(footprint "SerLog_CF3" (version 20221018) (generator pcbnew)
  (layer "F.Cu")
  (attr through_hole)
  (fp_text reference "REF**" (at 7.62 -33.02 unlocked) (layer "F.SilkS"))
  (fp_text value "SerLog_CF3" (at 0 -33.02 unlocked) (layer "F.Fab"))
  (fp_text user "x3.3v" (at 11.4 10.5 270 unlocked) (layer "B.SilkS"))
  (fp_text user "u5t" (at -0.0508 12.4692 270 unlocked) (layer "B.SilkS"))
  (fp_text user "mosi1" (at -0.0508 -10.4924 270 unlocked) (layer "B.SilkS"))
  (fp_text user "log3.3v" (at 11.38 -20.662 90 unlocked) (layer "B.SilkS"))
  (fp_text user "scl0" (at 0 -15.42 270 unlocked) (layer "B.SilkS"))
  (fp_text user "s0r" (at 2.5 25.5216 270 unlocked) (layer "B.SilkS"))
  (fp_text user "io69" (at 31.66 -13.3 90 unlocked) (layer "B.SilkS"))
  (fp_text user "io65" (at 26.58 -13.3 90 unlocked) (layer "B.SilkS"))
  (fp_text user "u3t" (at -0.0508 17.5492 270 unlocked) (layer "B.SilkS"))
  (fp_text user "rst\n" (at 2.5254 -27.7676 270 unlocked) (layer "B.SilkS"))
  (fp_text user "io79" (at 19.08 17.3 90 unlocked) (layer "B.SilkS"))
  (fp_text user "u2r" (at 2.4746 20.4416 270 unlocked) (layer "B.SilkS"))
  (fp_text user "io63" (at 24.04 -13.3 90 unlocked) (layer "B.SilkS"))
  (fp_text user "io83" (at 24.16 17.3 90 unlocked) (layer "B.SilkS"))
  (fp_text user "cs3" (at 0.0508 -2.5676 270 unlocked) (layer "B.SilkS"))
  (fp_text user "3.6v" (at 0 -28.1708 270 unlocked) (layer "B.SilkS"))
  (fp_text user "cantx" (at 16.42 -12.792 90 unlocked) (layer "B.SilkS"))
  (fp_text user "io28\n" (at 2.5 3 270 unlocked) (layer "B.SilkS"))
  (fp_text user "io78" (at 2.4746 28.0616 270 unlocked) (layer "B.SilkS"))
  (fp_text user "sck1" (at 2.5 -12.5784 270 unlocked) (layer "B.SilkS"))
  (fp_text user "s0t" (at -0.0508 25.22 270 unlocked) (layer "B.SilkS"))
  (fp_text user "io82" (at 2.5 30.5 270 unlocked) (layer "B.SilkS"))
  (fp_text user "s1r" (at 2.5 22.9308 270 unlocked) (layer "B.SilkS"))
  (fp_text user "vin5" (at 8.84 -19.9 270 unlocked) (layer "B.SilkS"))
  (fp_text user "io75" (at 14 17.3 90 unlocked) (layer "B.SilkS"))
  (fp_text user "Vrtc" (at 0 -20.6524 270 unlocked) (layer "B.SilkS"))
  (fp_text user "io67" (at 29.12 -13.3 90 unlocked) (layer "B.SilkS"))
  (fp_text user "Vin" (at 2.4746 -30.4092 270 unlocked) (layer "B.SilkS"))
  (fp_text user "miso2" (at 2.5254 -4.9 270 unlocked) (layer "B.SilkS"))
  (fp_text user "u3r" (at 2.5762 17.9524 270 unlocked) (layer "B.SilkS"))
  (fp_text user "io85" (at 26.7 17.3 90 unlocked) (layer "B.SilkS"))
  (fp_text user "sck3" (at 2.5762 -2.3 270 unlocked) (layer "B.SilkS"))
  (fp_text user "u2t" (at 0.0508 20.14 270 unlocked) (layer "B.SilkS"))
  (fp_text user "gnd" (at 8.8 -13.3 270 unlocked) (layer "B.SilkS"))
  (fp_text user "io62" (at 21.54 -19.9 270 unlocked) (layer "B.SilkS"))
  (fp_text user "gnd" (at 8.92 17.046 270 unlocked) (layer "B.SilkS"))
  (fp_text user "io66" (at 26.62 -19.9 270 unlocked) (layer "B.SilkS"))
  (fp_text user "cs2" (at 0 -7.7492 270 unlocked) (layer "B.SilkS"))
  (fp_text user "vin5x" (at 9 10.6 270 unlocked) (layer "B.SilkS"))
  (fp_text user "sda0" (at 2.5762 -15.1184 270 unlocked) (layer "B.SilkS"))
  (fp_text user "3.3v" (at 0.0508 -25.58 270 unlocked) (layer "B.SilkS"))
  (fp_text user "io86" (at 26.6 10.8 270 unlocked) (layer "B.SilkS"))
  (fp_text user "shdn" (at 2.5762 -25.2276 270 unlocked) (layer "B.SilkS"))
  (fp_text user "Bat" (at 0 -23.0908 270 unlocked) (layer "B.SilkS"))
  (fp_text user "3.6v" (at 11.34 -13.3 270 unlocked) (layer "B.SilkS"))
  (fp_text user "io27\n" (at -0.0508 2.6 270 unlocked) (layer "B.SilkS"))
  (fp_text user "io64" (at 24.08 -19.9 270 unlocked) (layer "B.SilkS"))
  (fp_text user "cs1" (at 0 -12.9308 270 unlocked) (layer "B.SilkS"))
  (fp_text user "u4r" (at 2.5 15.3616 270 unlocked) (layer "B.SilkS"))
  (fp_text user "io70" (at 31.7 -19.9 270 unlocked) (layer "B.SilkS"))
  (fp_text user "u7r" (at 2.4746 7.64 270 unlocked) (layer "B.SilkS"))
  (fp_text user "io84" (at 0 30.3 270 unlocked) (layer "B.SilkS"))
  (fp_text user "u7t" (at -0.0508 7.3384 270 unlocked) (layer "B.SilkS"))
  (fp_text user "miso3" (at 2.5762 0.3 270 unlocked) (layer "B.SilkS"))
  (fp_text user "io56" (at 13.92 -20.154 270 unlocked) (layer "B.SilkS"))
  (fp_text user "u5r" (at 2.5254 12.72 270 unlocked) (layer "B.SilkS"))
  (fp_text user "io77" (at 16.54 17.3 90 unlocked) (layer "B.SilkS"))
  (fp_text user "scl1" (at 0 -18.0108 270 unlocked) (layer "B.SilkS"))
  (fp_text user "gnd" (at 0.3048 -30.6346 270 unlocked) (layer "B.SilkS"))
  (fp_text user "3.6v" (at 11.46 17.3 270 unlocked) (layer "B.SilkS"))
  (fp_text user "io81" (at 21.62 17.3 90 unlocked) (layer "B.SilkS"))
  (fp_text user "miso1" (at 2.5762 -10 270 unlocked) (layer "B.SilkS"))
  (fp_text user "sda1" (at 2.5 -17.8616 270 unlocked) (layer "B.SilkS"))
  (fp_text user "mosi3" (at -0.0508 -0.18 270 unlocked) (layer "B.SilkS"))
  (fp_text user "u6r" (at 2.5 10.3324 270 unlocked) (layer "B.SilkS"))
  (fp_text user "u4t" (at -0.0508 15.0092 270 unlocked) (layer "B.SilkS"))
  (fp_text user "wake" (at 2.5254 -22.84 270 unlocked) (layer "B.SilkS"))
  (fp_text user "s1t" (at -0.0508 22.68 270 unlocked) (layer "B.SilkS"))
  (fp_text user "cnt1" (at 0 5 270 unlocked) (layer "B.SilkS"))
  (fp_text user "canrx" (at 16.46 -20.154 270 unlocked) (layer "B.SilkS"))
  (fp_text user "sck2" (at 2.5 -7.4476 270 unlocked) (layer "B.SilkS"))
  (fp_text user "mosi2" (at 0 -5.2092 270 unlocked) (layer "B.SilkS"))
  (fp_text user "io68" (at 29.16 -19.9 270 unlocked) (layer "B.SilkS"))
  (fp_text user "io80" (at 0 27.8616 270 unlocked) (layer "B.SilkS"))
  (fp_text user "cnr1" (at 2.5254 5.4556 270 unlocked) (layer "B.SilkS"))
  (fp_text user "u6t" (at -0.0508 9.9292 270 unlocked) (layer "B.SilkS"))
  (fp_text user "sck1" (at 2.5762 -12.6292 -270 unlocked) (layer "F.SilkS"))
  (fp_text user "u3r" (at 2.6016 17.9524 -270 unlocked) (layer "F.SilkS"))
  (fp_text user "u2r" (at 2.5762 20.5432 -270 unlocked) (layer "F.SilkS"))
  (fp_text user "u6t" (at -0.0508 9.98 -270 unlocked) (layer "F.SilkS"))
  (fp_text user "cs1" (at -0.0508 -12.88 -270 unlocked) (layer "F.SilkS"))
  (fp_text user "miso2" (at 2.5 -4.9076 -270 unlocked) (layer "F.SilkS"))
  (fp_text user "cnr1" (at 2.373 5.2016 -270 unlocked) (layer "F.SilkS"))
  (fp_text user "u6r" (at 2.5762 10.434 -270 unlocked) (layer "F.SilkS"))
  (fp_text user "s1t" (at -0.0254 22.7308 -270 unlocked) (layer "F.SilkS"))
  (fp_text user "shdn" (at 2.5508 -25.2276 -270 unlocked) (layer "F.SilkS"))
  (fp_text user "s0t" (at 0.0508 25.3216 -270 unlocked) (layer "F.SilkS"))
  (fp_text user "u5t" (at 2.6016 12.8216 -270 unlocked) (layer "F.SilkS"))
  (fp_text user "rst\n" (at 2.5508 -27.7168 90 unlocked) (layer "F.SilkS"))
  (fp_text user "u4t" (at 0 15.1616 -270 unlocked) (layer "F.SilkS"))
  (fp_text user "io28\n" (at 2.5762 3 -270 unlocked) (layer "F.SilkS"))
  (fp_text user "s1r" (at 2.5508 22.88 -270 unlocked) (layer "F.SilkS"))
  (fp_text user "Vrtc" (at 0 -20.5 -270 unlocked) (layer "F.SilkS"))
  (fp_text user "io78" (at 2.6016 28.0616 -270 unlocked) (layer "F.SilkS"))
  (fp_text user "cnt1" (at 0 4.9508 -270 unlocked) (layer "F.SilkS"))
  (fp_text user "mosi3" (at -0.0508 -0.0784 -270 unlocked) (layer "F.SilkS"))
  (fp_text user "sda1" (at 2.5 -17.6584 -270 unlocked) (layer "F.SilkS"))
  (fp_text user "u3t" (at 0 17.7016 -270 unlocked) (layer "F.SilkS"))
  (fp_text user "io27\n" (at 0.0508 2.5 -270 unlocked) (layer "F.SilkS"))
  (fp_text user "s0r" (at 2.5508 25.4708 -270 unlocked) (layer "F.SilkS"))
  (fp_text user "u2t" (at 0.0508 20.2416 -270 unlocked) (layer "F.SilkS"))
  (fp_text user "sck2" (at 2.5762 -7.3714 -270 unlocked) (layer "F.SilkS"))
  (fp_text user "3.6v" (at 0 -28.0692 -270 unlocked) (layer "F.SilkS"))
  (fp_text user "io80" (at 0 27.8616 -270 unlocked) (layer "F.SilkS"))
  (fp_text user "miso3" (at 2.5 0.3 -270 unlocked) (layer "F.SilkS"))
  (fp_text user "u4r" (at 2.6016 15.514 -270 unlocked) (layer "F.SilkS"))
  (fp_text user "3.3v" (at 0 -25.5292 -270 unlocked) (layer "F.SilkS"))
  (fp_text user "u7r" (at 0 7.4908 -270 unlocked) (layer "F.SilkS"))
  (fp_text user "wake" (at 2.5508 -22.7384 -270 unlocked) (layer "F.SilkS"))
  (fp_text user "io82" (at 2.5762 30.3476 -270 unlocked) (layer "F.SilkS"))
  (fp_text user "Bat" (at 0 -22.9892 -270 unlocked) (layer "F.SilkS"))
  (fp_text user "Vin" (at 2.5762 -30.3584 90 unlocked) (layer "F.SilkS"))
  (fp_text user "scl0" (at 0 -15.4708 -270 unlocked) (layer "F.SilkS"))
  (fp_text user "cs2" (at -0.0508 -7.6984 -270 unlocked) (layer "F.SilkS"))
  (fp_text user "io84" (at 0 30.3 -270 unlocked) (layer "F.SilkS"))
  (fp_text user "mosi1" (at -0.0508 -10.2384 -270 unlocked) (layer "F.SilkS"))
  (fp_text user "miso1" (at 2.4492 -10 -270 unlocked) (layer "F.SilkS"))
  (fp_text user "sda0" (at 2.5508 -14.966 -270 unlocked) (layer "F.SilkS"))
  (fp_text user "scl1" (at 0 -17.96 -270 unlocked) (layer "F.SilkS"))
  (fp_text user "mosi2" (at -0.0508 -5.1584 -270 unlocked) (layer "F.SilkS"))
  (fp_text user "cs3" (at 0 -2.72 -270 unlocked) (layer "F.SilkS"))
  (fp_text user "u5r" (at 0 12.52 -270 unlocked) (layer "F.SilkS"))
  (fp_text user "u7t" (at 2.5762 7.7416 -270 unlocked) (layer "F.SilkS"))
  (fp_text user "gnd" (at 0.381 -29.771 90 unlocked) (layer "F.SilkS"))
  (fp_text user "sck3" (at 2.5762 -2.3676 -270 unlocked) (layer "F.SilkS"))
  (fp_text user "${REFERENCE}" (at 0.02 0.03 90) (layer "F.Fab"))
  (pad "1" thru_hole rect (at -1.25 -30.45) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask"))
  (pad "2" thru_hole oval (at 1.29 -30.45) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask"))
  (pad "3" thru_hole oval (at -1.25 -27.91) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask"))
  (pad "4" thru_hole oval (at 1.29 -27.91) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask"))
  (pad "5" thru_hole oval (at -1.25 -25.37) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask"))
  (pad "6" thru_hole oval (at 1.29 -25.37) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask"))
  (pad "7" thru_hole oval (at -1.25 -22.83) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask"))
  (pad "8" thru_hole oval (at 1.29 -22.83) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask"))
  (pad "9" thru_hole oval (at -1.25 -20.29) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask"))
  (pad "10" thru_hole oval (at 1.29 -20.29) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask"))
  (pad "11" thru_hole oval (at -1.25 -17.75) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask"))
  (pad "12" thru_hole oval (at 1.29 -17.75) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask"))
  (pad "13" thru_hole oval (at -1.25 -15.21) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask"))
  (pad "14" thru_hole oval (at 1.29 -15.21) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask"))
  (pad "15" thru_hole oval (at -1.25 -12.67) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask"))
  (pad "16" thru_hole oval (at 1.29 -12.67) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask"))
  (pad "17" thru_hole oval (at -1.25 -10.13) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask"))
  (pad "18" thru_hole oval (at 1.29 -10.13) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask"))
  (pad "19" thru_hole oval (at -1.25 -7.59) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask"))
  (pad "20" thru_hole oval (at 1.29 -7.59) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask"))
  (pad "21" thru_hole oval (at -1.25 -5.05) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask"))
  (pad "22" thru_hole oval (at 1.29 -5.05) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask"))
  (pad "23" thru_hole oval (at -1.25 -2.51) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask"))
  (pad "24" thru_hole oval (at 1.29 -2.51) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask"))
  (pad "25" thru_hole oval (at -1.25 0.03) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask"))
  (pad "26" thru_hole oval (at 1.29 0.03) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask"))
  (pad "27" thru_hole oval (at -1.25 2.57) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask"))
  (pad "28" thru_hole oval (at 1.29 2.57) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask"))
  (pad "29" thru_hole oval (at -1.25 5.11) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask"))
  (pad "30" thru_hole oval (at 1.29 5.11) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask"))
  (pad "31" thru_hole oval (at -1.25 7.65) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask"))
  (pad "32" thru_hole oval (at 1.29 7.65) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask"))
  (pad "33" thru_hole oval (at -1.25 10.19) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask"))
  (pad "34" thru_hole oval (at 1.29 10.19) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask"))
  (pad "35" thru_hole oval (at -1.25 12.73) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask"))
  (pad "36" thru_hole oval (at 1.29 12.73) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask"))
  (pad "37" thru_hole oval (at -1.25 15.27) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask"))
  (pad "38" thru_hole oval (at 1.29 15.27) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask"))
  (pad "39" thru_hole oval (at -1.25 17.81) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask"))
  (pad "40" thru_hole oval (at 1.29 17.81) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask"))
  (pad "41" thru_hole oval (at -1.25 20.35) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask"))
  (pad "42" thru_hole oval (at 1.29 20.35) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask"))
  (pad "43" thru_hole oval (at -1.25 22.89) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask"))
  (pad "44" thru_hole oval (at 1.29 22.89) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask"))
  (pad "45" thru_hole oval (at -1.25 25.43) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask"))
  (pad "46" thru_hole oval (at 1.29 25.43) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask"))
  (pad "47" thru_hole oval (at -1.25 27.97) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask"))
  (pad "48" thru_hole oval (at 1.29 27.97) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask"))
  (pad "49" thru_hole oval (at -1.25 30.51) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask"))
  (pad "50" thru_hole oval (at 1.29 30.51) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask"))
  (pad "51" thru_hole rect (at 8.801 -15.262 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask"))
  (pad "52" thru_hole oval (at 8.801 -17.802 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask"))
  (pad "53" thru_hole oval (at 11.341 -15.262 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask"))
  (pad "54" thru_hole oval (at 11.341 -17.802 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask"))
  (pad "55" thru_hole oval (at 13.881 -15.262 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask"))
  (pad "56" thru_hole oval (at 13.881 -17.802 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask"))
  (pad "57" thru_hole oval (at 16.421 -15.262 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask"))
  (pad "58" thru_hole oval (at 16.421 -17.802 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask"))
  (pad "59" thru_hole oval (at 18.961 -15.262 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask"))
  (pad "60" thru_hole oval (at 18.961 -17.802 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask"))
  (pad "61" thru_hole oval (at 21.501 -15.262 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask"))
  (pad "62" thru_hole oval (at 21.501 -17.802 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask"))
  (pad "63" thru_hole oval (at 24.041 -15.262 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask"))
  (pad "64" thru_hole oval (at 24.041 -17.802 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask"))
  (pad "65" thru_hole oval (at 26.581 -15.262 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask"))
  (pad "66" thru_hole oval (at 26.581 -17.802 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask"))
  (pad "67" thru_hole oval (at 29.121 -15.262 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask"))
  (pad "68" thru_hole oval (at 29.121 -17.802 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask"))
  (pad "69" thru_hole oval (at 31.661 -15.262 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask"))
  (pad "70" thru_hole oval (at 31.661 -17.802 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask"))
  (pad "71" thru_hole rect (at 8.92 15.22 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask"))
  (pad "72" thru_hole oval (at 8.92 12.68 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask"))
  (pad "73" thru_hole oval (at 11.46 15.22 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask"))
  (pad "74" thru_hole oval (at 11.46 12.68 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask"))
  (pad "75" thru_hole oval (at 14 15.22 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask"))
  (pad "76" thru_hole oval (at 14 12.68 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask"))
  (pad "77" thru_hole oval (at 16.54 15.22 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask"))
  (pad "78" thru_hole oval (at 16.54 12.68 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask"))
  (pad "79" thru_hole oval (at 19.08 15.22 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask"))
  (pad "80" thru_hole oval (at 19.08 12.68 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask"))
  (pad "81" thru_hole oval (at 21.62 15.22 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask"))
  (pad "82" thru_hole oval (at 21.62 12.68 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask"))
  (pad "83" thru_hole oval (at 24.16 15.22 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask"))
  (pad "84" thru_hole oval (at 24.16 12.68 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask"))
  (pad "85" thru_hole oval (at 26.7 15.22 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask"))
  (pad "86" thru_hole oval (at 26.7 12.68 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask"))
  (pad "87" thru_hole oval (at 29.24 15.22 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask"))
  (pad "88" thru_hole oval (at 29.24 12.68 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask"))
  (pad "89" thru_hole oval (at 31.78 15.22 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask"))
  (pad "90" thru_hole oval (at 31.78 12.68 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask"))
)
