(footprint "SerLog_CF3_module" (version 20221018) (generator pcbnew)
  (layer "F.Cu")
  (fp_text reference "REF**" (at -1.29 -34.32 unlocked) (layer "F.SilkS"))
  (fp_text value "SerLog_CF3_module" (at 8.87 -34.32 unlocked) (layer "F.Fab"))
  (fp_text user "u5r" (at 2.5254 12.62 270 unlocked) (layer "B.SilkS"))
  (fp_text user "mosi1" (at -0.0508 -10.3924 270 unlocked) (layer "B.SilkS"))
  (fp_text user "sda0" (at 2.5762 -15.2184 270 unlocked) (layer "B.SilkS"))
  (fp_text user "sck3" (at 2.5762 -2.3152 270 unlocked) (layer "B.SilkS"))
  (fp_text user "u2r" (at 2.4746 20.3416 270 unlocked) (layer "B.SilkS"))
  (fp_text user "io77" (at 16.51 19.05 90 unlocked) (layer "B.SilkS"))
  (fp_text user "io86" (at 26.67 8.89 270 unlocked) (layer "B.SilkS"))
  (fp_text user "miso3" (at 2.5762 0.2756 270 unlocked) (layer "B.SilkS"))
  (fp_text user "mosi2" (at 0 -5.1092 270 unlocked) (layer "B.SilkS"))
  (fp_text user "cantx" (at 16.51 -10.922 90 unlocked) (layer "B.SilkS"))
  (fp_text user "cs2" (at 0 -7.6492 270 unlocked) (layer "B.SilkS"))
  (fp_text user "sck2" (at 2.5 -7.5476 270 unlocked) (layer "B.SilkS"))
  (fp_text user "u7t" (at -0.0508 7.4384 270 unlocked) (layer "B.SilkS"))
  (fp_text user "cs3" (at 0.0508 -2.4676 270 unlocked) (layer "B.SilkS"))
  (fp_text user "s0t" (at -0.0508 25.32 270 unlocked) (layer "B.SilkS"))
  (fp_text user "io70" (at 31.75 -21.59 270 unlocked) (layer "B.SilkS"))
  (fp_text user "u2t" (at 0.0508 20.24 270 unlocked) (layer "B.SilkS"))
  (fp_text user "io69" (at 31.75 -11.43 90 unlocked) (layer "B.SilkS"))
  (fp_text user "io65" (at 26.67 -11.43 90 unlocked) (layer "B.SilkS"))
  (fp_text user "u6r" (at 2.5 10.2324 270 unlocked) (layer "B.SilkS"))
  (fp_text user "u6t" (at -0.0508 10.0292 270 unlocked) (layer "B.SilkS"))
  (fp_text user "log3.3v" (at 11.43 -22.352 90 unlocked) (layer "B.SilkS"))
  (fp_text user "scl0" (at 0 -15.32 270 unlocked) (layer "B.SilkS"))
  (fp_text user "Bat" (at 0 -22.9908 270 unlocked) (layer "B.SilkS"))
  (fp_text user "io80" (at 0 27.9616 270 unlocked) (layer "B.SilkS"))
  (fp_text user "io63" (at 24.13 -11.43 90 unlocked) (layer "B.SilkS"))
  (fp_text user "s0r" (at 2.5 25.4216 270 unlocked) (layer "B.SilkS"))
  (fp_text user "io28\n" (at 2.5 2.6632 270 unlocked) (layer "B.SilkS"))
  (fp_text user "cs1" (at 0 -12.8308 270 unlocked) (layer "B.SilkS"))
  (fp_text user "3.6v" (at 0 -28.0708 270 unlocked) (layer "B.SilkS"))
  (fp_text user "u4r" (at 2.5 15.2616 270 unlocked) (layer "B.SilkS"))
  (fp_text user "io82" (at 2.5 30.4 270 unlocked) (layer "B.SilkS"))
  (fp_text user "gnd" (at 8.89 -11.43 270 unlocked) (layer "B.SilkS"))
  (fp_text user "io68" (at 29.21 -21.59 270 unlocked) (layer "B.SilkS"))
  (fp_text user "x3.3v" (at 11.43 8.636 270 unlocked) (layer "B.SilkS"))
  (fp_text user "io56" (at 13.97 -21.844 270 unlocked) (layer "B.SilkS"))
  (fp_text user "s1t" (at -0.0508 22.78 270 unlocked) (layer "B.SilkS"))
  (fp_text user "scl1" (at 0 -17.9108 270 unlocked) (layer "B.SilkS"))
  (fp_text user "io83" (at 24.13 19.05 90 unlocked) (layer "B.SilkS"))
  (fp_text user "io79" (at 19.05 19.05 90 unlocked) (layer "B.SilkS"))
  (fp_text user "rst\n" (at 2.5254 -27.8676 270 unlocked) (layer "B.SilkS"))
  (fp_text user "Vin" (at 2.4746 -30.5092 270 unlocked) (layer "B.SilkS"))
  (fp_text user "3.6v" (at 11.43 -11.43 270 unlocked) (layer "B.SilkS"))
  (fp_text user "u3r" (at 2.5762 17.8524 270 unlocked) (layer "B.SilkS"))
  (fp_text user "cnt1" (at 0 4.9492 270 unlocked) (layer "B.SilkS"))
  (fp_text user "io84" (at 0 30.4 270 unlocked) (layer "B.SilkS"))
  (fp_text user "sda1" (at 2.5 -17.9616 270 unlocked) (layer "B.SilkS"))
  (fp_text user "u3t" (at -0.0508 17.6492 270 unlocked) (layer "B.SilkS"))
  (fp_text user "io78" (at 2.4746 27.9616 270 unlocked) (layer "B.SilkS"))
  (fp_text user "wake" (at 2.5254 -22.94 270 unlocked) (layer "B.SilkS"))
  (fp_text user "cnr1" (at 2.5254 5.3556 270 unlocked) (layer "B.SilkS"))
  (fp_text user "io81" (at 21.59 19.05 90 unlocked) (layer "B.SilkS"))
  (fp_text user "canrx" (at 16.51 -21.844 270 unlocked) (layer "B.SilkS"))
  (fp_text user "u5t" (at -0.0508 12.5692 270 unlocked) (layer "B.SilkS"))
  (fp_text user "Vrtc" (at 0 -20.5524 270 unlocked) (layer "B.SilkS"))
  (fp_text user "io66" (at 26.67 -21.59 270 unlocked) (layer "B.SilkS"))
  (fp_text user "3.6v" (at 11.43 19.05 270 unlocked) (layer "B.SilkS"))
  (fp_text user "io64" (at 24.13 -21.59 270 unlocked) (layer "B.SilkS"))
  (fp_text user "io67" (at 29.21 -11.43 90 unlocked) (layer "B.SilkS"))
  (fp_text user "gnd" (at 0.3048 -30.5346 270 unlocked) (layer "B.SilkS"))
  (fp_text user "mosi3" (at -0.0508 -0.08 270 unlocked) (layer "B.SilkS"))
  (fp_text user "miso1" (at 2.5762 -9.8844 270 unlocked) (layer "B.SilkS"))
  (fp_text user "3.3v" (at 0.0508 -25.48 270 unlocked) (layer "B.SilkS"))
  (fp_text user "io27\n" (at -0.0508 2.46 270 unlocked) (layer "B.SilkS"))
  (fp_text user "io62" (at 21.59 -21.59 270 unlocked) (layer "B.SilkS"))
  (fp_text user "vin5x" (at 8.89 8.636 270 unlocked) (layer "B.SilkS"))
  (fp_text user "s1r" (at 2.5 22.8308 270 unlocked) (layer "B.SilkS"))
  (fp_text user "vin5" (at 8.89 -21.59 270 unlocked) (layer "B.SilkS"))
  (fp_text user "miso2" (at 2.5254 -5.1092 270 unlocked) (layer "B.SilkS"))
  (fp_text user "u7r" (at 2.4746 7.54 270 unlocked) (layer "B.SilkS"))
  (fp_text user "u4t" (at -0.0508 15.1092 270 unlocked) (layer "B.SilkS"))
  (fp_text user "io75" (at 13.97 19.05 90 unlocked) (layer "B.SilkS"))
  (fp_text user "sck1" (at 2.5 -12.6784 270 unlocked) (layer "B.SilkS"))
  (fp_text user "gnd" (at 8.89 18.796 270 unlocked) (layer "B.SilkS"))
  (fp_text user "io85" (at 26.67 19.05 90 unlocked) (layer "B.SilkS"))
  (fp_text user "shdn" (at 2.5762 -25.3276 270 unlocked) (layer "B.SilkS"))
  (fp_text user "io80" (at 0 27.9616 -270 unlocked) (layer "F.SilkS"))
  (fp_text user "Bat" (at 0 -22.8892 -270 unlocked) (layer "F.SilkS"))
  (fp_text user "wake" (at 2.5508 -22.8384 -270 unlocked) (layer "F.SilkS"))
  (fp_text user "rst\n" (at 2.5508 -27.8168 90 unlocked) (layer "F.SilkS"))
  (fp_text user "u2t" (at 0.0508 20.3416 -270 unlocked) (layer "F.SilkS"))
  (fp_text user "cs3" (at 0 -2.62 -270 unlocked) (layer "F.SilkS"))
  (fp_text user "u5r" (at 0 12.62 -270 unlocked) (layer "F.SilkS"))
  (fp_text user "io27\n" (at 0.0508 2.4092 -270 unlocked) (layer "F.SilkS"))
  (fp_text user "cnr1" (at 2.373 5.1016 -270 unlocked) (layer "F.SilkS"))
  (fp_text user "u3r" (at 2.6016 17.8524 -270 unlocked) (layer "F.SilkS"))
  (fp_text user "u5t" (at 2.6016 12.7216 -270 unlocked) (layer "F.SilkS"))
  (fp_text user "gnd" (at 0.381 -29.671 90 unlocked) (layer "F.SilkS"))
  (fp_text user "io84" (at 0 30.4 -270 unlocked) (layer "F.SilkS"))
  (fp_text user "u6r" (at 2.5762 10.334 -270 unlocked) (layer "F.SilkS"))
  (fp_text user "mosi3" (at -0.0508 0.0216 -270 unlocked) (layer "F.SilkS"))
  (fp_text user "s0r" (at 2.5508 25.3708 -270 unlocked) (layer "F.SilkS"))
  (fp_text user "s0t" (at 0.0508 25.4216 -270 unlocked) (layer "F.SilkS"))
  (fp_text user "miso3" (at 2.5 0.1232 -270 unlocked) (layer "F.SilkS"))
  (fp_text user "mosi1" (at -0.0508 -10.1384 -270 unlocked) (layer "F.SilkS"))
  (fp_text user "io82" (at 2.5762 30.2476 -270 unlocked) (layer "F.SilkS"))
  (fp_text user "s1r" (at 2.5508 22.78 -270 unlocked) (layer "F.SilkS"))
  (fp_text user "Vin" (at 2.5762 -30.4584 90 unlocked) (layer "F.SilkS"))
  (fp_text user "sda0" (at 2.5508 -15.066 -270 unlocked) (layer "F.SilkS"))
  (fp_text user "sda1" (at 2.5762 -17.7584 -270 unlocked) (layer "F.SilkS"))
  (fp_text user "u7r" (at 0 7.5908 -270 unlocked) (layer "F.SilkS"))
  (fp_text user "s1t" (at -0.0254 22.8308 -270 unlocked) (layer "F.SilkS"))
  (fp_text user "3.3v" (at 0 -25.4292 -270 unlocked) (layer "F.SilkS"))
  (fp_text user "miso1" (at 2.4492 -9.9352 -270 unlocked) (layer "F.SilkS"))
  (fp_text user "u3t" (at 0 17.8016 -270 unlocked) (layer "F.SilkS"))
  (fp_text user "sck1" (at 2.5762 -12.7292 -270 unlocked) (layer "F.SilkS"))
  (fp_text user "shdn" (at 2.5508 -25.3276 -270 unlocked) (layer "F.SilkS"))
  (fp_text user "u4r" (at 2.6016 15.414 -270 unlocked) (layer "F.SilkS"))
  (fp_text user "Vrtc" (at 0 -20.4 -270 unlocked) (layer "F.SilkS"))
  (fp_text user "u7t" (at 2.5762 7.6416 -270 unlocked) (layer "F.SilkS"))
  (fp_text user "scl0" (at 0 -15.3708 -270 unlocked) (layer "F.SilkS"))
  (fp_text user "miso2" (at 2.5 -5.0076 -270 unlocked) (layer "F.SilkS"))
  (fp_text user "cs1" (at -0.0508 -12.78 -270 unlocked) (layer "F.SilkS"))
  (fp_text user "u4t" (at 0 15.2616 -270 unlocked) (layer "F.SilkS"))
  (fp_text user "cs2" (at -0.0508 -7.5984 -270 unlocked) (layer "F.SilkS"))
  (fp_text user "mosi2" (at -0.0508 -5.0584 -270 unlocked) (layer "F.SilkS"))
  (fp_text user "io78" (at 2.6016 27.9616 -270 unlocked) (layer "F.SilkS"))
  (fp_text user "u6t" (at -0.0508 10.08 -270 unlocked) (layer "F.SilkS"))
  (fp_text user "u2r" (at 2.5762 20.4432 -270 unlocked) (layer "F.SilkS"))
  (fp_text user "3.6v" (at 0 -27.9692 -270 unlocked) (layer "F.SilkS"))
  (fp_text user "sck3" (at 2.5762 -2.4676 -270 unlocked) (layer "F.SilkS"))
  (fp_text user "sck2" (at 2.5762 -7.4714 -270 unlocked) (layer "F.SilkS"))
  (fp_text user "cnt1" (at 0 5.0508 -270 unlocked) (layer "F.SilkS"))
  (fp_text user "io28\n" (at 2.5762 2.6124 -270 unlocked) (layer "F.SilkS"))
  (fp_text user "scl1" (at 0 -17.86 -270 unlocked) (layer "F.SilkS"))
  (fp_text user "${REFERENCE}" (at -0.02 1.24 90 unlocked) (layer "F.Fab"))
  (pad "1" thru_hole rect (at -1.27 -30.48) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask"))
  (pad "2" thru_hole oval (at 1.27 -30.48) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask"))
  (pad "3" thru_hole oval (at -1.27 -27.94) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask"))
  (pad "4" thru_hole oval (at 1.27 -27.94) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask"))
  (pad "5" thru_hole oval (at -1.27 -25.4) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask"))
  (pad "6" thru_hole oval (at 1.27 -25.4) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask"))
  (pad "7" thru_hole oval (at -1.27 -22.86) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask"))
  (pad "8" thru_hole oval (at 1.27 -22.86) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask"))
  (pad "9" thru_hole oval (at -1.27 -20.32) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask"))
  (pad "10" thru_hole oval (at 1.27 -20.32) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask"))
  (pad "11" thru_hole oval (at -1.27 -17.78) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask"))
  (pad "12" thru_hole oval (at 1.27 -17.78) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask"))
  (pad "13" thru_hole oval (at -1.27 -15.24) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask"))
  (pad "14" thru_hole oval (at 1.27 -15.24) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask"))
  (pad "15" thru_hole oval (at -1.27 -12.7) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask"))
  (pad "16" thru_hole oval (at 1.27 -12.7) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask"))
  (pad "17" thru_hole oval (at -1.27 -10.16) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask"))
  (pad "18" thru_hole oval (at 1.27 -10.16) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask"))
  (pad "19" thru_hole oval (at -1.27 -7.62) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask"))
  (pad "20" thru_hole oval (at 1.27 -7.62) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask"))
  (pad "21" thru_hole oval (at -1.27 -5.08) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask"))
  (pad "22" thru_hole oval (at 1.27 -5.08) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask"))
  (pad "23" thru_hole oval (at -1.27 -2.54) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask"))
  (pad "24" thru_hole oval (at 1.27 -2.54) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask"))
  (pad "25" thru_hole oval (at -1.27 0) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask"))
  (pad "26" thru_hole oval (at 1.27 0) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask"))
  (pad "27" thru_hole oval (at -1.27 2.54) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask"))
  (pad "28" thru_hole oval (at 1.27 2.54) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask"))
  (pad "29" thru_hole oval (at -1.27 5.08) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask"))
  (pad "30" thru_hole oval (at 1.27 5.08) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask"))
  (pad "31" thru_hole oval (at -1.27 7.62) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask"))
  (pad "32" thru_hole oval (at 1.27 7.62) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask"))
  (pad "33" thru_hole oval (at -1.27 10.16) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask"))
  (pad "34" thru_hole oval (at 1.27 10.16) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask"))
  (pad "35" thru_hole oval (at -1.27 12.7) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask"))
  (pad "36" thru_hole oval (at 1.27 12.7) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask"))
  (pad "37" thru_hole oval (at -1.27 15.24) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask"))
  (pad "38" thru_hole oval (at 1.27 15.24) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask"))
  (pad "39" thru_hole oval (at -1.27 17.78) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask"))
  (pad "40" thru_hole oval (at 1.27 17.78) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask"))
  (pad "41" thru_hole oval (at -1.27 20.32) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask"))
  (pad "42" thru_hole oval (at 1.27 20.32) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask"))
  (pad "43" thru_hole oval (at -1.27 22.86) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask"))
  (pad "44" thru_hole oval (at 1.27 22.86) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask"))
  (pad "45" thru_hole oval (at -1.27 25.4) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask"))
  (pad "46" thru_hole oval (at 1.27 25.4) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask"))
  (pad "47" thru_hole oval (at -1.27 27.94) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask"))
  (pad "48" thru_hole oval (at 1.27 27.94) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask"))
  (pad "49" thru_hole oval (at -1.27 30.48) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask"))
  (pad "50" thru_hole oval (at 1.27 30.48) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask"))
  (pad "51" smd rect (at 8.89 -13.9984 270) (size 3 1) (layers "B.Cu" "B.Paste" "B.Mask"))
  (pad "52" smd rect (at 8.89 -19.0384 270) (size 3 1) (layers "B.Cu" "B.Paste" "B.Mask"))
  (pad "53" smd rect (at 11.43 -13.9984 270) (size 3 1) (layers "B.Cu" "B.Paste" "B.Mask"))
  (pad "54" smd rect (at 11.43 -19.0384 270) (size 3 1) (layers "B.Cu" "B.Paste" "B.Mask"))
  (pad "55" smd rect (at 13.97 -13.9984 270) (size 3 1) (layers "B.Cu" "B.Paste" "B.Mask"))
  (pad "56" smd rect (at 13.97 -19.0384 270) (size 3 1) (layers "B.Cu" "B.Paste" "B.Mask"))
  (pad "57" smd rect (at 16.51 -13.9984 270) (size 3 1) (layers "B.Cu" "B.Paste" "B.Mask"))
  (pad "58" smd rect (at 16.51 -19.0384 270) (size 3 1) (layers "B.Cu" "B.Paste" "B.Mask"))
  (pad "59" smd rect (at 19.05 -13.9984 270) (size 3 1) (layers "B.Cu" "B.Paste" "B.Mask"))
  (pad "60" smd rect (at 19.05 -19.0384 270) (size 3 1) (layers "B.Cu" "B.Paste" "B.Mask"))
  (pad "61" smd rect (at 21.59 -13.9984 270) (size 3 1) (layers "B.Cu" "B.Paste" "B.Mask"))
  (pad "62" smd rect (at 21.59 -19.0384 270) (size 3 1) (layers "B.Cu" "B.Paste" "B.Mask"))
  (pad "63" smd rect (at 24.13 -13.9984 270) (size 3 1) (layers "B.Cu" "B.Paste" "B.Mask"))
  (pad "64" smd rect (at 24.13 -19.0384 270) (size 3 1) (layers "B.Cu" "B.Paste" "B.Mask"))
  (pad "65" smd rect (at 26.67 -13.9984 270) (size 3 1) (layers "B.Cu" "B.Paste" "B.Mask"))
  (pad "66" smd rect (at 26.67 -19.0384 270) (size 3 1) (layers "B.Cu" "B.Paste" "B.Mask"))
  (pad "67" smd rect (at 29.21 -13.9984 270) (size 3 1) (layers "B.Cu" "B.Paste" "B.Mask"))
  (pad "68" smd rect (at 29.21 -19.0384 270) (size 3 1) (layers "B.Cu" "B.Paste" "B.Mask"))
  (pad "69" smd rect (at 31.75 -13.9984 270) (size 3 1) (layers "B.Cu" "B.Paste" "B.Mask"))
  (pad "70" smd rect (at 31.75 -19.0384 270) (size 3 1) (layers "B.Cu" "B.Paste" "B.Mask"))
  (pad "71" smd rect (at 8.89 16.507 270) (size 3 1) (layers "B.Cu" "B.Paste" "B.Mask"))
  (pad "72" smd rect (at 8.89 11.467 270) (size 3 1) (layers "B.Cu" "B.Paste" "B.Mask"))
  (pad "73" smd rect (at 11.43 16.507 270) (size 3 1) (layers "B.Cu" "B.Paste" "B.Mask"))
  (pad "74" smd rect (at 11.43 11.467 270) (size 3 1) (layers "B.Cu" "B.Paste" "B.Mask"))
  (pad "75" smd rect (at 13.97 16.507 270) (size 3 1) (layers "B.Cu" "B.Paste" "B.Mask"))
  (pad "76" smd rect (at 13.97 11.467 270) (size 3 1) (layers "B.Cu" "B.Paste" "B.Mask"))
  (pad "77" smd rect (at 16.51 16.507 270) (size 3 1) (layers "B.Cu" "B.Paste" "B.Mask"))
  (pad "78" smd rect (at 16.51 11.467 270) (size 3 1) (layers "B.Cu" "B.Paste" "B.Mask"))
  (pad "79" smd rect (at 19.05 16.507 270) (size 3 1) (layers "B.Cu" "B.Paste" "B.Mask"))
  (pad "80" smd rect (at 19.05 11.467 270) (size 3 1) (layers "B.Cu" "B.Paste" "B.Mask"))
  (pad "81" smd rect (at 21.59 16.507 270) (size 3 1) (layers "B.Cu" "B.Paste" "B.Mask"))
  (pad "82" smd rect (at 21.59 11.467 270) (size 3 1) (layers "B.Cu" "B.Paste" "B.Mask"))
  (pad "83" smd rect (at 24.13 16.507 270) (size 3 1) (layers "B.Cu" "B.Paste" "B.Mask"))
  (pad "84" smd rect (at 24.13 11.467 270) (size 3 1) (layers "B.Cu" "B.Paste" "B.Mask"))
  (pad "85" smd rect (at 26.67 16.507 270) (size 3 1) (layers "B.Cu" "B.Paste" "B.Mask"))
  (pad "86" smd rect (at 26.67 11.467 270) (size 3 1) (layers "B.Cu" "B.Paste" "B.Mask"))
  (pad "87" smd rect (at 29.21 16.507 270) (size 3 1) (layers "B.Cu" "B.Paste" "B.Mask"))
  (pad "88" smd rect (at 29.21 11.467 270) (size 3 1) (layers "B.Cu" "B.Paste" "B.Mask"))
  (pad "89" smd rect (at 31.75 16.507 270) (size 3 1) (layers "B.Cu" "B.Paste" "B.Mask"))
  (pad "90" smd rect (at 31.75 11.467 270) (size 3 1) (layers "B.Cu" "B.Paste" "B.Mask"))
)
