(footprint "SerMonK_v3_0" (version 20211014) (generator pcbnew)
  (layer "F.Cu")
  (tedit 0)
  (attr through_hole)
  (fp_text reference "REF**" (at 14.986 -27.8412 unlocked) (layer "F.SilkS"))
  (fp_text value "SerMonK_v3_0" (at 14.986 -26.3412 unlocked) (layer "F.Fab"))
  (fp_text user "${REFERENCE}" (at 3.07 -28.1212 90) (layer "F.Fab"))
  (fp_text user "${REFERENCE}" (at 14.986 -24.8412 unlocked) (layer "F.Fab"))
  (fp_text user "${REFERENCE}" (at 14.79 -30.3792 180) (layer "F.Fab"))
  (pad "1" thru_hole rect (at 2.032 -52.2732) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  (pad "2" thru_hole oval (at 2.032 -49.7078) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  (pad "3" thru_hole oval (at 2.032 -47.1932) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  (pad "4" thru_hole oval (at 2.032 -44.6532) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  (pad "5" thru_hole oval (at 2.032 -42.1132) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  (pad "6" thru_hole oval (at 2.032 -39.5732) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  (pad "7" thru_hole oval (at 2.032 -37.0332) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  (pad "8" thru_hole oval (at 2.032 -34.4932) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  (pad "9" thru_hole oval (at 2.032 -31.9532) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  (pad "10" thru_hole oval (at 2.032 -29.4132) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  (pad "11" thru_hole oval (at 2.032 -26.8732) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  (pad "12" thru_hole oval (at 2.032 -24.3332) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  (pad "13" thru_hole oval (at 2.032 -21.7932) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  (pad "14" thru_hole oval (at 2.032 -19.2532) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  (pad "15" thru_hole oval (at 2.032 -16.7132) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  (pad "16" thru_hole oval (at 2.032 -14.1732) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  (pad "17" thru_hole oval (at 2.032 -11.6332) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  (pad "18" thru_hole oval (at 2.032 -9.0932) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  (pad "19" thru_hole oval (at 2.032 -6.5532) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  (pad "20" thru_hole oval (at 2.032 -4.0132) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  (pad "21" thru_hole oval (at 27.432 -4.0132) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  (pad "22" thru_hole oval (at 27.432 -6.5532) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  (pad "23" thru_hole oval (at 27.432 -9.0932) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  (pad "24" thru_hole oval (at 27.432 -11.6332) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  (pad "25" thru_hole oval (at 27.432 -14.1732) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  (pad "26" thru_hole oval (at 27.432 -16.7132) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  (pad "27" thru_hole oval (at 27.432 -19.2532) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  (pad "28" thru_hole oval (at 27.432 -21.7932) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  (pad "29" thru_hole oval (at 27.432 -24.3332) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  (pad "30" thru_hole oval (at 27.432 -26.8732) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  (pad "31" thru_hole oval (at 27.432 -29.4132) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  (pad "32" thru_hole oval (at 27.432 -31.9532) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  (pad "33" thru_hole oval (at 27.432 -34.4932) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  (pad "34" thru_hole oval (at 27.432 -37.0332) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  (pad "35" thru_hole oval (at 27.432 -39.5732) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  (pad "36" thru_hole oval (at 27.432 -42.1132) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  (pad "37" thru_hole oval (at 27.432 -44.6532) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  (pad "38" thru_hole oval (at 27.432 -47.1932) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  (pad "39" thru_hole oval (at 27.432 -49.7332) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  (pad "40" thru_hole oval (at 27.432 -52.2732) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  (pad "41" thru_hole oval (at 4.572 -52.2732) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  (pad "42" thru_hole oval (at 4.572 -49.7332) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  (pad "43" thru_hole oval (at 4.572 -47.1932) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  (pad "44" thru_hole oval (at 4.572 -44.6532) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  (pad "45" thru_hole oval (at 4.572 -42.1132) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  (pad "46" thru_hole oval (at 4.572 -39.5732) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  (pad "47" thru_hole oval (at 4.572 -37.0332) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  (pad "48" thru_hole oval (at 4.572 -34.4932) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  (pad "49" thru_hole oval (at 24.892 -34.4932) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  (pad "50" thru_hole oval (at 24.892 -37.0332) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  (pad "51" thru_hole oval (at 24.892 -39.5732) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  (pad "52" thru_hole oval (at 24.892 -42.1132) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  (pad "53" thru_hole oval (at 24.892 -44.6532) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  (pad "54" thru_hole oval (at 24.892 -47.1932) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  (pad "55" thru_hole oval (at 24.892 -49.7332) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  (pad "56" thru_hole oval (at 24.892 -52.2732) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
)
