(footprint "Sullins2x5_SFH11-PBPC-D05-ST-BK" (version 20211014) (generator pcbnew)
  (layer "F.Cu")
  (tedit 0)
  (attr through_hole)
  (fp_text reference "REF**" (at 10.1 -2.6) (layer "F.SilkS"))
  (fp_text value "CONN_SFH11-xxxC-D05-ST-XX_SUL" (at 5.45 6.55) (layer "F.SilkS"))
  (fp_text user "*" (at 0 0) (layer "F.SilkS"))
  (fp_text user "*" (at 0 0) (layer "F.Fab"))
  (pad "1" thru_hole rect (at 0 0) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask))
  (pad "2" thru_hole circle (at 0 2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask))
  (pad "3" thru_hole circle (at 2.54 0) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask))
  (pad "4" thru_hole circle (at 2.54 2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask))
  (pad "5" thru_hole circle (at 5.08 0) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask))
  (pad "6" thru_hole circle (at 5.08 2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask))
  (pad "7" thru_hole circle (at 7.62 0) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask))
  (pad "8" thru_hole circle (at 7.62 2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask))
  (pad "9" thru_hole circle (at 10.16 0) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask))
  (pad "10" thru_hole circle (at 10.16 2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask))
)
