(module IC8_TPH1R306P1_TOS (layer F.Cu)
  (fp_text reference REF** (at 0 0) (layer F.SilkS))
  (fp_text value IC8_TPH1R306P1_TOS (at 0 0) (layer F.SilkS))
  (fp_text user "Copyright 2021 Accelerated Designs. All rights reserved." (at 0 0) (layer Cmts.User))
  (fp_text user "*" (at 0 0) (layer F.SilkS))
  (fp_text user "*" (at 0 0) (layer F.Fab))
  (fp_text user "0.05in/1.27mm" (at -5.9059 -1.27) (layer Cmts.User))
  (fp_text user "0.018in/0.457mm" (at 5.9059 -1.905) (layer Cmts.User))
  (fp_text user "0.225in/5.716mm" (at 0 -5.0165) (layer Cmts.User))
  (fp_text user "0.047in/1.194mm" (at -2.8579 4.3815) (layer Cmts.User))
  (fp_text user "0.17in/4.318mm" (at 5.0165 0) (layer Cmts.User))
  (fp_text user "0.146in/3.708mm" (at 0 5.6515) (layer Cmts.User))
  (pad 1 smd rect (at -2.857899 -1.905) (size 1.1938 .4572) (layers F.Cu F.Paste F.Mask))
  (pad 2 smd rect (at -2.857899 -.635) (size 1.1938 .4572) (layers F.Cu F.Paste F.Mask))
  (pad 3 smd rect (at -2.857899 .635) (size 1.1938 .4572) (layers F.Cu F.Paste F.Mask))
  (pad 4 smd rect (at -2.857899 1.905) (size 1.1938 .4572) (layers F.Cu F.Paste F.Mask))
  (pad 5 smd rect (at 2.857899 1.905) (size 1.1938 .4572) (layers F.Cu F.Paste F.Mask))
  (pad 6 smd rect (at 2.857899 .635) (size 1.1938 .4572) (layers F.Cu F.Paste F.Mask))
  (pad 7 smd rect (at 2.857899 -.635) (size 1.1938 .4572) (layers F.Cu F.Paste F.Mask))
  (pad 8 smd rect (at 2.857899 -1.905) (size 1.1938 .4572) (layers F.Cu F.Paste F.Mask))
)
