(footprint "boostr_v1_0" (version 20211014) (generator pcbnew)
  (layer "F.Cu")
  (tedit 0)
  (attr through_hole)
  (fp_text reference "REF**" (at 0 -0.5 unlocked) (layer "F.SilkS"))
  (fp_text value "boostr_v1_0" (at 0 1 unlocked) (layer "F.Fab"))
  (fp_text user "${REFERENCE}" (at 0 2.5 unlocked) (layer "F.Fab"))
  (pad "1" thru_hole rect (at 13.462 -2.286 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  (pad "2" thru_hole oval (at 13.462 -4.826 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  (pad "3" thru_hole oval (at 16.002 -2.286 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  (pad "4" thru_hole oval (at 16.002 -4.826 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  (pad "5" thru_hole oval (at 18.542 -2.286 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  (pad "6" thru_hole oval (at 18.542 -4.826 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  (pad "7" thru_hole oval (at 21.082 -2.286 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  (pad "8" thru_hole oval (at 21.082 -4.826 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  (pad "9" thru_hole oval (at 23.622 -2.286 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  (pad "10" thru_hole oval (at 23.622 -4.826 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  (pad "11" thru_hole rect (at 3.302 -52.324 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  (pad "12" thru_hole oval (at 5.842 -52.324 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  (pad "13" thru_hole oval (at 8.382 -52.324 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  (pad "14" thru_hole oval (at 10.922 -52.324 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  (pad "15" thru_hole oval (at 13.462 -52.324 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  (pad "16" thru_hole oval (at 16.002 -52.324 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  (pad "17" thru_hole oval (at 18.542 -52.324 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  (pad "18" thru_hole oval (at 21.082 -52.324 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  (pad "19" thru_hole oval (at 23.622 -52.324 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
)
