(footprint "fsa1208-mlp" (version 20211014) (generator pcbnew)
  (layer "F.Cu")
  (tedit 0)
  (attr through_hole)
  (fp_text reference "REF**" (at 4.75 2.5 unlocked) (layer "F.SilkS"))
  (fp_text value "fsa1208-mlp" (at 0.65 -3.85 unlocked) (layer "F.Fab"))
  (fp_text user "${REFERENCE}" (at 4.75 2.5 unlocked) (layer "F.Fab"))
  (pad "1" smd rect (at -0.25 -2.35 90) (size 0.9 0.24) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "2" smd rect (at -1.35 -1.75) (size 0.9 0.24) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "3" smd rect (at -1.35 -1.25) (size 0.9 0.24) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "4" smd rect (at -1.35 -0.75) (size 0.9 0.24) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "5" smd rect (at -1.35 -0.25) (size 0.9 0.24) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "6" smd rect (at -1.35 0.25) (size 0.9 0.24) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "7" smd rect (at -1.35 0.75) (size 0.9 0.24) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "8" smd rect (at -1.35 1.25) (size 0.9 0.24) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "9" smd rect (at -1.35 1.75) (size 0.9 0.24) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "10" smd rect (at -0.25 2.35 90) (size 0.9 0.24) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "11" smd rect (at 0.25 2.35 90) (size 0.9 0.24) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "12" smd rect (at 1.35 1.75 180) (size 0.9 0.24) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "13" smd rect (at 1.35 1.25 180) (size 0.9 0.24) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "14" smd rect (at 1.35 0.75 180) (size 0.9 0.24) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "15" smd rect (at 1.35 0.25 180) (size 0.9 0.24) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "16" smd rect (at 1.35 -0.25 180) (size 0.9 0.24) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "17" smd rect (at 1.35 -0.75 180) (size 0.9 0.24) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "18" smd rect (at 1.35 -1.25 180) (size 0.9 0.24) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "19" smd rect (at 1.35 -1.75 180) (size 0.9 0.24) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "20" smd rect (at 0.25 -2.35 270) (size 0.9 0.24) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "21" smd rect (at 0 0 90) (size 3.15 1.15) (layers "F.Cu" "F.Paste" "F.Mask"))
)
