(footprint "wakestr_slim_v1" (version 20211014) (generator pcbnew)
  (layer "F.Cu")
  (tedit 0)
  (attr through_hole)
  (fp_text reference "REF**" (at 0.254 0 unlocked) (layer "F.SilkS"))
  (fp_text value "wakestr_slim_v1" (at 0 1 unlocked) (layer "F.Fab"))
  (fp_text user "${REFERENCE}" (at 0.254 0 unlocked) (layer "F.Fab"))
  (pad "1" thru_hole rect (at -16.764 10.033) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  (pad "2" thru_hole circle (at -16.764 7.493) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  (pad "3" thru_hole circle (at -16.764 4.953) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  (pad "4" thru_hole circle (at -16.764 2.413) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  (pad "5" thru_hole circle (at -16.764 -0.127) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  (pad "6" thru_hole circle (at -16.764 -2.667) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  (pad "7" thru_hole circle (at -16.764 -5.207) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  (pad "8" thru_hole circle (at -16.764 -7.747) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  (pad "9" thru_hole circle (at -16.764 -10.287) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  (pad "10" thru_hole circle (at 18.796 -5.207) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  (pad "11" thru_hole circle (at 18.796 -2.667) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  (pad "12" thru_hole circle (at 18.796 -0.127) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  (pad "13" thru_hole circle (at 18.796 2.413) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  (pad "14" thru_hole circle (at 18.796 4.953) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  (pad "15" thru_hole circle (at 18.796 7.493) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  (pad "16" thru_hole rect (at 18.796 10.033) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x09_P2.54mm_Vertical.wrl"
    (offset (xyz -25.4 -5.08 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
  (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x07_P2.54mm_Vertical.wrl"
    (offset (xyz 10.16 -10.16 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)
