(kicad_symbol_lib (version 20211014) (generator kicad_symbol_editor)
  (symbol "DM3AT-SF-PEJM5" (pin_names (offset 1.016)) (in_bom yes) (on_board yes)
    (property "Reference" "J" (id 0) (at -7.62 18.3148 0))
    (property "Value" "DM3AT-SF-PEJM5" (id 1) (at -7.62 -20.8538 0))
    (property "Footprint" "HRS_DM3AT-SF-PEJM5" (id 2) (at 0 0 0))
    (property "DESCRIPTION" "DM3 RA SMT microSD memory card push/push" (id 4) (at 0 0 0))
    (property "MF" "Hirose" (id 5) (at 0 0 0))
    (property "AVAILABILITY" "Unavailable" (id 6) (at 0 0 0))
    (property "MP" "DM3AT-SF-PEJM5" (id 7) (at 0 0 0))
    (property "PRICE" "None" (id 8) (at 0 0 0))
    (property "PACKAGE" "None" (id 9) (at 0 0 0))
    (symbol "DM3AT-SF-PEJM5_0_0"
      (text "A" (at -3.048 -13.208 0))
      (text "B" (at -3.048 -16.51 0))
      (pin bidirectional line (at -12.7 12.7 0) (length 5.08)
        (name "DAT0")
        (number "7")
      )
      (pin bidirectional line (at -12.7 10.16 0) (length 5.08)
        (name "DAT1")
        (number "8")
      )
      (pin bidirectional line (at -12.7 7.62 0) (length 5.08)
        (name "DAT2")
        (number "1")
      )
      (pin bidirectional line (at -12.7 5.08 0) (length 5.08)
        (name "CD/DAT3")
        (number "2")
      )
      (pin bidirectional line (at -12.7 2.54 0) (length 5.08)
        (name "CMD")
        (number "3")
      )
      (pin bidirectional clock (at -12.7 0.0 0) (length 5.08)
        (name "CLK")
        (number "5")
      )
      (pin power_in line (at -12.7 15.24 0) (length 5.08)
        (name "VDD")
        (number "4")
      )
      (pin power_in line (at -12.7 -2.54 0) (length 5.08)
        (name "VSS")
        (number "6")
      )
      (pin bidirectional line (at -12.7 -12.7 0) (length 5.08)
        (name "~")
        (number "SWA")
      )
      (pin bidirectional line (at -12.7 -15.24 0) (length 5.08)
        (name "~")
        (number "SWB")
      )
      (pin passive line (at -12.7 -7.62 0) (length 5.08)
        (name "SHIELD")
        (number "P1")
      )
      (pin passive line (at -12.7 -7.62 0) (length 5.08)
        (name "SHIELD")
        (number "P2")
      )
      (pin passive line (at -12.7 -7.62 0) (length 5.08)
        (name "SHIELD")
        (number "P3")
      )
      (pin passive line (at -12.7 -7.62 0) (length 5.08)
        (name "SHIELD")
        (number "P4")
      )
    )
  )
)