(kicad_symbol_lib (version 20211014) (generator kicad_symbol_editor)
  (symbol "I7C4W008A120V-001-R" (pin_names (offset 1.016)) (in_bom yes) (on_board yes)
    (property "Reference" "PS" (id 0) (at -20.32 10.922 0))
    (property "Value" "I7C4W008A120V-001-R" (id 1) (at -20.32 -12.7 0))
    (property "Footprint" "CONV_I7C4W008A120V-001-R" (id 2) (at 0 0 0))
    (property "STANDARD" "Manufacturer Recommendations" (id 4) (at 0 0 0))
    (property "PARTREV" "V5" (id 5) (at 0 0 0))
    (property "MANUFACTURER" "TDK-Lambda" (id 6) (at 0 0 0))
    (property "MAXIMUM_PACKAGE_HEIGHT" "12.7mm" (id 7) (at 0 0 0))
    (symbol "I7C4W008A120V-001-R_0_0"
      (pin input line (at -25.4 7.62 0) (length 5.08)
        (name "VIN(+)")
        (number "1")
      )
      (pin input line (at -25.4 0.0 0) (length 5.08)
        (name "~{ON/OFF}")
        (number "2")
      )
      (pin input line (at -25.4 -7.62 0) (length 5.08)
        (name "VIN(-)/GND")
        (number "3")
      )
      (pin output line (at 25.4 -7.62 180.0) (length 5.08)
        (name "VOUT(-)/GND")
        (number "4")
      )
      (pin passive line (at 25.4 -2.54 180.0) (length 5.08)
        (name "TRIM")
        (number "6")
      )
      (pin output line (at 25.4 7.62 180.0) (length 5.08)
        (name "VOUT(+)")
        (number "8")
      )
      (pin input line (at 25.4 2.54 180.0) (length 5.08)
        (name "SENSE+")
        (number "7")
      )
    )
  )
)