(kicad_symbol_lib
	(version 20231120)
	(generator "kicad_symbol_editor")
	(generator_version "8.0")
	(symbol "01550900M(Holder)"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "F"
			(at 0 2.54 0)
		)
		(property "Value" "01550900M(Holder)"
			(at 0 -3.81 0)
		)
		(property "Footprint" "ProjectFootprints:01550900M"
			(at -1.27 -11.43 0)
		)
		(property "Datasheet" "https://www.littelfuse.com/~/media/electronics/datasheets/fuses/littelfuse_fuse_154_154t_154l_154tl_datasheet.pdf.pdf"
			(at 1.27 -2.54 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(property "Part Number" "F1889-ND"
			(at -1.27 -8.89 0)
		)
		(property "Supplier" "Digikey"
			(at 0 -6.35 0)
		)
		(property "Link" "https://www.digikey.com/products/en/circuit-protection/fuseholders/140?k=little%20fuse%20nano"
			(at -1.27 -13.97 0)
		)
		(symbol "01550900M(Holder)_0_1")
		(symbol "01550900M(Holder)_1_1"
			(pin passive line
				(at -5.08 0 0)
				(length 2.54)
				(name "1")
				(number "1")
			)
			(pin passive line
				(at 5.08 0 180)
				(length 2.54)
				(name "2")
				(number "2")
			)
		)
	)
	(symbol "12401598E4_2A"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at -7.632 35.612 0)
		)
		(property "Value" "12401598E4_2A"
			(at -7.6336 -38.1632 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" "\nUSB3.2 GEN2, Type C, Top mount, CH 1.58mm, Dual Row SMT\n"
			(at 0 0 0)
		)
		(property "MF" ""
			(at 0 0 0)
		)
		(property "MAXIMUM_PACKAGE_HEIGHT" ""
			(at 0 0 0)
		)
		(property "Package" ""
			(at 0 0 0)
		)
		(property "Price" ""
			(at 0 0 0)
		)
		(property "Check_prices" ""
			(at 0 0 0)
		)
		(property "STANDARD" ""
			(at 0 0 0)
		)
		(property "PARTREV" "4"
			(at 0 0 0)
		)
		(property "SnapEDA_Link" ""
			(at 0 0 0)
		)
		(property "MP" ""
			(at 0 0 0)
		)
		(property "Purchase-URL" ""
			(at 0 0 0)
		)
		(property "Availability" ""
			(at 0 0 0)
		)
		(property "MANUFACTURER" ""
			(at 0 0 0)
		)
		(symbol "12401598E4_2A_0_0"
			(pin power_in line
				(at 12.7 -30.48 180)
				(length 5.08)
				(name "GND")
				(number "A1")
			)
			(pin passive line
				(at 12.7 -7.62 180)
				(length 5.08)
				(name "SSRXN2")
				(number "A10")
			)
			(pin passive line
				(at 12.7 -10.16 180)
				(length 5.08)
				(name "SSRXP2")
				(number "A11")
			)
			(pin power_in line
				(at 12.7 -30.48 180)
				(length 5.08)
				(name "GND")
				(number "A12")
			)
			(pin passive line
				(at 12.7 2.54 180)
				(length 5.08)
				(name "SSTXP1")
				(number "A2")
			)
			(pin passive line
				(at 12.7 5.08 180)
				(length 5.08)
				(name "SSTXN1")
				(number "A3")
			)
			(pin power_in line
				(at 12.7 30.48 180)
				(length 5.08)
				(name "VBUS")
				(number "A4")
			)
			(pin passive line
				(at 12.7 0 180)
				(length 5.08)
				(name "CC1")
				(number "A5")
			)
			(pin passive line
				(at 12.7 22.86 180)
				(length 5.08)
				(name "DP1")
				(number "A6")
			)
			(pin passive line
				(at 12.7 25.4 180)
				(length 5.08)
				(name "DN1")
				(number "A7")
			)
			(pin passive line
				(at 12.7 -2.54 180)
				(length 5.08)
				(name "SBU1")
				(number "A8")
			)
			(pin power_in line
				(at 12.7 30.48 180)
				(length 5.08)
				(name "VBUS")
				(number "A9")
			)
			(pin power_in line
				(at 12.7 -30.48 180)
				(length 5.08)
				(name "GND")
				(number "B1")
			)
			(pin passive line
				(at 12.7 10.16 180)
				(length 5.08)
				(name "SSRXN1")
				(number "B10")
			)
			(pin passive line
				(at 12.7 7.62 180)
				(length 5.08)
				(name "SSRXP1")
				(number "B11")
			)
			(pin power_in line
				(at 12.7 -30.48 180)
				(length 5.08)
				(name "GND")
				(number "B12")
			)
			(pin passive line
				(at 12.7 -15.24 180)
				(length 5.08)
				(name "SSTXP2")
				(number "B2")
			)
			(pin passive line
				(at 12.7 -12.7 180)
				(length 5.08)
				(name "SSTXN2")
				(number "B3")
			)
			(pin power_in line
				(at 12.7 30.48 180)
				(length 5.08)
				(name "VBUS")
				(number "B4")
			)
			(pin passive line
				(at 12.7 -17.78 180)
				(length 5.08)
				(name "CC2")
				(number "B5")
			)
			(pin passive line
				(at 12.7 15.24 180)
				(length 5.08)
				(name "DP2")
				(number "B6")
			)
			(pin passive line
				(at 12.7 17.78 180)
				(length 5.08)
				(name "DN2")
				(number "B7")
			)
			(pin passive line
				(at 12.7 -20.32 180)
				(length 5.08)
				(name "SBU2")
				(number "B8")
			)
			(pin power_in line
				(at 12.7 30.48 180)
				(length 5.08)
				(name "VBUS")
				(number "B9")
			)
			(pin power_in line
				(at 12.7 -25.4 180)
				(length 5.08)
				(name "SHIELD")
				(number "SH1")
			)
			(pin power_in line
				(at 12.7 -25.4 180)
				(length 5.08)
				(name "SHIELD")
				(number "SH2")
			)
			(pin power_in line
				(at 12.7 -25.4 180)
				(length 5.08)
				(name "SHIELD")
				(number "SH3")
			)
			(pin power_in line
				(at 12.7 -25.4 180)
				(length 5.08)
				(name "SHIELD")
				(number "SH4")
			)
		)
		(symbol "12401598E4_2A_0_1")
		(symbol "12401598E4_2A_1_1")
	)
	(symbol "1EDN8511BXUSA1"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 0 0)
		)
		(property "Value" "1EDN8511BXUSA1"
			(at 0 15.24 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "1EDN8511BXUSA1_0_1")
		(symbol "1EDN8511BXUSA1_1_1"
			(pin power_in line
				(at -8.89 2.54 0)
				(length 2.54)
				(name "VDD")
				(number "1")
			)
			(pin output line
				(at -8.89 0 0)
				(length 2.54)
				(name "OUT")
				(number "2")
			)
			(pin output line
				(at -8.89 -2.54 0)
				(length 2.54)
				(name "OUT_SNK")
				(number "3")
			)
			(pin power_in line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "GND")
				(number "4")
			)
			(pin input line
				(at 10.16 0 180)
				(length 2.54)
				(name "IN-")
				(number "5")
			)
			(pin input line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "IN+")
				(number "6")
			)
		)
	)
	(symbol "2N7002DW_small_symbol"
		(pin_names
			(offset 0)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "Q"
			(at 0 8.89 0)
		)
		(property "Value" "2N7002DW_small_symbol"
			(at -5.08 -15.24 0)
		)
		(property "Footprint" "digikey-footprints:SOT-363"
			(at 16.51 5.08 0)
		)
		(property "Datasheet" "https://www.onsemi.com/pub/Collateral/2N7002DW-D.PDF"
			(at 16.51 7.62 0)
		)
		(property "Description" "MOSFET 2N-CH 60V 0.115A SC70-6"
			(at 16.51 25.4 0)
		)
		(property "Digi-Key_PN" "2N7002DWCT-ND"
			(at 16.51 10.16 0)
		)
		(property "MPN" "2N7002DW"
			(at 16.51 12.7 0)
		)
		(property "Category" "Discrete Semiconductor Products"
			(at 16.51 15.24 0)
		)
		(property "Family" "Transistors - FETs, MOSFETs - Arrays"
			(at 16.51 17.78 0)
		)
		(property "DK_Datasheet_Link" "https://www.onsemi.com/pub/Collateral/2N7002DW-D.PDF"
			(at 16.51 20.32 0)
		)
		(property "DK_Detail_Page" "/product-detail/en/on-semiconductor/2N7002DW/2N7002DWCT-ND/1785790"
			(at 16.51 22.86 0)
		)
		(property "Manufacturer" "ON Semiconductor"
			(at 16.51 27.94 0)
		)
		(property "Status" "Active"
			(at 16.51 30.48 0)
		)
		(property "ki_keywords" "2N7002DWCT-ND"
			(at 0 0 0)
		)
		(symbol "2N7002DW_small_symbol_0_1")
		(symbol "2N7002DW_small_symbol_1_1"
			(pin input line
				(at -6.35 5.08 0)
				(length 2.54)
				(name "S2")
				(number "1")
			)
			(pin input line
				(at -6.35 0 0)
				(length 2.54)
				(name "G2")
				(number "2")
			)
			(pin output line
				(at -6.35 -5.08 0)
				(length 2.54)
				(name "D1")
				(number "3")
			)
			(pin input line
				(at 6.35 -5.08 180)
				(length 2.54)
				(name "S1")
				(number "4")
			)
			(pin input line
				(at 6.35 0 180)
				(length 2.54)
				(name "G1")
				(number "5")
			)
			(pin output line
				(at 6.35 5.08 180)
				(length 2.54)
				(name "D2")
				(number "6")
			)
		)
	)
	(symbol "35SVPF82M"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "C"
			(at -2.54 3.81 0)
		)
		(property "Value" "35SVPF82M"
			(at -2.54 -5.08 0)
		)
		(property "Footprint" "ProjectFootprints:CAP_35SVPF82M"
			(at 0 0 0)
		)
		(property "Datasheet" "https://industrial.panasonic.com/ww/products/pt/os-con/models/35SVPF82M"
			(at 0 0 0)
		)
		(property "Description" "82 µF 35 V Aluminum - Polymer Capacitors Radial, Can - SMD 20mOhm 5000 Hrs @ 105°C"
			(at 0 0 0)
		)
		(property "PartNum" "35SVPF82M"
			(at 0 0 0)
		)
		(property "VendorNum" "P16562CT-ND"
			(at 0 0 0)
		)
		(property "Subst" "No"
			(at 0 0 0)
		)
		(symbol "35SVPF82M_0_0"
			(pin passive line
				(at -2.54 0 0)
				(length 2.54)
				(name "~")
				(number "1")
			)
			(pin passive line
				(at 5.08 0 180)
				(length 2.54)
				(name "~")
				(number "2")
			)
		)
	)
	(symbol "74HC4051"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 13.97 0)
		)
		(property "Value" "74HC4051"
			(at 0 11.43 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "74HC4051_0_1")
		(symbol "74HC4051_1_1"
			(pin passive line
				(at -8.89 7.62 0)
				(length 2.54)
				(name "A4")
				(number "1")
			)
			(pin input line
				(at 8.89 -7.62 180)
				(length 2.54)
				(name "S1")
				(number "10")
			)
			(pin input line
				(at 8.89 -5.08 180)
				(length 2.54)
				(name "S0")
				(number "11")
			)
			(pin passive line
				(at 8.89 -2.54 180)
				(length 2.54)
				(name "A3")
				(number "12")
			)
			(pin passive line
				(at 8.89 0 180)
				(length 2.54)
				(name "A0")
				(number "13")
			)
			(pin passive line
				(at 8.89 2.54 180)
				(length 2.54)
				(name "A1")
				(number "14")
			)
			(pin passive line
				(at 8.89 5.08 180)
				(length 2.54)
				(name "A2")
				(number "15")
			)
			(pin power_in line
				(at 8.89 7.62 180)
				(length 2.54)
				(name "VCC")
				(number "16")
			)
			(pin passive line
				(at -8.89 5.08 0)
				(length 2.54)
				(name "A6")
				(number "2")
			)
			(pin passive line
				(at -8.89 2.54 0)
				(length 2.54)
				(name "A")
				(number "3")
			)
			(pin passive line
				(at -8.89 0 0)
				(length 2.54)
				(name "A7")
				(number "4")
			)
			(pin passive line
				(at -8.89 -2.54 0)
				(length 2.54)
				(name "A5")
				(number "5")
			)
			(pin input line
				(at -8.89 -5.08 0)
				(length 2.54)
				(name "~{E}")
				(number "6")
			)
			(pin power_in line
				(at -8.89 -7.62 0)
				(length 2.54)
				(name "VEE")
				(number "7")
			)
			(pin power_in line
				(at -8.89 -10.16 0)
				(length 2.54)
				(name "GND")
				(number "8")
			)
			(pin input line
				(at 8.89 -10.16 180)
				(length 2.54)
				(name "S2")
				(number "9")
			)
		)
	)
	(symbol "74LVCV2G66"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -4.572 7.62 0)
		)
		(property "Value" "74LVCV2G66"
			(at 0 -7.112 0)
		)
		(property "Footprint" ""
			(at 1.27 0 0)
		)
		(property "Datasheet" ""
			(at 1.27 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "74LVCV2G66_0_1")
		(symbol "74LVCV2G66_1_1"
			(pin passive line
				(at -8.89 3.81 0)
				(length 2.54)
				(name "1Z")
				(number "1")
			)
			(pin passive line
				(at -8.89 1.27 0)
				(length 2.54)
				(name "1Y")
				(number "2")
			)
			(pin input line
				(at -8.89 -1.27 0)
				(length 2.54)
				(name "2E")
				(number "3")
			)
			(pin power_in line
				(at -8.89 -3.81 0)
				(length 2.54)
				(name "GND")
				(number "4")
			)
			(pin passive line
				(at 8.89 -3.81 180)
				(length 2.54)
				(name "2Z")
				(number "5")
			)
			(pin passive line
				(at 8.89 -1.27 180)
				(length 2.54)
				(name "2Y")
				(number "6")
			)
			(pin passive line
				(at 8.89 1.27 180)
				(length 2.54)
				(name "1E")
				(number "7")
			)
			(pin power_in line
				(at 8.89 3.81 180)
				(length 2.54)
				(name "VCC")
				(number "8")
			)
		)
	)
	(symbol "ACPL-244"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 11.43 0)
		)
		(property "Value" "ACPL-244"
			(at 0 -11.43 0)
		)
		(property "Footprint" ""
			(at 1.27 -1.27 0)
		)
		(property "Datasheet" ""
			(at 1.27 -1.27 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "ACPL-244_0_1")
		(symbol "ACPL-244_1_1"
			(pin bidirectional line
				(at -8.89 8.89 0)
				(length 2.54)
				(name "~")
				(number "1")
			)
			(pin bidirectional line
				(at 8.89 -6.35 180)
				(length 2.54)
				(name "~")
				(number "10")
			)
			(pin bidirectional line
				(at 8.89 -3.81 180)
				(length 2.54)
				(name "~")
				(number "11")
			)
			(pin bidirectional line
				(at 8.89 -1.27 180)
				(length 2.54)
				(name "~")
				(number "12")
			)
			(pin bidirectional line
				(at 8.89 1.27 180)
				(length 2.54)
				(name "~")
				(number "13")
			)
			(pin bidirectional line
				(at 8.89 3.81 180)
				(length 2.54)
				(name "~")
				(number "14")
			)
			(pin bidirectional line
				(at 8.89 6.35 180)
				(length 2.54)
				(name "~")
				(number "15")
			)
			(pin bidirectional line
				(at 8.89 8.89 180)
				(length 2.54)
				(name "~")
				(number "16")
			)
			(pin bidirectional line
				(at -8.89 6.35 0)
				(length 2.54)
				(name "~")
				(number "2")
			)
			(pin bidirectional line
				(at -8.89 3.81 0)
				(length 2.54)
				(name "~")
				(number "3")
			)
			(pin bidirectional line
				(at -8.89 1.27 0)
				(length 2.54)
				(name "~")
				(number "4")
			)
			(pin bidirectional line
				(at -8.89 -1.27 0)
				(length 2.54)
				(name "~")
				(number "5")
			)
			(pin bidirectional line
				(at -8.89 -3.81 0)
				(length 2.54)
				(name "~")
				(number "6")
			)
			(pin bidirectional line
				(at -8.89 -6.35 0)
				(length 2.54)
				(name "~")
				(number "7")
			)
			(pin bidirectional line
				(at -8.89 -8.89 0)
				(length 2.54)
				(name "~")
				(number "8")
			)
			(pin bidirectional line
				(at 8.89 -8.89 180)
				(length 2.54)
				(name "~")
				(number "9")
			)
		)
	)
	(symbol "AD5259"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 8.89 11.43 0)
		)
		(property "Value" "AD5259"
			(at -6.35 11.43 0)
		)
		(property "Footprint" ""
			(at 29.21 -19.05 0)
		)
		(property "Datasheet" ""
			(at 29.21 -19.05 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "AD5259_1_1"
			(pin passive line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "W")
				(number "1")
			)
			(pin passive line
				(at 12.7 7.62 180)
				(length 2.54)
				(name "A")
				(number "10")
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "AD0")
				(number "2")
			)
			(pin input line
				(at -12.7 -7.62 0)
				(length 2.54)
				(name "AD1")
				(number "3")
			)
			(pin bidirectional line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "SDA")
				(number "4")
			)
			(pin input line
				(at -12.7 7.62 0)
				(length 2.54)
				(name "SCL")
				(number "5")
			)
			(pin power_in line
				(at 2.54 12.7 270)
				(length 2.54)
				(name "VLOG")
				(number "6")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "GND")
				(number "7")
			)
			(pin power_in line
				(at 0 12.7 270)
				(length 2.54)
				(name "VDD")
				(number "8")
			)
			(pin passive line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "B")
				(number "9")
			)
		)
	)
	(symbol "AD7980BRMZRL7"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -5.08 10.16 0)
		)
		(property "Value" "AD7980"
			(at -2.54 -11.43 0)
		)
		(property "Footprint" "ProjectDevices:AD7980_SOP50P490X110-10N"
			(at 1.27 -20.32 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/AD7980.pdf"
			(at 1.27 -22.86 0)
		)
		(property "Description" "16-Bit, 1 MSPS, PulSAR ADC in MSOP/LFCSP"
			(at 1.27 -26.67 0)
		)
		(property "PartNum" "AD7980BRMZ"
			(at 0 -12.7 0)
		)
		(property "VendorNum" "AD7980BRMZ-ND"
			(at 0 -15.24 0)
		)
		(property "Vendor" "Digikey"
			(at 0 -17.78 0)
		)
		(property "Subst" "No"
			(at 0 -7.62 0)
		)
		(symbol "AD7980BRMZRL7_0_0"
			(pin input line
				(at -13.97 5.08 0)
				(length 5.08)
				(name "REF")
				(number "1")
			)
			(pin power_in line
				(at 13.97 5.08 180)
				(length 5.08)
				(name "VIO")
				(number "10")
			)
			(pin power_in line
				(at -13.97 2.54 0)
				(length 5.08)
				(name "VDD")
				(number "2")
			)
			(pin input line
				(at -13.97 0 0)
				(length 5.08)
				(name "IN+")
				(number "3")
			)
			(pin input line
				(at -13.97 -2.54 0)
				(length 5.08)
				(name "IN-")
				(number "4")
			)
			(pin power_in line
				(at -13.97 -5.08 0)
				(length 5.08)
				(name "GND")
				(number "5")
			)
			(pin input line
				(at 13.97 -5.08 180)
				(length 5.08)
				(name "CNV")
				(number "6")
			)
			(pin output line
				(at 13.97 -2.54 180)
				(length 5.08)
				(name "SDO")
				(number "7")
			)
			(pin input line
				(at 13.97 0 180)
				(length 5.08)
				(name "SCK")
				(number "8")
			)
			(pin input line
				(at 13.97 2.54 180)
				(length 5.08)
				(name "SDI")
				(number "9")
			)
		)
	)
	(symbol "AD8217"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 5.08 7.62 0)
		)
		(property "Value" "AD8217"
			(at 0 0 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "AD8217_0_1")
		(symbol "AD8217_1_1"
			(pin input line
				(at -10.16 3.81 0)
				(length 2.54)
				(name "+IN")
				(number "1")
			)
			(pin input line
				(at 10.16 3.81 180)
				(length 2.54)
				(name "-IN")
				(number "1")
			)
			(pin no_connect line
				(at -10.16 1.27 0)
				(length 2.54)
				(name "NC")
				(number "2")
			)
			(pin no_connect line
				(at -10.16 -1.27 0)
				(length 2.54)
				(name "NC")
				(number "3")
			)
			(pin input line
				(at -10.16 -3.81 0)
				(length 2.54)
				(name "GND")
				(number "4")
			)
			(pin output line
				(at 10.16 -3.81 180)
				(length 2.54)
				(name "OUT")
				(number "5")
			)
			(pin no_connect line
				(at 10.16 -1.27 180)
				(length 2.54)
				(name "NC")
				(number "6")
			)
			(pin no_connect line
				(at 10.16 1.27 180)
				(length 2.54)
				(name "NC")
				(number "7")
			)
		)
	)
	(symbol "ADA4510"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -3.81 8.89 0)
		)
		(property "Value" "ADA4510"
			(at 3.81 8.89 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 1.27 -8.89 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/ada4510-2.pdf"
			(at -1.27 -6.35 0)
		)
		(property "Description" "Precision, 40 V, ±70 nV/°C, Rail-to-Rail Input and Output Op Amp with DigiTrim"
			(at 0 0 0)
		)
		(property "PartNum" "ADA4510-2ARZ-RL"
			(at 1.27 -11.43 0)
		)
		(property "VendorNum" "505-ADA4510-2ARZ-RLCT-ND"
			(at 1.27 -13.97 0)
		)
		(property "Vendor" "Digikey"
			(at 0 -16.51 0)
		)
		(property "Subst" "No"
			(at 6.35 -16.51 0)
		)
		(symbol "ADA4510_1_1"
			(pin output line
				(at -8.89 5.08 0)
				(length 2.54)
				(name "OUTA")
				(number "1")
			)
			(pin input line
				(at -8.89 2.54 0)
				(length 2.54)
				(name "-IN_A")
				(number "2")
			)
			(pin input line
				(at -8.89 0 0)
				(length 2.54)
				(name "+IN_A")
				(number "3")
			)
			(pin power_in line
				(at -8.89 -2.54 0)
				(length 2.54)
				(name "V-")
				(number "4")
			)
			(pin input line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "+IN_B")
				(number "5")
			)
			(pin input line
				(at 10.16 0 180)
				(length 2.54)
				(name "-IN_B")
				(number "6")
			)
			(pin output line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "OUT_B")
				(number "7")
			)
			(pin power_in line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "V+")
				(number "8")
			)
		)
	)
	(symbol "ADA4622-4ACPZ-R7"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 2.54 3.175 0)
		)
		(property "Value" "ADA4622-4ACPZ-R7"
			(at 2.54 -5.08 0)
		)
		(property "Footprint" "ProjectFootprints:ADA4622_QFN65P400X400X80-17N"
			(at 1.27 -15.24 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/ada4622-1-4622-2-4622-4.pdf"
			(at 1.27 -17.78 0)
		)
		(property "Description" "30 V, 8 MHz, Low Bias Current, Single-Supply, RRO, Precision Quad Op Amp"
			(at -2.54 16.51 0)
		)
		(property "Package" "LFCSP -16 Analog Devices"
			(at -3.81 13.97 0)
		)
		(property "PartNum" "ADA4622-4ACPZ-R7"
			(at 13.97 6.35 0)
		)
		(property "VendorNum" "ADA4622-4ACPZ-R7"
			(at 12.7 8.89 0)
		)
		(symbol "ADA4622-4ACPZ-R7_1_0"
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "~")
				(number "1")
			)
			(pin power_in line
				(at -2.54 -7.62 90)
				(length 2.54)
				(name "~")
				(number "10")
			)
			(pin output line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "15")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 5.08)
				(name "~")
				(number "17")
			)
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "~")
				(number "2")
			)
			(pin power_in line
				(at -2.54 7.62 270)
				(length 2.54)
				(name "~")
				(number "3")
			)
		)
		(symbol "ADA4622-4ACPZ-R7_2_0"
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "~")
				(number "4")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "~")
				(number "5")
			)
			(pin output line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "6")
			)
		)
		(symbol "ADA4622-4ACPZ-R7_3_0"
			(pin output line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "7")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "~")
				(number "8")
			)
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "~")
				(number "9")
			)
		)
		(symbol "ADA4622-4ACPZ-R7_4_0"
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "~")
				(number "11")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "~")
				(number "12")
			)
			(pin output line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "14")
			)
		)
	)
	(symbol "ADA4805-2"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -5.08 6.35 0)
		)
		(property "Value" "ADA4805"
			(at 5.08 6.35 0)
		)
		(property "Footprint" "ProjectDevices:ADA4805_SOP65P490X110-8N"
			(at 2.54 -12.7 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/ADA4805-1_4805-2.pdf"
			(at 2.54 -15.24 0)
		)
		(property "Description" "Voff 125uV, 0.2 µV/°C Offset Drift, 105 MHz Low Power, Low noise: 5.9 nV/√Hz, Ibias 470nA"
			(at 0 0 0)
		)
		(property "PartNum" "ADA4805-2ARMZ"
			(at -1.27 -10.16 0)
		)
		(property "VendorNum" "505-ADA4805-2ARMZ-ND"
			(at -2.54 -20.32 0)
		)
		(property "Vendor" "Digikey"
			(at -6.35 -17.78 0)
		)
		(property "Subst" "No"
			(at 0 -17.78 0)
		)
		(symbol "ADA4805-2_1_1"
			(pin output line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "OUTA")
				(number "1")
			)
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "-IN_A")
				(number "2")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "+IN_A")
				(number "3")
			)
			(pin power_in line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "Vs-")
				(number "4")
			)
			(pin input line
				(at 8.89 -5.08 180)
				(length 2.54)
				(name "+IN_B")
				(number "5")
			)
			(pin input line
				(at 8.89 -2.54 180)
				(length 2.54)
				(name "-IN_B")
				(number "6")
			)
			(pin output line
				(at 8.89 0 180)
				(length 2.54)
				(name "OUT_B")
				(number "7")
			)
			(pin power_in line
				(at 8.89 2.54 180)
				(length 2.54)
				(name "Vs+")
				(number "8")
			)
		)
	)
	(symbol "ADM2561EBRNZ"
		(pin_names
			(offset 0.254)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 22.86 10.16 0)
		)
		(property "Value" "ADM2561EBRNZ"
			(at 22.86 7.62 0)
		)
		(property "Footprint" "RN-28-1_ADI"
			(at 22.86 6.096 0)
		)
		(property "Datasheet" ""
			(at 6.35 1.27 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_fp_filters" "RN-28-1_ADI RN-28-1_ADI-M RN-28-1_ADI-L"
			(at 0 0 0)
		)
		(symbol "ADM2561EBRNZ_1_1"
			(pin power_in line
				(at 6.35 1.27 0)
				(length 7.62)
				(name "GND1")
				(number "1")
			)
			(pin unspecified line
				(at 6.35 -21.59 0)
				(length 7.62)
				(name "DE")
				(number "10")
			)
			(pin unspecified line
				(at 6.35 -24.13 0)
				(length 7.62)
				(name "TXD")
				(number "11")
			)
			(pin unspecified line
				(at 6.35 -26.67 0)
				(length 7.62)
				(name "INV")
				(number "12")
			)
			(pin unspecified line
				(at 6.35 -29.21 0)
				(length 7.62)
				(name "NIC")
				(number "13")
			)
			(pin power_in line
				(at 6.35 -31.75 0)
				(length 7.62)
				(name "GND1")
				(number "14")
			)
			(pin power_in line
				(at 39.37 -31.75 180)
				(length 7.62)
				(name "GND2")
				(number "15")
			)
			(pin power_in line
				(at 39.37 -29.21 180)
				(length 7.62)
				(name "GND2")
				(number "16")
			)
			(pin bidirectional line
				(at 39.37 -26.67 180)
				(length 7.62)
				(name "A")
				(number "17")
			)
			(pin bidirectional line
				(at 39.37 -24.13 180)
				(length 7.62)
				(name "B")
				(number "18")
			)
			(pin unspecified line
				(at 39.37 -21.59 180)
				(length 7.62)
				(name "NIC")
				(number "19")
			)
			(pin power_in line
				(at 6.35 -1.27 0)
				(length 7.62)
				(name "GND1")
				(number "2")
			)
			(pin unspecified line
				(at 39.37 -19.05 180)
				(length 7.62)
				(name "NIC")
				(number "20")
			)
			(pin power_in line
				(at 39.37 -16.51 180)
				(length 7.62)
				(name "GND2")
				(number "21")
			)
			(pin power_in line
				(at 39.37 -13.97 180)
				(length 7.62)
				(name "GND2")
				(number "22")
			)
			(pin unspecified line
				(at 39.37 -11.43 180)
				(length 7.62)
				(name "VISOIN")
				(number "23")
			)
			(pin power_in line
				(at 39.37 -8.89 180)
				(length 7.62)
				(name "GNDISO")
				(number "24")
			)
			(pin power_out line
				(at 39.37 -6.35 180)
				(length 7.62)
				(name "VISOOUT")
				(number "25")
			)
			(pin power_in line
				(at 39.37 -3.81 180)
				(length 7.62)
				(name "GNDISO")
				(number "26")
			)
			(pin unspecified line
				(at 39.37 -1.27 180)
				(length 7.62)
				(name "VSEL")
				(number "27")
			)
			(pin power_in line
				(at 39.37 1.27 180)
				(length 7.62)
				(name "GNDISO")
				(number "28")
			)
			(pin power_in line
				(at 6.35 -3.81 0)
				(length 7.62)
				(name "GND1")
				(number "3")
			)
			(pin power_in line
				(at 6.35 -6.35 0)
				(length 7.62)
				(name "VCC")
				(number "4")
			)
			(pin power_in line
				(at 6.35 -8.89 0)
				(length 7.62)
				(name "GND1")
				(number "5")
			)
			(pin power_in line
				(at 6.35 -11.43 0)
				(length 7.62)
				(name "GND1")
				(number "6")
			)
			(pin unspecified line
				(at 6.35 -13.97 0)
				(length 7.62)
				(name "VIO")
				(number "7")
			)
			(pin unspecified line
				(at 6.35 -16.51 0)
				(length 7.62)
				(name "RXD")
				(number "8")
			)
			(pin unspecified line
				(at 6.35 -19.05 0)
				(length 7.62)
				(name "*RE")
				(number "9")
			)
		)
	)
	(symbol "ADP150"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 5.08 0)
		)
		(property "Value" "ADP150"
			(at 0 -5.08 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "ADP150_0_0"
			(pin power_in line
				(at -7.62 1.27 0)
				(length 2.54)
				(name "Vin")
				(number "1A")
			)
			(pin input line
				(at -7.62 -1.27 0)
				(length 2.54)
				(name "EN")
				(number "1B")
			)
			(pin power_out line
				(at 7.62 1.27 180)
				(length 2.54)
				(name "Vout")
				(number "2A")
			)
			(pin power_in line
				(at 7.62 -1.27 180)
				(length 2.54)
				(name "GND")
				(number "2B")
			)
		)
		(symbol "ADP150_0_1")
	)
	(symbol "ADS124S08IPBSR"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.2406 46.357 0)
		)
		(property "Value" "ADS124S08"
			(at -15.2672 -45.8017 0)
		)
		(property "Footprint" "ProjectDevices:ADS124S08_QFP50P700X700X120-32N"
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" "24bit ADC, 12 chan, PGA, differential, Sigma-Delta, 4Ksps, 32pin TQFP 5x5"
			(at 0 0 0)
		)
		(property "PartNum" "ADS124S08IPBSR"
			(at 0 0 0)
		)
		(property "VendorNum" ""
			(at 0 0 0)
		)
		(property "Vendor" ""
			(at 0 0 0)
		)
		(property "Subst" "No"
			(at 0 0 0)
		)
		(symbol "ADS124S08IPBSR_0_0"
			(pin input line
				(at -20.32 7.62 0)
				(length 5.08)
				(name "AINCOM")
				(number "1")
			)
			(pin input line
				(at -20.32 22.86 0)
				(length 5.08)
				(name "DIN")
				(number "10")
			)
			(pin input clock
				(at -20.32 25.4 0)
				(length 5.08)
				(name "SCLK")
				(number "11")
			)
			(pin output line
				(at -20.32 20.32 0)
				(length 5.08)
				(name "DOUT/~{DRDY}")
				(number "12")
			)
			(pin output line
				(at 20.32 20.32 180)
				(length 5.08)
				(name "~{DRDY}")
				(number "13")
			)
			(pin power_in line
				(at 20.32 -40.64 180)
				(length 5.08)
				(name "DGND")
				(number "14")
			)
			(pin power_in line
				(at 20.32 43.18 180)
				(length 5.08)
				(name "IOVDD")
				(number "15")
			)
			(pin power_in line
				(at 20.32 40.64 180)
				(length 5.08)
				(name "DVDD")
				(number "16")
			)
			(pin input clock
				(at -20.32 12.7 0)
				(length 5.08)
				(name "CLK")
				(number "17")
			)
			(pin input line
				(at -20.32 33.02 0)
				(length 5.08)
				(name "~{RESET}")
				(number "18")
			)
			(pin bidirectional line
				(at -20.32 -22.86 0)
				(length 5.08)
				(name "GPIO3/AIN11")
				(number "19")
			)
			(pin input line
				(at -20.32 -7.62 0)
				(length 5.08)
				(name "AIN5")
				(number "2")
			)
			(pin bidirectional line
				(at -20.32 -20.32 0)
				(length 5.08)
				(name "GPIO2/AIN10")
				(number "20")
			)
			(pin bidirectional line
				(at -20.32 -17.78 0)
				(length 5.08)
				(name "GPIO1/AIN9")
				(number "21")
			)
			(pin bidirectional line
				(at -20.32 -15.24 0)
				(length 5.08)
				(name "GPIO0/AIN8")
				(number "22")
			)
			(pin output line
				(at 20.32 33.02 180)
				(length 5.08)
				(name "REFOUT")
				(number "23")
			)
			(pin output line
				(at 20.32 30.48 180)
				(length 5.08)
				(name "REFCOM")
				(number "24")
			)
			(pin power_in line
				(at 20.32 38.1 180)
				(length 5.08)
				(name "AVDD")
				(number "26")
			)
			(pin power_in line
				(at 20.32 -38.1 180)
				(length 5.08)
				(name "AVSS")
				(number "27")
			)
			(pin power_in line
				(at 20.32 -35.56 180)
				(length 5.08)
				(name "AVSS-SW")
				(number "28")
			)
			(pin input line
				(at -20.32 -27.94 0)
				(length 5.08)
				(name "REFN0")
				(number "29")
			)
			(pin input line
				(at -20.32 -5.08 0)
				(length 5.08)
				(name "AIN4")
				(number "3")
			)
			(pin input line
				(at -20.32 -30.48 0)
				(length 5.08)
				(name "REFP0")
				(number "30")
			)
			(pin input line
				(at -20.32 -12.7 0)
				(length 5.08)
				(name "REFN1/AIN7")
				(number "31")
			)
			(pin input line
				(at -20.32 -10.16 0)
				(length 5.08)
				(name "REFP1/AIN6")
				(number "32")
			)
			(pin input line
				(at -20.32 -2.54 0)
				(length 5.08)
				(name "AIN3")
				(number "4")
			)
			(pin input line
				(at -20.32 0 0)
				(length 5.08)
				(name "AIN2")
				(number "5")
			)
			(pin input line
				(at -20.32 2.54 0)
				(length 5.08)
				(name "AIN1")
				(number "6")
			)
			(pin input line
				(at -20.32 5.08 0)
				(length 5.08)
				(name "AIN0")
				(number "7")
			)
			(pin input line
				(at -20.32 30.48 0)
				(length 5.08)
				(name "START/SYNC")
				(number "8")
			)
			(pin input line
				(at -20.32 27.94 0)
				(length 5.08)
				(name "~{CS}")
				(number "9")
			)
		)
	)
	(symbol "ADS4130-8"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 6.35 30.48 0)
		)
		(property "Value" "ADS4130-8"
			(at 6.35 27.94 0)
		)
		(property "Footprint" ""
			(at 0 10.16 0)
		)
		(property "Datasheet" ""
			(at 0 10.16 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "ADS4130-8_0_1")
		(symbol "ADS4130-8_1_1"
			(pin power_in line
				(at 25.4 22.86 180)
				(length 2.54)
				(name "AVDD")
				(number "A1")
			)
			(pin output line
				(at 25.4 -17.78 180)
				(length 2.54)
				(name "INT")
				(number "A2")
			)
			(pin input line
				(at 25.4 -5.08 180)
				(length 2.54)
				(name "DIN")
				(number "A3")
			)
			(pin bidirectional line
				(at 25.4 -7.62 180)
				(length 2.54)
				(name "SCLK")
				(number "A4")
			)
			(pin bidirectional line
				(at 25.4 -10.16 180)
				(length 2.54)
				(name "~{CS}")
				(number "A5")
			)
			(pin power_out line
				(at 25.4 20.32 180)
				(length 2.54)
				(name "RCAPA")
				(number "B1")
			)
			(pin input line
				(at 25.4 -15.24 180)
				(length 2.54)
				(name "~{SYNC}")
				(number "B2")
			)
			(pin output line
				(at 25.4 -2.54 180)
				(length 2.54)
				(name "DOUT")
				(number "B3")
			)
			(pin bidirectional line
				(at 25.4 -20.32 180)
				(length 2.54)
				(name "CLK")
				(number "B4")
			)
			(pin input line
				(at 25.4 15.24 180)
				(length 2.54)
				(name "IOVDD")
				(number "B5")
			)
			(pin power_in line
				(at 25.4 -25.4 180)
				(length 2.54)
				(name "AVSS")
				(number "C1")
			)
			(pin input line
				(at -15.24 -22.86 0)
				(length 2.54)
				(name "PSW")
				(number "C2")
			)
			(pin input line
				(at -15.24 -27.94 0)
				(length 2.54)
				(name "NC")
				(number "C3")
			)
			(pin input line
				(at -15.24 -30.48 0)
				(length 2.54)
				(name "NC")
				(number "C4")
			)
			(pin power_in line
				(at 25.4 -27.94 180)
				(length 2.54)
				(name "DGND")
				(number "C5")
			)
			(pin power_out line
				(at 25.4 7.62 180)
				(length 2.54)
				(name "REFOUT")
				(number "D1")
			)
			(pin bidirectional line
				(at -15.24 -12.7 0)
				(length 2.54)
				(name "A13/IO/VB")
				(number "D2")
			)
			(pin bidirectional line
				(at -15.24 0 0)
				(length 2.54)
				(name "A8/IO/VB")
				(number "D3")
			)
			(pin bidirectional line
				(at -15.24 15.24 0)
				(length 2.54)
				(name "A2/IO/VB/P1")
				(number "D4")
			)
			(pin power_out line
				(at 25.4 12.7 180)
				(length 2.54)
				(name "RCAPD")
				(number "D5")
			)
			(pin bidirectional line
				(at -15.24 -17.78 0)
				(length 2.54)
				(name "A15/IO/VB/REFIN2-")
				(number "E1")
			)
			(pin bidirectional line
				(at -15.24 -10.16 0)
				(length 2.54)
				(name "A12/IO/VB")
				(number "E2")
			)
			(pin bidirectional line
				(at -15.24 2.54 0)
				(length 2.54)
				(name "A7/IO/VB")
				(number "E3")
			)
			(pin bidirectional line
				(at -15.24 12.7 0)
				(length 2.54)
				(name "A3/IO/VB/P2")
				(number "E4")
			)
			(pin bidirectional line
				(at -15.24 20.32 0)
				(length 2.54)
				(name "A0/IO/VB")
				(number "E5")
			)
			(pin bidirectional line
				(at -15.24 -15.24 0)
				(length 2.54)
				(name "A14/IO/VB/REFIN2+")
				(number "F1")
			)
			(pin bidirectional line
				(at -15.24 -5.08 0)
				(length 2.54)
				(name "A10/IO/VB")
				(number "F2")
			)
			(pin input line
				(at 25.4 5.08 180)
				(length 2.54)
				(name "REFIN1+")
				(number "F3")
			)
			(pin bidirectional line
				(at -15.24 7.62 0)
				(length 2.54)
				(name "A5/IO/VB/P4")
				(number "F4")
			)
			(pin bidirectional line
				(at -15.24 17.78 0)
				(length 2.54)
				(name "A1/IO/VB")
				(number "F5")
			)
			(pin bidirectional line
				(at -15.24 -7.62 0)
				(length 2.54)
				(name "A11/IO/VB")
				(number "G1")
			)
			(pin bidirectional line
				(at -15.24 -2.54 0)
				(length 2.54)
				(name "A9/IO/VB")
				(number "G2")
			)
			(pin input line
				(at 25.4 2.54 180)
				(length 2.54)
				(name "REFIN1-")
				(number "G3")
			)
			(pin bidirectional line
				(at -15.24 5.08 0)
				(length 2.54)
				(name "A6/IO/VB")
				(number "G4")
			)
			(pin bidirectional line
				(at -15.24 10.16 0)
				(length 2.54)
				(name "A4/IO/VB/P3")
				(number "G5")
			)
		)
	)
	(symbol "ADUCM355BCCZ"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -22.86 81.28 0)
		)
		(property "Value" "ADUCM355BCCZ"
			(at -22.86 -81.28 0)
		)
		(property "Footprint" "LGA72S50P11X9_600X500X100N"
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(property "PARTREV" "A"
			(at 0 0 0)
		)
		(property "STANDARD" "IPC-7351B"
			(at 0 0 0)
		)
		(property "MAXIMUM_PACKAGE_HEIGHT" "1.0mm"
			(at 0 0 0)
		)
		(property "MANUFACTURER" "Analog Devices"
			(at 0 0 0)
		)
		(symbol "ADUCM355BCCZ_0_0"
			(pin input line
				(at -27.94 22.86 0)
				(length 5.08)
				(name "RE0")
				(number "A1")
			)
			(pin input line
				(at -27.94 -7.62 0)
				(length 5.08)
				(name "DE1")
				(number "A10")
			)
			(pin input line
				(at -27.94 -2.54 0)
				(length 5.08)
				(name "RE1")
				(number "A11")
			)
			(pin input line
				(at -27.94 17.78 0)
				(length 5.08)
				(name "DE0")
				(number "A2")
			)
			(pin input line
				(at -27.94 20.32 0)
				(length 5.08)
				(name "SE0")
				(number "A3")
			)
			(pin bidirectional line
				(at -27.94 -43.18 0)
				(length 5.08)
				(name "AIN4_LPF0")
				(number "A4")
			)
			(pin bidirectional line
				(at -27.94 -55.88 0)
				(length 5.08)
				(name "VREF_1.8V")
				(number "A5")
			)
			(pin input line
				(at -27.94 -27.94 0)
				(length 5.08)
				(name "RCAL1")
				(number "A6")
			)
			(pin input line
				(at -27.94 -25.4 0)
				(length 5.08)
				(name "RCAL0")
				(number "A7")
			)
			(pin bidirectional line
				(at -27.94 -50.8 0)
				(length 5.08)
				(name "AIN7_LPF1")
				(number "A8")
			)
			(pin input line
				(at -27.94 -5.08 0)
				(length 5.08)
				(name "SE1")
				(number "A9")
			)
			(pin bidirectional line
				(at -27.94 25.4 0)
				(length 5.08)
				(name "CE0")
				(number "B1")
			)
			(pin bidirectional line
				(at -27.94 -12.7 0)
				(length 5.08)
				(name "VZERO1")
				(number "B10")
			)
			(pin bidirectional line
				(at -27.94 0 0)
				(length 5.08)
				(name "CE1")
				(number "B11")
			)
			(pin bidirectional line
				(at -27.94 12.7 0)
				(length 5.08)
				(name "VZERO0")
				(number "B2")
			)
			(pin input line
				(at -27.94 -48.26 0)
				(length 5.08)
				(name "AIN6")
				(number "B3")
			)
			(pin input line
				(at -27.94 -45.72 0)
				(length 5.08)
				(name "AIN5")
				(number "B4")
			)
			(pin power_in line
				(at 27.94 -66.04 180)
				(length 5.08)
				(name "AGND_REF")
				(number "B5")
			)
			(pin input line
				(at -27.94 -38.1 0)
				(length 5.08)
				(name "AIN2")
				(number "B6")
			)
			(pin bidirectional line
				(at -27.94 -40.64 0)
				(length 5.08)
				(name "AIN3/BUF_VREF1V8")
				(number "B7")
			)
			(pin input line
				(at -27.94 -35.56 0)
				(length 5.08)
				(name "AIN1")
				(number "B8")
			)
			(pin input line
				(at -27.94 -33.02 0)
				(length 5.08)
				(name "AIN0")
				(number "B9")
			)
			(pin input line
				(at -27.94 5.08 0)
				(length 5.08)
				(name "CAP_POT0")
				(number "C1")
			)
			(pin bidirectional line
				(at -27.94 -10.16 0)
				(length 5.08)
				(name "VBIAS1")
				(number "C10")
			)
			(pin input line
				(at -27.94 -20.32 0)
				(length 5.08)
				(name "CAP_POT1")
				(number "C11")
			)
			(pin bidirectional line
				(at -27.94 15.24 0)
				(length 5.08)
				(name "VBIAS0")
				(number "C2")
			)
			(pin input line
				(at -27.94 10.16 0)
				(length 5.08)
				(name "RC0_0")
				(number "D1")
			)
			(pin input line
				(at -27.94 -15.24 0)
				(length 5.08)
				(name "RC1_0")
				(number "D10")
			)
			(pin input line
				(at -27.94 -17.78 0)
				(length 5.08)
				(name "RC1_1")
				(number "D11")
			)
			(pin input line
				(at -27.94 7.62 0)
				(length 5.08)
				(name "RC0_1")
				(number "D2")
			)
			(pin bidirectional line
				(at 27.94 0 180)
				(length 5.08)
				(name "BM/P1.1")
				(number "D5")
			)
			(pin bidirectional line
				(at 27.94 -10.16 180)
				(length 5.08)
				(name "P1.5/SPI1_~{CS}")
				(number "D6")
			)
			(pin bidirectional line
				(at 27.94 -5.08 180)
				(length 5.08)
				(name "P1.3/SPI1_MOSI")
				(number "D7")
			)
			(pin power_in line
				(at 27.94 60.96 180)
				(length 5.08)
				(name "AVDD_REG")
				(number "E1")
			)
			(pin bidirectional line
				(at -27.94 -60.96 0)
				(length 5.08)
				(name "ADCVBIAS_CAP")
				(number "E11")
			)
			(pin bidirectional line
				(at -27.94 -58.42 0)
				(length 5.08)
				(name "VREF_2.5V")
				(number "E2")
			)
			(pin bidirectional line
				(at 27.94 -2.54 180)
				(length 5.08)
				(name "P1.2/SPI1_CLK")
				(number "E7")
			)
			(pin power_in line
				(at 27.94 76.2 180)
				(length 5.08)
				(name "DVDD_AD")
				(number "F1")
			)
			(pin power_in line
				(at 27.94 -71.12 180)
				(length 5.08)
				(name "AGND")
				(number "F10")
			)
			(pin power_in line
				(at 27.94 63.5 180)
				(length 5.08)
				(name "AVDD")
				(number "F11")
			)
			(pin power_in line
				(at 27.94 -76.2 180)
				(length 5.08)
				(name "DGND_AD")
				(number "F2")
			)
			(pin bidirectional line
				(at 27.94 2.54 180)
				(length 5.08)
				(name "P1.0/SYS_WAKE")
				(number "F5")
			)
			(pin bidirectional line
				(at 27.94 -7.62 180)
				(length 5.08)
				(name "P1.4/SPI1_MISO")
				(number "F6")
			)
			(pin power_in line
				(at 27.94 -73.66 180)
				(length 5.08)
				(name "DGND")
				(number "F7")
			)
			(pin power_in line
				(at 27.94 68.58 180)
				(length 5.08)
				(name "DVDD_REG_AD")
				(number "G1")
			)
			(pin bidirectional line
				(at 27.94 -20.32 180)
				(length 5.08)
				(name "GPIO0/PWM0")
				(number "G10")
			)
			(pin power_in line
				(at 27.94 48.26 180)
				(length 5.08)
				(name "VDCDC_CAP2P")
				(number "G11")
			)
			(pin power_in line
				(at 27.94 66.04 180)
				(length 5.08)
				(name "AVDD_DD")
				(number "G2")
			)
			(pin input clock
				(at 27.94 -27.94 180)
				(length 5.08)
				(name "XTALI")
				(number "H1")
			)
			(pin bidirectional line
				(at 27.94 -22.86 180)
				(length 5.08)
				(name "GPIO1/PWM1")
				(number "H10")
			)
			(pin power_in line
				(at 27.94 45.72 180)
				(length 5.08)
				(name "VDCDC_CAP2N")
				(number "H11")
			)
			(pin power_in line
				(at 27.94 -68.58 180)
				(length 5.08)
				(name "AGND_DD")
				(number "H2")
			)
			(pin input clock
				(at -27.94 33.02 0)
				(length 5.08)
				(name "SWCLK")
				(number "H3")
			)
			(pin bidirectional line
				(at -27.94 30.48 0)
				(length 5.08)
				(name "SWDIO")
				(number "H4")
			)
			(pin bidirectional line
				(at 27.94 12.7 180)
				(length 5.08)
				(name "P0.5/I2C_SDA")
				(number "H5")
			)
			(pin bidirectional line
				(at 27.94 17.78 180)
				(length 5.08)
				(name "P0.3/SPI0_~{CS}")
				(number "H6")
			)
			(pin bidirectional line
				(at 27.94 20.32 180)
				(length 5.08)
				(name "P0.2/SPI0_MISO")
				(number "H7")
			)
			(pin bidirectional line
				(at 27.94 22.86 180)
				(length 5.08)
				(name "P0.1/SPI0_MOSI")
				(number "H8")
			)
			(pin bidirectional line
				(at 27.94 25.4 180)
				(length 5.08)
				(name "P0.0/SPI0_CLK")
				(number "H9")
			)
			(pin output clock
				(at 27.94 -30.48 180)
				(length 5.08)
				(name "XTALO")
				(number "J1")
			)
			(pin input line
				(at -27.94 35.56 0)
				(length 5.08)
				(name "~{RESET}")
				(number "J10")
			)
			(pin power_in line
				(at 27.94 40.64 180)
				(length 5.08)
				(name "VDCDC_CAPOUT")
				(number "J11")
			)
			(pin bidirectional line
				(at 27.94 7.62 180)
				(length 5.08)
				(name "P0.11/UART_SIN")
				(number "J2")
			)
			(pin bidirectional line
				(at 27.94 10.16 180)
				(length 5.08)
				(name "P0.10/UART_SOUT")
				(number "J3")
			)
			(pin bidirectional line
				(at 27.94 -15.24 180)
				(length 5.08)
				(name "P2.4")
				(number "J4")
			)
			(pin bidirectional line
				(at 27.94 15.24 180)
				(length 5.08)
				(name "P0.4/I2C_SCL")
				(number "J5")
			)
			(pin power_in line
				(at 27.94 73.66 180)
				(length 5.08)
				(name "DVDD")
				(number "J6")
			)
			(pin power_in line
				(at 27.94 71.12 180)
				(length 5.08)
				(name "DVDD_REG")
				(number "J7")
			)
			(pin power_in line
				(at 27.94 53.34 180)
				(length 5.08)
				(name "VDCDC_CAP1N")
				(number "J8")
			)
			(pin power_in line
				(at 27.94 55.88 180)
				(length 5.08)
				(name "VDCDC_CAP1P")
				(number "J9")
			)
		)
	)
	(symbol "AP2112K-3.3"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -5.08 8.89 0)
		)
		(property "Value" "AP2112K-3.3"
			(at 0 6.35 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "AP2112K-3.3_0_1")
		(symbol "AP2112K-3.3_1_1"
			(pin input line
				(at -8.89 2.54 0)
				(length 2.54)
				(name "VIN")
				(number "1")
			)
			(pin input line
				(at -8.89 0 0)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin input line
				(at -8.89 -2.54 0)
				(length 2.54)
				(name "EN")
				(number "3")
			)
			(pin input line
				(at 8.89 -2.54 180)
				(length 2.54)
				(name "NC")
				(number "4")
			)
			(pin input line
				(at 8.89 2.54 180)
				(length 2.54)
				(name "VOUT")
				(number "5")
			)
		)
	)
	(symbol "ATP304"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "Q"
			(at 3.81 1.27 0)
		)
		(property "Value" "ATP304"
			(at 6.35 -1.27 0)
		)
		(property "Footprint" ""
			(at -10.16 1.27 0)
		)
		(property "Datasheet" ""
			(at -10.16 1.27 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "ATP304_1_1"
			(pin bidirectional line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "G")
				(number "1")
			)
			(pin bidirectional line
				(at 0 5.08 270)
				(length 2.54)
				(name "D")
				(number "2")
			)
			(pin bidirectional line
				(at 0 -5.08 90)
				(length 2.54)
				(name "S")
				(number "3")
			)
		)
	)
	(symbol "Adafruit_BME280"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 7.62 0)
		)
		(property "Value" "Adafruit_BME280"
			(at 0 -15.24 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "Adafruit_BME280_0_1")
		(symbol "Adafruit_BME280_1_1"
			(pin bidirectional line
				(at -10.16 3.81 0)
				(length 2.54)
				(name "Vin")
				(number "1")
			)
			(pin bidirectional line
				(at -10.16 1.27 0)
				(length 2.54)
				(name "3Vo")
				(number "2")
			)
			(pin bidirectional line
				(at -10.16 -1.27 0)
				(length 2.54)
				(name "Gnd")
				(number "3")
			)
			(pin bidirectional line
				(at -10.16 -3.81 0)
				(length 2.54)
				(name "SCK")
				(number "4")
			)
			(pin bidirectional line
				(at -10.16 -6.35 0)
				(length 2.54)
				(name "SDO")
				(number "5")
			)
			(pin bidirectional line
				(at -10.16 -8.89 0)
				(length 2.54)
				(name "SDI")
				(number "6")
			)
			(pin bidirectional line
				(at -10.16 -11.43 0)
				(length 2.54)
				(name "CS")
				(number "7")
			)
		)
	)
	(symbol "Adafruit_INA260"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 8.89 11.43 0)
		)
		(property "Value" "Adafruit_INA260"
			(at -2.54 11.43 0)
		)
		(property "Footprint" ""
			(at -3.81 2.54 0)
		)
		(property "Datasheet" ""
			(at -3.81 2.54 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "Adafruit_INA260_0_1")
		(symbol "Adafruit_INA260_1_1"
			(pin bidirectional line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "Vcc")
				(number "1")
			)
			(pin bidirectional line
				(at -12.7 0 0)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin bidirectional line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "SCL")
				(number "3")
			)
			(pin bidirectional line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "SDA")
				(number "4")
			)
			(pin bidirectional line
				(at -12.7 -7.62 0)
				(length 2.54)
				(name "ALERT")
				(number "5")
			)
			(pin bidirectional line
				(at -12.7 -10.16 0)
				(length 2.54)
				(name "Vbus")
				(number "6")
			)
			(pin bidirectional line
				(at -12.7 7.62 0)
				(length 2.54)
				(name "Vin+")
				(number "7")
			)
			(pin bidirectional line
				(at 12.7 7.62 180)
				(length 2.54)
				(name "Vin-")
				(number "8")
			)
		)
	)
	(symbol "B82559B2102A027"
		(pin_names
			(offset 0.254) hide)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "L"
			(at 16.51 10.16 0)
		)
		(property "Value" "B82559B2102A027"
			(at 16.51 7.62 0)
		)
		(property "Footprint" "B82559B_TDK"
			(at 16.51 6.096 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_fp_filters" "B82559B_TDK B82559B_TDK-M B82559B_TDK-L"
			(at 0 0 0)
		)
		(symbol "B82559B2102A027_1_1"
			(pin bidirectional line
				(at 0 0 0)
				(length 7.62)
				(name "1")
				(number "1")
			)
			(pin bidirectional line
				(at 33.02 0 180)
				(length 7.62)
				(name "2")
				(number "2")
			)
			(pin bidirectional line
				(at 33.02 2.54 180)
				(length 7.62)
				(name "3")
				(number "3")
			)
		)
	)
	(symbol "BAS21"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 0 0)
		)
		(property "Value" "BAS21"
			(at 0 0 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "BAS21_0_1")
		(symbol "BAS21_1_1"
			(pin passive line
				(at 3.81 0 180)
				(length 2.54)
				(name "A")
				(number "A")
			)
			(pin passive line
				(at -3.81 0 0)
				(length 2.54)
				(name "K")
				(number "K")
			)
		)
	)
	(symbol "BD5232G"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 12.7 0)
		)
		(property "Value" "BD5232G"
			(at 0 10.16 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "BD5232G_0_1")
		(symbol "BD5232G_1_1"
			(pin output line
				(at -8.89 5.08 0)
				(length 2.54)
				(name "~{RST}")
				(number "1")
			)
			(pin power_in line
				(at -8.89 2.54 0)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin input line
				(at -8.89 0 0)
				(length 2.54)
				(name "Ct")
				(number "3")
			)
			(pin power_in line
				(at 8.89 1.27 180)
				(length 2.54)
				(name "GND")
				(number "4")
			)
			(pin power_in line
				(at 8.89 3.81 180)
				(length 2.54)
				(name "VDD")
				(number "5")
			)
		)
	)
	(symbol "BGS13S4N8"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 2.54 7.62 0)
		)
		(property "Value" "BGS13S4N8"
			(at 7.62 -7.62 0)
		)
		(property "Footprint" "ProjectDevices:BGS13SN8"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.infineon.com/dgdl/Infineon-BGS13SN8-DS-v02_02-EN.pdf"
			(at 0 15.24 0)
		)
		(property "Description" "Infineon RF SWITCH SP3T 6GHZ TSNP8-1"
			(at 0 0 0)
		)
		(symbol "BGS13S4N8_1_1"
			(pin passive line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "V1")
				(number "1")
			)
			(pin passive line
				(at -10.16 0 0)
				(length 2.54)
				(name "RF3")
				(number "2")
			)
			(pin passive line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "RF1")
				(number "3")
			)
			(pin passive line
				(at 0 -7.62 90)
				(length 2.54)
				(name "RFIN")
				(number "4")
			)
			(pin passive line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "RF2")
				(number "5")
			)
			(pin passive line
				(at 10.16 0 180)
				(length 2.54)
				(name "DGND")
				(number "6")
			)
			(pin passive line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "VCC")
				(number "7")
			)
			(pin passive line
				(at 0 7.62 270)
				(length 2.54)
				(name "V2")
				(number "8")
			)
		)
	)
	(symbol "BME280"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 5.08 8.89 0)
		)
		(property "Value" "BME280"
			(at -2.54 8.89 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "BME280_0_1")
		(symbol "BME280_1_1"
			(pin power_in line
				(at -12.7 5.08 0)
				(length 5.08)
				(name "GND")
				(number "1")
			)
			(pin input line
				(at -12.7 2.54 0)
				(length 5.08)
				(name "CSB")
				(number "2")
			)
			(pin bidirectional line
				(at -12.7 0 0)
				(length 5.08)
				(name "SDI")
				(number "3")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 5.08)
				(name "SCK")
				(number "4")
			)
			(pin bidirectional line
				(at 12.7 -2.54 180)
				(length 5.08)
				(name "SDO")
				(number "5")
			)
			(pin power_in line
				(at 12.7 0 180)
				(length 5.08)
				(name "VDDIO")
				(number "6")
			)
			(pin power_in line
				(at 12.7 2.54 180)
				(length 5.08)
				(name "GND")
				(number "7")
			)
			(pin power_in line
				(at 12.7 5.08 180)
				(length 5.08)
				(name "VDD")
				(number "8")
			)
		)
	)
	(symbol "BQ24040DSQR"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -10.16 7.35 0)
		)
		(property "Value" "BQ24040DSQR"
			(at 0 7.62 0)
		)
		(property "Footprint" "ProjectFootprints:BQ2040_SON40P200X200X80-11N"
			(at 0 34.29 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/bq24040.pdf"
			(at 3.81 -10.16 0)
		)
		(property "Description" "IC BATT CHG LI-ION 1CELL 10SON"
			(at 2.54 -1.27 0)
		)
		(symbol "BQ24040DSQR_0_0"
			(pin input line
				(at -13.97 3.81 0)
				(length 5.08)
				(name "IN")
				(number "1")
			)
			(pin output line
				(at 13.97 3.81 180)
				(length 5.08)
				(name "OUT")
				(number "10")
			)
			(pin power_in line
				(at 0 -13.97 90)
				(length 5.08)
				(name "EXP")
				(number "11")
			)
			(pin input line
				(at -13.97 1.27 0)
				(length 5.08)
				(name "ISET")
				(number "2")
			)
			(pin power_in line
				(at -13.97 -1.27 0)
				(length 5.08)
				(name "VSS")
				(number "3")
			)
			(pin input line
				(at -13.97 -3.81 0)
				(length 5.08)
				(name "PRETERM")
				(number "4")
			)
			(pin output line
				(at -13.97 -6.35 0)
				(length 5.08)
				(name "~{PG}")
				(number "5")
			)
			(pin input line
				(at 13.97 -6.35 180)
				(length 5.08)
				(name "NC")
				(number "6")
			)
			(pin input line
				(at 13.97 -3.81 180)
				(length 5.08)
				(name "ISET2")
				(number "7")
			)
			(pin output line
				(at 13.97 -1.27 180)
				(length 5.08)
				(name "~{CHG}")
				(number "8")
			)
			(pin input line
				(at 13.97 1.27 180)
				(length 5.08)
				(name "TS")
				(number "9")
			)
		)
	)
	(symbol "BTT6050-1ERA"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 3.81 13.97 0)
		)
		(property "Value" "BTT6050-1ERA"
			(at 0 -8.89 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "BTT6050-1ERA_0_1")
		(symbol "BTT6050-1ERA_1_1"
			(pin passive line
				(at -7.62 10.16 0)
				(length 2.54)
				(name "NC")
				(number "1")
			)
			(pin output line
				(at 7.62 0 180)
				(length 2.54)
				(name "OUT")
				(number "10")
			)
			(pin output line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "OUT")
				(number "11")
			)
			(pin output line
				(at 7.62 5.08 180)
				(length 2.54)
				(name "OUT")
				(number "12")
			)
			(pin passive line
				(at 7.62 7.62 180)
				(length 2.54)
				(name "NC")
				(number "13")
			)
			(pin passive line
				(at 7.62 10.16 180)
				(length 2.54)
				(name "NC")
				(number "14")
			)
			(pin input line
				(at 0 15.24 270)
				(length 2.54)
				(name "VS")
				(number "15")
			)
			(pin passive line
				(at -7.62 7.62 0)
				(length 2.54)
				(name "NC")
				(number "2")
			)
			(pin passive line
				(at -7.62 5.08 0)
				(length 2.54)
				(name "GND")
				(number "3")
			)
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "IN")
				(number "4")
			)
			(pin input line
				(at -7.62 0 0)
				(length 2.54)
				(name "DEN")
				(number "5")
			)
			(pin output line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "IS")
				(number "6")
			)
			(pin passive line
				(at -7.62 -5.08 0)
				(length 2.54)
				(name "NC")
				(number "7")
			)
			(pin passive line
				(at 7.62 -5.08 180)
				(length 2.54)
				(name "NC")
				(number "8")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 2.54)
				(name "NC")
				(number "9")
			)
		)
	)
	(symbol "BTT6200-4ESA"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 17.78 0)
		)
		(property "Value" "BTT6200-4ESA"
			(at 7.62 17.78 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "BTT6200-4ESA_0_1")
		(symbol "BTT6200-4ESA_1_1"
			(pin input line
				(at -12.7 12.7 0)
				(length 2.54)
				(name "NC")
				(number "1")
			)
			(pin input line
				(at -12.7 -10.16 0)
				(length 2.54)
				(name "IN3")
				(number "10")
			)
			(pin input line
				(at -12.7 -12.7 0)
				(length 2.54)
				(name "DSEL1")
				(number "11")
			)
			(pin input line
				(at -12.7 -15.24 0)
				(length 2.54)
				(name "NC")
				(number "12")
			)
			(pin output line
				(at 11.43 -15.24 180)
				(length 2.54)
				(name "OUT3")
				(number "13")
			)
			(pin input line
				(at 11.43 -12.7 180)
				(length 2.54)
				(name "NC")
				(number "14")
			)
			(pin input line
				(at 11.43 -10.16 180)
				(length 2.54)
				(name "NC")
				(number "15")
			)
			(pin input line
				(at 11.43 -7.62 180)
				(length 2.54)
				(name "NC")
				(number "16")
			)
			(pin output line
				(at 11.43 -5.08 180)
				(length 2.54)
				(name "OUT2")
				(number "17")
			)
			(pin input line
				(at 11.43 -2.54 180)
				(length 2.54)
				(name "NC")
				(number "18")
			)
			(pin input line
				(at 11.43 0 180)
				(length 2.54)
				(name "NC")
				(number "19")
			)
			(pin input line
				(at -12.7 10.16 0)
				(length 2.54)
				(name "IN0")
				(number "2")
			)
			(pin output line
				(at 11.43 2.54 180)
				(length 2.54)
				(name "OUT1")
				(number "20")
			)
			(pin input line
				(at 11.43 5.08 180)
				(length 2.54)
				(name "NC")
				(number "21")
			)
			(pin input line
				(at 11.43 7.62 180)
				(length 2.54)
				(name "NC")
				(number "22")
			)
			(pin input line
				(at 11.43 10.16 180)
				(length 2.54)
				(name "NC")
				(number "23")
			)
			(pin output line
				(at 11.43 12.7 180)
				(length 2.54)
				(name "OUT0")
				(number "24")
			)
			(pin input line
				(at -1.27 19.05 270)
				(length 2.54)
				(name "VS")
				(number "25")
			)
			(pin input line
				(at -12.7 7.62 0)
				(length 2.54)
				(name "NC")
				(number "3")
			)
			(pin input line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "GND")
				(number "4")
			)
			(pin input line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "IN1")
				(number "5")
			)
			(pin input line
				(at -12.7 0 0)
				(length 2.54)
				(name "DEN")
				(number "6")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "IS")
				(number "7")
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "DSEL0")
				(number "8")
			)
			(pin input line
				(at -12.7 -7.62 0)
				(length 2.54)
				(name "IN2")
				(number "9")
			)
		)
	)
	(symbol "CR2032_tabthruhole"
		(pin_numbers hide)
		(pin_names
			(offset 1.651) hide)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "B"
			(at 4.826 3.81 0)
		)
		(property "Value" "CR2032_tabthruhole"
			(at 3.81 -7.62 0)
		)
		(property "Footprint" "BAT_CR-2032_PAN"
			(at 3.81 -9.144 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(property "ki_fp_filters" "BAT_CR-2032_PAN"
			(at 0 0 0)
		)
		(symbol "CR2032_tabthruhole_0_1"
			(pin power_out line
				(at 0 0 0)
				(length 2.54)
				(name "Pos")
				(number "2")
			)
		)
		(symbol "CR2032_tabthruhole_1_1"
			(pin power_out line
				(at 10.16 0 180)
				(length 2.54)
				(name "Neg")
				(number "1")
			)
		)
	)
	(symbol "CVS-04TB"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "SW"
			(at 1.27 8.89 0)
		)
		(property "Value" "CVS-04TB"
			(at 1.27 6.35 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "CVS-04TB_0_1")
		(symbol "CVS-04TB_1_1"
			(pin input line
				(at -5.08 2.54 0)
				(length 2.54)
				(name "~")
				(number "1")
			)
			(pin input line
				(at -5.08 0 0)
				(length 2.54)
				(name "~")
				(number "2")
			)
			(pin input line
				(at -5.08 -2.54 0)
				(length 2.54)
				(name "~")
				(number "3")
			)
			(pin input line
				(at -5.08 -5.08 0)
				(length 2.54)
				(name "~")
				(number "4")
			)
			(pin input line
				(at 5.08 -5.08 180)
				(length 2.54)
				(name "~")
				(number "5")
			)
			(pin input line
				(at 5.08 -2.54 180)
				(length 2.54)
				(name "~")
				(number "6")
			)
			(pin input line
				(at 5.08 0 180)
				(length 2.54)
				(name "~")
				(number "7")
			)
			(pin input line
				(at 5.08 2.54 180)
				(length 2.54)
				(name "~")
				(number "8")
			)
		)
	)
	(symbol "CY62148"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 0 0)
		)
		(property "Value" ""
			(at 0 0 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "CY62148_1_0"
			(pin input line
				(at -17.78 -12.7 0)
				(length 2.54)
				(name "")
				(number "10")
			)
			(pin input line
				(at -17.78 -15.24 0)
				(length 2.54)
				(name "")
				(number "11")
			)
			(pin input line
				(at -17.78 -17.78 0)
				(length 2.54)
				(name "")
				(number "12")
			)
			(pin input line
				(at -17.78 -20.32 0)
				(length 2.54)
				(name "")
				(number "13")
			)
			(pin input line
				(at -17.78 -22.86 0)
				(length 2.54)
				(name "")
				(number "14")
			)
			(pin input line
				(at -17.78 -25.4 0)
				(length 2.54)
				(name "")
				(number "15")
			)
			(pin input line
				(at -17.78 -27.94 0)
				(length 2.54)
				(name "")
				(number "16")
			)
			(pin input line
				(at 0 -27.94 180)
				(length 2.54)
				(name "")
				(number "17")
			)
			(pin input line
				(at 0 -25.4 180)
				(length 2.54)
				(name "")
				(number "18")
			)
			(pin input line
				(at 0 -22.86 180)
				(length 2.54)
				(name "")
				(number "19")
			)
			(pin input line
				(at -17.78 7.62 0)
				(length 2.54)
				(name "")
				(number "2")
			)
			(pin input line
				(at 0 -20.32 180)
				(length 2.54)
				(name "")
				(number "20")
			)
			(pin input line
				(at 0 -17.78 180)
				(length 2.54)
				(name "")
				(number "21")
			)
			(pin input line
				(at 0 -15.24 180)
				(length 2.54)
				(name "")
				(number "22")
			)
			(pin input line
				(at 0 -12.7 180)
				(length 2.54)
				(name "")
				(number "23")
			)
			(pin input line
				(at 0 -10.16 180)
				(length 2.54)
				(name "")
				(number "24")
			)
			(pin input line
				(at 0 -7.62 180)
				(length 2.54)
				(name "")
				(number "25")
			)
			(pin input line
				(at 0 -5.08 180)
				(length 2.54)
				(name "")
				(number "26")
			)
			(pin input line
				(at 0 -2.54 180)
				(length 2.54)
				(name "")
				(number "27")
			)
			(pin input line
				(at 0 0 180)
				(length 2.54)
				(name "")
				(number "28")
			)
			(pin input line
				(at 0 2.54 180)
				(length 2.54)
				(name "")
				(number "29")
			)
			(pin input line
				(at -17.78 5.08 0)
				(length 2.54)
				(name "")
				(number "3")
			)
			(pin input line
				(at 0 5.08 180)
				(length 2.54)
				(name "")
				(number "30")
			)
			(pin input line
				(at 0 7.62 180)
				(length 2.54)
				(name "")
				(number "31")
			)
			(pin input line
				(at 0 10.16 180)
				(length 2.54)
				(name "")
				(number "32")
			)
			(pin input line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "")
				(number "4")
			)
			(pin input line
				(at -17.78 0 0)
				(length 2.54)
				(name "")
				(number "5")
			)
			(pin input line
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "")
				(number "6")
			)
			(pin input line
				(at -17.78 -5.08 0)
				(length 2.54)
				(name "")
				(number "7")
			)
			(pin input line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "")
				(number "8")
			)
			(pin input line
				(at -17.78 -10.16 0)
				(length 2.54)
				(name "")
				(number "9")
			)
		)
		(symbol "CY62148_1_1"
			(pin input line
				(at -17.78 10.16 0)
				(length 2.54)
				(name "1")
				(number "1")
			)
		)
	)
	(symbol "ChargR_ltc4162_v1"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "M"
			(at 13.97 22.86 0)
		)
		(property "Value" "ChargR_ltc4162_v1"
			(at 0 11.43 0)
		)
		(property "Footprint" ""
			(at -6.35 1.27 90)
		)
		(property "Datasheet" ""
			(at -6.35 1.27 90)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "ChargR_ltc4162_v1_0_1")
		(symbol "ChargR_ltc4162_v1_1_1"
			(pin power_in line
				(at -11.43 25.4 270)
				(length 2.54)
				(name "Gnd")
				(number "1")
			)
			(pin bidirectional line
				(at 6.35 -10.16 90)
				(length 2.54)
				(name "~{SMBALERT}")
				(number "10")
			)
			(pin power_out line
				(at 3.81 -10.16 90)
				(length 2.54)
				(name "Vout")
				(number "11")
			)
			(pin power_out line
				(at 1.27 -10.16 90)
				(length 2.54)
				(name "Vout")
				(number "12")
			)
			(pin power_out line
				(at -1.27 -10.16 90)
				(length 2.54)
				(name "Vbat")
				(number "13")
			)
			(pin power_out line
				(at -3.81 -10.16 90)
				(length 2.54)
				(name "Vbat")
				(number "14")
			)
			(pin power_in line
				(at -6.35 -10.16 90)
				(length 2.54)
				(name "Gnd")
				(number "15")
			)
			(pin power_in line
				(at -8.89 -10.16 90)
				(length 2.54)
				(name "Gnd")
				(number "16")
			)
			(pin power_in line
				(at 13.97 3.81 180)
				(length 2.54)
				(name "GND")
				(number "17")
			)
			(pin power_in line
				(at 13.97 6.35 180)
				(length 2.54)
				(name "4S_BAT")
				(number "18")
			)
			(pin power_in line
				(at -8.89 25.4 270)
				(length 2.54)
				(name "Gnd")
				(number "2")
			)
			(pin power_in line
				(at -6.35 25.4 270)
				(length 2.54)
				(name "Vin")
				(number "3")
			)
			(pin power_in line
				(at -3.81 25.4 270)
				(length 2.54)
				(name "Vin")
				(number "4")
			)
			(pin bidirectional line
				(at -1.27 25.4 270)
				(length 2.54)
				(name "SDA")
				(number "5")
			)
			(pin bidirectional line
				(at 1.27 25.4 270)
				(length 2.54)
				(name "SCL")
				(number "6")
			)
			(pin power_in line
				(at 3.81 25.4 270)
				(length 2.54)
				(name "DVcc")
				(number "7")
			)
			(pin input line
				(at 6.35 25.4 270)
				(length 2.54)
				(name "A0")
				(number "8")
			)
			(pin input line
				(at 8.89 25.4 270)
				(length 2.54)
				(name "A1")
				(number "9")
			)
		)
	)
	(symbol "ChargR_ltc4162_v2"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 1.27 0)
		)
		(property "Value" "ChargR_ltc4162_v2"
			(at 1.27 -2.54 0)
		)
		(property "Footprint" ""
			(at -3.81 1.27 0)
		)
		(property "Datasheet" ""
			(at -3.81 1.27 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "ChargR_ltc4162_v2_0_0"
			(text "1"
				(at 7.366 7.366 0)
			)
			(text "12"
				(at -7.874 5.334 0)
			)
			(text "13"
				(at -7.874 -9.906 0)
			)
			(text "18"
				(at 7.366 -9.906 0)
			)
			(text "2"
				(at 7.366 5.334 0)
			)
			(text "3"
				(at 4.318 7.366 0)
			)
		)
		(symbol "ChargR_ltc4162_v2_0_1")
		(symbol "ChargR_ltc4162_v2_1_1"
			(pin power_in line
				(at 13.97 16.51 270)
				(length 2.54)
				(name "Gnd")
				(number "1")
			)
			(pin bidirectional line
				(at -8.89 16.51 270)
				(length 2.54)
				(name "SCL")
				(number "10")
			)
			(pin output line
				(at -11.43 16.51 270)
				(length 2.54)
				(name "~{SMBALERT}")
				(number "11")
			)
			(pin bidirectional line
				(at -13.97 16.51 270)
				(length 2.54)
				(name "SDA")
				(number "12")
			)
			(pin power_out line
				(at -6.35 -19.05 90)
				(length 2.54)
				(name "Vout")
				(number "13")
			)
			(pin power_out line
				(at -3.81 -19.05 90)
				(length 2.54)
				(name "Vout")
				(number "14")
			)
			(pin power_out line
				(at -1.27 -19.05 90)
				(length 2.54)
				(name "Vout")
				(number "15")
			)
			(pin power_in line
				(at 1.27 -19.05 90)
				(length 2.54)
				(name "Gnd")
				(number "16")
			)
			(pin power_in line
				(at 3.81 -19.05 90)
				(length 2.54)
				(name "Gnd")
				(number "17")
			)
			(pin power_in line
				(at 6.35 -19.05 90)
				(length 2.54)
				(name "Gnd")
				(number "18")
			)
			(pin power_in line
				(at 11.43 -19.05 90)
				(length 2.54)
				(name "H1")
				(number "19")
			)
			(pin power_in line
				(at 11.43 16.51 270)
				(length 2.54)
				(name "Gnd")
				(number "2")
			)
			(pin power_in line
				(at 13.97 -19.05 90)
				(length 2.54)
				(name "H2")
				(number "20")
			)
			(pin power_in line
				(at 8.89 16.51 270)
				(length 2.54)
				(name "Vin")
				(number "3")
			)
			(pin power_in line
				(at 6.35 16.51 270)
				(length 2.54)
				(name "Vin")
				(number "4")
			)
			(pin power_in line
				(at 3.81 16.51 270)
				(length 2.54)
				(name "Vbat")
				(number "5")
			)
			(pin power_in line
				(at 1.27 16.51 270)
				(length 2.54)
				(name "Vbat")
				(number "6")
			)
			(pin power_in line
				(at -1.27 16.51 270)
				(length 2.54)
				(name "Gnd")
				(number "7")
			)
			(pin power_in line
				(at -3.81 16.51 270)
				(length 2.54)
				(name "Gnd")
				(number "8")
			)
			(pin power_in line
				(at -6.35 16.51 270)
				(length 2.54)
				(name "DVcc")
				(number "9")
			)
		)
	)
	(symbol "Conn_01x03_02"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 0 0 0)
		)
		(property "Value" "Conn_01x03_02"
			(at 0 0 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "Conn_01x03_02_0_1")
		(symbol "Conn_01x03_02_1_1"
			(pin input line
				(at -2.54 2.54 0)
				(length 2.54)
				(name "1")
				(number "1")
			)
			(pin input line
				(at -2.54 -3.81 0)
				(length 2.54)
				(name "3")
				(number "3")
			)
		)
	)
	(symbol "Conn_02x50"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 67.31 0)
		)
		(property "Value" "Conn_02x50"
			(at 0 64.77 0)
		)
		(property "Footprint" ""
			(at 0 17.78 0)
		)
		(property "Datasheet" ""
			(at 0 17.78 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "Conn_02x50_1_1"
			(pin passive line
				(at -6.35 62.23 0)
				(length 3.81)
				(name "Pin_1")
				(number "1")
			)
			(pin passive line
				(at 6.35 52.07 180)
				(length 3.81)
				(name "Pin_10")
				(number "10")
			)
			(pin passive line
				(at 6.35 -62.23 180)
				(length 3.81)
				(name "Pin_100")
				(number "100")
			)
			(pin passive line
				(at -6.35 49.53 0)
				(length 3.81)
				(name "Pin_11")
				(number "11")
			)
			(pin passive line
				(at 6.35 49.53 180)
				(length 3.81)
				(name "Pin_12")
				(number "12")
			)
			(pin passive line
				(at -6.35 46.99 0)
				(length 3.81)
				(name "Pin_13")
				(number "13")
			)
			(pin passive line
				(at 6.35 46.99 180)
				(length 3.81)
				(name "Pin_14")
				(number "14")
			)
			(pin passive line
				(at -6.35 44.45 0)
				(length 3.81)
				(name "Pin_15")
				(number "15")
			)
			(pin passive line
				(at 6.35 44.45 180)
				(length 3.81)
				(name "Pin_16")
				(number "16")
			)
			(pin passive line
				(at -6.35 41.91 0)
				(length 3.81)
				(name "Pin_17")
				(number "17")
			)
			(pin passive line
				(at 6.35 41.91 180)
				(length 3.81)
				(name "Pin_18")
				(number "18")
			)
			(pin passive line
				(at -6.35 39.37 0)
				(length 3.81)
				(name "Pin_19")
				(number "19")
			)
			(pin passive line
				(at 6.35 62.23 180)
				(length 3.81)
				(name "Pin_2")
				(number "2")
			)
			(pin passive line
				(at 6.35 39.37 180)
				(length 3.81)
				(name "Pin_20")
				(number "20")
			)
			(pin passive line
				(at -6.35 36.83 0)
				(length 3.81)
				(name "Pin_21")
				(number "21")
			)
			(pin passive line
				(at 6.35 36.83 180)
				(length 3.81)
				(name "Pin_22")
				(number "22")
			)
			(pin passive line
				(at -6.35 34.29 0)
				(length 3.81)
				(name "Pin_23")
				(number "23")
			)
			(pin passive line
				(at 6.35 34.29 180)
				(length 3.81)
				(name "Pin_24")
				(number "24")
			)
			(pin passive line
				(at -6.35 31.75 0)
				(length 3.81)
				(name "Pin_25")
				(number "25")
			)
			(pin passive line
				(at 6.35 31.75 180)
				(length 3.81)
				(name "Pin_26")
				(number "26")
			)
			(pin passive line
				(at -6.35 29.21 0)
				(length 3.81)
				(name "Pin_27")
				(number "27")
			)
			(pin passive line
				(at 6.35 29.21 180)
				(length 3.81)
				(name "Pin_28")
				(number "28")
			)
			(pin passive line
				(at -6.35 26.67 0)
				(length 3.81)
				(name "Pin_29")
				(number "29")
			)
			(pin passive line
				(at -6.35 59.69 0)
				(length 3.81)
				(name "Pin_3")
				(number "3")
			)
			(pin passive line
				(at 6.35 26.67 180)
				(length 3.81)
				(name "Pin_30")
				(number "30")
			)
			(pin passive line
				(at -6.35 24.13 0)
				(length 3.81)
				(name "Pin_31")
				(number "31")
			)
			(pin passive line
				(at 6.35 24.13 180)
				(length 3.81)
				(name "Pin_32")
				(number "32")
			)
			(pin passive line
				(at -6.35 21.59 0)
				(length 3.81)
				(name "Pin_33")
				(number "33")
			)
			(pin passive line
				(at 6.35 21.59 180)
				(length 3.81)
				(name "Pin_34")
				(number "34")
			)
			(pin passive line
				(at -6.35 19.05 0)
				(length 3.81)
				(name "Pin_35")
				(number "35")
			)
			(pin passive line
				(at 6.35 19.05 180)
				(length 3.81)
				(name "Pin_36")
				(number "36")
			)
			(pin passive line
				(at -6.35 16.51 0)
				(length 3.81)
				(name "Pin_37")
				(number "37")
			)
			(pin passive line
				(at 6.35 16.51 180)
				(length 3.81)
				(name "Pin_38")
				(number "38")
			)
			(pin passive line
				(at -6.35 13.97 0)
				(length 3.81)
				(name "Pin_39")
				(number "39")
			)
			(pin passive line
				(at 6.35 59.69 180)
				(length 3.81)
				(name "Pin_4")
				(number "4")
			)
			(pin passive line
				(at 6.35 13.97 180)
				(length 3.81)
				(name "Pin_40")
				(number "40")
			)
			(pin passive line
				(at -6.35 11.43 0)
				(length 3.81)
				(name "Pin_41")
				(number "41")
			)
			(pin passive line
				(at 6.35 11.43 180)
				(length 3.81)
				(name "Pin_42")
				(number "42")
			)
			(pin passive line
				(at -6.35 8.89 0)
				(length 3.81)
				(name "Pin_43")
				(number "43")
			)
			(pin passive line
				(at 6.35 8.89 180)
				(length 3.81)
				(name "Pin_44")
				(number "44")
			)
			(pin passive line
				(at -6.35 6.35 0)
				(length 3.81)
				(name "Pin_45")
				(number "45")
			)
			(pin passive line
				(at 6.35 6.35 180)
				(length 3.81)
				(name "Pin_46")
				(number "46")
			)
			(pin passive line
				(at -6.35 3.81 0)
				(length 3.81)
				(name "Pin_47")
				(number "47")
			)
			(pin passive line
				(at 6.35 3.81 180)
				(length 3.81)
				(name "Pin_48")
				(number "48")
			)
			(pin passive line
				(at -6.35 1.27 0)
				(length 3.81)
				(name "Pin_49")
				(number "49")
			)
			(pin passive line
				(at -6.35 57.15 0)
				(length 3.81)
				(name "Pin_5")
				(number "5")
			)
			(pin passive line
				(at 6.35 1.27 180)
				(length 3.81)
				(name "Pin_50")
				(number "50")
			)
			(pin passive line
				(at -6.35 -1.27 0)
				(length 3.81)
				(name "Pin_51")
				(number "51")
			)
			(pin passive line
				(at 6.35 -1.27 180)
				(length 3.81)
				(name "Pin_52")
				(number "52")
			)
			(pin passive line
				(at -6.35 -3.81 0)
				(length 3.81)
				(name "Pin_53")
				(number "53")
			)
			(pin passive line
				(at 6.35 -3.81 180)
				(length 3.81)
				(name "Pin_54")
				(number "54")
			)
			(pin passive line
				(at -6.35 -6.35 0)
				(length 3.81)
				(name "Pin_55")
				(number "55")
			)
			(pin passive line
				(at 6.35 -6.35 180)
				(length 3.81)
				(name "Pin_56")
				(number "56")
			)
			(pin passive line
				(at -6.35 -8.89 0)
				(length 3.81)
				(name "Pin_57")
				(number "57")
			)
			(pin passive line
				(at 6.35 -8.89 180)
				(length 3.81)
				(name "Pin_58")
				(number "58")
			)
			(pin passive line
				(at -6.35 -11.43 0)
				(length 3.81)
				(name "Pin_59")
				(number "59")
			)
			(pin passive line
				(at 6.35 57.15 180)
				(length 3.81)
				(name "Pin_6")
				(number "6")
			)
			(pin passive line
				(at 6.35 -11.43 180)
				(length 3.81)
				(name "Pin_60")
				(number "60")
			)
			(pin passive line
				(at -6.35 -13.97 0)
				(length 3.81)
				(name "Pin_61")
				(number "61")
			)
			(pin passive line
				(at 6.35 -13.97 180)
				(length 3.81)
				(name "Pin_62")
				(number "62")
			)
			(pin passive line
				(at -6.35 -16.51 0)
				(length 3.81)
				(name "Pin_63")
				(number "63")
			)
			(pin passive line
				(at 6.35 -16.51 180)
				(length 3.81)
				(name "Pin_64")
				(number "64")
			)
			(pin passive line
				(at -6.35 -19.05 0)
				(length 3.81)
				(name "Pin_65")
				(number "65")
			)
			(pin passive line
				(at 6.35 -19.05 180)
				(length 3.81)
				(name "Pin_66")
				(number "66")
			)
			(pin passive line
				(at -6.35 -21.59 0)
				(length 3.81)
				(name "Pin_67")
				(number "67")
			)
			(pin passive line
				(at 6.35 -21.59 180)
				(length 3.81)
				(name "Pin_68")
				(number "68")
			)
			(pin passive line
				(at -6.35 -24.13 0)
				(length 3.81)
				(name "Pin_69")
				(number "69")
			)
			(pin passive line
				(at -6.35 54.61 0)
				(length 3.81)
				(name "Pin_7")
				(number "7")
			)
			(pin passive line
				(at 6.35 -24.13 180)
				(length 3.81)
				(name "Pin_70")
				(number "70")
			)
			(pin passive line
				(at -6.35 -26.67 0)
				(length 3.81)
				(name "Pin_71")
				(number "71")
			)
			(pin passive line
				(at 6.35 -26.67 180)
				(length 3.81)
				(name "Pin_72")
				(number "72")
			)
			(pin passive line
				(at -6.35 -29.21 0)
				(length 3.81)
				(name "Pin_73")
				(number "73")
			)
			(pin passive line
				(at 6.35 -29.21 180)
				(length 3.81)
				(name "Pin_74")
				(number "74")
			)
			(pin passive line
				(at -6.35 -31.75 0)
				(length 3.81)
				(name "Pin_75")
				(number "75")
			)
			(pin passive line
				(at 6.35 -31.75 180)
				(length 3.81)
				(name "Pin_76")
				(number "76")
			)
			(pin passive line
				(at -6.35 -34.29 0)
				(length 3.81)
				(name "Pin_77")
				(number "77")
			)
			(pin passive line
				(at 6.35 -34.29 180)
				(length 3.81)
				(name "Pin_78")
				(number "78")
			)
			(pin passive line
				(at -6.35 -36.83 0)
				(length 3.81)
				(name "Pin_79")
				(number "79")
			)
			(pin passive line
				(at 6.35 54.61 180)
				(length 3.81)
				(name "Pin_8")
				(number "8")
			)
			(pin passive line
				(at 6.35 -36.83 180)
				(length 3.81)
				(name "Pin_80")
				(number "80")
			)
			(pin passive line
				(at -6.35 -39.37 0)
				(length 3.81)
				(name "Pin_81")
				(number "81")
			)
			(pin passive line
				(at 6.35 -39.37 180)
				(length 3.81)
				(name "Pin_82")
				(number "82")
			)
			(pin passive line
				(at -6.35 -41.91 0)
				(length 3.81)
				(name "Pin_83")
				(number "83")
			)
			(pin passive line
				(at 6.35 -41.91 180)
				(length 3.81)
				(name "Pin_84")
				(number "84")
			)
			(pin passive line
				(at -6.35 -44.45 0)
				(length 3.81)
				(name "Pin_85")
				(number "85")
			)
			(pin passive line
				(at 6.35 -44.45 180)
				(length 3.81)
				(name "Pin_86")
				(number "86")
			)
			(pin passive line
				(at -6.35 -46.99 0)
				(length 3.81)
				(name "Pin_87")
				(number "87")
			)
			(pin passive line
				(at 6.35 -46.99 180)
				(length 3.81)
				(name "Pin_88")
				(number "88")
			)
			(pin passive line
				(at -6.35 -49.53 0)
				(length 3.81)
				(name "Pin_89")
				(number "89")
			)
			(pin passive line
				(at -6.35 52.07 0)
				(length 3.81)
				(name "Pin_9")
				(number "9")
			)
			(pin passive line
				(at 6.35 -49.53 180)
				(length 3.81)
				(name "Pin_90")
				(number "90")
			)
			(pin passive line
				(at -6.35 -52.07 0)
				(length 3.81)
				(name "Pin_91")
				(number "91")
			)
			(pin passive line
				(at 6.35 -52.07 180)
				(length 3.81)
				(name "Pin_92")
				(number "92")
			)
			(pin passive line
				(at -6.35 -54.61 0)
				(length 3.81)
				(name "Pin_93")
				(number "93")
			)
			(pin passive line
				(at 6.35 -54.61 180)
				(length 3.81)
				(name "Pin_94")
				(number "94")
			)
			(pin passive line
				(at -6.35 -57.15 0)
				(length 3.81)
				(name "Pin_95")
				(number "95")
			)
			(pin passive line
				(at 6.35 -57.15 180)
				(length 3.81)
				(name "Pin_96")
				(number "96")
			)
			(pin passive line
				(at -6.35 -59.69 0)
				(length 3.81)
				(name "Pin_97")
				(number "97")
			)
			(pin passive line
				(at 6.35 -59.69 180)
				(length 3.81)
				(name "Pin_98")
				(number "98")
			)
			(pin passive line
				(at -6.35 -62.23 0)
				(length 3.81)
				(name "Pin_99")
				(number "99")
			)
		)
	)
	(symbol "Conn_ST_STDC14_tm"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at -8.89 15.24 0)
		)
		(property "Value" "Conn_ST_STDC14_tm"
			(at 0 12.7 0)
		)
		(property "Footprint" ""
			(at -1.27 0 0)
		)
		(property "Datasheet" ""
			(at -1.27 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "Conn_ST_STDC14_tm_0_1")
		(symbol "Conn_ST_STDC14_tm_1_1"
			(pin no_connect line
				(at -13.97 7.62 0)
				(length 2.54)
				(name "NC")
				(number "1")
			)
			(pin output line
				(at 13.97 2.54 180)
				(length 2.54)
				(name "JTDI/NC")
				(number "10")
			)
			(pin passive line
				(at 13.97 0 180)
				(length 2.54)
				(name "GNDDet")
				(number "11")
			)
			(pin open_collector line
				(at 13.97 -2.54 180)
				(length 2.54)
				(name "~{RST}")
				(number "12")
			)
			(pin output line
				(at 13.97 -5.08 180)
				(length 2.54)
				(name "VCP_RX")
				(number "13")
			)
			(pin input line
				(at 13.97 -7.62 180)
				(length 2.54)
				(name "VCP_TX")
				(number "14")
			)
			(pin no_connect line
				(at -13.97 5.08 0)
				(length 2.54)
				(name "NC")
				(number "2")
			)
			(pin power_in line
				(at -13.97 2.54 0)
				(length 2.54)
				(name "VCC")
				(number "3")
			)
			(pin bidirectional line
				(at -13.97 0 0)
				(length 2.54)
				(name "JTMS/SWDIO")
				(number "4")
			)
			(pin power_in line
				(at -13.97 -2.54 0)
				(length 2.54)
				(name "GND")
				(number "5")
			)
			(pin output line
				(at -13.97 -5.08 0)
				(length 2.54)
				(name "JCLK/SWCLK")
				(number "6")
			)
			(pin passive line
				(at -13.97 -7.62 0)
				(length 2.54)
				(name "GND")
				(number "7")
			)
			(pin input line
				(at 13.97 7.62 180)
				(length 2.54)
				(name "JTDO/SWO")
				(number "8")
			)
			(pin input line
				(at 13.97 5.08 180)
				(length 2.54)
				(name "JRCLK/NC")
				(number "9")
			)
		)
	)
	(symbol "Cree-XP-G3"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "D"
			(at 0 -8.89 0)
		)
		(property "Value" "Cree-XP-G3"
			(at 0 -5.08 0)
		)
		(property "Footprint" "ProjectFootprints:Cree-XP-L-HI"
			(at 24.13 -2.54 0)
		)
		(property "Datasheet" "https://cree-led.com/media/documents/dsXPG3.pdf"
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(property "Part Number" "XPGDPR-L1-0000-00F01CT-ND"
			(at 24.13 0 0)
		)
		(property "Supplier" "Digikey"
			(at 11.43 2.54 0)
		)
		(property "Link" "https://www.digikey.com/en/products/detail/cree-inc/XPGDPR-L1-0000-00F01/10131728?s=N4IgjCBcoMwOxVAYygMwIYBsDOBTANCAPZQDaIMAHAGwCs1ALCALqEAOALlCAMocBOASwB2AcxABfQgFoATIhApIAgK4FiZELRYSpIeZHJJ%2BuXAAIAGgAVpAcRg6gA"
			(at 128.27 -5.08 0)
		)
		(symbol "Cree-XP-G3_1_1"
			(pin passive line
				(at -2.54 0 0)
				(length 1.778)
				(name "A")
				(number "1")
			)
			(pin passive line
				(at 2.54 0 180)
				(length 1.778)
				(name "K")
				(number "2")
			)
			(pin output line
				(at 0 2.54 270)
				(length 2.54)
				(name "THERM")
				(number "3")
			)
		)
	)
	(symbol "CreeXD16"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 5.08 0)
		)
		(property "Value" "CreeXD16"
			(at 0 -3.81 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "CreeXD16_1_1"
			(pin passive line
				(at -2.54 0 0)
				(length 1.778)
				(name "A")
				(number "1")
			)
			(pin passive line
				(at 2.54 0 180)
				(length 1.778)
				(name "K")
				(number "2")
			)
		)
	)
	(symbol "Cree_XE-G"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 7.62 0)
		)
		(property "Value" "Cree_XE-G"
			(at 0 5.08 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "Cree_XE-G_0_1")
		(symbol "Cree_XE-G_1_1"
			(pin power_in line
				(at -7.62 -1.27 0)
				(length 2.54)
				(name "A")
				(number "1")
			)
			(pin power_in line
				(at 7.62 -1.27 180)
				(length 2.54)
				(name "K")
				(number "2")
			)
			(pin bidirectional line
				(at -7.62 -3.81 0)
				(length 2.54)
				(name "Iso")
				(number "3")
			)
		)
	)
	(symbol "Cree_XHP70.3"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "D"
			(at 2.54 6.35 0)
		)
		(property "Value" "Cree_XHP70.3"
			(at -7.62 7.62 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "Cree_XHP70.3_0_1")
		(symbol "Cree_XHP70.3_1_1"
			(pin power_in line
				(at -7.62 1.27 0)
				(length 2.54)
				(name "A1")
				(number "1")
			)
			(pin power_in line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "A2")
				(number "2")
			)
			(pin power_in line
				(at 7.62 -2.54 180)
				(length 2.54)
				(name "K2")
				(number "3")
			)
			(pin power_in line
				(at 7.62 1.27 180)
				(length 2.54)
				(name "K1")
				(number "4")
			)
			(pin bidirectional line
				(at 0 -7.62 90)
				(length 2.54)
				(name "T")
				(number "5")
			)
		)
	)
	(symbol "Cree_XPGDWT"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "D"
			(at -8.89 5.08 0)
		)
		(property "Value" "Cree_XPGDWT"
			(at -7.62 -10.16 0)
		)
		(property "Footprint" "LED_XPGDWT-B1-0000-00LE1"
			(at 0 7.62 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(property "MAXIMUM_PACKAGE_HEIGHT" "2.26mm"
			(at 0 13.97 0)
		)
		(property "STANDARD" "Manufacturer Recommendations"
			(at 1.27 10.16 0)
		)
		(property "PARTREV" ""
			(at 0 0 0)
		)
		(property "MANUFACTURER" "CREE"
			(at 0 11.43 0)
		)
		(symbol "Cree_XPGDWT_0_0"
			(pin passive line
				(at -10.16 0 0)
				(length 2.54)
				(name "~")
				(number "A")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 5.08)
				(name "~")
				(number "C")
			)
			(pin passive line
				(at 6.35 -5.08 180)
				(length 2.54)
				(name "EP")
				(number "EP")
			)
		)
	)
	(symbol "D24V10F5"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 7.62 0)
		)
		(property "Value" "D24V10F5"
			(at 5.08 7.62 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "D24V10F5_0_1")
		(symbol "D24V10F5_1_1"
			(pin bidirectional line
				(at -11.43 5.08 0)
				(length 2.54)
				(name "PG")
				(number "1")
			)
			(pin bidirectional line
				(at -11.43 2.54 0)
				(length 2.54)
				(name "~{SHDN}")
				(number "2")
			)
			(pin bidirectional line
				(at -11.43 0 0)
				(length 2.54)
				(name "Vin")
				(number "3")
			)
			(pin bidirectional line
				(at -11.43 -2.54 0)
				(length 2.54)
				(name "GND")
				(number "4")
			)
			(pin bidirectional line
				(at 11.43 3.81 180)
				(length 2.54)
				(name "Vout")
				(number "5")
			)
		)
	)
	(symbol "D24V22F5"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 -10.16 0)
		)
		(property "Value" "D24V22F5"
			(at 0 10.16 0)
		)
		(property "Footprint" ""
			(at 0 3.81 0)
		)
		(property "Datasheet" ""
			(at 0 3.81 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "D24V22F5_0_1")
		(symbol "D24V22F5_1_1"
			(pin bidirectional line
				(at -8.89 5.08 0)
				(length 2.54)
				(name "Vout")
				(number "1")
			)
			(pin bidirectional line
				(at -8.89 2.54 0)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin bidirectional line
				(at -8.89 0 0)
				(length 2.54)
				(name "Vin")
				(number "3")
			)
			(pin bidirectional line
				(at -8.89 -2.54 0)
				(length 2.54)
				(name "EN")
				(number "4")
			)
			(pin bidirectional line
				(at -8.89 -5.08 0)
				(length 2.54)
				(name "PG")
				(number "5")
			)
		)
	)
	(symbol "D24V25F5"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 7.62 7.62 0)
		)
		(property "Value" "D24V25F5"
			(at -3.81 7.62 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "D24V25F5_0_1")
		(symbol "D24V25F5_1_1"
			(pin bidirectional line
				(at -11.43 3.81 0)
				(length 2.54)
				(name "Vin")
				(number "1")
			)
			(pin bidirectional line
				(at -11.43 0 0)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin bidirectional line
				(at -11.43 -5.08 0)
				(length 2.54)
				(name "ENABLE")
				(number "3")
			)
			(pin bidirectional line
				(at 11.43 0 180)
				(length 2.54)
				(name "GND")
				(number "4")
			)
			(pin bidirectional line
				(at 11.43 3.81 180)
				(length 2.54)
				(name "Vout")
				(number "5")
			)
		)
	)
	(symbol "D24V50F5"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 -8.89 0)
		)
		(property "Value" "D24V50F5"
			(at 0 8.89 0)
		)
		(property "Footprint" ""
			(at 3.81 -2.54 0)
		)
		(property "Datasheet" ""
			(at 3.81 -2.54 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "D24V50F5_0_1")
		(symbol "D24V50F5_1_1"
			(pin bidirectional line
				(at -8.89 5.08 0)
				(length 2.54)
				(name "Out")
				(number "1")
			)
			(pin bidirectional line
				(at -8.89 2.54 0)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin bidirectional line
				(at -8.89 0 0)
				(length 2.54)
				(name "GND")
				(number "3")
			)
			(pin bidirectional line
				(at -8.89 -2.54 0)
				(length 2.54)
				(name "Vin")
				(number "4")
			)
			(pin bidirectional line
				(at -8.89 -5.08 0)
				(length 2.54)
				(name "EN")
				(number "5")
			)
		)
	)
	(symbol "D24V5F3"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 3.81 10.16 0)
		)
		(property "Value" "D24V5F3"
			(at 5.08 7.62 0)
		)
		(property "Footprint" ""
			(at 0 1.27 0)
		)
		(property "Datasheet" ""
			(at 0 1.27 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "D24V5F3_0_1")
		(symbol "D24V5F3_1_1"
			(pin input line
				(at -5.08 3.81 0)
				(length 2.54)
				(name "~{SHDN}")
				(number "1")
			)
			(pin power_in line
				(at -5.08 1.27 0)
				(length 2.54)
				(name "VIN")
				(number "2")
			)
			(pin power_in line
				(at -5.08 -1.27 0)
				(length 2.54)
				(name "GND")
				(number "3")
			)
			(pin power_out line
				(at -5.08 -3.81 0)
				(length 2.54)
				(name "VOUT")
				(number "4")
			)
		)
	)
	(symbol "D36V50F3"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 -21.59 0)
		)
		(property "Value" "D36V50F3"
			(at 0 13.97 0)
		)
		(property "Footprint" ""
			(at 3.81 7.62 0)
		)
		(property "Datasheet" ""
			(at 3.81 7.62 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "D36V50F3_0_1")
		(symbol "D36V50F3_1_1"
			(pin output line
				(at 8.89 10.16 180)
				(length 2.54)
				(name "Vout")
				(number "1")
			)
			(pin output line
				(at 8.89 -12.7 180)
				(length 2.54)
				(name "Vrp")
				(number "10")
			)
			(pin output line
				(at 8.89 -15.24 180)
				(length 2.54)
				(name "EN")
				(number "11")
			)
			(pin output line
				(at 8.89 -17.78 180)
				(length 2.54)
				(name "PG")
				(number "12")
			)
			(pin output line
				(at 8.89 7.62 180)
				(length 2.54)
				(name "Vout")
				(number "2")
			)
			(pin output line
				(at 8.89 5.08 180)
				(length 2.54)
				(name "GND")
				(number "3")
			)
			(pin output line
				(at 8.89 2.54 180)
				(length 2.54)
				(name "GND")
				(number "4")
			)
			(pin output line
				(at 8.89 0 180)
				(length 2.54)
				(name "GND")
				(number "5")
			)
			(pin output line
				(at 8.89 -2.54 180)
				(length 2.54)
				(name "GND")
				(number "6")
			)
			(pin output line
				(at 8.89 -5.08 180)
				(length 2.54)
				(name "Vin")
				(number "7")
			)
			(pin output line
				(at 8.89 -7.62 180)
				(length 2.54)
				(name "Vin")
				(number "8")
			)
			(pin output line
				(at 8.89 -10.16 180)
				(length 2.54)
				(name "Vrp")
				(number "9")
			)
		)
	)
	(symbol "DCDC_AM1P"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 7.62 0)
		)
		(property "Value" "AM1P-0507DZ"
			(at 0 -10.16 0)
		)
		(property "Footprint" "Package_DIP:PowerIntegrations_PDIP-8C"
			(at 0 -15.24 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(property "PartNum" "AM1P-0507DZ"
			(at 0 -12.7 0)
		)
		(property "VendorNum" ""
			(at 0 0 0)
		)
		(property "Vendor" ""
			(at 0 0 0)
		)
		(property "Subst" ""
			(at 0 0 0)
		)
		(symbol "DCDC_AM1P_1_1"
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "GND")
				(number "1")
			)
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "NC")
				(number "2")
			)
			(pin input line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "+Vin")
				(number "4")
			)
			(pin output line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "+V1out")
				(number "5")
			)
			(pin input line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "-V1out")
				(number "6")
			)
			(pin output line
				(at 12.7 0 180)
				(length 2.54)
				(name "-V2out")
				(number "7")
			)
			(pin output line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "-V2out")
				(number "8")
			)
		)
	)
	(symbol "DM3AT-SF-PEJM5"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at -7.62 18.3148 0)
		)
		(property "Value" "DM3AT-SF-PEJM5"
			(at -7.62 -20.8538 0)
		)
		(property "Footprint" "ProjectFootprints:HRS_DM3AT-SF-PEJM5"
			(at 2.54 -22.86 0)
		)
		(property "Datasheet" "https://www.hirose.com/product/document?clcode=CL0609-0033-6-00&productname=DM3AT-SF-PEJ2M5&series=DM3&documenttype=Catalog&lang=en&documentid=D49662_en"
			(at 7.62 0 0)
		)
		(property "Description" ""
			(at 0 19.05 0)
		)
		(symbol "DM3AT-SF-PEJM5_0_0"
			(text "A"
				(at -3.048 -13.208 0)
			)
			(text "B"
				(at -3.048 -16.51 0)
			)
			(pin bidirectional line
				(at -12.7 15.24 0)
				(length 5.08)
				(name "DAT2")
				(number "1")
			)
			(pin bidirectional line
				(at -12.7 12.7 0)
				(length 5.08)
				(name "CD/DAT3")
				(number "2")
			)
			(pin bidirectional line
				(at -12.7 10.16 0)
				(length 5.08)
				(name "CMD")
				(number "3")
			)
			(pin power_in line
				(at -12.7 7.62 0)
				(length 5.08)
				(name "VDD")
				(number "4")
			)
			(pin bidirectional clock
				(at -12.7 5.08 0)
				(length 5.08)
				(name "CLK")
				(number "5")
			)
			(pin power_in line
				(at -12.7 2.54 0)
				(length 5.08)
				(name "VSS")
				(number "6")
			)
			(pin bidirectional line
				(at -12.7 0 0)
				(length 5.08)
				(name "DAT0")
				(number "7")
			)
			(pin bidirectional line
				(at -12.7 -2.54 0)
				(length 5.08)
				(name "DAT1")
				(number "8")
			)
			(pin passive line
				(at -12.7 -5.08 0)
				(length 5.08)
				(name "SHIELD")
				(number "P1")
			)
			(pin passive line
				(at -12.7 -6.35 0)
				(length 5.08)
				(name "SHIELD")
				(number "P2")
			)
			(pin passive line
				(at -12.7 -7.62 0)
				(length 5.08)
				(name "SHIELD")
				(number "P3")
			)
			(pin passive line
				(at -12.7 -8.89 0)
				(length 5.08)
				(name "SHIELD")
				(number "P4")
			)
			(pin bidirectional line
				(at -12.7 -12.7 0)
				(length 5.08)
				(name "~")
				(number "SWA")
			)
			(pin bidirectional line
				(at -12.7 -15.24 0)
				(length 5.08)
				(name "~")
				(number "SWB")
			)
		)
		(symbol "DM3AT-SF-PEJM5_0_1")
	)
	(symbol "DS3211M"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 3.81 8.89 0)
		)
		(property "Value" "DS3211M"
			(at -5.08 8.89 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "DS3211M_0_1")
		(symbol "DS3211M_1_1"
			(pin open_collector line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "32KHZ")
				(number "1")
			)
			(pin passive line
				(at 12.7 -10.16 180)
				(length 2.54)
				(name "GND")
				(number "10")
			)
			(pin passive line
				(at 12.7 -7.62 180)
				(length 2.54)
				(name "GND")
				(number "11")
			)
			(pin passive line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "GND")
				(number "12")
			)
			(pin power_in line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "GND")
				(number "13")
			)
			(pin power_in line
				(at 12.7 0 180)
				(length 2.54)
				(name "VBAT")
				(number "14")
			)
			(pin bidirectional line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "SDA")
				(number "15")
			)
			(pin input line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "SCL")
				(number "16")
			)
			(pin power_in line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "VCC")
				(number "2")
			)
			(pin open_collector line
				(at -12.7 0 0)
				(length 2.54)
				(name "~{INT}/SQW")
				(number "3")
			)
			(pin bidirectional line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "~{RST}")
				(number "4")
			)
			(pin passive line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "GND")
				(number "5")
			)
			(pin passive line
				(at -12.7 -7.62 0)
				(length 2.54)
				(name "GND")
				(number "6")
			)
			(pin passive line
				(at -12.7 -10.16 0)
				(length 2.54)
				(name "GND")
				(number "7")
			)
			(pin passive line
				(at -12.7 -12.7 0)
				(length 2.54)
				(name "GND")
				(number "8")
			)
			(pin passive line
				(at 12.7 -12.7 180)
				(length 2.54)
				(name "GND")
				(number "9")
			)
		)
	)
	(symbol "DS3231MZ"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 5.08 7.62 0)
		)
		(property "Value" "DS3231MZ"
			(at -3.81 7.62 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/DS3231M.pdf"
			(at 0 0 0)
		)
		(property "Description" "RTC 5ppm  2uA standby 200uA active"
			(at 0 0 0)
		)
		(property "ki_keywords" "RTC"
			(at 0 0 0)
		)
		(symbol "DS3231MZ_0_1")
		(symbol "DS3231MZ_1_1"
			(pin open_collector line
				(at -11.43 3.81 0)
				(length 2.54)
				(name "32KHZ")
				(number "1")
			)
			(pin power_in line
				(at -11.43 1.27 0)
				(length 2.54)
				(name "VCC")
				(number "2")
			)
			(pin open_collector line
				(at -11.43 -1.27 0)
				(length 2.54)
				(name "~{INT}/SQW")
				(number "3")
			)
			(pin bidirectional line
				(at -11.43 -3.81 0)
				(length 2.54)
				(name "~{RST}")
				(number "4")
			)
			(pin power_in line
				(at 11.43 -3.81 180)
				(length 2.54)
				(name "GND")
				(number "5")
			)
			(pin power_in line
				(at 11.43 -1.27 180)
				(length 2.54)
				(name "VBAT")
				(number "6")
			)
			(pin bidirectional line
				(at 11.43 1.27 180)
				(length 2.54)
				(name "SDA")
				(number "7")
			)
			(pin input line
				(at 11.43 3.81 180)
				(length 2.54)
				(name "SCL")
				(number "8")
			)
		)
	)
	(symbol "ECS-3953M-120-BN-TR"
		(pin_names
			(offset 0.254)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "OSC"
			(at 26.67 3.81 0)
		)
		(property "Value" "ECS-3953M-120-BN-TR"
			(at 25.4 -7.62 0)
		)
		(property "Footprint" "ECS-3951M/3953M-BN_ECS"
			(at 26.67 -7.62 0)
		)
		(property "Datasheet" ""
			(at 12.7 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_fp_filters" "ECS-3951M/3953M-BN_ECS ECS-3951M/3953M-BN_ECS-M ECS-3951M/3953M-BN_ECS-L"
			(at 0 0 0)
		)
		(symbol "ECS-3953M-120-BN-TR_1_1"
			(pin unspecified line
				(at 12.7 0 0)
				(length 7.62)
				(name "EN")
				(number "1")
			)
			(pin power_in line
				(at 12.7 -2.54 0)
				(length 7.62)
				(name "GND")
				(number "2")
			)
			(pin output line
				(at 38.1 -2.54 180)
				(length 7.62)
				(name "Out")
				(number "3")
			)
			(pin power_in line
				(at 38.1 0 180)
				(length 7.62)
				(name "VDD")
				(number "4")
			)
		)
	)
	(symbol "EK-TM4C123GXL"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -0.762 40.894 0)
		)
		(property "Value" "EK-TM4C123GXL"
			(at -7.366 37.846 0)
		)
		(property "Footprint" "EK-TM4C123GXL:MODULE_EK-TM4C123GXL"
			(at 1.27 -43.942 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/spms376e/spms376e.pdf"
			(at 2.54 -49.53 0)
		)
		(property "Description" "Tiva TM4c123g...PM 64pin Launchpad daughter card"
			(at 1.524 -40.894 0)
		)
		(property "PartNum" "EK-TM4C123GXL"
			(at 0.762 -38.354 0)
		)
		(property "VendorNum" "595-EK-TM4C123GXL"
			(at 1.778 -47.752 0)
		)
		(property "Subst" "No"
			(at 0.508 -52.07 0)
		)
		(property "Vendor" "Mouser"
			(at 1.016 -45.72 0)
		)
		(symbol "EK-TM4C123GXL_0_0"
			(pin power_in line
				(at -71.12 11.43 0)
				(length 5.08)
				(name "+3.3V")
				(number "J1_1")
			)
			(pin bidirectional line
				(at -71.12 -11.43 0)
				(length 5.08)
				(name "PA7")
				(number "J1_10")
			)
			(pin bidirectional line
				(at -71.12 8.89 0)
				(length 5.08)
				(name "PB5")
				(number "J1_2")
			)
			(pin bidirectional line
				(at -71.12 6.35 0)
				(length 5.08)
				(name "PB0")
				(number "J1_3")
			)
			(pin bidirectional line
				(at -71.12 3.81 0)
				(length 5.08)
				(name "PB1")
				(number "J1_4")
			)
			(pin bidirectional line
				(at -71.12 1.27 0)
				(length 5.08)
				(name "PE4")
				(number "J1_5")
			)
			(pin bidirectional line
				(at -71.12 -1.27 0)
				(length 5.08)
				(name "PE5")
				(number "J1_6")
			)
			(pin bidirectional line
				(at -71.12 -3.81 0)
				(length 5.08)
				(name "PB4")
				(number "J1_7")
			)
			(pin bidirectional line
				(at -71.12 -6.35 0)
				(length 5.08)
				(name "PA5")
				(number "J1_8")
			)
			(pin bidirectional line
				(at -71.12 -8.89 0)
				(length 5.08)
				(name "PA6")
				(number "J1_9")
			)
			(pin power_in line
				(at 68.58 11.43 180)
				(length 5.08)
				(name "GND")
				(number "J2_1")
			)
			(pin bidirectional line
				(at 68.58 -11.43 180)
				(length 5.08)
				(name "PA2")
				(number "J2_10")
			)
			(pin bidirectional line
				(at 68.58 8.89 180)
				(length 5.08)
				(name "PB2")
				(number "J2_2")
			)
			(pin bidirectional line
				(at 68.58 6.35 180)
				(length 5.08)
				(name "PE0")
				(number "J2_3")
			)
			(pin bidirectional line
				(at 68.58 3.81 180)
				(length 5.08)
				(name "PF0")
				(number "J2_4")
			)
			(pin bidirectional line
				(at 68.58 -1.27 180)
				(length 5.08)
				(name "PB7")
				(number "J2_6")
			)
			(pin bidirectional line
				(at 68.58 -3.81 180)
				(length 5.08)
				(name "PB6")
				(number "J2_7")
			)
			(pin bidirectional line
				(at 68.58 -6.35 180)
				(length 5.08)
				(name "PA4")
				(number "J2_8")
			)
			(pin bidirectional line
				(at 68.58 -8.89 180)
				(length 5.08)
				(name "PA3")
				(number "J2_9")
			)
			(pin power_in line
				(at -48.26 11.43 180)
				(length 5.08)
				(name "+VBUS")
				(number "J3_1")
			)
			(pin bidirectional line
				(at -48.26 -11.43 180)
				(length 5.08)
				(name "PF1")
				(number "J3_10")
			)
			(pin power_in line
				(at -48.26 8.89 180)
				(length 5.08)
				(name "GND")
				(number "J3_2")
			)
			(pin bidirectional line
				(at -48.26 6.35 180)
				(length 5.08)
				(name "PD0")
				(number "J3_3")
			)
			(pin bidirectional line
				(at -48.26 3.81 180)
				(length 5.08)
				(name "PD1")
				(number "J3_4")
			)
			(pin bidirectional line
				(at -48.26 1.27 180)
				(length 5.08)
				(name "PD2")
				(number "J3_5")
			)
			(pin bidirectional line
				(at -48.26 -1.27 180)
				(length 5.08)
				(name "PD3")
				(number "J3_6")
			)
			(pin bidirectional line
				(at -48.26 -3.81 180)
				(length 5.08)
				(name "PE1")
				(number "J3_7")
			)
			(pin bidirectional line
				(at -48.26 -6.35 180)
				(length 5.08)
				(name "PE2")
				(number "J3_8")
			)
			(pin bidirectional line
				(at -48.26 -8.89 180)
				(length 5.08)
				(name "PE3")
				(number "J3_9")
			)
			(pin bidirectional line
				(at 45.72 11.43 0)
				(length 5.08)
				(name "PF2")
				(number "J4_1")
			)
			(pin bidirectional line
				(at 45.72 -11.43 0)
				(length 5.08)
				(name "PF4")
				(number "J4_10")
			)
			(pin bidirectional line
				(at 45.72 8.89 0)
				(length 5.08)
				(name "PF3")
				(number "J4_2")
			)
			(pin bidirectional line
				(at 45.72 6.35 0)
				(length 5.08)
				(name "PB3")
				(number "J4_3")
			)
			(pin bidirectional line
				(at 45.72 3.81 0)
				(length 5.08)
				(name "PC4")
				(number "J4_4")
			)
			(pin bidirectional line
				(at 45.72 1.27 0)
				(length 5.08)
				(name "PC5")
				(number "J4_5")
			)
			(pin bidirectional line
				(at 45.72 -1.27 0)
				(length 5.08)
				(name "PC6")
				(number "J4_6")
			)
			(pin bidirectional line
				(at 45.72 -3.81 0)
				(length 5.08)
				(name "PC7")
				(number "J4_7")
			)
			(pin bidirectional line
				(at 45.72 -6.35 0)
				(length 5.08)
				(name "PD6")
				(number "J4_8")
			)
			(pin bidirectional line
				(at 45.72 -8.89 0)
				(length 5.08)
				(name "PD7")
				(number "J4_9")
			)
		)
		(symbol "EK-TM4C123GXL_1_0"
			(pin input line
				(at 68.58 1.27 180)
				(length 5.08)
				(name "~{RESET}")
				(number "J2_5")
			)
		)
		(symbol "EK-TM4C123GXL_1_1")
	)
	(symbol "ESD16"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 2.54 3.81 0)
		)
		(property "Value" "ESD16"
			(at 1.27 -6.35 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "ESD16_0_0"
			(pin passive line
				(at -2.54 -7.62 90)
				(length 2.54)
				(name "G")
				(number "3")
			)
		)
		(symbol "ESD16_0_1")
		(symbol "ESD16_1_1"
			(pin passive line
				(at -5.08 5.08 270)
				(length 2.54)
				(name "1")
				(number "1")
			)
			(pin passive line
				(at 0 5.08 270)
				(length 2.54)
				(name "2")
				(number "2")
			)
		)
	)
	(symbol "FDMC007N08LC"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "Q"
			(at 10.16 1.27 0)
		)
		(property "Value" "FDMC007N08LC"
			(at 11.43 -1.27 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "FDMC007N08LC_0_1")
		(symbol "FDMC007N08LC_1_1"
			(pin power_in line
				(at 3.81 -6.35 90)
				(length 1.27)
				(name "S")
				(number "1")
			)
			(pin bidirectional line
				(at 2.54 -6.35 90)
				(length 1.27)
				(name "S")
				(number "2")
			)
			(pin bidirectional line
				(at 1.27 -6.35 90)
				(length 1.27)
				(name "S")
				(number "3")
			)
			(pin passive line
				(at -5.08 -1.27 0)
				(length 1.27)
				(name "G")
				(number "4")
			)
			(pin power_in line
				(at 1.27 5.08 270)
				(length 1.27)
				(name "D")
				(number "5")
			)
		)
	)
	(symbol "FDMC8327L"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "M"
			(at 5.08 0 0)
		)
		(property "Value" "FDMC8327L"
			(at 8.89 -2.54 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "FDMC8327L_1_1"
			(pin bidirectional line
				(at 0 -5.08 90)
				(length 1.27)
				(name "S")
				(number "1")
			)
			(pin bidirectional line
				(at 1.27 -5.08 90)
				(length 1.27)
				(name "S")
				(number "2")
			)
			(pin power_in line
				(at 2.54 -5.08 90)
				(length 1.27)
				(name "S")
				(number "3")
			)
			(pin passive line
				(at -5.08 -1.27 0)
				(length 1.27)
				(name "G")
				(number "4")
			)
			(pin passive line
				(at -1.27 5.08 270)
				(length 1.27)
				(name "D")
				(number "5")
			)
			(pin power_in line
				(at 0 5.08 270)
				(length 1.27)
				(name "D")
				(number "5")
			)
			(pin power_in line
				(at 1.27 5.08 270)
				(length 1.27)
				(name "D")
				(number "5")
			)
			(pin power_in line
				(at 2.54 5.08 270)
				(length 1.27)
				(name "D")
				(number "5")
			)
		)
	)
	(symbol "FDS4935BZ"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -8.89 0 0)
		)
		(property "Value" "FDS4935BZ"
			(at -8.89 -2.54 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "FDS4935BZ_0_1")
		(symbol "FDS4935BZ_1_1"
			(pin bidirectional line
				(at 0 -5.08 90)
				(length 1.27)
				(name "S")
				(number "1")
			)
			(pin passive line
				(at 6.35 -1.27 180)
				(length 1.27)
				(name "G")
				(number "2")
			)
			(pin power_in line
				(at 0 5.08 270)
				(length 1.27)
				(name "D")
				(number "7")
			)
			(pin power_in line
				(at -1.27 5.08 270)
				(length 1.27)
				(name "D")
				(number "8")
			)
		)
		(symbol "FDS4935BZ_2_1"
			(pin bidirectional line
				(at 0 -5.08 90)
				(length 1.27)
				(name "S")
				(number "3")
			)
			(pin passive line
				(at 6.35 -1.27 180)
				(length 1.27)
				(name "G")
				(number "4")
			)
			(pin power_in line
				(at 0 5.08 270)
				(length 1.27)
				(name "D")
				(number "5")
			)
			(pin power_in line
				(at -1.27 5.08 270)
				(length 1.27)
				(name "D")
				(number "6")
			)
		)
	)
	(symbol "FDS6990"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 8.89 2.54 0)
		)
		(property "Value" "FDS6990"
			(at 10.16 0 0)
		)
		(property "Footprint" ""
			(at -2.54 -13.97 0)
		)
		(property "Datasheet" ""
			(at -2.54 -13.97 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "FDS6990_1_1"
			(pin bidirectional line
				(at 1.27 -5.08 90)
				(length 1.27)
				(name "S")
				(number "1")
			)
			(pin bidirectional line
				(at -5.08 -1.27 0)
				(length 1.27)
				(name "G")
				(number "2")
			)
			(pin power_in line
				(at 1.27 5.08 270)
				(length 1.27)
				(name "D")
				(number "7")
			)
			(pin power_in line
				(at 2.54 5.08 270)
				(length 1.27)
				(name "D")
				(number "8")
			)
		)
		(symbol "FDS6990_2_1"
			(pin bidirectional line
				(at 1.27 -5.08 90)
				(length 1.27)
				(name "S")
				(number "3")
			)
			(pin bidirectional line
				(at -5.08 -1.27 0)
				(length 1.27)
				(name "G")
				(number "4")
			)
			(pin power_in line
				(at 1.27 5.08 270)
				(length 1.27)
				(name "D")
				(number "5")
			)
			(pin power_in line
				(at 2.54 5.08 270)
				(length 1.27)
				(name "D")
				(number "6")
			)
		)
	)
	(symbol "FSA1208"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 5.08 20.32 0)
		)
		(property "Value" "FSA1208"
			(at 7.62 17.78 0)
		)
		(property "Footprint" ""
			(at -87.63 91.44 0)
		)
		(property "Datasheet" ""
			(at -87.63 91.44 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "FSA1208_0_1")
		(symbol "FSA1208_1_1"
			(pin power_in line
				(at -1.27 17.78 270)
				(length 2.54)
				(name "VCC")
				(number "1")
			)
			(pin power_in line
				(at -1.27 -16.51 90)
				(length 2.54)
				(name "GND")
				(number "10")
			)
			(pin passive line
				(at 1.27 -16.51 90)
				(length 2.54)
				(name "NC")
				(number "11")
			)
			(pin passive line
				(at 8.89 -7.62 180)
				(length 2.54)
				(name "D8")
				(number "12")
			)
			(pin passive line
				(at 8.89 -5.08 180)
				(length 2.54)
				(name "D7")
				(number "13")
			)
			(pin passive line
				(at 8.89 -2.54 180)
				(length 2.54)
				(name "D6")
				(number "14")
			)
			(pin passive line
				(at 8.89 0 180)
				(length 2.54)
				(name "D5")
				(number "15")
			)
			(pin passive line
				(at 8.89 2.54 180)
				(length 2.54)
				(name "D4")
				(number "16")
			)
			(pin passive line
				(at 8.89 5.08 180)
				(length 2.54)
				(name "D3")
				(number "17")
			)
			(pin passive line
				(at 8.89 7.62 180)
				(length 2.54)
				(name "D2")
				(number "18")
			)
			(pin passive line
				(at 8.89 10.16 180)
				(length 2.54)
				(name "D1")
				(number "19")
			)
			(pin passive line
				(at -8.89 10.16 0)
				(length 2.54)
				(name "S1")
				(number "2")
			)
			(pin input line
				(at 1.27 17.78 270)
				(length 2.54)
				(name "~{OE}")
				(number "20")
			)
			(pin passive line
				(at -8.89 7.62 0)
				(length 2.54)
				(name "S2")
				(number "3")
			)
			(pin passive line
				(at -8.89 5.08 0)
				(length 2.54)
				(name "S3")
				(number "4")
			)
			(pin passive line
				(at -8.89 2.54 0)
				(length 2.54)
				(name "S4")
				(number "5")
			)
			(pin passive line
				(at -8.89 0 0)
				(length 2.54)
				(name "S5")
				(number "6")
			)
			(pin passive line
				(at -8.89 -2.54 0)
				(length 2.54)
				(name "S6")
				(number "7")
			)
			(pin passive line
				(at -8.89 -5.08 0)
				(length 2.54)
				(name "S7")
				(number "8")
			)
			(pin passive line
				(at -8.89 -7.62 0)
				(length 2.54)
				(name "S8")
				(number "9")
			)
		)
	)
	(symbol "Grove-110990030"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at -2.54 8.89 0)
		)
		(property "Value" "Grove-110990030"
			(at 1.27 -6.35 0)
		)
		(property "Footprint" ""
			(at 0 1.27 0)
		)
		(property "Datasheet" ""
			(at 0 1.27 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "Grove-110990030_0_1")
		(symbol "Grove-110990030_1_1"
			(pin passive line
				(at -10.16 5.08 0)
				(length 5.08)
				(name "1")
				(number "1")
			)
			(pin passive line
				(at -10.16 2.54 0)
				(length 5.08)
				(name "2")
				(number "2")
			)
			(pin passive line
				(at -10.16 0 0)
				(length 5.08)
				(name "3")
				(number "3")
			)
			(pin passive line
				(at -10.16 -2.54 0)
				(length 5.08)
				(name "4")
				(number "4")
			)
		)
	)
	(symbol "HV508"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -8.89 -12.7 0)
		)
		(property "Value" "HV508"
			(at 6.35 -12.7 0)
		)
		(property "Footprint" ""
			(at 3.81 -2.54 0)
		)
		(property "Datasheet" ""
			(at 3.81 -2.54 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "HV508_0_1")
		(symbol "HV508_1_1"
			(pin bidirectional line
				(at -12.7 7.62 0)
				(length 2.54)
				(name "LVIN")
				(number "1")
			)
			(pin bidirectional line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "POL")
				(number "2")
			)
			(pin bidirectional line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "HVEN")
				(number "3")
			)
			(pin bidirectional line
				(at -12.7 -7.62 0)
				(length 2.54)
				(name "GND")
				(number "4")
			)
			(pin bidirectional line
				(at 11.43 -7.62 180)
				(length 2.54)
				(name "HVOUT2")
				(number "5")
			)
			(pin bidirectional line
				(at 11.43 -2.54 180)
				(length 2.54)
				(name "VDD")
				(number "6")
			)
			(pin bidirectional line
				(at 11.43 2.54 180)
				(length 2.54)
				(name "HVIN")
				(number "7")
			)
			(pin bidirectional line
				(at 11.43 7.62 180)
				(length 2.54)
				(name "HVOUT1")
				(number "8")
			)
		)
	)
	(symbol "INA236"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 3.81 11.43 0)
		)
		(property "Value" "INA236"
			(at -2.54 11.43 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "INA236_0_1")
		(symbol "INA236_1_1"
			(pin input line
				(at -8.89 6.35 0)
				(length 2.54)
				(name "Vin+")
				(number "1")
			)
			(pin input line
				(at -8.89 3.81 0)
				(length 2.54)
				(name "Vin-")
				(number "2")
			)
			(pin power_in line
				(at -8.89 1.27 0)
				(length 2.54)
				(name "GND")
				(number "3")
			)
			(pin power_in line
				(at -8.89 -1.27 0)
				(length 2.54)
				(name "VS")
				(number "4")
			)
			(pin input line
				(at 8.89 -1.27 180)
				(length 2.54)
				(name "SCL")
				(number "5")
			)
			(pin bidirectional line
				(at 8.89 1.27 180)
				(length 2.54)
				(name "SDA")
				(number "6")
			)
			(pin input line
				(at 8.89 3.81 180)
				(length 2.54)
				(name "A0")
				(number "7")
			)
			(pin open_collector line
				(at 8.89 6.35 180)
				(length 2.54)
				(name "~{Alert}")
				(number "8")
			)
		)
	)
	(symbol "INA237"
		(pin_names
			(offset 0.254)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 11.43 0)
		)
		(property "Value" "INA237"
			(at 1.27 8.89 0)
		)
		(property "Footprint" "VSSOP10_DGS_TEX"
			(at 0 -10.16 0)
		)
		(property "Datasheet" ""
			(at -15.24 5.08 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_fp_filters" "VSSOP10_DGS_TEX VSSOP10_DGS_TEX-M VSSOP10_DGS_TEX-L"
			(at 0 0 0)
		)
		(symbol "INA237_1_1"
			(pin input line
				(at -11.43 5.08 0)
				(length 3.81)
				(name "A1")
				(number "1")
			)
			(pin input line
				(at 11.43 5.08 180)
				(length 3.81)
				(name "IN+")
				(number "10")
			)
			(pin input line
				(at -11.43 2.54 0)
				(length 3.81)
				(name "A0")
				(number "2")
			)
			(pin output line
				(at -11.43 0 0)
				(length 3.81)
				(name "ALERT")
				(number "3")
			)
			(pin bidirectional line
				(at -11.43 -2.54 0)
				(length 3.81)
				(name "SDA")
				(number "4")
			)
			(pin input line
				(at -11.43 -5.08 0)
				(length 3.81)
				(name "SCL")
				(number "5")
			)
			(pin power_in line
				(at 11.43 -5.08 180)
				(length 3.81)
				(name "VS")
				(number "6")
			)
			(pin power_in line
				(at 11.43 -2.54 180)
				(length 3.81)
				(name "GND")
				(number "7")
			)
			(pin input line
				(at 11.43 0 180)
				(length 3.81)
				(name "VBUS")
				(number "8")
			)
			(pin input line
				(at 11.43 2.54 180)
				(length 3.81)
				(name "IN-")
				(number "9")
			)
		)
	)
	(symbol "INA260"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 5.08 12.7 0)
		)
		(property "Value" "INA260"
			(at -5.08 12.7 0)
		)
		(property "Footprint" ""
			(at 0 -5.08 0)
		)
		(property "Datasheet" ""
			(at 0 -5.08 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "INA260_0_1")
		(symbol "INA260_1_1"
			(pin input line
				(at -10.16 7.62 0)
				(length 2.54)
				(name "IN+")
				(number "1")
			)
			(pin input line
				(at 10.16 -7.62 180)
				(length 2.54)
				(name "VS")
				(number "10")
			)
			(pin power_in line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "GND")
				(number "11")
			)
			(pin input line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "VBUS")
				(number "12")
			)
			(pin no_connect line
				(at 10.16 0 180)
				(length 2.54)
				(name "NC")
				(number "13")
			)
			(pin input line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "IN-")
				(number "14")
			)
			(pin input line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "IN-")
				(number "15")
			)
			(pin input line
				(at 10.16 7.62 180)
				(length 2.54)
				(name "IN-")
				(number "16")
			)
			(pin input line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "IN+")
				(number "2")
			)
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "IN+")
				(number "3")
			)
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "A1")
				(number "4")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "A0")
				(number "5")
			)
			(pin power_in line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "GND")
				(number "6")
			)
			(pin input line
				(at -10.16 -7.62 0)
				(length 2.54)
				(name "ALERT")
				(number "7")
			)
			(pin bidirectional line
				(at -10.16 -10.16 0)
				(length 2.54)
				(name "SDA")
				(number "8")
			)
			(pin input line
				(at 10.16 -10.16 180)
				(length 2.54)
				(name "SCL")
				(number "9")
			)
		)
	)
	(symbol "IRS2008"
		(pin_names
			(offset 0.254)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 19.05 6.35 0)
		)
		(property "Value" "IRS2008"
			(at 19.05 3.81 0)
		)
		(property "Footprint" "SOIC8_INF"
			(at 19.05 -10.16 0)
		)
		(property "Datasheet" ""
			(at 5.08 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC8_INF SOIC8_INF-M SOIC8_INF-L"
			(at 0 0 0)
		)
		(symbol "IRS2008_1_1"
			(pin power_in line
				(at 5.08 0 0)
				(length 7.62)
				(name "VCC")
				(number "1")
			)
			(pin power_in line
				(at 5.08 -2.54 0)
				(length 7.62)
				(name "HIN")
				(number "2")
			)
			(pin input line
				(at 5.08 -5.08 0)
				(length 7.62)
				(name "SD")
				(number "3")
			)
			(pin input line
				(at 5.08 -7.62 0)
				(length 7.62)
				(name "COM")
				(number "4")
			)
			(pin output line
				(at 33.02 -7.62 180)
				(length 7.62)
				(name "LO")
				(number "5")
			)
			(pin output line
				(at 33.02 -5.08 180)
				(length 7.62)
				(name "VS")
				(number "6")
			)
			(pin output line
				(at 33.02 -2.54 180)
				(length 7.62)
				(name "HO")
				(number "7")
			)
			(pin power_in line
				(at 33.02 0 180)
				(length 7.62)
				(name "VB")
				(number "8")
			)
		)
	)
	(symbol "ISO7041"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 6.35 11.43 0)
		)
		(property "Value" "ISO7041"
			(at 1.27 -13.97 0)
		)
		(property "Footprint" ""
			(at 1.27 2.54 0)
		)
		(property "Datasheet" ""
			(at 1.27 2.54 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "ISO7041_0_0"
			(pin power_in line
				(at -8.89 7.62 0)
				(length 2.54)
				(name "VCC1")
				(number "1")
			)
			(pin input line
				(at 10.16 -7.62 180)
				(length 2.54)
				(name "EN2")
				(number "10")
			)
			(pin input line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "IND")
				(number "11")
			)
			(pin output line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "OUTC")
				(number "12")
			)
			(pin output line
				(at 10.16 0 180)
				(length 2.54)
				(name "OUTB")
				(number "13")
			)
			(pin output line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "OUTA")
				(number "14")
			)
			(pin power_in line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "GND2")
				(number "15")
			)
			(pin power_in line
				(at 10.16 7.62 180)
				(length 2.54)
				(name "VCC2")
				(number "16")
			)
			(pin power_in line
				(at -8.89 5.08 0)
				(length 2.54)
				(name "GND1")
				(number "2")
			)
			(pin input line
				(at -8.89 2.54 0)
				(length 2.54)
				(name "INA")
				(number "3")
			)
			(pin input line
				(at -8.89 0 0)
				(length 2.54)
				(name "INB")
				(number "4")
			)
			(pin input line
				(at -8.89 -2.54 0)
				(length 2.54)
				(name "INC")
				(number "5")
			)
			(pin output line
				(at -8.89 -5.08 0)
				(length 2.54)
				(name "OUTD")
				(number "6")
			)
			(pin input line
				(at -8.89 -7.62 0)
				(length 2.54)
				(name "EN")
				(number "7")
			)
			(pin power_in line
				(at -8.89 -10.16 0)
				(length 2.54)
				(name "GND1")
				(number "8")
			)
			(pin power_in line
				(at 10.16 -10.16 180)
				(length 2.54)
				(name "GND2")
				(number "9")
			)
		)
		(symbol "ISO7041_0_1")
	)
	(symbol "L450P1600MM"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "LD"
			(at 0 1.27 0)
		)
		(property "Value" "L450P1600MM"
			(at 0 3.81 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "L450P1600MM_0_1")
		(symbol "L450P1600MM_1_1"
			(pin passive line
				(at -6.35 -3.81 0)
				(length 2.54)
				(name "K")
				(number "1")
			)
			(pin passive line
				(at 0 -7.62 90)
				(length 2.54)
				(name "~")
				(number "2")
			)
			(pin passive line
				(at 6.35 -3.81 180)
				(length 2.54)
				(name "A")
				(number "3")
			)
		)
	)
	(symbol "LLS1J222MELA"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "C"
			(at 8.89 3.81 0)
		)
		(property "Value" "LLS1J222MELA"
			(at 15.24 1.27 0)
		)
		(property "Footprint" "Capacitor_THT:CP_Radial_D25.0mm_P10.00mm_SnapIn"
			(at 0 0 0)
		)
		(property "Datasheet" "http://nichicon-us.com/english/products/pdfs/e-lls.pdf"
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(property "Supplier" "Digikey"
			(at 0 0 0)
		)
		(property "Link" "https://www.digikey.com/en/products/detail/nichicon/LLS1J222MELA/2428146"
			(at 0 0 0)
		)
		(property "Part Number" "LLS1J222MELA-ND"
			(at 0 0 0)
		)
		(symbol "LLS1J222MELA_0_0"
			(text "+"
				(at 3.81 7.62 0)
			)
		)
		(symbol "LLS1J222MELA_1_1"
			(pin input line
				(at 0 11.43 270)
				(length 5.0038)
				(name "+")
				(number "1")
			)
			(pin input line
				(at 0 -1.27 90)
				(length 5.0038)
				(name "-")
				(number "2")
			)
		)
	)
	(symbol "LM5134"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -5.08 5.08 0)
		)
		(property "Value" "LM5134"
			(at -2.54 -5.08 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "LM5134_0_1")
		(symbol "LM5134_1_1"
			(pin power_in line
				(at -8.89 2.54 0)
				(length 2.54)
				(name "VDD")
				(number "1")
			)
			(pin power_out line
				(at -8.89 0 0)
				(length 2.54)
				(name "PILOT")
				(number "2")
			)
			(pin power_out line
				(at -8.89 -2.54 0)
				(length 2.54)
				(name "OUT")
				(number "3")
			)
			(pin power_in line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "VSS")
				(number "4")
			)
			(pin input line
				(at 12.7 0 180)
				(length 2.54)
				(name "INB")
				(number "5")
			)
			(pin input line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "IN")
				(number "6")
			)
		)
	)
	(symbol "LM66200DRLR"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "IC"
			(at -10.16 8.255 0)
		)
		(property "Value" "LM66200DRLR"
			(at -10.16 -7.62 0)
		)
		(property "Footprint" "ProjectFootprints:LM66200_SOT8"
			(at 0 -13.97 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/lm66200.pdf"
			(at 0 -10.16 0)
		)
		(property "Description" "\n1.6-V to 5.5-V, 40-mΩ, 2.5-A, low-IQ, dual ideal diode\n"
			(at 1.27 -8.89 0)
		)
		(symbol "LM66200DRLR_0_0")
		(symbol "LM66200DRLR_1_0"
			(pin passive line
				(at -15.24 5.08 0)
				(length 5.08)
				(name "GND")
				(number "1")
			)
			(pin power_out line
				(at -15.24 2.54 0)
				(length 5.08)
				(name "VOUT")
				(number "2")
			)
			(pin power_in line
				(at -15.24 0 0)
				(length 5.08)
				(name "VIN1")
				(number "3")
			)
			(pin input line
				(at -15.24 -2.54 0)
				(length 5.08)
				(name "~{ON}")
				(number "4")
			)
			(pin passive line
				(at 15.24 -2.54 180)
				(length 5.08)
				(name "GND")
				(number "5")
			)
			(pin power_in line
				(at 15.24 0 180)
				(length 5.08)
				(name "VIN2")
				(number "6")
			)
			(pin power_out line
				(at 15.24 2.54 180)
				(length 5.08)
				(name "VOUT")
				(number "7")
			)
			(pin output line
				(at 15.24 5.08 180)
				(length 5.08)
				(name "ST")
				(number "8")
			)
		)
	)
	(symbol "LPC11E37FBD48"
		(pin_names
			(offset 0.254)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 50.8 3.81 0)
		)
		(property "Value" "LPC11E37FBD48"
			(at 21.59 -68.58 0)
		)
		(property "Footprint" "LQFP48_SOT313-2_NXP"
			(at 21.59 -64.77 0)
		)
		(property "Datasheet" ""
			(at -22.86 -2.54 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP48_SOT313-2_NXP LQFP48_SOT313-2_NXP-M LQFP48_SOT313-2_NXP-L"
			(at 0 0 0)
		)
		(symbol "LPC11E37FBD48_1_1"
			(pin bidirectional line
				(at -22.86 -2.54 0)
				(length 7.62)
				(name "PIO1_25/CT32B0_MAT1")
				(number "1")
			)
			(pin bidirectional line
				(at -22.86 -25.4 0)
				(length 7.62)
				(name "PIO0_2/SSEL0/CT16B0_CAP0")
				(number "10")
			)
			(pin bidirectional line
				(at -22.86 -27.94 0)
				(length 7.62)
				(name "PIO1_26/CT32B0_MAT2/RXD")
				(number "11")
			)
			(pin bidirectional line
				(at -22.86 -30.48 0)
				(length 7.62)
				(name "PIO1_27/CT32B0_MAT3/TXD")
				(number "12")
			)
			(pin bidirectional line
				(at -22.86 -33.02 0)
				(length 7.62)
				(name "PIO1_20/DSR/SCK1")
				(number "13")
			)
			(pin bidirectional line
				(at -22.86 -35.56 0)
				(length 7.62)
				(name "PIO0_3")
				(number "14")
			)
			(pin bidirectional line
				(at -22.86 -38.1 0)
				(length 7.62)
				(name "PIO0_4/SCL")
				(number "15")
			)
			(pin bidirectional line
				(at -22.86 -40.64 0)
				(length 7.62)
				(name "PIO0_5/SDA")
				(number "16")
			)
			(pin bidirectional line
				(at -22.86 -43.18 0)
				(length 7.62)
				(name "PIO0_21/CT16B1_MAT0/MOSI1")
				(number "17")
			)
			(pin bidirectional line
				(at -22.86 -45.72 0)
				(length 7.62)
				(name "PIO1_23/CT16B1_MAT1/SSEL1")
				(number "18")
			)
			(pin no_connect line
				(at -22.86 -48.26 0)
				(length 7.62)
				(name "NC")
				(number "19")
			)
			(pin bidirectional line
				(at -22.86 -5.08 0)
				(length 7.62)
				(name "PIO1_19/DTR/SSEL1")
				(number "2")
			)
			(pin no_connect line
				(at -22.86 -50.8 0)
				(length 7.62)
				(name "NC")
				(number "20")
			)
			(pin bidirectional line
				(at -22.86 -53.34 0)
				(length 7.62)
				(name "PIO1_24/CT32B0_MAT0")
				(number "21")
			)
			(pin bidirectional line
				(at -22.86 -55.88 0)
				(length 7.62)
				(name "PIO0_6/SCK0")
				(number "22")
			)
			(pin bidirectional line
				(at -22.86 -58.42 0)
				(length 7.62)
				(name "PIO0_7/CTS")
				(number "23")
			)
			(pin bidirectional line
				(at -22.86 -60.96 0)
				(length 7.62)
				(name "PIO1_28/CT32B0_CAP0/SCLK")
				(number "24")
			)
			(pin bidirectional line
				(at 71.12 -60.96 180)
				(length 7.62)
				(name "PIO1_31")
				(number "25")
			)
			(pin bidirectional line
				(at 71.12 -58.42 180)
				(length 7.62)
				(name "PIO1_21/DCD/MISO1")
				(number "26")
			)
			(pin bidirectional line
				(at 71.12 -55.88 180)
				(length 7.62)
				(name "PIO0_8/MISO0/CT16B0_MAT0")
				(number "27")
			)
			(pin bidirectional line
				(at 71.12 -53.34 180)
				(length 7.62)
				(name "PIO0_9/MOSI0/CT16B0_MAT1")
				(number "28")
			)
			(pin bidirectional line
				(at 71.12 -50.8 180)
				(length 7.62)
				(name "SWCLK/PIO0_10/SCK0/CT16B0_MAT2")
				(number "29")
			)
			(pin bidirectional line
				(at -22.86 -7.62 0)
				(length 7.62)
				(name "RESET/PIO0_0")
				(number "3")
			)
			(pin bidirectional line
				(at 71.12 -48.26 180)
				(length 7.62)
				(name "PIO0_22/AD6/CT16B1_MAT1/MISO1")
				(number "30")
			)
			(pin bidirectional line
				(at 71.12 -45.72 180)
				(length 7.62)
				(name "PIO1_29/SCK0/CT32B0_CAP1")
				(number "31")
			)
			(pin bidirectional line
				(at 71.12 -43.18 180)
				(length 7.62)
				(name "TDI/PIO0_11/AD0/CT32B0_MAT3")
				(number "32")
			)
			(pin bidirectional line
				(at 71.12 -40.64 180)
				(length 7.62)
				(name "TMS/PIO0_12/AD1/CT32B1_CAP0")
				(number "33")
			)
			(pin bidirectional line
				(at 71.12 -38.1 180)
				(length 7.62)
				(name "TDO/PIO0_13/AD2/CT32B1_MAT0")
				(number "34")
			)
			(pin bidirectional line
				(at 71.12 -35.56 180)
				(length 7.62)
				(name "TRST/PIO0_14/AD3/CT32B1_MAT1")
				(number "35")
			)
			(pin bidirectional line
				(at 71.12 -33.02 180)
				(length 7.62)
				(name "PIO1_13/DTR/CT16B0_MAT0/TXD")
				(number "36")
			)
			(pin bidirectional line
				(at 71.12 -30.48 180)
				(length 7.62)
				(name "PIO1_14/DSR/CT16B0_MAT1/RXD")
				(number "37")
			)
			(pin bidirectional line
				(at 71.12 -27.94 180)
				(length 7.62)
				(name "PIO1_22/RI/MOSI1")
				(number "38")
			)
			(pin bidirectional line
				(at 71.12 -25.4 180)
				(length 7.62)
				(name "SWDIO/PIO0_15/AD4/CT32B1_MAT2")
				(number "39")
			)
			(pin output line
				(at -22.86 -10.16 0)
				(length 7.62)
				(name "PIO0_1/CLKOUT/CT32B0_MAT2")
				(number "4")
			)
			(pin bidirectional line
				(at 71.12 -22.86 180)
				(length 7.62)
				(name "PIO0_16/AD5/CT32B1_MAT3/WAKEUP")
				(number "40")
			)
			(pin power_in line
				(at 71.12 -20.32 180)
				(length 7.62)
				(name "VSS")
				(number "41")
			)
			(pin bidirectional line
				(at 71.12 -17.78 180)
				(length 7.62)
				(name "PIO0_23/AD7")
				(number "42")
			)
			(pin bidirectional line
				(at 71.12 -15.24 180)
				(length 7.62)
				(name "PIO1_15/DCD/CT16B0_MAT2/SCK1")
				(number "43")
			)
			(pin power_in line
				(at 71.12 -12.7 180)
				(length 7.62)
				(name "VDD")
				(number "44")
			)
			(pin bidirectional line
				(at 71.12 -10.16 180)
				(length 7.62)
				(name "PIO0_17/RTS/CT32B0_CAP0/SCLK")
				(number "45")
			)
			(pin bidirectional line
				(at 71.12 -7.62 180)
				(length 7.62)
				(name "PIO0_18/RXD/CT32B0_MAT0")
				(number "46")
			)
			(pin bidirectional line
				(at 71.12 -5.08 180)
				(length 7.62)
				(name "PIO0_19/TXD/CT32B0_MAT1")
				(number "47")
			)
			(pin bidirectional line
				(at 71.12 -2.54 180)
				(length 7.62)
				(name "PIO1_16/RI/CT16B0_CAP0")
				(number "48")
			)
			(pin power_in line
				(at -22.86 -12.7 0)
				(length 7.62)
				(name "VSS")
				(number "5")
			)
			(pin input line
				(at -22.86 -15.24 0)
				(length 7.62)
				(name "XTALIN")
				(number "6")
			)
			(pin output line
				(at -22.86 -17.78 0)
				(length 7.62)
				(name "XTALOUT")
				(number "7")
			)
			(pin power_in line
				(at -22.86 -20.32 0)
				(length 7.62)
				(name "VDD")
				(number "8")
			)
			(pin bidirectional line
				(at -22.86 -22.86 0)
				(length 7.62)
				(name "PIO0_20/CT16B1_CAP0")
				(number "9")
			)
		)
	)
	(symbol "LT3012"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -3.81 11.43 0)
		)
		(property "Value" "LT3012"
			(at 8.89 11.43 0)
		)
		(property "Footprint" ""
			(at -2.54 5.08 0)
		)
		(property "Datasheet" ""
			(at -2.54 5.08 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "LT3012_0_1")
		(symbol "LT3012_1_1"
			(pin bidirectional line
				(at -2.54 -11.43 90)
				(length 2.54)
				(name "GND")
				(number "1")
			)
			(pin bidirectional line
				(at 20.32 -11.43 90)
				(length 2.54) hide
				(name "NC")
				(number "10")
			)
			(pin bidirectional line
				(at -7.62 -1.27 0)
				(length 2.54)
				(name "~{SHDN}")
				(number "11")
			)
			(pin bidirectional line
				(at 22.86 -11.43 90)
				(length 2.54) hide
				(name "NC")
				(number "12")
			)
			(pin bidirectional line
				(at -7.62 5.08 0)
				(length 2.54)
				(name "IN")
				(number "13")
			)
			(pin bidirectional line
				(at -7.62 7.62 0)
				(length 2.54)
				(name "IN")
				(number "14")
			)
			(pin bidirectional line
				(at 25.4 -11.43 90)
				(length 2.54) hide
				(name "NC")
				(number "15")
			)
			(pin bidirectional line
				(at 7.62 -11.43 90)
				(length 2.54)
				(name "GND")
				(number "16")
			)
			(pin bidirectional line
				(at 10.16 -11.43 90)
				(length 2.54)
				(name "GND")
				(number "17")
			)
			(pin bidirectional line
				(at 15.24 -11.43 90)
				(length 2.54) hide
				(name "NC")
				(number "2")
			)
			(pin bidirectional line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "OUT")
				(number "3")
			)
			(pin bidirectional line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "OUT")
				(number "4")
			)
			(pin bidirectional line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "ADJ")
				(number "5")
			)
			(pin bidirectional line
				(at 0 -11.43 90)
				(length 2.54)
				(name "GND")
				(number "6")
			)
			(pin bidirectional line
				(at 17.78 -11.43 90)
				(length 2.54) hide
				(name "NC")
				(number "7")
			)
			(pin bidirectional line
				(at 2.54 -11.43 90)
				(length 2.54)
				(name "GND")
				(number "8")
			)
			(pin bidirectional line
				(at 5.08 -11.43 90)
				(length 2.54)
				(name "GND")
				(number "9")
			)
		)
	)
	(symbol "LT3063EMS8E"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 2.54 13.97 0)
		)
		(property "Value" "LT3063EMS8E"
			(at 0 7.62 0)
		)
		(property "Footprint" "Package_SO:TSSOP-8_3x3mm_P0.65mm"
			(at 36.83 -3.81 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/3063fa.pdf"
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(property "Part Number" "LT3063EMS8E#PBF"
			(at 27.94 -6.35 0)
		)
		(property "Supplier" "Digikey"
			(at 21.59 -1.27 0)
		)
		(property "Link" "https://www.digikey.com/en/products/detail/analog-devices-inc/LT3063EMS8E-PBF/4864071"
			(at 66.04 -8.89 0)
		)
		(symbol "LT3063EMS8E_1_1"
			(pin bidirectional line
				(at 1.27 -10.16 90)
				(length 2.54)
				(name "REF/BYP")
				(number "1")
			)
			(pin bidirectional line
				(at 10.16 0 180)
				(length 2.54)
				(name "ADJ")
				(number "2")
			)
			(pin bidirectional line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "OUT")
				(number "3")
			)
			(pin bidirectional line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "OUT")
				(number "4")
			)
			(pin bidirectional line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "IN")
				(number "5")
			)
			(pin bidirectional line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "IN")
				(number "6")
			)
			(pin bidirectional line
				(at -10.16 0 0)
				(length 2.54)
				(name "~{SHDN}")
				(number "7")
			)
			(pin bidirectional line
				(at -3.81 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "8")
			)
		)
	)
	(symbol "LT3063EMS8E-3.3"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 16.51 0)
		)
		(property "Value" "LT3063EMS8E-3.3"
			(at 0 13.97 0)
		)
		(property "Footprint" "Package_SO:MSOP-8-1EP_3x3mm_P0.65mm_EP1.68x1.88mm_ThermalVias"
			(at 57.15 -7.62 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/3063fa.pdf"
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(property "Part Number" "LT3063EMS8E-3.3#PBF-ND"
			(at 34.29 -5.08 0)
		)
		(property "Supplier" "Digikey"
			(at 24.13 -2.54 0)
		)
		(property "Link" "https://www.digikey.com/en/products/detail/linear-technology-analog-devices/lt3063ems8e-3-3-pbf/6569167"
			(at 77.47 -10.16 0)
		)
		(symbol "LT3063EMS8E-3.3_0_1")
		(symbol "LT3063EMS8E-3.3_1_1"
			(pin bidirectional line
				(at 1.27 -3.81 90)
				(length 2.54)
				(name "REF/BYP")
				(number "1")
			)
			(pin bidirectional line
				(at 10.16 6.35 180)
				(length 2.54)
				(name "ADJ")
				(number "2")
			)
			(pin bidirectional line
				(at 10.16 8.89 180)
				(length 2.54)
				(name "OUT")
				(number "3")
			)
			(pin bidirectional line
				(at 10.16 11.43 180)
				(length 2.54)
				(name "OUT")
				(number "4")
			)
			(pin bidirectional line
				(at -10.16 11.43 0)
				(length 2.54)
				(name "IN")
				(number "5")
			)
			(pin bidirectional line
				(at -10.16 8.89 0)
				(length 2.54)
				(name "IN")
				(number "6")
			)
			(pin bidirectional line
				(at -10.16 6.35 0)
				(length 2.54)
				(name "~{SHDN}")
				(number "7")
			)
			(pin bidirectional line
				(at -3.81 -3.81 90)
				(length 2.54)
				(name "GND")
				(number "8")
			)
		)
	)
	(symbol "LT3083xTSSOP"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 -20.32 0)
		)
		(property "Value" "LT3083xTSSOP"
			(at 0 7.62 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "LT3083xTSSOP_1_1"
			(pin power_out line
				(at 12.7 3.81 180)
				(length 2.54)
				(name "OUT")
				(number "1")
			)
			(pin input line
				(at -12.7 -10.16 0)
				(length 2.54)
				(name "VCONTROL")
				(number "10")
			)
			(pin input line
				(at -12.7 -12.7 0)
				(length 2.54)
				(name "VCONTROL")
				(number "11")
			)
			(pin power_in line
				(at -12.7 3.81 0)
				(length 2.54)
				(name "IN")
				(number "12")
			)
			(pin power_in line
				(at -12.7 1.27 0)
				(length 2.54)
				(name "IN")
				(number "13")
			)
			(pin power_in line
				(at -12.7 -1.27 0)
				(length 2.54)
				(name "IN")
				(number "14")
			)
			(pin power_in line
				(at -12.7 -3.81 0)
				(length 2.54)
				(name "IN")
				(number "15")
			)
			(pin power_out line
				(at 12.7 -16.51 180)
				(length 2.54)
				(name "OUT")
				(number "16")
			)
			(pin power_out line
				(at 3.81 -21.59 90)
				(length 2.54)
				(name "OUT")
				(number "17")
			)
			(pin power_out line
				(at 12.7 1.27 180)
				(length 2.54)
				(name "OUT")
				(number "2")
			)
			(pin power_out line
				(at 12.7 -1.27 180)
				(length 2.54)
				(name "OUT")
				(number "3")
			)
			(pin power_out line
				(at 12.7 -3.81 180)
				(length 2.54)
				(name "OUT")
				(number "4")
			)
			(pin power_out line
				(at 12.7 -6.35 180)
				(length 2.54)
				(name "OUT")
				(number "5")
			)
			(pin power_out line
				(at 12.7 -8.89 180)
				(length 2.54)
				(name "OUT")
				(number "6")
			)
			(pin input line
				(at -12.7 -16.51 0)
				(length 2.54)
				(name "SET")
				(number "7")
			)
			(pin power_out line
				(at 12.7 -11.43 180)
				(length 2.54)
				(name "OUT")
				(number "8")
			)
			(pin power_out line
				(at 12.7 -13.97 180)
				(length 2.54)
				(name "OUT")
				(number "9")
			)
		)
	)
	(symbol "LT3991EMS-3.3"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 11.43 0)
		)
		(property "Value" "LT3991EMS-3.3"
			(at 0 8.89 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "LT3991EMS-3.3_0_1")
		(symbol "LT3991EMS-3.3_1_1"
			(pin input line
				(at -8.89 5.08 0)
				(length 2.54)
				(name "BD")
				(number "1")
			)
			(pin input line
				(at 8.89 5.08 180)
				(length 2.54)
				(name "SYNC")
				(number "10")
			)
			(pin input line
				(at 0 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "11")
			)
			(pin output line
				(at -8.89 2.54 0)
				(length 2.54)
				(name "BOOST")
				(number "2")
			)
			(pin output line
				(at -8.89 0 0)
				(length 2.54)
				(name "SW")
				(number "3")
			)
			(pin input line
				(at -8.89 -2.54 0)
				(length 2.54)
				(name "VIN")
				(number "4")
			)
			(pin input line
				(at -8.89 -5.08 0)
				(length 2.54)
				(name "EN")
				(number "5")
			)
			(pin output line
				(at 8.89 -5.08 180)
				(length 2.54)
				(name "VOUT")
				(number "6")
			)
			(pin input line
				(at 8.89 -2.54 180)
				(length 2.54)
				(name "SS")
				(number "7")
			)
			(pin input line
				(at 8.89 0 180)
				(length 2.54)
				(name "RT")
				(number "8")
			)
			(pin output line
				(at 8.89 2.54 180)
				(length 2.54)
				(name "PG")
				(number "9")
			)
		)
	)
	(symbol "LT3991EMS-ADJ"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 11.43 0)
		)
		(property "Value" "LT3991EMS-ADJ"
			(at 0 8.89 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "LT3991EMS-ADJ_0_1")
		(symbol "LT3991EMS-ADJ_1_1"
			(pin input line
				(at -8.89 5.08 0)
				(length 2.54)
				(name "BD")
				(number "1")
			)
			(pin input line
				(at 8.89 5.08 180)
				(length 2.54)
				(name "SYNC")
				(number "10")
			)
			(pin input line
				(at 0 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "11")
			)
			(pin output line
				(at -8.89 2.54 0)
				(length 2.54)
				(name "BOOST")
				(number "2")
			)
			(pin output line
				(at -8.89 0 0)
				(length 2.54)
				(name "SW")
				(number "3")
			)
			(pin input line
				(at -8.89 -2.54 0)
				(length 2.54)
				(name "VIN")
				(number "4")
			)
			(pin input line
				(at -8.89 -5.08 0)
				(length 2.54)
				(name "EN")
				(number "5")
			)
			(pin input line
				(at 8.89 -5.08 180)
				(length 2.54)
				(name "FB")
				(number "6")
			)
			(pin input line
				(at 8.89 -2.54 180)
				(length 2.54)
				(name "SS")
				(number "7")
			)
			(pin input line
				(at 8.89 0 180)
				(length 2.54)
				(name "RT")
				(number "8")
			)
			(pin output line
				(at 8.89 2.54 180)
				(length 2.54)
				(name "PG")
				(number "9")
			)
		)
	)
	(symbol "LT8300"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 2.54 5.08 0)
		)
		(property "Value" "LT8300"
			(at -3.81 5.08 0)
		)
		(property "Footprint" ""
			(at 0 -3.81 0)
		)
		(property "Datasheet" ""
			(at 0 -3.81 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "LT8300_0_0"
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "EN/UVLO")
				(number "1")
			)
			(pin power_in line
				(at -10.16 0 0)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "RFB")
				(number "3")
			)
			(pin input line
				(at 7.62 -1.27 180)
				(length 2.54)
				(name "SW")
				(number "4")
			)
			(pin power_in line
				(at 7.62 1.27 180)
				(length 2.54)
				(name "VIN")
				(number "5")
			)
		)
		(symbol "LT8300_0_1")
	)
	(symbol "LT8391D"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 16.51 30.48 0)
		)
		(property "Value" "LT8391D"
			(at 0 8.89 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "LT8391D_0_0"
			(pin passive line
				(at -15.24 7.62 0)
				(length 2.54)
				(name "TG1")
				(number "1")
			)
			(pin input line
				(at -15.24 -15.24 0)
				(length 2.54)
				(name "CTRL")
				(number "10")
			)
			(pin input line
				(at 17.78 -7.62 180)
				(length 2.54)
				(name "ISP")
				(number "11")
			)
			(pin input line
				(at 17.78 -11.43 180)
				(length 2.54)
				(name "ISN")
				(number "12")
			)
			(pin input line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "GND")
				(number "13")
			)
			(pin output line
				(at -15.24 -12.7 0)
				(length 2.54)
				(name "~{FAULT}")
				(number "14")
			)
			(pin passive line
				(at -5.08 -30.48 90)
				(length 2.54)
				(name "SS")
				(number "15")
			)
			(pin input line
				(at 17.78 -5.08 180)
				(length 2.54)
				(name "FB")
				(number "16")
			)
			(pin output line
				(at 2.54 -30.48 90)
				(length 2.54)
				(name "VC")
				(number "17")
			)
			(pin input line
				(at 10.16 -30.48 90)
				(length 2.54)
				(name "RT")
				(number "18")
			)
			(pin input line
				(at -15.24 -17.78 0)
				(length 2.54)
				(name "SPRD")
				(number "19")
			)
			(pin passive line
				(at -2.54 27.94 270)
				(length 2.54)
				(name "LSP")
				(number "2")
			)
			(pin no_connect line
				(at 17.78 -20.32 180)
				(length 2.54)
				(name "NC")
				(number "20")
			)
			(pin output line
				(at 17.78 0 180)
				(length 2.54)
				(name "VOUT")
				(number "21")
			)
			(pin input line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "TG2")
				(number "22")
			)
			(pin input line
				(at 10.16 27.94 270)
				(length 2.54)
				(name "SW2")
				(number "23")
			)
			(pin input line
				(at 17.78 17.78 180)
				(length 2.54)
				(name "BST2")
				(number "24")
			)
			(pin input line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "BG2")
				(number "25")
			)
			(pin input line
				(at -15.24 12.7 0)
				(length 2.54)
				(name "BG1")
				(number "26")
			)
			(pin input line
				(at -15.24 17.78 0)
				(length 2.54)
				(name "BST1")
				(number "27")
			)
			(pin input line
				(at -7.62 27.94 270)
				(length 2.54)
				(name "SW1")
				(number "28")
			)
			(pin power_in line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "GND")
				(number "29")
			)
			(pin passive line
				(at 2.54 27.94 270)
				(length 2.54)
				(name "LSN")
				(number "3")
			)
			(pin power_in line
				(at -15.24 2.54 0)
				(length 2.54)
				(name "VIN")
				(number "4")
			)
			(pin input line
				(at -15.24 -7.62 0)
				(length 2.54)
				(name "INTVCC")
				(number "5")
			)
			(pin input line
				(at -15.24 -5.08 0)
				(length 2.54)
				(name "ENUVLO")
				(number "6")
			)
			(pin input line
				(at 17.78 -22.86 180)
				(length 2.54)
				(name "RP")
				(number "7")
			)
			(pin input line
				(at 17.78 -15.24 180)
				(length 2.54)
				(name "PWM")
				(number "8")
			)
			(pin output line
				(at -15.24 -22.86 0)
				(length 2.54)
				(name "VREF")
				(number "9")
			)
		)
	)
	(symbol "LT8391IUFD#TRPBF"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -12.7244 26.7212 0)
		)
		(property "Value" "LT8391IUFD#TRPBF"
			(at -7.62 -36.83 0)
		)
		(property "Footprint" "QFN50P400X500X80-29N"
			(at 0 -43.18 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(property "MANUFACTURER" "Linear Technology"
			(at -1.27 -39.37 0)
		)
		(symbol "LT8391IUFD#TRPBF_0_0"
			(pin passive line
				(at -15.24 8.89 0)
				(length 2.54)
				(name "TG1")
				(number "1")
			)
			(pin input line
				(at -15.24 -11.43 0)
				(length 2.54)
				(name "CTRL1")
				(number "10")
			)
			(pin input line
				(at 17.78 -6.35 180)
				(length 2.54)
				(name "ISP")
				(number "11")
			)
			(pin input line
				(at 17.78 -10.16 180)
				(length 2.54)
				(name "ISN")
				(number "12")
			)
			(pin input line
				(at -15.24 -13.97 0)
				(length 2.54)
				(name "CTRL2")
				(number "13")
			)
			(pin output line
				(at -15.24 -8.89 0)
				(length 2.54)
				(name "~{FAULT}")
				(number "14")
			)
			(pin passive line
				(at -5.08 -27.94 90)
				(length 2.54)
				(name "SS")
				(number "15")
			)
			(pin input line
				(at 17.78 0 180)
				(length 2.54)
				(name "FB")
				(number "16")
			)
			(pin output line
				(at 2.54 -27.94 90)
				(length 2.54)
				(name "VC")
				(number "17")
			)
			(pin input line
				(at 10.16 -27.94 90)
				(length 2.54)
				(name "RT")
				(number "18")
			)
			(pin input line
				(at -15.24 -16.51 0)
				(length 2.54)
				(name "SYNC")
				(number "19")
			)
			(pin passive line
				(at -2.54 27.94 270)
				(length 2.54)
				(name "LSP")
				(number "2")
			)
			(pin input line
				(at 17.78 -16.51 180)
				(length 2.54)
				(name "PWMTG")
				(number "20")
			)
			(pin output line
				(at 17.78 2.54 180)
				(length 2.54)
				(name "VOUT")
				(number "21")
			)
			(pin input line
				(at 17.78 8.89 180)
				(length 2.54)
				(name "TG2")
				(number "22")
			)
			(pin input line
				(at 10.16 27.94 270)
				(length 2.54)
				(name "SW2")
				(number "23")
			)
			(pin input line
				(at 17.78 19.05 180)
				(length 2.54)
				(name "BST2")
				(number "24")
			)
			(pin input line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "BG2")
				(number "25")
			)
			(pin input line
				(at -15.24 15.24 0)
				(length 2.54)
				(name "BG1")
				(number "26")
			)
			(pin input line
				(at -15.24 19.05 0)
				(length 2.54)
				(name "BST1")
				(number "27")
			)
			(pin input line
				(at -7.62 27.94 270)
				(length 2.54)
				(name "SW1")
				(number "28")
			)
			(pin power_in line
				(at 17.78 11.43 180)
				(length 2.54)
				(name "GND")
				(number "29")
			)
			(pin passive line
				(at 2.54 27.94 270)
				(length 2.54)
				(name "LSN")
				(number "3")
			)
			(pin power_in line
				(at -15.24 5.08 0)
				(length 2.54)
				(name "VIN")
				(number "4")
			)
			(pin input line
				(at -15.24 -5.08 0)
				(length 2.54)
				(name "INTVCC")
				(number "5")
			)
			(pin input line
				(at -15.24 0 0)
				(length 2.54)
				(name "ENUVLO")
				(number "6")
			)
			(pin input line
				(at 17.78 -19.05 180)
				(length 2.54)
				(name "RP")
				(number "7")
			)
			(pin input line
				(at 17.78 -13.97 180)
				(length 2.54)
				(name "PWM")
				(number "8")
			)
			(pin output line
				(at -15.24 -19.05 0)
				(length 2.54)
				(name "VREF")
				(number "9")
			)
		)
	)
	(symbol "LT8392"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 2.54 0)
		)
		(property "Value" "LT8392"
			(at 0 0 0)
		)
		(property "Footprint" ""
			(at -5.08 -6.35 0)
		)
		(property "Datasheet" ""
			(at -5.08 -6.35 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "LT8392_0_1")
		(symbol "LT8392_1_1"
			(pin bidirectional line
				(at 20.32 10.16 180)
				(length 2.54)
				(name "BG1")
				(number "1")
			)
			(pin bidirectional line
				(at -20.32 -6.35 0)
				(length 2.54)
				(name "TEST")
				(number "10")
			)
			(pin bidirectional line
				(at -20.32 19.05 0)
				(length 2.54)
				(name "TRIM")
				(number "11")
			)
			(pin bidirectional line
				(at -20.32 11.43 0)
				(length 2.54)
				(name "VREF")
				(number "12")
			)
			(pin bidirectional line
				(at -20.32 2.54 0)
				(length 2.54)
				(name "CTRL")
				(number "13")
			)
			(pin bidirectional line
				(at 20.32 -29.21 180)
				(length 2.54)
				(name "ISP")
				(number "14")
			)
			(pin bidirectional line
				(at 20.32 -35.56 180)
				(length 2.54)
				(name "ISN")
				(number "15")
			)
			(pin bidirectional line
				(at -20.32 -13.97 0)
				(length 2.54)
				(name "ISMON")
				(number "16")
			)
			(pin bidirectional line
				(at -20.32 27.94 0)
				(length 2.54)
				(name "~{PGOOD}")
				(number "17")
			)
			(pin bidirectional line
				(at -6.35 -52.07 90)
				(length 2.54)
				(name "SS")
				(number "18")
			)
			(pin bidirectional line
				(at 20.32 -44.45 180)
				(length 2.54)
				(name "FB")
				(number "19")
			)
			(pin bidirectional line
				(at 20.32 33.02 180)
				(length 2.54)
				(name "BST1")
				(number "2")
			)
			(pin bidirectional line
				(at 3.81 -52.07 90)
				(length 2.54)
				(name "VC")
				(number "20")
			)
			(pin bidirectional line
				(at -1.27 -52.07 90)
				(length 2.54)
				(name "RT")
				(number "21")
			)
			(pin bidirectional line
				(at -20.32 -22.86 0)
				(length 2.54)
				(name "SYNC/SPRD")
				(number "22")
			)
			(pin bidirectional line
				(at -20.32 -44.45 0)
				(length 2.54)
				(name "EXTVCC")
				(number "23")
			)
			(pin bidirectional line
				(at 20.32 40.64 180)
				(length 2.54)
				(name "VOUT")
				(number "24")
			)
			(pin bidirectional line
				(at 20.32 -22.86 180)
				(length 2.54)
				(name "TG2")
				(number "25")
			)
			(pin bidirectional line
				(at 20.32 -19.05 180)
				(length 2.54)
				(name "SW2")
				(number "26")
			)
			(pin bidirectional line
				(at 20.32 36.83 180)
				(length 2.54)
				(name "BST2")
				(number "27")
			)
			(pin bidirectional line
				(at 20.32 -15.24 180)
				(length 2.54)
				(name "BG2")
				(number "28")
			)
			(pin bidirectional line
				(at 8.89 -52.07 90)
				(length 2.54)
				(name "GND")
				(number "29")
			)
			(pin bidirectional line
				(at 20.32 17.78 180)
				(length 2.54)
				(name "SW1")
				(number "3")
			)
			(pin bidirectional line
				(at 20.32 24.13 180)
				(length 2.54)
				(name "TG1")
				(number "4")
			)
			(pin bidirectional line
				(at 20.32 -2.54 180)
				(length 2.54)
				(name "LSP")
				(number "5")
			)
			(pin bidirectional line
				(at 20.32 -8.89 180)
				(length 2.54)
				(name "LSN")
				(number "6")
			)
			(pin bidirectional line
				(at 6.35 50.8 270)
				(length 2.54)
				(name "VIN")
				(number "7")
			)
			(pin bidirectional line
				(at -20.32 40.64 0)
				(length 2.54)
				(name "INTVCC")
				(number "8")
			)
			(pin bidirectional line
				(at -5.08 50.8 270)
				(length 2.54)
				(name "EN/UVLO")
				(number "9")
			)
		)
	)
	(symbol "LT8392smt"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 2.54 35.56 0)
		)
		(property "Value" "LT8392smt"
			(at 2.54 33.02 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "LT8392smt_0_1")
		(symbol "LT8392smt_1_1"
			(pin bidirectional line
				(at -22.86 38.1 0)
				(length 2.54)
				(name "TG1")
				(number "1")
			)
			(pin bidirectional line
				(at -5.08 -10.16 90)
				(length 2.54)
				(name "CTRL")
				(number "10")
			)
			(pin bidirectional line
				(at 0 -10.16 90)
				(length 2.54)
				(name "ISP")
				(number "11")
			)
			(pin bidirectional line
				(at 5.08 -10.16 90)
				(length 2.54)
				(name "ISN")
				(number "12")
			)
			(pin bidirectional line
				(at 10.16 -10.16 90)
				(length 2.54)
				(name "ISMON")
				(number "13")
			)
			(pin bidirectional line
				(at 15.24 -10.16 90)
				(length 2.54)
				(name "~{PGOOD}")
				(number "14")
			)
			(pin bidirectional line
				(at 27.94 2.54 180)
				(length 2.54)
				(name "SS")
				(number "15")
			)
			(pin bidirectional line
				(at 27.94 7.62 180)
				(length 2.54)
				(name "FB")
				(number "16")
			)
			(pin bidirectional line
				(at 27.94 12.7 180)
				(length 2.54)
				(name "VC")
				(number "17")
			)
			(pin bidirectional line
				(at 27.94 17.78 180)
				(length 2.54)
				(name "RT")
				(number "18")
			)
			(pin bidirectional line
				(at 27.94 22.86 180)
				(length 2.54)
				(name "SYNC/SPRD")
				(number "19")
			)
			(pin bidirectional line
				(at -22.86 33.02 0)
				(length 2.54)
				(name "LSP")
				(number "2")
			)
			(pin bidirectional line
				(at 27.94 27.94 180)
				(length 2.54)
				(name "EXTVCC")
				(number "20")
			)
			(pin bidirectional line
				(at 27.94 33.02 180)
				(length 2.54)
				(name "VOUT")
				(number "21")
			)
			(pin bidirectional line
				(at 27.94 38.1 180)
				(length 2.54)
				(name "TG2")
				(number "22")
			)
			(pin bidirectional line
				(at 15.24 50.8 270)
				(length 2.54)
				(name "SW2")
				(number "23")
			)
			(pin bidirectional line
				(at 10.16 50.8 270)
				(length 2.54)
				(name "BST2")
				(number "24")
			)
			(pin bidirectional line
				(at 5.08 50.8 270)
				(length 2.54)
				(name "BG2")
				(number "25")
			)
			(pin bidirectional line
				(at 0 50.8 270)
				(length 2.54)
				(name "BG1")
				(number "26")
			)
			(pin bidirectional line
				(at -5.08 50.8 270)
				(length 2.54)
				(name "BST1")
				(number "27")
			)
			(pin bidirectional line
				(at -10.16 50.8 270)
				(length 2.54)
				(name "SW1")
				(number "28")
			)
			(pin bidirectional line
				(at -15.24 50.8 270)
				(length 2.54)
				(name "GND")
				(number "29")
			)
			(pin bidirectional line
				(at -22.86 27.94 0)
				(length 2.54)
				(name "LSN")
				(number "3")
			)
			(pin bidirectional line
				(at -22.86 22.86 0)
				(length 2.54)
				(name "VIN")
				(number "4")
			)
			(pin bidirectional line
				(at -22.86 17.78 0)
				(length 2.54)
				(name "INTVCC")
				(number "5")
			)
			(pin bidirectional line
				(at -22.86 12.7 0)
				(length 2.54)
				(name "EN/UVLO")
				(number "6")
			)
			(pin bidirectional line
				(at -22.86 7.62 0)
				(length 2.54)
				(name "TEST")
				(number "7")
			)
			(pin bidirectional line
				(at -22.86 2.54 0)
				(length 2.54)
				(name "TRIM")
				(number "8")
			)
			(pin bidirectional line
				(at -10.16 -10.16 90)
				(length 2.54)
				(name "VREF")
				(number "9")
			)
		)
	)
	(symbol "LT8612IUDE#PBF"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -8.89 24.13 0)
		)
		(property "Value" "LT8612IUDE#PBF"
			(at -7.62 21.59 0)
		)
		(property "Footprint" "QFN50P300X600X80-29N"
			(at 0 2.54 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(property "PARTREV" "A"
			(at 0 0 0)
		)
		(property "MANUFACTURER" "ANALOG DEVICES"
			(at 0 -2.54 0)
		)
		(property "STANDARD" "IPC-7351B"
			(at -6.35 0 0)
		)
		(symbol "LT8612IUDE#PBF_0_0"
			(pin input clock
				(at -8.89 -12.7 90)
				(length 5.08)
				(name "SYNC")
				(number "1")
			)
			(pin power_in line
				(at 3.81 -12.7 90)
				(length 5.08)
				(name "PGND")
				(number "10")
			)
			(pin power_in line
				(at 1.27 -12.7 90)
				(length 5.08)
				(name "GND")
				(number "11")
			)
			(pin power_in line
				(at -1.27 -12.7 90)
				(length 5.08)
				(name "GND")
				(number "12")
			)
			(pin power_in line
				(at -3.81 -12.7 90)
				(length 5.08)
				(name "GND")
				(number "13")
			)
			(pin power_in line
				(at -6.35 -12.7 90)
				(length 5.08)
				(name "GND")
				(number "14")
			)
			(pin output line
				(at 17.78 17.78 180)
				(length 5.08)
				(name "SW")
				(number "15")
			)
			(pin output line
				(at 17.78 15.24 180)
				(length 5.08)
				(name "SW")
				(number "16")
			)
			(pin output line
				(at 17.78 12.7 180)
				(length 5.08)
				(name "SW")
				(number "17")
			)
			(pin output line
				(at 17.78 10.16 180)
				(length 5.08)
				(name "SW")
				(number "18")
			)
			(pin output line
				(at 17.78 7.62 180)
				(length 5.08)
				(name "SW")
				(number "19")
			)
			(pin output line
				(at -17.78 7.62 0)
				(length 5.08)
				(name "TR/SS")
				(number "2")
			)
			(pin passive line
				(at 17.78 20.32 180)
				(length 5.08)
				(name "BST")
				(number "20")
			)
			(pin output line
				(at -17.78 10.16 0)
				(length 5.08)
				(name "INTVCC")
				(number "21")
			)
			(pin input line
				(at 17.78 2.54 180)
				(length 5.08)
				(name "BIAS")
				(number "22")
			)
			(pin open_collector line
				(at 17.78 5.08 180)
				(length 5.08)
				(name "PG")
				(number "23")
			)
			(pin input line
				(at 17.78 0 180)
				(length 5.08)
				(name "FB")
				(number "24")
			)
			(pin passive line
				(at 17.78 -2.54 180)
				(length 5.08)
				(name "EP")
				(number "29")
			)
			(pin passive line
				(at -17.78 5.08 0)
				(length 5.08)
				(name "RT")
				(number "3")
			)
			(pin input line
				(at -17.78 12.7 0)
				(length 5.08)
				(name "EN/UV")
				(number "4")
			)
			(pin input line
				(at -17.78 20.32 0)
				(length 5.08)
				(name "VIN")
				(number "5")
			)
			(pin input line
				(at -17.78 17.78 0)
				(length 5.08)
				(name "VIN")
				(number "6")
			)
			(pin input line
				(at -17.78 15.24 0)
				(length 5.08)
				(name "VIN")
				(number "7")
			)
			(pin power_in line
				(at 6.35 -12.7 90)
				(length 5.08)
				(name "PGND")
				(number "8")
			)
			(pin power_in line
				(at 8.89 -12.7 90)
				(length 5.08)
				(name "PGND")
				(number "9")
			)
		)
	)
	(symbol "LT8618EDDB#TRMPBF"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -5.08 12.7 0)
		)
		(property "Value" "LT8618EDDB#TRMPBF"
			(at -11.43 16.51 0)
		)
		(property "Footprint" "SON50P300X200X80-11N"
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(property "MAXIMUM_PACKAGE_HEIGHT" "0.8mm"
			(at 0 0 0)
		)
		(property "MANUFACTURER" "Analog Devices"
			(at 0 0 0)
		)
		(property "PARTREV" "A"
			(at 0 0 0)
		)
		(property "STANDARD" "IPC 7351B"
			(at 0 0 0)
		)
		(symbol "LT8618EDDB#TRMPBF_0_0"
			(pin passive line
				(at 13.97 10.16 180)
				(length 5.08)
				(name "BST")
				(number "1")
			)
			(pin input line
				(at -13.97 10.16 0)
				(length 5.08)
				(name "VIN")
				(number "10")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 5.08)
				(name "GND")
				(number "11")
			)
			(pin output line
				(at 13.97 5.08 180)
				(length 5.08)
				(name "SW")
				(number "2")
			)
			(pin passive line
				(at 13.97 2.54 180)
				(length 5.08)
				(name "BIAS")
				(number "3")
			)
			(pin output line
				(at -13.97 0 0)
				(length 5.08)
				(name "INTVCC")
				(number "4")
			)
			(pin input line
				(at -13.97 -5.08 0)
				(length 5.08)
				(name "RT")
				(number "5")
			)
			(pin output line
				(at 13.97 -2.54 180)
				(length 5.08)
				(name "FB")
				(number "6")
			)
			(pin input line
				(at -13.97 -2.54 0)
				(length 5.08)
				(name "TR/SS")
				(number "7")
			)
			(pin output line
				(at -13.97 2.54 0)
				(length 5.08)
				(name "PG")
				(number "8")
			)
			(pin input line
				(at -13.97 5.08 0)
				(length 5.08)
				(name "EN/UV")
				(number "9")
			)
		)
	)
	(symbol "LT8645SIV#PBF"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -11.43 16.51 0)
		)
		(property "Value" "LT8645SIV#PBF"
			(at -6.35 11.43 0)
		)
		(property "Footprint" "CONV_T8645SIV#PBF"
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(property "PARTREV" "A"
			(at 0 0 0)
		)
		(property "MAXIMUM_PACKAGE_HEIGHT" "1.03mm"
			(at 0 0 0)
		)
		(property "STANDARD" "Manufacturer Recommendations"
			(at 0 0 0)
		)
		(property "MANUFACTURER" "Analog Devices"
			(at 0 0 0)
		)
		(symbol "LT8645SIV#PBF_0_0"
			(pin passive line
				(at 17.78 -12.7 180)
				(length 5.08)
				(name "BIAS")
				(number "1")
			)
			(pin power_in line
				(at -6.35 -27.94 90)
				(length 5.08)
				(name "GND")
				(number "10")
			)
			(pin passive line
				(at 17.78 5.08 180)
				(length 5.08)
				(name "BST")
				(number "11")
			)
			(pin output line
				(at 17.78 -7.62 180)
				(length 5.08)
				(name "SW")
				(number "12")
			)
			(pin output line
				(at 17.78 -5.08 180)
				(length 5.08)
				(name "SW")
				(number "13")
			)
			(pin output line
				(at 17.78 -2.54 180)
				(length 5.08)
				(name "SW")
				(number "14")
			)
			(pin output line
				(at 17.78 0 180)
				(length 5.08)
				(name "SW")
				(number "15")
			)
			(pin output line
				(at 17.78 2.54 180)
				(length 5.08)
				(name "SW")
				(number "16")
			)
			(pin power_in line
				(at -5.08 -27.94 90)
				(length 5.08)
				(name "GND")
				(number "17")
			)
			(pin power_in line
				(at -3.81 -27.94 90)
				(length 5.08)
				(name "GND")
				(number "18")
			)
			(pin power_in line
				(at -2.54 -27.94 90)
				(length 5.08)
				(name "GND")
				(number "19")
			)
			(pin power_in line
				(at -17.78 -5.08 0)
				(length 5.08)
				(name "INTVCC")
				(number "2")
			)
			(pin input line
				(at -17.78 5.08 0)
				(length 5.08)
				(name "VIN")
				(number "21")
			)
			(pin input line
				(at -17.78 2.54 0)
				(length 5.08)
				(name "VIN")
				(number "22")
			)
			(pin input line
				(at -17.78 0 0)
				(length 5.08)
				(name "VIN")
				(number "23")
			)
			(pin input line
				(at -17.78 -2.54 0)
				(length 5.08)
				(name "EN/UV")
				(number "25")
			)
			(pin passive line
				(at -17.78 -10.16 0)
				(length 5.08)
				(name "RT")
				(number "26")
			)
			(pin output clock
				(at 17.78 10.16 180)
				(length 5.08)
				(name "CLKOUT")
				(number "27")
			)
			(pin input line
				(at -17.78 -12.7 0)
				(length 5.08)
				(name "SYNC/MODE")
				(number "28")
			)
			(pin output line
				(at -17.78 -7.62 0)
				(length 5.08)
				(name "TR/SS")
				(number "29")
			)
			(pin power_in line
				(at -1.27 -27.94 90)
				(length 5.08)
				(name "GND")
				(number "30")
			)
			(pin output line
				(at 17.78 -10.16 180)
				(length 5.08)
				(name "PG")
				(number "31")
			)
			(pin input line
				(at 17.78 -15.24 180)
				(length 5.08)
				(name "FB")
				(number "32")
			)
			(pin power_in line
				(at 0 -27.94 90)
				(length 5.08)
				(name "GND")
				(number "33")
			)
			(pin power_in line
				(at 1.27 -27.94 90)
				(length 5.08)
				(name "GND")
				(number "34")
			)
			(pin power_in line
				(at 2.54 -27.94 90)
				(length 5.08)
				(name "GND")
				(number "35")
			)
			(pin power_in line
				(at 3.81 -27.94 90)
				(length 5.08)
				(name "GND")
				(number "36")
			)
			(pin power_in line
				(at 5.08 -27.94 90)
				(length 5.08)
				(name "GND")
				(number "37")
			)
			(pin power_in line
				(at 6.35 -27.94 90)
				(length 5.08)
				(name "GND")
				(number "38")
			)
			(pin input line
				(at -17.78 12.7 0)
				(length 5.08)
				(name "VIN")
				(number "4")
			)
			(pin input line
				(at -17.78 10.16 0)
				(length 5.08)
				(name "VIN")
				(number "5")
			)
			(pin input line
				(at -17.78 7.62 0)
				(length 5.08)
				(name "VIN")
				(number "6")
			)
			(pin power_in line
				(at 7.62 -27.94 90)
				(length 5.08)
				(name "GND")
				(number "8")
			)
			(pin power_in line
				(at 8.89 -27.94 90)
				(length 5.08)
				(name "GND")
				(number "9")
			)
		)
	)
	(symbol "LTC1760"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -12.7 -39.37 0)
		)
		(property "Value" "LTC1760"
			(at 7.62 -39.37 0)
		)
		(property "Footprint" ""
			(at -1.27 2.54 0)
		)
		(property "Datasheet" ""
			(at -1.27 2.54 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "LTC1760_0_1")
		(symbol "LTC1760_1_1"
			(pin passive line
				(at -15.24 12.7 0)
				(length 2.54)
				(name "VPLUS")
				(number "1")
			)
			(pin passive line
				(at 13.97 -7.62 180)
				(length 2.54)
				(name "GB2O")
				(number "10")
			)
			(pin passive line
				(at 13.97 -10.16 180)
				(length 2.54)
				(name "GB2I")
				(number "11")
			)
			(pin passive line
				(at 13.97 20.32 180)
				(length 2.54)
				(name "LOPWR")
				(number "12")
			)
			(pin passive line
				(at 13.97 0 180)
				(length 2.54)
				(name "VSET")
				(number "13")
			)
			(pin passive line
				(at -15.24 17.78 0)
				(length 2.54)
				(name "ITH")
				(number "14")
			)
			(pin passive line
				(at -15.24 15.24 0)
				(length 2.54)
				(name "ISET")
				(number "15")
			)
			(pin passive line
				(at -15.24 30.48 0)
				(length 2.54)
				(name "DCDIV")
				(number "16")
			)
			(pin passive line
				(at 13.97 -22.86 180)
				(length 2.54)
				(name "SCL_B2")
				(number "17")
			)
			(pin passive line
				(at -15.24 -20.32 0)
				(length 2.54)
				(name "SCL")
				(number "18")
			)
			(pin passive line
				(at 13.97 -33.02 180)
				(length 2.54)
				(name "SCL_B1")
				(number "19")
			)
			(pin passive line
				(at -15.24 -10.16 0)
				(length 2.54)
				(name "BAT2")
				(number "2")
			)
			(pin passive line
				(at -15.24 -25.4 0)
				(length 2.54)
				(name "VDDS")
				(number "20")
			)
			(pin passive line
				(at 13.97 -25.4 180)
				(length 2.54)
				(name "SDA_B2")
				(number "21")
			)
			(pin passive line
				(at -15.24 -22.86 0)
				(length 2.54)
				(name "SDA")
				(number "22")
			)
			(pin passive line
				(at 13.97 -35.56 180)
				(length 2.54)
				(name "SDA_B1")
				(number "23")
			)
			(pin passive line
				(at -15.24 7.62 0)
				(length 2.54)
				(name "GND")
				(number "24")
			)
			(pin passive line
				(at -15.24 -15.24 0)
				(length 2.54)
				(name "VCC2")
				(number "25")
			)
			(pin passive line
				(at -15.24 -33.02 0)
				(length 2.54)
				(name "MODE")
				(number "26")
			)
			(pin passive line
				(at 13.97 -20.32 180)
				(length 2.54)
				(name "TH2B")
				(number "27")
			)
			(pin passive line
				(at 13.97 -17.78 180)
				(length 2.54)
				(name "TH2A")
				(number "28")
			)
			(pin passive line
				(at -15.24 -17.78 0)
				(length 2.54)
				(name "INTB")
				(number "29")
			)
			(pin passive line
				(at -15.24 -7.62 0)
				(length 2.54)
				(name "BAT1")
				(number "3")
			)
			(pin passive line
				(at 13.97 -27.94 180)
				(length 2.54)
				(name "TH1A")
				(number "30")
			)
			(pin passive line
				(at 13.97 -30.48 180)
				(length 2.54)
				(name "TH1B")
				(number "31")
			)
			(pin passive line
				(at -15.24 -30.48 0)
				(length 2.54)
				(name "ILIM")
				(number "32")
			)
			(pin passive line
				(at -15.24 -27.94 0)
				(length 2.54)
				(name "VLIM")
				(number "33")
			)
			(pin passive line
				(at 13.97 2.54 180)
				(length 2.54)
				(name "CSN")
				(number "34")
			)
			(pin passive line
				(at 13.97 5.08 180)
				(length 2.54)
				(name "CSP")
				(number "35")
			)
			(pin passive line
				(at -15.24 33.02 0)
				(length 2.54)
				(name "CLP")
				(number "36")
			)
			(pin passive line
				(at -15.24 10.16 0)
				(length 2.54)
				(name "COMP1")
				(number "37")
			)
			(pin passive line
				(at -15.24 5.08 0)
				(length 2.54)
				(name "PGND")
				(number "38")
			)
			(pin passive line
				(at 13.97 7.62 180)
				(length 2.54)
				(name "BGATE")
				(number "39")
			)
			(pin passive line
				(at 13.97 22.86 180)
				(length 2.54)
				(name "SCN")
				(number "4")
			)
			(pin passive line
				(at 13.97 10.16 180)
				(length 2.54)
				(name "VCC")
				(number "40")
			)
			(pin passive line
				(at 13.97 33.02 180)
				(length 2.54)
				(name "DCIN")
				(number "41")
			)
			(pin passive line
				(at 13.97 12.7 180)
				(length 2.54)
				(name "SW")
				(number "42")
			)
			(pin passive line
				(at 13.97 15.24 180)
				(length 2.54)
				(name "BOOST")
				(number "43")
			)
			(pin passive line
				(at 13.97 17.78 180)
				(length 2.54)
				(name "TGATE")
				(number "44")
			)
			(pin passive line
				(at -15.24 0 0)
				(length 2.54)
				(name "SHC1")
				(number "45")
			)
			(pin passive line
				(at -15.24 2.54 0)
				(length 2.54)
				(name "GHC1")
				(number "46")
			)
			(pin passive line
				(at -15.24 -2.54 0)
				(length 2.54)
				(name "GHC2")
				(number "47")
			)
			(pin passive line
				(at -15.24 -5.08 0)
				(length 2.54)
				(name "SHC2")
				(number "48")
			)
			(pin passive line
				(at 13.97 25.4 180)
				(length 2.54)
				(name "SCP")
				(number "5")
			)
			(pin passive line
				(at 13.97 27.94 180)
				(length 2.54)
				(name "GDCO")
				(number "6")
			)
			(pin passive line
				(at 13.97 30.48 180)
				(length 2.54)
				(name "GDCI")
				(number "7")
			)
			(pin passive line
				(at 13.97 -2.54 180)
				(length 2.54)
				(name "GB1O")
				(number "8")
			)
			(pin passive line
				(at 13.97 -5.08 180)
				(length 2.54)
				(name "GB1I")
				(number "9")
			)
		)
	)
	(symbol "LTC1867"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -10.16 12.7 0)
		)
		(property "Value" "LTC1867"
			(at 7.62 12.7 0)
		)
		(property "Footprint" ""
			(at -2.54 15.24 0)
		)
		(property "Datasheet" ""
			(at -2.54 15.24 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "LTC1867_1_1"
			(pin input line
				(at -13.97 8.89 0)
				(length 2.54)
				(name "CH0")
				(number "1")
			)
			(pin input line
				(at 13.97 -6.35 180)
				(length 2.54)
				(name "VREF")
				(number "10")
			)
			(pin input line
				(at 13.97 -3.81 180)
				(length 2.54)
				(name "~{CS/CONV}")
				(number "11")
			)
			(pin input line
				(at 13.97 -1.27 180)
				(length 2.54)
				(name "SCK")
				(number "12")
			)
			(pin input line
				(at 13.97 1.27 180)
				(length 2.54)
				(name "SDO")
				(number "13")
			)
			(pin input line
				(at 13.97 3.81 180)
				(length 2.54)
				(name "SDI")
				(number "14")
			)
			(pin input line
				(at 13.97 6.35 180)
				(length 2.54)
				(name "GND")
				(number "15")
			)
			(pin input line
				(at 13.97 8.89 180)
				(length 2.54)
				(name "VDD")
				(number "16")
			)
			(pin input line
				(at -13.97 6.35 0)
				(length 2.54)
				(name "CH1")
				(number "2")
			)
			(pin input line
				(at -13.97 3.81 0)
				(length 2.54)
				(name "CH2")
				(number "3")
			)
			(pin input line
				(at -13.97 1.27 0)
				(length 2.54)
				(name "CH3")
				(number "4")
			)
			(pin input line
				(at -13.97 -1.27 0)
				(length 2.54)
				(name "CH4")
				(number "5")
			)
			(pin input line
				(at -13.97 -3.81 0)
				(length 2.54)
				(name "CH5")
				(number "6")
			)
			(pin input line
				(at -13.97 -6.35 0)
				(length 2.54)
				(name "CH6")
				(number "7")
			)
			(pin input line
				(at -13.97 -8.89 0)
				(length 2.54)
				(name "CH7/COM")
				(number "8")
			)
			(pin input line
				(at 13.97 -8.89 180)
				(length 2.54)
				(name "REFCOMP")
				(number "9")
			)
		)
	)
	(symbol "LTC2066"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 6.35 2.54 0)
		)
		(property "Value" "LTC2066"
			(at 15.24 2.54 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "LTC2066_0_0"
			(text "+"
				(at 10.922 -5.08 0)
			)
			(text "-"
				(at 10.922 -7.366 0)
			)
		)
		(symbol "LTC2066_0_1")
		(symbol "LTC2066_1_1"
			(pin input line
				(at 2.54 -1.27 0)
				(length 2.54)
				(name "IN+")
				(number "1")
			)
			(pin bidirectional line
				(at 2.54 -6.35 0)
				(length 2.54)
				(name "V-")
				(number "2")
			)
			(pin bidirectional line
				(at 2.54 -11.43 0)
				(length 2.54)
				(name "IN-")
				(number "3")
			)
			(pin bidirectional line
				(at 19.05 -11.43 180)
				(length 2.54)
				(name "OUT")
				(number "4")
			)
			(pin bidirectional line
				(at 19.05 -6.35 180)
				(length 2.54)
				(name "~{SH}")
				(number "5")
			)
			(pin bidirectional line
				(at 19.05 -1.27 180)
				(length 2.54)
				(name "V+")
				(number "6")
			)
		)
	)
	(symbol "LTC2496"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 16.51 0)
		)
		(property "Value" "LTC2496"
			(at 10.16 16.51 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "LTC2496_0_0"
			(text "Exposed Pad, Solder Side"
				(at -1.27 -19.05 900)
			)
		)
		(symbol "LTC2496_0_1")
		(symbol "LTC2496_1_1"
			(pin bidirectional line
				(at -6.35 -49.53 90)
				(length 2.54)
				(name "GND")
				(number "1")
			)
			(pin input line
				(at -11.43 6.35 0)
				(length 2.54)
				(name "CH2")
				(number "10")
			)
			(pin input line
				(at -11.43 3.81 0)
				(length 2.54)
				(name "CH3")
				(number "11")
			)
			(pin input line
				(at -11.43 1.27 0)
				(length 2.54)
				(name "CH4")
				(number "12")
			)
			(pin input line
				(at -11.43 -1.27 0)
				(length 2.54)
				(name "CH5")
				(number "13")
			)
			(pin input line
				(at -11.43 -3.81 0)
				(length 2.54)
				(name "CH6")
				(number "14")
			)
			(pin input line
				(at -11.43 -6.35 0)
				(length 2.54)
				(name "CH7")
				(number "15")
			)
			(pin input line
				(at -11.43 -8.89 0)
				(length 2.54)
				(name "CH8")
				(number "16")
			)
			(pin input line
				(at -11.43 -11.43 0)
				(length 2.54)
				(name "CH9")
				(number "17")
			)
			(pin input line
				(at -11.43 -13.97 0)
				(length 2.54)
				(name "CH10")
				(number "18")
			)
			(pin input line
				(at -11.43 -16.51 0)
				(length 2.54)
				(name "CH11")
				(number "19")
			)
			(pin bidirectional line
				(at 16.51 -11.43 180)
				(length 2.54)
				(name "NC")
				(number "2")
			)
			(pin input line
				(at -11.43 -19.05 0)
				(length 2.54)
				(name "CH12")
				(number "20")
			)
			(pin input line
				(at -11.43 -21.59 0)
				(length 2.54)
				(name "CH13")
				(number "21")
			)
			(pin input line
				(at -11.43 -24.13 0)
				(length 2.54)
				(name "CH14")
				(number "22")
			)
			(pin input line
				(at -11.43 -26.67 0)
				(length 2.54)
				(name "CH15")
				(number "23")
			)
			(pin bidirectional line
				(at 16.51 -6.35 180)
				(length 2.54)
				(name "MUXOUTP")
				(number "24")
			)
			(pin bidirectional line
				(at 16.51 0 180)
				(length 2.54)
				(name "ADCINP")
				(number "25")
			)
			(pin bidirectional line
				(at 16.51 6.35 180)
				(length 2.54)
				(name "ADCINN")
				(number "26")
			)
			(pin bidirectional line
				(at 16.51 12.7 180)
				(length 2.54)
				(name "MUXOUTN")
				(number "27")
			)
			(pin bidirectional line
				(at 2.54 17.78 270)
				(length 2.54)
				(name "VCC")
				(number "28")
			)
			(pin input line
				(at -11.43 -35.56 0)
				(length 2.54)
				(name "REF+")
				(number "29")
			)
			(pin bidirectional line
				(at -3.81 -49.53 90)
				(length 2.54)
				(name "GND")
				(number "3")
			)
			(pin input line
				(at -11.43 -39.37 0)
				(length 2.54)
				(name "REF-")
				(number "30")
			)
			(pin bidirectional line
				(at 6.35 -49.53 90)
				(length 2.54)
				(name "GND")
				(number "31")
			)
			(pin bidirectional line
				(at 8.89 -49.53 90)
				(length 2.54)
				(name "GND")
				(number "32")
			)
			(pin bidirectional line
				(at 11.43 -49.53 90)
				(length 2.54)
				(name "GND")
				(number "33")
			)
			(pin bidirectional line
				(at 16.51 -16.51 180)
				(length 2.54)
				(name "SDI")
				(number "34")
			)
			(pin bidirectional line
				(at 16.51 -20.32 180)
				(length 2.54)
				(name "FO")
				(number "35")
			)
			(pin bidirectional line
				(at 16.51 -25.4 180)
				(length 2.54)
				(name "~{CS}")
				(number "36")
			)
			(pin bidirectional line
				(at 16.51 -27.94 180)
				(length 2.54)
				(name "SDO")
				(number "37")
			)
			(pin bidirectional line
				(at 16.51 -30.48 180)
				(length 2.54)
				(name "SCK")
				(number "38")
			)
			(pin bidirectional line
				(at 16.51 -38.1 180)
				(length 2.54)
				(name "GND")
				(number "39")
			)
			(pin bidirectional line
				(at -1.27 -49.53 90)
				(length 2.54)
				(name "GND")
				(number "4")
			)
			(pin bidirectional line
				(at 1.27 -49.53 90)
				(length 2.54)
				(name "GND")
				(number "5")
			)
			(pin bidirectional line
				(at 3.81 -49.53 90)
				(length 2.54)
				(name "GND")
				(number "6")
			)
			(pin input line
				(at -11.43 -30.48 0)
				(length 2.54)
				(name "COM")
				(number "7")
			)
			(pin input line
				(at -11.43 11.43 0)
				(length 2.54)
				(name "CH0")
				(number "8")
			)
			(pin input line
				(at -11.43 8.89 0)
				(length 2.54)
				(name "CH1")
				(number "9")
			)
		)
	)
	(symbol "LTC4162"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -20.32 -40.64 0)
		)
		(property "Value" "LTC4162"
			(at 17.78 -40.64 0)
		)
		(property "Footprint" ""
			(at -2.54 15.24 0)
		)
		(property "Datasheet" ""
			(at -2.54 15.24 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "LTC4162_0_1")
		(symbol "LTC4162_1_1"
			(pin passive line
				(at 24.13 8.89 180)
				(length 2.54)
				(name "BOOST")
				(number "1")
			)
			(pin passive line
				(at -24.13 -30.48 0)
				(length 2.54)
				(name "NTC")
				(number "10")
			)
			(pin passive line
				(at -24.13 -17.78 0)
				(length 2.54)
				(name "RT")
				(number "11")
			)
			(pin passive line
				(at -24.13 -10.16 0)
				(length 2.54)
				(name "~{SMBALERT}")
				(number "12")
			)
			(pin passive line
				(at -24.13 -5.08 0)
				(length 2.54)
				(name "SCL")
				(number "13")
			)
			(pin passive line
				(at -24.13 -7.62 0)
				(length 2.54)
				(name "SDA")
				(number "14")
			)
			(pin passive line
				(at -24.13 10.16 0)
				(length 2.54)
				(name "DVCC")
				(number "15")
			)
			(pin passive line
				(at -24.13 -15.24 0)
				(length 2.54)
				(name "SYNC")
				(number "16")
			)
			(pin passive line
				(at -24.13 15.24 0)
				(length 2.54)
				(name "CELLS0")
				(number "17")
			)
			(pin passive line
				(at -24.13 12.7 0)
				(length 2.54)
				(name "CELLS1")
				(number "18")
			)
			(pin passive line
				(at 24.13 -33.02 180)
				(length 2.54)
				(name "BATSENS+")
				(number "19")
			)
			(pin passive line
				(at -24.13 26.67 0)
				(length 2.54)
				(name "INTVCC")
				(number "2")
			)
			(pin passive line
				(at 24.13 -24.13 180)
				(length 2.54)
				(name "CSN")
				(number "20")
			)
			(pin passive line
				(at 24.13 -16.51 180)
				(length 2.54)
				(name "CSP")
				(number "21")
			)
			(pin passive line
				(at 24.13 16.51 180)
				(length 2.54)
				(name "BATFET")
				(number "22")
			)
			(pin passive line
				(at -5.08 -40.64 90)
				(length 2.54)
				(name "PGND1")
				(number "23")
			)
			(pin passive line
				(at 0 -40.64 90)
				(length 2.54)
				(name "PGND2")
				(number "24")
			)
			(pin passive line
				(at 24.13 -1.27 180)
				(length 2.54)
				(name "SW")
				(number "25")
			)
			(pin passive line
				(at 24.13 -3.81 180)
				(length 2.54)
				(name "SW")
				(number "26")
			)
			(pin passive line
				(at 24.13 26.67 180)
				(length 2.54)
				(name "VOUT")
				(number "27")
			)
			(pin passive line
				(at 24.13 24.13 180)
				(length 2.54)
				(name "VOUT")
				(number "28")
			)
			(pin passive line
				(at 5.08 -40.64 90)
				(length 2.54)
				(name "EPAD")
				(number "29")
			)
			(pin passive line
				(at 13.97 35.56 270)
				(length 2.54)
				(name "VOUTA")
				(number "3")
			)
			(pin passive line
				(at 7.62 35.56 270)
				(length 2.54)
				(name "CLN")
				(number "4")
			)
			(pin passive line
				(at 0 35.56 270)
				(length 2.54)
				(name "CLP")
				(number "5")
			)
			(pin passive line
				(at -8.89 35.56 270)
				(length 2.54)
				(name "INFET")
				(number "6")
			)
			(pin passive line
				(at -15.24 35.56 270)
				(length 2.54)
				(name "VIN")
				(number "7")
			)
			(pin passive line
				(at -24.13 24.13 0)
				(length 2.54)
				(name "VCC2P5")
				(number "8")
			)
			(pin passive line
				(at -24.13 -33.02 0)
				(length 2.54)
				(name "NTCBIAS")
				(number "9")
			)
		)
	)
	(symbol "LTC4162EUFD-L42"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 20.32 38.1 0)
		)
		(property "Value" "LTC4162EUFD-L42"
			(at 2.54 20.32 0)
		)
		(property "Footprint" ""
			(at 0 15.24 0)
		)
		(property "Datasheet" ""
			(at 0 15.24 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "LTC4162EUFD-L42_0_1")
		(symbol "LTC4162EUFD-L42_1_1"
			(pin passive line
				(at 25.4 11.43 180)
				(length 2.54)
				(name "BOOST")
				(number "1")
			)
			(pin passive line
				(at -22.86 -27.94 0)
				(length 2.54)
				(name "NTC")
				(number "10")
			)
			(pin passive line
				(at -22.86 -15.24 0)
				(length 2.54)
				(name "RT")
				(number "11")
			)
			(pin passive line
				(at -22.86 -7.62 0)
				(length 2.54)
				(name "~{SMBALERT}")
				(number "12")
			)
			(pin passive line
				(at -22.86 -2.54 0)
				(length 2.54)
				(name "SCL")
				(number "13")
			)
			(pin passive line
				(at -22.86 -5.08 0)
				(length 2.54)
				(name "SDA")
				(number "14")
			)
			(pin passive line
				(at -22.86 12.7 0)
				(length 2.54)
				(name "DVCC")
				(number "15")
			)
			(pin passive line
				(at -22.86 -12.7 0)
				(length 2.54)
				(name "SYNC")
				(number "16")
			)
			(pin passive line
				(at -22.86 17.78 0)
				(length 2.54)
				(name "CELLS0")
				(number "17")
			)
			(pin passive line
				(at -22.86 15.24 0)
				(length 2.54)
				(name "CELLS1")
				(number "18")
			)
			(pin passive line
				(at 25.4 -30.48 180)
				(length 2.54)
				(name "BATSENS+")
				(number "19")
			)
			(pin passive line
				(at -22.86 29.21 0)
				(length 2.54)
				(name "INTVCC")
				(number "2")
			)
			(pin passive line
				(at 25.4 -21.59 180)
				(length 2.54)
				(name "CSN")
				(number "20")
			)
			(pin passive line
				(at 25.4 -13.97 180)
				(length 2.54)
				(name "CSP")
				(number "21")
			)
			(pin passive line
				(at 25.4 19.05 180)
				(length 2.54)
				(name "BATFET")
				(number "22")
			)
			(pin passive line
				(at -3.81 -38.1 90)
				(length 2.54)
				(name "PGND1")
				(number "23")
			)
			(pin passive line
				(at 1.27 -38.1 90)
				(length 2.54)
				(name "PGND2")
				(number "24")
			)
			(pin passive line
				(at 25.4 1.27 180)
				(length 2.54)
				(name "SW")
				(number "25")
			)
			(pin passive line
				(at 25.4 -1.27 180)
				(length 2.54)
				(name "SW")
				(number "26")
			)
			(pin passive line
				(at 25.4 29.21 180)
				(length 2.54)
				(name "VOUT")
				(number "27")
			)
			(pin passive line
				(at 25.4 26.67 180)
				(length 2.54)
				(name "VOUT")
				(number "28")
			)
			(pin passive line
				(at 6.35 -38.1 90)
				(length 2.54)
				(name "EPAD")
				(number "29")
			)
			(pin passive line
				(at 15.24 38.1 270)
				(length 2.54)
				(name "VOUTA")
				(number "3")
			)
			(pin passive line
				(at 8.89 38.1 270)
				(length 2.54)
				(name "CLN")
				(number "4")
			)
			(pin passive line
				(at 1.27 38.1 270)
				(length 2.54)
				(name "CLP")
				(number "5")
			)
			(pin passive line
				(at -7.62 38.1 270)
				(length 2.54)
				(name "INFET")
				(number "6")
			)
			(pin passive line
				(at -13.97 38.1 270)
				(length 2.54)
				(name "VIN")
				(number "7")
			)
			(pin passive line
				(at -22.86 26.67 0)
				(length 2.54)
				(name "VCC2P5")
				(number "8")
			)
			(pin passive line
				(at -22.86 -30.48 0)
				(length 2.54)
				(name "NTCBIAS")
				(number "9")
			)
		)
	)
	(symbol "LTC4372"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -13.97 10.16 0)
		)
		(property "Value" "LTC4372"
			(at -12.7 7.62 0)
		)
		(property "Footprint" ""
			(at -5.08 5.08 0)
		)
		(property "Datasheet" ""
			(at -5.08 5.08 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "LTC4372_0_1")
		(symbol "LTC4372_1_1"
			(pin bidirectional line
				(at 5.08 8.89 270)
				(length 2.54)
				(name "OUT")
				(number "1")
			)
			(pin bidirectional line
				(at 1.27 8.89 270)
				(length 2.54)
				(name "GATE")
				(number "2")
			)
			(pin bidirectional line
				(at -2.54 8.89 270)
				(length 2.54)
				(name "SRC")
				(number "3")
			)
			(pin bidirectional line
				(at -6.35 8.89 270)
				(length 2.54)
				(name "IN")
				(number "4")
			)
			(pin bidirectional line
				(at -6.35 -8.89 90)
				(length 2.54)
				(name "INTVcc")
				(number "5")
			)
			(pin bidirectional line
				(at 5.08 -8.89 90)
				(length 2.54)
				(name "GND")
				(number "6")
			)
			(pin bidirectional line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "2UPU")
				(number "7")
			)
			(pin bidirectional line
				(at -17.78 -1.27 0)
				(length 2.54)
				(name "SHDN")
				(number "8")
			)
			(pin bidirectional line
				(at 2.54 -8.89 90)
				(length 2.54)
				(name "GND")
				(number "9")
			)
		)
	)
	(symbol "LTC4420IMSE-PBF"
		(pin_names
			(offset 0.254)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 27.94 6.35 0)
		)
		(property "Value" "LTC4420IMSE-PBF"
			(at 24.13 3.81 0)
		)
		(property "Footprint" "MSE_12_ADI"
			(at 25.4 -6.35 90)
		)
		(property "Datasheet" ""
			(at 5.08 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_fp_filters" "MSE_12_ADI MSE_12_ADI-M MSE_12_ADI-L"
			(at 0 0 0)
		)
		(symbol "LTC4420IMSE-PBF_1_1"
			(pin bidirectional line
				(at 5.08 0 0)
				(length 7.62)
				(name "V1")
				(number "1")
			)
			(pin unspecified line
				(at 43.18 -5.08 180)
				(length 7.62)
				(name "V2UV")
				(number "10")
			)
			(pin unspecified line
				(at 43.18 -2.54 180)
				(length 7.62)
				(name "*V2DIS")
				(number "11")
			)
			(pin bidirectional line
				(at 43.18 0 180)
				(length 7.62)
				(name "V2")
				(number "12")
			)
			(pin bidirectional line
				(at 5.08 -2.54 0)
				(length 7.62)
				(name "V2TEST")
				(number "2")
			)
			(pin unspecified line
				(at 5.08 -5.08 0)
				(length 7.62)
				(name "CMP1")
				(number "3")
			)
			(pin unspecified line
				(at 5.08 -7.62 0)
				(length 7.62)
				(name "ADJ")
				(number "4")
			)
			(pin power_in line
				(at 5.08 -10.16 0)
				(length 7.62)
				(name "GND")
				(number "5")
			)
			(pin output line
				(at 5.08 -12.7 0)
				(length 7.62)
				(name "CMPOUT1")
				(number "6")
			)
			(pin power_in line
				(at 43.18 -12.7 180)
				(length 7.62)
				(name "GNDSW")
				(number "7")
			)
			(pin bidirectional line
				(at 43.18 -10.16 180)
				(length 7.62)
				(name "V2OK")
				(number "8")
			)
			(pin output line
				(at 43.18 -7.62 180)
				(length 7.62)
				(name "OUT")
				(number "9")
			)
			(pin unspecified line
				(at 25.4 -22.86 90)
				(length 7.62)
				(name "EPAD")
				(number "EPAD")
			)
		)
	)
	(symbol "LTC4440-5ES6"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 8.89 0)
		)
		(property "Value" "LTC4440-5ES6"
			(at -1.27 8.89 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-6"
			(at 0 -10.16 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/4440fb.pdf"
			(at -2.54 11.43 0)
		)
		(property "Description" "High-side, N-Channel, Mosfet driver, 80V input, -40°C to +85°C, SOT23-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "high-side mosfet-driver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
		(symbol "LTC4440-5ES6_0_1")
		(symbol "LTC4440-5ES6_1_1"
			(pin power_in line
				(at -2.54 10.16 270)
				(length 2.54)
				(name "VCC")
				(number "1")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "INP")
				(number "3")
			)
			(pin input line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "TS")
				(number "4")
			)
			(pin output line
				(at 10.16 0 180)
				(length 2.54)
				(name "TG")
				(number "5")
			)
			(pin input line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "BOOST")
				(number "6")
			)
		)
	)
	(symbol "Lambda_300W_I7C4W008A120V-001-R"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "M"
			(at 2.54 6.35 0)
		)
		(property "Value" "Lambda_300W_I7C4W008A120V-001-R"
			(at -2.54 -10.16 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "Lambda_300W_I7C4W008A120V-001-R_0_1")
		(symbol "Lambda_300W_I7C4W008A120V-001-R_1_1"
			(pin power_in line
				(at -15.24 2.54 0)
				(length 2.54)
				(name "Vin")
				(number "1")
			)
			(pin input line
				(at -15.24 0 0)
				(length 2.54)
				(name "~{Enable}")
				(number "2")
			)
			(pin power_in line
				(at -15.24 -2.54 0)
				(length 2.54)
				(name "GND")
				(number "3")
			)
			(pin power_in line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "GND")
				(number "4")
			)
			(pin input line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "Trim")
				(number "5")
			)
			(pin input line
				(at 10.16 0 180)
				(length 2.54)
				(name "Sense")
				(number "6")
			)
			(pin power_in line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "Vout")
				(number "7")
			)
		)
	)
	(symbol "Lambda_300W_I7C4W008A120V-002-R"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "M"
			(at 5.08 10.16 0)
		)
		(property "Value" "Lambda_300W_I7C4W008A120V-002-R"
			(at 1.27 12.7 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "Lambda_300W_I7C4W008A120V-002-R_0_1")
		(symbol "Lambda_300W_I7C4W008A120V-002-R_1_1"
			(pin power_in line
				(at -12.7 3.81 0)
				(length 2.54)
				(name "Vin")
				(number "1")
			)
			(pin input line
				(at -12.7 1.27 0)
				(length 2.54)
				(name "Enable")
				(number "2")
			)
			(pin power_in line
				(at -12.7 -1.27 0)
				(length 2.54)
				(name "GND")
				(number "3")
			)
			(pin input line
				(at -2.54 -8.89 90)
				(length 2.54)
				(name "Sync")
				(number "32")
			)
			(pin output line
				(at 0 -8.89 90)
				(length 2.54)
				(name "ISMON")
				(number "34")
			)
			(pin power_in line
				(at 12.7 -3.81 180)
				(length 2.54)
				(name "GND")
				(number "4")
			)
			(pin output line
				(at 12.7 -1.27 180)
				(length 2.54)
				(name "Pgood")
				(number "5")
			)
			(pin input line
				(at 12.7 1.27 180)
				(length 2.54)
				(name "Trim")
				(number "6")
			)
			(pin input line
				(at 12.7 3.81 180)
				(length 2.54)
				(name "Vsense")
				(number "7")
			)
			(pin power_out line
				(at 12.7 6.35 180)
				(length 2.54)
				(name "Vout")
				(number "8")
			)
		)
	)
	(symbol "LowPowerLab-SD-Card"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -8.128 12.954 0)
		)
		(property "Value" "LowPowerLab-SD-Card"
			(at 0 -11.43 0)
		)
		(property "Footprint" ""
			(at 3.81 2.54 0)
		)
		(property "Datasheet" ""
			(at 3.81 2.54 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "LowPowerLab-SD-Card_0_1")
		(symbol "LowPowerLab-SD-Card_1_1"
			(pin input line
				(at -10.16 7.62 0)
				(length 2.54)
				(name "GND")
				(number "1")
			)
			(pin input line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "CS")
				(number "10")
			)
			(pin input line
				(at 10.16 0 180)
				(length 2.54)
				(name "EN")
				(number "11")
			)
			(pin input line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "CD")
				(number "12")
			)
			(pin input line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "NC")
				(number "13")
			)
			(pin input line
				(at 10.16 7.62 180)
				(length 2.54)
				(name "GND")
				(number "14")
			)
			(pin input line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "3V")
				(number "2")
			)
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "NC")
				(number "3")
			)
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "NC")
				(number "4")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "MI")
				(number "5")
			)
			(pin input line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "SCK")
				(number "6")
			)
			(pin input line
				(at -10.16 -7.62 0)
				(length 2.54)
				(name "MO")
				(number "7")
			)
			(pin input line
				(at 10.16 -7.62 180)
				(length 2.54)
				(name "NC")
				(number "8")
			)
			(pin input line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "NC")
				(number "9")
			)
		)
	)
	(symbol "Luxeon-L1C1"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "D"
			(at 2.54 2.54 0)
		)
		(property "Value" "Luxeon-L1C1"
			(at 0 -3.81 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "Luxeon-L1C1_1_1"
			(pin passive line
				(at -2.54 0 0)
				(length 1.778)
				(name "A")
				(number "1")
			)
			(pin passive line
				(at 2.54 0 180)
				(length 1.778)
				(name "K")
				(number "2")
			)
			(pin output line
				(at 0 2.54 270)
				(length 2.54)
				(name "THERM")
				(number "3")
			)
		)
	)
	(symbol "MAX1562"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 5.08 7.62 0)
		)
		(property "Value" "MAX1562"
			(at -2.54 7.62 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "MAX1562_0_1")
		(symbol "MAX1562_1_1"
			(pin input line
				(at -8.89 3.81 0)
				(length 2.54)
				(name "~{ON}")
				(number "1")
			)
			(pin input line
				(at -8.89 1.27 0)
				(length 2.54)
				(name "~{FAULT}")
				(number "2")
			)
			(pin input line
				(at -8.89 -1.27 0)
				(length 2.54)
				(name "GND")
				(number "3")
			)
			(pin input line
				(at -8.89 -3.81 0)
				(length 2.54)
				(name "ISET")
				(number "4")
			)
			(pin input line
				(at 7.62 -3.81 180)
				(length 2.54)
				(name "IN")
				(number "5")
			)
			(pin output line
				(at 7.62 -1.27 180)
				(length 2.54)
				(name "OUT")
				(number "6")
			)
			(pin input line
				(at 7.62 1.27 180)
				(length 2.54)
				(name "IN")
				(number "7")
			)
			(pin output line
				(at 7.62 3.81 180)
				(length 2.54)
				(name "OUT")
				(number "8")
			)
		)
	)
	(symbol "MAX22027"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 2.54 7.62 0)
		)
		(property "Value" "MAX22027"
			(at -6.35 7.62 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "MAX22027_0_0"
			(pin input line
				(at -10.16 3.81 0)
				(length 2.54)
				(name "RXD")
				(number "1")
			)
			(pin output line
				(at -10.16 1.27 0)
				(length 2.54)
				(name "TXD")
				(number "2")
			)
			(pin power_in line
				(at -10.16 -1.27 0)
				(length 2.54)
				(name "VDDA")
				(number "3")
			)
			(pin power_in line
				(at -10.16 -3.81 0)
				(length 2.54)
				(name "GNDA")
				(number "4")
			)
			(pin power_in line
				(at 7.62 -3.81 180)
				(length 2.54)
				(name "GNDB")
				(number "5")
			)
			(pin bidirectional line
				(at 7.62 -1.27 180)
				(length 2.54)
				(name "A")
				(number "6")
			)
			(pin bidirectional line
				(at 7.62 1.27 180)
				(length 2.54)
				(name "B")
				(number "7")
			)
			(pin power_in line
				(at 7.62 3.81 180)
				(length 2.54)
				(name "VDDB")
				(number "8")
			)
		)
		(symbol "MAX22027_0_1")
	)
	(symbol "MAX3223"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 10.16 43.18 0)
		)
		(property "Value" "MAX3223"
			(at -7.62 43.18 0)
		)
		(property "Footprint" ""
			(at 0 16.51 0)
		)
		(property "Datasheet" ""
			(at 0 16.51 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "MAX3223_0_0"
			(pin input line
				(at -15.24 36.83 0)
				(length 5.08)
				(name "~{EN}")
				(number "1")
			)
			(pin output line
				(at -15.24 6.35 0)
				(length 5.08)
				(name "RX2_OUT")
				(number "10")
			)
			(pin bidirectional line
				(at 17.78 31.75 180)
				(length 5.08)
				(name "~{INVALID}")
				(number "11")
			)
			(pin input line
				(at -15.24 11.43 0)
				(length 5.08)
				(name "TX2_IN")
				(number "12")
			)
			(pin input line
				(at -15.24 13.97 0)
				(length 5.08)
				(name "TX1_IN")
				(number "13")
			)
			(pin input line
				(at 17.78 34.29 180)
				(length 5.08)
				(name "FORCEON")
				(number "14")
			)
			(pin output line
				(at -15.24 8.89 0)
				(length 5.08)
				(name "RX1_OUT")
				(number "15")
			)
			(pin input line
				(at 17.78 8.89 180)
				(length 5.08)
				(name "RX1_232")
				(number "16")
			)
			(pin output line
				(at 17.78 13.97 180)
				(length 5.08)
				(name "TX1_232")
				(number "17")
			)
			(pin power_in line
				(at 1.27 -5.08 90)
				(length 5.08)
				(name "GND")
				(number "18")
			)
			(pin power_in line
				(at 1.27 45.72 270)
				(length 5.08)
				(name "VCC")
				(number "19")
			)
			(pin input line
				(at -15.24 34.29 0)
				(length 5.08)
				(name "C1+")
				(number "2")
			)
			(pin input line
				(at 17.78 36.83 180)
				(length 5.08)
				(name "~{FORCEOFF}")
				(number "20")
			)
			(pin power_in line
				(at 17.78 26.67 180)
				(length 5.08)
				(name "VS+")
				(number "3")
			)
			(pin input line
				(at -15.24 29.21 0)
				(length 5.08)
				(name "C1-")
				(number "4")
			)
			(pin input line
				(at -15.24 24.13 0)
				(length 5.08)
				(name "C2+")
				(number "5")
			)
			(pin input line
				(at -15.24 19.05 0)
				(length 5.08)
				(name "C2-")
				(number "6")
			)
			(pin power_in line
				(at 17.78 21.59 180)
				(length 5.08)
				(name "VS-")
				(number "7")
			)
			(pin output line
				(at 17.78 11.43 180)
				(length 5.08)
				(name "TX2_232")
				(number "8")
			)
			(pin input line
				(at 17.78 6.35 180)
				(length 5.08)
				(name "RX2_232")
				(number "9")
			)
		)
		(symbol "MAX3223_0_1")
	)
	(symbol "MB85RC1M"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.6346 13.4877 0)
		)
		(property "Value" "MB85RC1M"
			(at -11.43 -8.89 0)
		)
		(property "Footprint" "ProjectFootprints:MB85R_SOIC127P600X88-8N"
			(at 0 16.51 0)
		)
		(property "Datasheet" "https://www.fujitsu.com/jp/group/fsl/en/imagesgig5/MB85RC1MT-DS501-00027-4v0-E.pdf"
			(at 0 0 0)
		)
		(property "Description" "IC FRAM 1MBIT I2C 3.4MHZ 8SOP"
			(at 0 0 0)
		)
		(property "PartNum" "MB85RC1MTPNF-G-JNERE1"
			(at 0 0 0)
		)
		(property "VendorNum" "865-1268-1-ND"
			(at 0 0 0)
		)
		(property "Vendor" "Digikey"
			(at 0 0 0)
		)
		(property "Subst" "No"
			(at 0 0 0)
		)
		(symbol "MB85RC1M_0_0"
			(pin no_connect line
				(at -12.7 5.08 0)
				(length 5.08)
				(name "NC")
				(number "1")
			)
			(pin input line
				(at -12.7 2.54 0)
				(length 5.08)
				(name "A1")
				(number "2")
			)
			(pin input line
				(at -12.7 0 0)
				(length 5.08)
				(name "A2")
				(number "3")
			)
			(pin power_in line
				(at -12.7 -2.54 0)
				(length 5.08)
				(name "VSS")
				(number "4")
			)
			(pin bidirectional line
				(at 12.7 -2.54 180)
				(length 5.08)
				(name "SDA")
				(number "5")
			)
			(pin input clock
				(at 12.7 0 180)
				(length 5.08)
				(name "SCL")
				(number "6")
			)
			(pin input line
				(at 12.7 2.54 180)
				(length 5.08)
				(name "WP")
				(number "7")
			)
			(pin power_in line
				(at 12.7 5.08 180)
				(length 5.08)
				(name "VDD")
				(number "8")
			)
		)
	)
	(symbol "MBC-180"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 16.51 0)
		)
		(property "Value" "MBC-180"
			(at 0 -16.51 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "MBC-180_1_1"
			(pin input line
				(at 33.02 -10.16 180)
				(length 2.54)
				(name "FAN+VE")
				(number "1")
			)
			(pin input line
				(at -12.7 8.89 0)
				(length 2.54)
				(name "L")
				(number "1")
			)
			(pin input line
				(at 33.02 10.16 180)
				(length 2.54)
				(name "V1+VE")
				(number "1")
			)
			(pin input line
				(at 33.02 -24.13 180)
				(length 2.54)
				(name "Vs")
				(number "1")
			)
			(pin input line
				(at 33.02 -12.7 180)
				(length 2.54)
				(name "FAN-VE")
				(number "2")
			)
			(pin input line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "NC")
				(number "2")
			)
			(pin input line
				(at 33.02 -26.67 180)
				(length 2.54)
				(name "PGPF")
				(number "2")
			)
			(pin input line
				(at 33.02 7.62 180)
				(length 2.54)
				(name "V1+VE")
				(number "2")
			)
			(pin input line
				(at 33.02 -29.21 180)
				(length 2.54)
				(name "GND")
				(number "3")
			)
			(pin input line
				(at -12.7 1.27 0)
				(length 2.54)
				(name "N")
				(number "3")
			)
			(pin input line
				(at 33.02 5.08 180)
				(length 2.54)
				(name "V1+VE")
				(number "3")
			)
			(pin input line
				(at 33.02 2.54 180)
				(length 2.54)
				(name "V1-VE")
				(number "4")
			)
			(pin input line
				(at 33.02 0 180)
				(length 2.54)
				(name "V1-VE")
				(number "5")
			)
			(pin input line
				(at 33.02 -2.54 180)
				(length 2.54)
				(name "V1-VE")
				(number "6")
			)
		)
	)
	(symbol "MBT3904DW1T1G"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 0 0)
		)
		(property "Value" "MBT3904DW1T1G"
			(at 2.54 -12.7 0)
		)
		(property "Footprint" "MBT3904DW1T1G:SOT236"
			(at -2.54 -20.32 0)
		)
		(property "Datasheet" "https://www.onsemi.com/pdf/datasheet/mbt2222adw1t1-d.pdf"
			(at 0 -17.78 0)
		)
		(property "Description" "BJT 2 NPN (Dual) 40V 200mA 300MHz 150mW SC-88/SC70-6/SOT-363\n (3904), 2222 is 600mA"
			(at 0 0 0)
		)
		(symbol "MBT3904DW1T1G_0_0")
		(symbol "MBT3904DW1T1G_1_0"
			(pin bidirectional line
				(at 10.16 7.62 270)
				(length 2.54)
				(name "E")
				(number "1")
			)
			(pin bidirectional line
				(at 2.54 7.62 270)
				(length 2.54)
				(name "B")
				(number "2")
			)
			(pin bidirectional line
				(at -10.16 7.62 270)
				(length 2.54)
				(name "C")
				(number "3")
			)
			(pin bidirectional line
				(at -10.16 -7.62 90)
				(length 2.54)
				(name "E")
				(number "4")
			)
			(pin bidirectional line
				(at -2.54 -7.62 90)
				(length 2.54)
				(name "B")
				(number "5")
			)
			(pin bidirectional line
				(at 10.16 -7.62 90)
				(length 2.54)
				(name "C")
				(number "6")
			)
		)
	)
	(symbol "MCP6006"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 2.54 6.35 0)
		)
		(property "Value" "MCP6006"
			(at 5.08 3.81 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "MCP6006_0_1"
			(pin power_in line
				(at -1.27 -7.62 90)
				(length 3.81)
				(name "V-")
				(number "2")
			)
			(pin power_in line
				(at -1.27 7.62 270)
				(length 3.81)
				(name "V+")
				(number "5")
			)
		)
		(symbol "MCP6006_1_1"
			(pin output line
				(at 8.89 0 180)
				(length 2.54)
				(name "~")
				(number "1")
			)
			(pin input line
				(at -6.35 2.54 0)
				(length 2.54)
				(name "+")
				(number "3")
			)
			(pin input line
				(at -6.35 -2.54 0)
				(length 2.54)
				(name "-")
				(number "4")
			)
		)
	)
	(symbol "MCP73832"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 7.62 8.89 0)
		)
		(property "Value" "MCP73832"
			(at -3.81 8.89 0)
		)
		(property "Footprint" "ProjectFootprints:MCP73832_SON50P200X300X100-9N"
			(at -2.54 0 0)
		)
		(property "Datasheet" "https://ww1.microchip.com/downloads/en/DeviceDoc/MCP73831-Family-Data-Sheet-DS20001984H.pdf"
			(at -2.54 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "MCP73832_0_1")
		(symbol "MCP73832_1_1"
			(pin power_in line
				(at -11.43 3.81 0)
				(length 2.54)
				(name "VDD")
				(number "1")
			)
			(pin power_in line
				(at -11.43 1.27 0)
				(length 2.54)
				(name "VDD")
				(number "2")
			)
			(pin power_in line
				(at -11.43 -1.27 0)
				(length 2.54)
				(name "VBAT")
				(number "3")
			)
			(pin power_in line
				(at -11.43 -3.81 0)
				(length 2.54)
				(name "VBAT")
				(number "4")
			)
			(pin output line
				(at 12.7 -3.81 180)
				(length 2.54)
				(name "STAT")
				(number "5")
			)
			(pin power_in line
				(at 12.7 -1.27 180)
				(length 2.54)
				(name "VSS")
				(number "6")
			)
			(pin no_connect line
				(at 12.7 1.27 180)
				(length 2.54)
				(name "NC")
				(number "7")
			)
			(pin bidirectional line
				(at 12.7 3.81 180)
				(length 2.54)
				(name "PROG")
				(number "8")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "PAD")
				(number "9")
			)
		)
	)
	(symbol "MMS_UV_S5713"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 12.7 0)
		)
		(property "Value" "MMS UV S5713"
			(at 0 -11.43 0)
		)
		(property "Footprint" "ProjectDevices:MMS_UV_S5731"
			(at 0 -13.97 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" "S3904-256Q (maybe N)"
			(at 0 0 0)
		)
		(symbol "MMS_UV_S5713_1_1"
			(pin power_in line
				(at -10.16 7.62 0)
				(length 2.54)
				(name "Vss")
				(number "1")
			)
			(pin input line
				(at 8.89 2.54 180)
				(length 2.54)
				(name "CLK2")
				(number "10")
			)
			(pin input line
				(at 8.89 5.08 180)
				(length 2.54)
				(name "CLK1")
				(number "11")
			)
			(pin input line
				(at 8.89 7.62 180)
				(length 2.54)
				(name "ST")
				(number "12")
			)
			(pin input line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "Vscg")
				(number "2")
			)
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "Vsub")
				(number "3")
			)
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "Vbias")
				(number "4")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "NC")
				(number "5")
			)
			(pin power_in line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "Vss")
				(number "6")
			)
			(pin output line
				(at 8.89 -5.08 180)
				(length 2.54)
				(name "Video")
				(number "7")
			)
			(pin output line
				(at 8.89 -2.54 180)
				(length 2.54)
				(name "Dummy")
				(number "8")
			)
			(pin output line
				(at 8.89 0 180)
				(length 2.54)
				(name "~{EOS}")
				(number "9")
			)
		)
	)
	(symbol "MT29F2G"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 5.08 7.62 0)
		)
		(property "Value" "MT29F2G"
			(at -2.54 7.62 0)
		)
		(property "Footprint" "ProjectFootprints:MT29F2G_SON127P600X800X65-8N"
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" "256Mx8 NAND SLC Flash"
			(at 0 0 0)
		)
		(symbol "MT29F2G_0_0"
			(pin input line
				(at -12.7 3.81 0)
				(length 5.08)
				(name "~{CS}")
				(number "1")
			)
			(pin input line
				(at -12.7 1.27 0)
				(length 5.08)
				(name "SO")
				(number "2")
			)
			(pin input line
				(at -12.7 -1.27 0)
				(length 5.08)
				(name "~{WP}")
				(number "3")
			)
			(pin input line
				(at -12.7 -3.81 0)
				(length 5.08)
				(name "VSS")
				(number "4")
			)
			(pin input line
				(at 12.7 -3.81 180)
				(length 5.08)
				(name "SI")
				(number "5")
			)
			(pin input line
				(at 12.7 -1.27 180)
				(length 5.08)
				(name "SCK")
				(number "6")
			)
			(pin input line
				(at 12.7 1.27 180)
				(length 5.08)
				(name "~{HOLD}")
				(number "7")
			)
			(pin input line
				(at 12.7 3.81 180)
				(length 5.08)
				(name "VDD")
				(number "8")
			)
		)
		(symbol "MT29F2G_0_1")
	)
	(symbol "MicroSD_DM3AT"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 63.5 -3.81 0)
		)
		(property "Value" "MicroSD_DM3AT"
			(at 1.27 17.78 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "MicroSD_DM3AT_0_0"
			(text "A"
				(at -8.89 -13.97 0)
			)
			(text "B"
				(at -8.89 -16.51 0)
			)
		)
		(symbol "MicroSD_DM3AT_0_1")
		(symbol "MicroSD_DM3AT_1_1"
			(pin bidirectional line
				(at -21.59 8.89 0)
				(length 3.81)
				(name "DAT2")
				(number "1")
			)
			(pin bidirectional line
				(at -21.59 6.35 0)
				(length 3.81)
				(name "DAT3/CD")
				(number "2")
			)
			(pin input line
				(at -21.59 3.81 0)
				(length 3.81)
				(name "CMD")
				(number "3")
			)
			(pin power_in line
				(at -21.59 1.27 0)
				(length 3.81)
				(name "VDD")
				(number "4")
			)
			(pin input line
				(at -21.59 -1.27 0)
				(length 3.81)
				(name "CLK")
				(number "5")
			)
			(pin power_in line
				(at -21.59 -3.81 0)
				(length 3.81)
				(name "VSS")
				(number "6")
			)
			(pin bidirectional line
				(at -21.59 -6.35 0)
				(length 3.81)
				(name "DAT0")
				(number "7")
			)
			(pin bidirectional line
				(at -21.59 -8.89 0)
				(length 3.81)
				(name "DAT1")
				(number "8")
			)
			(pin passive line
				(at 21.59 -12.7 180)
				(length 3.81)
				(name "SHIELD")
				(number "P1")
			)
			(pin passive line
				(at 21.59 -13.97 180)
				(length 3.81)
				(name "SHIELD")
				(number "P2")
			)
			(pin passive line
				(at 21.59 -15.24 180)
				(length 3.81)
				(name "SHIELD")
				(number "P3")
			)
			(pin passive line
				(at 21.59 -16.51 180)
				(length 3.81)
				(name "SHIELD")
				(number "P4")
			)
			(pin passive line
				(at -21.59 -11.43 0)
				(length 3.81)
				(name "DET_A")
				(number "SWA")
			)
			(pin passive line
				(at -21.59 -13.97 0)
				(length 3.81)
				(name "DET_B")
				(number "SWB")
			)
		)
	)
	(symbol "Monster_02x34_mod"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -13.97 49.53 0)
		)
		(property "Value" "Monster_02x34_mod"
			(at -12.7 46.99 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "Monster_02x34_mod_0_0"
			(text "Boot: USART2, SPI1, USB"
				(at -3.81 34.29 0)
			)
		)
		(symbol "Monster_02x34_mod_0_1")
		(symbol "Monster_02x34_mod_1_1"
			(pin passive line
				(at -35.56 43.18 0)
				(length 3.81)
				(name "USART1_RX")
				(number "1")
			)
			(pin passive line
				(at -35.56 20.32 0)
				(length 3.81)
				(name "USART3_CK")
				(number "10")
			)
			(pin passive line
				(at -35.56 17.78 0)
				(length 3.81)
				(name "UART4_RX")
				(number "11")
			)
			(pin passive line
				(at -35.56 15.24 0)
				(length 3.81)
				(name "UART4_TX")
				(number "12")
			)
			(pin passive line
				(at -35.56 12.7 0)
				(length 3.81)
				(name "UART5_RX")
				(number "13")
			)
			(pin passive line
				(at -35.56 10.16 0)
				(length 3.81)
				(name "UART5_TX")
				(number "14")
			)
			(pin passive line
				(at -35.56 7.62 0)
				(length 3.81)
				(name "GPIO_A")
				(number "15")
			)
			(pin passive line
				(at -35.56 5.08 0)
				(length 3.81)
				(name "GPIO_B")
				(number "16")
			)
			(pin passive line
				(at -35.56 2.54 0)
				(length 3.81)
				(name "GND")
				(number "17")
			)
			(pin passive line
				(at -35.56 0 0)
				(length 3.81)
				(name "GPIO_C")
				(number "18")
			)
			(pin passive line
				(at -35.56 -2.54 0)
				(length 3.81)
				(name "GPIO_D")
				(number "19")
			)
			(pin passive line
				(at -35.56 40.64 0)
				(length 3.81)
				(name "USART1_TX")
				(number "2")
			)
			(pin passive line
				(at -35.56 -5.08 0)
				(length 3.81)
				(name "PWM_A")
				(number "20")
			)
			(pin passive line
				(at -35.56 -7.62 0)
				(length 3.81)
				(name "PWM_B")
				(number "21")
			)
			(pin passive line
				(at -35.56 -10.16 0)
				(length 3.81)
				(name "PWM_C")
				(number "22")
			)
			(pin passive line
				(at -35.56 -12.7 0)
				(length 3.81)
				(name "AVCC")
				(number "23")
			)
			(pin passive line
				(at -35.56 -15.24 0)
				(length 3.81)
				(name "ADC_A")
				(number "24")
			)
			(pin passive line
				(at -35.56 -17.78 0)
				(length 3.81)
				(name "ADC_B")
				(number "25")
			)
			(pin passive line
				(at -35.56 -20.32 0)
				(length 3.81)
				(name "ADC_C")
				(number "26")
			)
			(pin passive line
				(at -35.56 -22.86 0)
				(length 3.81)
				(name "AGND")
				(number "27")
			)
			(pin passive line
				(at -35.56 -25.4 0)
				(length 3.81)
				(name "I2C_A_SDA")
				(number "28")
			)
			(pin passive line
				(at -35.56 -27.94 0)
				(length 3.81)
				(name "I2C_A_SCL")
				(number "29")
			)
			(pin passive line
				(at -35.56 38.1 0)
				(length 3.81)
				(name "USART1_CK")
				(number "3")
			)
			(pin passive line
				(at -35.56 -30.48 0)
				(length 3.81)
				(name "SPI_A_COPI")
				(number "30")
			)
			(pin passive line
				(at -35.56 -33.02 0)
				(length 3.81)
				(name "SPI_A_CIPO")
				(number "31")
			)
			(pin passive line
				(at -35.56 -35.56 0)
				(length 3.81)
				(name "SPI_A_SCLK")
				(number "32")
			)
			(pin passive line
				(at -35.56 -38.1 0)
				(length 3.81)
				(name "SPI_A_CS")
				(number "33")
			)
			(pin passive line
				(at -35.56 -40.64 0)
				(length 3.81)
				(name "SPI_A_NSS")
				(number "34")
			)
			(pin passive line
				(at 35.56 -40.64 180)
				(length 3.81)
				(name "SPI_C_CS")
				(number "35")
			)
			(pin passive line
				(at 35.56 -38.1 180)
				(length 3.81)
				(name "SPI_C_SCLK")
				(number "36")
			)
			(pin passive line
				(at 35.56 -35.56 180)
				(length 3.81)
				(name "SPI_C_CIPO")
				(number "37")
			)
			(pin passive line
				(at 35.56 -33.02 180)
				(length 3.81)
				(name "SPI_C_COPI")
				(number "38")
			)
			(pin passive line
				(at 35.56 -30.48 180)
				(length 3.81)
				(name "GPIO_E")
				(number "39")
			)
			(pin passive line
				(at -35.56 35.56 0)
				(length 3.81)
				(name "USART2_RX")
				(number "4")
			)
			(pin passive line
				(at 35.56 -27.94 180)
				(length 3.81)
				(name "SPARE_CS_NSS")
				(number "40")
			)
			(pin passive line
				(at 35.56 -25.4 180)
				(length 3.81)
				(name "SPI_B_CS")
				(number "41")
			)
			(pin passive line
				(at 35.56 -22.86 180)
				(length 3.81)
				(name "SPI_B_SCLK")
				(number "42")
			)
			(pin passive line
				(at 35.56 -20.32 180)
				(length 3.81)
				(name "SPI_B_CIPO")
				(number "43")
			)
			(pin passive line
				(at 35.56 -17.78 180)
				(length 3.81)
				(name "SPI_B_COPI")
				(number "44")
			)
			(pin passive line
				(at 35.56 -15.24 180)
				(length 3.81)
				(name "I2C_C_SCL")
				(number "45")
			)
			(pin passive line
				(at 35.56 -12.7 180)
				(length 3.81)
				(name "I2C_C_SDA")
				(number "46")
			)
			(pin passive line
				(at 35.56 -10.16 180)
				(length 3.81)
				(name "I2C_B_SCL")
				(number "47")
			)
			(pin passive line
				(at 35.56 -7.62 180)
				(length 3.81)
				(name "I2C_B_SDA")
				(number "48")
			)
			(pin passive line
				(at 35.56 -5.08 180)
				(length 3.81)
				(name "SPARE_TX")
				(number "49")
			)
			(pin passive line
				(at -35.56 33.02 0)
				(length 3.81)
				(name "USART2_TX")
				(number "5")
			)
			(pin passive line
				(at 35.56 -2.54 180)
				(length 3.81)
				(name "SPARE_RX")
				(number "50")
			)
			(pin passive line
				(at 35.56 0 180)
				(length 3.81)
				(name "UART10_TX")
				(number "51")
			)
			(pin passive line
				(at 35.56 2.54 180)
				(length 3.81)
				(name "UART10_RX")
				(number "52")
			)
			(pin passive line
				(at 35.56 5.08 180)
				(length 3.81)
				(name "UART9_TX")
				(number "53")
			)
			(pin passive line
				(at 35.56 7.62 180)
				(length 3.81)
				(name "UART9_RX")
				(number "54")
			)
			(pin passive line
				(at 35.56 10.16 180)
				(length 3.81)
				(name "UART8_TX")
				(number "55")
			)
			(pin passive line
				(at 35.56 12.7 180)
				(length 3.81)
				(name "UART8_RX")
				(number "56")
			)
			(pin passive line
				(at 35.56 15.24 180)
				(length 3.81)
				(name "USART7_TX")
				(number "57")
			)
			(pin passive line
				(at 35.56 17.78 180)
				(length 3.81)
				(name "USART7_RX")
				(number "58")
			)
			(pin passive line
				(at 35.56 20.32 180)
				(length 3.81)
				(name "USART6_TX")
				(number "59")
			)
			(pin passive line
				(at -35.56 30.48 0)
				(length 3.81)
				(name "USART2_CTS")
				(number "6")
			)
			(pin passive line
				(at 35.56 22.86 180)
				(length 3.81)
				(name "USART6_RX")
				(number "60")
			)
			(pin passive line
				(at 35.56 25.4 180)
				(length 3.81)
				(name "WAKE")
				(number "61")
			)
			(pin passive line
				(at 35.56 27.94 180)
				(length 3.81)
				(name "~{SLEEP}")
				(number "62")
			)
			(pin passive line
				(at 35.56 30.48 180)
				(length 3.81)
				(name "GND")
				(number "63")
			)
			(pin passive line
				(at 35.56 33.02 180)
				(length 3.81)
				(name "+3V_COIN")
				(number "64")
			)
			(pin passive line
				(at 35.56 35.56 180)
				(length 3.81)
				(name "+5V_USB")
				(number "65")
			)
			(pin passive line
				(at 35.56 38.1 180)
				(length 3.81)
				(name "+VBAT_LION")
				(number "66")
			)
			(pin passive line
				(at 35.56 40.64 180)
				(length 3.81)
				(name "+3V6_IN")
				(number "67")
			)
			(pin passive line
				(at 35.56 43.18 180)
				(length 3.81)
				(name "+3V3_OUT")
				(number "68")
			)
			(pin passive line
				(at -35.56 27.94 0)
				(length 3.81)
				(name "USART2_RTS")
				(number "7")
			)
			(pin passive line
				(at -35.56 25.4 0)
				(length 3.81)
				(name "USART3_RX")
				(number "8")
			)
			(pin passive line
				(at -35.56 22.86 0)
				(length 3.81)
				(name "USART3_TX")
				(number "9")
			)
		)
	)
	(symbol "Monster_02x34_mod_v1_1"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -13.97 49.53 0)
		)
		(property "Value" "Monster_02x34_mod_v1_1"
			(at -12.7 46.99 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "Monster_02x34_mod_v1_1_0_0"
			(text "Boot: USART2, SPI1, USB"
				(at -3.81 34.29 0)
			)
		)
		(symbol "Monster_02x34_mod_v1_1_0_1")
		(symbol "Monster_02x34_mod_v1_1_1_1"
			(pin passive line
				(at -35.56 43.18 0)
				(length 3.81)
				(name "USART1_RX")
				(number "1")
			)
			(pin passive line
				(at -35.56 20.32 0)
				(length 3.81)
				(name "USART3_CK")
				(number "10")
			)
			(pin passive line
				(at -35.56 17.78 0)
				(length 3.81)
				(name "UART4_RX")
				(number "11")
			)
			(pin passive line
				(at -35.56 15.24 0)
				(length 3.81)
				(name "UART4_TX")
				(number "12")
			)
			(pin passive line
				(at -35.56 12.7 0)
				(length 3.81)
				(name "UART5_RX")
				(number "13")
			)
			(pin passive line
				(at -35.56 10.16 0)
				(length 3.81)
				(name "UART5_TX")
				(number "14")
			)
			(pin passive line
				(at -35.56 7.62 0)
				(length 3.81)
				(name "GPIO_A")
				(number "15")
			)
			(pin passive line
				(at -35.56 5.08 0)
				(length 3.81)
				(name "GPIO_B")
				(number "16")
			)
			(pin passive line
				(at -35.56 2.54 0)
				(length 3.81)
				(name "GND")
				(number "17")
			)
			(pin passive line
				(at -35.56 0 0)
				(length 3.81)
				(name "GPIO_C")
				(number "18")
			)
			(pin passive line
				(at -35.56 -2.54 0)
				(length 3.81)
				(name "GPIO_D")
				(number "19")
			)
			(pin passive line
				(at -35.56 40.64 0)
				(length 3.81)
				(name "USART1_TX")
				(number "2")
			)
			(pin passive line
				(at -35.56 -5.08 0)
				(length 3.81)
				(name "PWM_A")
				(number "20")
			)
			(pin passive line
				(at -35.56 -7.62 0)
				(length 3.81)
				(name "PWM_B")
				(number "21")
			)
			(pin passive line
				(at -35.56 -10.16 0)
				(length 3.81)
				(name "PWM_C")
				(number "22")
			)
			(pin passive line
				(at -35.56 -12.7 0)
				(length 3.81)
				(name "AVCC")
				(number "23")
			)
			(pin passive line
				(at -35.56 -15.24 0)
				(length 3.81)
				(name "ADC_A")
				(number "24")
			)
			(pin passive line
				(at -35.56 -17.78 0)
				(length 3.81)
				(name "ADC_B")
				(number "25")
			)
			(pin passive line
				(at -35.56 -20.32 0)
				(length 3.81)
				(name "ADC_C")
				(number "26")
			)
			(pin passive line
				(at -35.56 -22.86 0)
				(length 3.81)
				(name "AGND")
				(number "27")
			)
			(pin passive line
				(at -35.56 -25.4 0)
				(length 3.81)
				(name "I2C_A_SDA")
				(number "28")
			)
			(pin passive line
				(at -35.56 -27.94 0)
				(length 3.81)
				(name "I2C_A_SCL")
				(number "29")
			)
			(pin passive line
				(at -35.56 38.1 0)
				(length 3.81)
				(name "USART1_CK")
				(number "3")
			)
			(pin passive line
				(at -35.56 -30.48 0)
				(length 3.81)
				(name "SPI_A_COPI")
				(number "30")
			)
			(pin passive line
				(at -35.56 -33.02 0)
				(length 3.81)
				(name "SPI_A_CIPO")
				(number "31")
			)
			(pin passive line
				(at -35.56 -35.56 0)
				(length 3.81)
				(name "SPI_A_SCLK")
				(number "32")
			)
			(pin passive line
				(at -35.56 -38.1 0)
				(length 3.81)
				(name "SPI_A_CS")
				(number "33")
			)
			(pin passive line
				(at -35.56 -40.64 0)
				(length 3.81)
				(name "SPI_A_NSS")
				(number "34")
			)
			(pin passive line
				(at 35.56 -40.64 180)
				(length 3.81)
				(name "SPI_C_CS")
				(number "35")
			)
			(pin passive line
				(at 35.56 -38.1 180)
				(length 3.81)
				(name "SPI_C_SCLK")
				(number "36")
			)
			(pin passive line
				(at 35.56 -35.56 180)
				(length 3.81)
				(name "SPI_C_CIPO")
				(number "37")
			)
			(pin passive line
				(at 35.56 -33.02 180)
				(length 3.81)
				(name "SPI_C_COPI")
				(number "38")
			)
			(pin passive line
				(at 35.56 -30.48 180)
				(length 3.81)
				(name "GPIO_E")
				(number "39")
			)
			(pin passive line
				(at -35.56 35.56 0)
				(length 3.81)
				(name "USART2_RX")
				(number "4")
			)
			(pin passive line
				(at 35.56 -27.94 180)
				(length 3.81)
				(name "SPARE_CS_NSS")
				(number "40")
			)
			(pin passive line
				(at 35.56 -25.4 180)
				(length 3.81)
				(name "SPI_B_CS")
				(number "41")
			)
			(pin passive line
				(at 35.56 -22.86 180)
				(length 3.81)
				(name "SPI_B_SCLK")
				(number "42")
			)
			(pin passive line
				(at 35.56 -20.32 180)
				(length 3.81)
				(name "SPI_B_CIPO")
				(number "43")
			)
			(pin passive line
				(at 35.56 -17.78 180)
				(length 3.81)
				(name "SPI_B_COPI")
				(number "44")
			)
			(pin passive line
				(at 35.56 -15.24 180)
				(length 3.81)
				(name "I2C_C_SCL")
				(number "45")
			)
			(pin passive line
				(at 35.56 -12.7 180)
				(length 3.81)
				(name "I2C_C_SDA")
				(number "46")
			)
			(pin passive line
				(at 35.56 -10.16 180)
				(length 3.81)
				(name "I2C_B_SCL")
				(number "47")
			)
			(pin passive line
				(at 35.56 -7.62 180)
				(length 3.81)
				(name "I2C_B_SDA")
				(number "48")
			)
			(pin passive line
				(at 35.56 -5.08 180)
				(length 3.81)
				(name "UART11_TX")
				(number "49")
			)
			(pin passive line
				(at -35.56 33.02 0)
				(length 3.81)
				(name "USART2_TX")
				(number "5")
			)
			(pin passive line
				(at 35.56 -2.54 180)
				(length 3.81)
				(name "UART11_RX")
				(number "50")
			)
			(pin passive line
				(at 35.56 0 180)
				(length 3.81)
				(name "UART10_TX")
				(number "51")
			)
			(pin passive line
				(at 35.56 2.54 180)
				(length 3.81)
				(name "UART10_RX")
				(number "52")
			)
			(pin passive line
				(at 35.56 5.08 180)
				(length 3.81)
				(name "UART9_TX")
				(number "53")
			)
			(pin passive line
				(at 35.56 7.62 180)
				(length 3.81)
				(name "UART9_RX")
				(number "54")
			)
			(pin passive line
				(at 35.56 10.16 180)
				(length 3.81)
				(name "UART8_TX")
				(number "55")
			)
			(pin passive line
				(at 35.56 12.7 180)
				(length 3.81)
				(name "UART8_RX")
				(number "56")
			)
			(pin passive line
				(at 35.56 15.24 180)
				(length 3.81)
				(name "USART7_TX")
				(number "57")
			)
			(pin passive line
				(at 35.56 17.78 180)
				(length 3.81)
				(name "USART7_RX")
				(number "58")
			)
			(pin passive line
				(at 35.56 20.32 180)
				(length 3.81)
				(name "USART6_TX")
				(number "59")
			)
			(pin passive line
				(at -35.56 30.48 0)
				(length 3.81)
				(name "USART2_CTS")
				(number "6")
			)
			(pin passive line
				(at 35.56 22.86 180)
				(length 3.81)
				(name "USART6_RX")
				(number "60")
			)
			(pin passive line
				(at 35.56 25.4 180)
				(length 3.81)
				(name "GPIO_F")
				(number "61")
			)
			(pin passive line
				(at 35.56 27.94 180)
				(length 3.81)
				(name "GPIO_G")
				(number "62")
			)
			(pin passive line
				(at 35.56 30.48 180)
				(length 3.81)
				(name "~{WAKE_IN}")
				(number "63")
			)
			(pin passive line
				(at 35.56 33.02 180)
				(length 3.81)
				(name "~{SLEEP_OUT}")
				(number "64")
			)
			(pin passive line
				(at 35.56 35.56 180)
				(length 3.81)
				(name "GND")
				(number "65")
			)
			(pin passive line
				(at 35.56 38.1 180)
				(length 3.81)
				(name "+3V_COIN")
				(number "66")
			)
			(pin passive line
				(at 35.56 40.64 180)
				(length 3.81)
				(name "+5V_USB_OUT")
				(number "67")
			)
			(pin passive line
				(at 35.56 43.18 180)
				(length 3.81)
				(name "+3V3_IN")
				(number "68")
			)
			(pin passive line
				(at -35.56 27.94 0)
				(length 3.81)
				(name "USART2_RTS")
				(number "7")
			)
			(pin passive line
				(at -35.56 25.4 0)
				(length 3.81)
				(name "USART3_RX")
				(number "8")
			)
			(pin passive line
				(at -35.56 22.86 0)
				(length 3.81)
				(name "USART3_TX")
				(number "9")
			)
		)
	)
	(symbol "MoteinoM0"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 26.67 0)
		)
		(property "Value" "MoteinoM0"
			(at 49.53 26.67 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "MoteinoM0_0_1")
		(symbol "MoteinoM0_1_1"
			(pin bidirectional line
				(at -19.05 21.59 0)
				(length 2.54)
				(name "~{RST}")
				(number "1")
			)
			(pin bidirectional line
				(at -19.05 -1.27 0)
				(length 2.54)
				(name "A4(PA05(AIN5/SER0:1/TC0:1))")
				(number "10")
			)
			(pin bidirectional line
				(at -19.05 -3.81 0)
				(length 2.54)
				(name "A3(PA04(AIN4/REFB/SER0:0/TC0:0))")
				(number "11")
			)
			(pin bidirectional line
				(at -19.05 -6.35 0)
				(length 2.54)
				(name "A2(PB09(AIN3/SER4:1/TC4:1))")
				(number "12")
			)
			(pin bidirectional line
				(at -19.05 -8.89 0)
				(length 2.54)
				(name "A1(PB08(AIN2/SER4:0/TC4:0))")
				(number "13")
			)
			(pin bidirectional line
				(at -19.05 -11.43 0)
				(length 2.54)
				(name "A0(PA02(AIN0/DAC))")
				(number "14")
			)
			(pin bidirectional line
				(at -19.05 -13.97 0)
				(length 2.54)
				(name "D9(PA07/AIN7/SER0:3/TC1:1))")
				(number "15")
			)
			(pin bidirectional line
				(at -19.05 -16.51 0)
				(length 2.54)
				(name "D8(PA06/AIN6/SER0:2/TC1:0)")
				(number "16")
			)
			(pin bidirectional line
				(at 57.15 -16.51 180)
				(length 2.54)
				(name "D7(PA21(SER5:3+))")
				(number "17")
			)
			(pin bidirectional line
				(at 57.15 -13.97 180)
				(length 2.54)
				(name "D6(PA20(SER5:2+))")
				(number "18")
			)
			(pin bidirectional line
				(at 57.15 -11.43 180)
				(length 2.54)
				(name "D5(PA15(XOUT/SER2:3+))")
				(number "19")
			)
			(pin bidirectional line
				(at -19.05 19.05 0)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin bidirectional line
				(at 57.15 -8.89 180)
				(length 2.54)
				(name "D4(PA08(I2C/AIN16/SER0:0+))")
				(number "20")
			)
			(pin bidirectional line
				(at 57.15 -6.35 180)
				(length 2.54)
				(name "D3(PA09(I2C/AIN17/SER0:1+))")
				(number "21")
			)
			(pin bidirectional line
				(at 57.15 -3.81 180)
				(length 2.54)
				(name "D2(PA14(XIN/SER2:2+))")
				(number "22")
			)
			(pin bidirectional line
				(at 57.15 -1.27 180)
				(length 2.54)
				(name "D1(PA10(AIN18/SER0:2+))")
				(number "23")
			)
			(pin bidirectional line
				(at 57.15 1.27 180)
				(length 2.54)
				(name "D0(PA11(AIN19/SER0:3+))")
				(number "24")
			)
			(pin bidirectional line
				(at 57.15 3.81 180)
				(length 2.54)
				(name "SPI_MOSI(PB10(SER4:2+))")
				(number "25")
			)
			(pin bidirectional line
				(at 57.15 6.35 180)
				(length 2.54)
				(name "SPI_SCK(PB11(SER4:3+))")
				(number "26")
			)
			(pin bidirectional line
				(at 57.15 8.89 180)
				(length 2.54)
				(name "SPI_MISO(PA12(I2C/SER2:0+))")
				(number "27")
			)
			(pin bidirectional line
				(at 57.15 11.43 180)
				(length 2.54)
				(name "SDA(PA22(I2C/SER3:0+))")
				(number "28")
			)
			(pin bidirectional line
				(at 57.15 13.97 180)
				(length 2.54)
				(name "SCL(PA23(I2C/SER3:0+))")
				(number "29")
			)
			(pin bidirectional line
				(at -19.05 16.51 0)
				(length 2.54)
				(name "D13(PA17(I2C/SER1:1+))")
				(number "3")
			)
			(pin bidirectional line
				(at 57.15 16.51 180)
				(length 2.54)
				(name "3.3V_LDO")
				(number "30")
			)
			(pin bidirectional line
				(at 57.15 19.05 180)
				(length 2.54)
				(name "GND")
				(number "31")
			)
			(pin bidirectional line
				(at 57.15 21.59 180)
				(length 2.54)
				(name "Vin_(3.6V-6V)")
				(number "32")
			)
			(pin bidirectional line
				(at 57.15 -38.1 180)
				(length 2.54)
				(name "GND")
				(number "33")
			)
			(pin bidirectional line
				(at 57.15 -35.56 180)
				(length 2.54)
				(name "3.3V_LDO")
				(number "34")
			)
			(pin bidirectional line
				(at 57.15 -33.02 180)
				(length 2.54)
				(name "SWCLK(PA30(SWCLK/SER1:2+))")
				(number "35")
			)
			(pin bidirectional line
				(at 57.15 -30.48 180)
				(length 2.54)
				(name "SWDIO(PA31(SWDIO/SER1:3+))")
				(number "36")
			)
			(pin bidirectional line
				(at 57.15 -27.94 180)
				(length 2.54)
				(name "AREF(PA03(AIN1/REFA))")
				(number "37")
			)
			(pin bidirectional line
				(at 57.15 -25.4 180)
				(length 2.54)
				(name "ATN(PA13(I2C/SER2:1+))")
				(number "38")
			)
			(pin bidirectional line
				(at -19.05 13.97 0)
				(length 2.54)
				(name "D12(PA19(SER1:3+))")
				(number "4")
			)
			(pin bidirectional line
				(at -19.05 11.43 0)
				(length 2.54)
				(name "D11(PA16(I2C/SER1:0+))")
				(number "5")
			)
			(pin bidirectional line
				(at -19.05 8.89 0)
				(length 2.54)
				(name "D10(PA18(SER1:2+))")
				(number "6")
			)
			(pin bidirectional line
				(at -19.05 6.35 0)
				(length 2.54)
				(name "D30(PB22(SER5:2+))")
				(number "7")
			)
			(pin bidirectional line
				(at -19.05 3.81 0)
				(length 2.54)
				(name "D31(PB23(SER5:3+))")
				(number "8")
			)
			(pin bidirectional line
				(at -19.05 1.27 0)
				(length 2.54)
				(name "A5(PB02(AIN10/SER5:0)")
				(number "9")
			)
		)
	)
	(symbol "NVMFS5C604NLWFAFT1G"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "Q"
			(at 6.35 0 0)
		)
		(property "Value" "NVMFS5C604NLWFAFT1G"
			(at 15.24 -2.54 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "NVMFS5C604NLWFAFT1G_1_1"
			(pin power_in line
				(at 2.54 -5.08 90)
				(length 1.27)
				(name "S")
				(number "1")
			)
			(pin bidirectional line
				(at 1.27 -5.08 90)
				(length 1.27)
				(name "S")
				(number "2")
			)
			(pin bidirectional line
				(at 0 -5.08 90)
				(length 1.27)
				(name "S")
				(number "3")
			)
			(pin passive line
				(at -5.08 -1.27 0)
				(length 1.27)
				(name "G")
				(number "4")
			)
			(pin bidirectional line
				(at -1.27 5.08 270)
				(length 1.27)
				(name "D")
				(number "5")
			)
			(pin power_in line
				(at 0 5.08 270)
				(length 1.27)
				(name "D")
				(number "5")
			)
			(pin power_in line
				(at 1.27 5.08 270)
				(length 1.27)
				(name "D")
				(number "5")
			)
			(pin power_in line
				(at 2.54 5.08 270)
				(length 1.27)
				(name "D")
				(number "5")
			)
		)
	)
	(symbol "OM-7605-C8-32.768KHZ-20PPM-TA-QC"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 10.16 0)
		)
		(property "Value" "OM-7605-C8-32.768KHZ-20PPM-TA-QC"
			(at 0 7.62 0)
		)
		(property "Footprint" "ProjectFootprints:OSC_OM-7605-C8-32.768KHZ-20PPM-TA-QC"
			(at 0 -10.16 0)
		)
		(property "Datasheet" "https://www.microcrystal.com/fileadmin/Media/Products/kHzOSC/Datasheet/OM-7605-C8.pdf"
			(at 2.54 -7.62 0)
		)
		(property "Description" "32.768 kHz XO Osc, 20ppm, 1.6V-5.5V, 0.5uA, En, 4-SMD"
			(at 0 0 0)
		)
		(symbol "OM-7605-C8-32.768KHZ-20PPM-TA-QC_1_1"
			(pin output line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "CLK")
				(number "1")
			)
			(pin power_in line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin input line
				(at 7.62 -2.54 180)
				(length 2.54)
				(name "OE")
				(number "3")
			)
			(pin power_in line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "VDD")
				(number "4")
			)
		)
	)
	(symbol "PCA6408A"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 3.302 14.224 0)
		)
		(property "Value" "PCA6408A"
			(at 0.508 -13.97 0)
		)
		(property "Footprint" "ProjectFootprints:PCA6408A_SOP65P640X110-16N"
			(at 0.762 -16.256 0)
		)
		(property "Datasheet" "https://www.nxp.com/docs/en/data-sheet/PCA6408A.pdf"
			(at 1.778 -14.732 0)
		)
		(property "Description" "Port IO expander 8-bit I2C-bus 400khz"
			(at 1.524 -17.78 0)
		)
		(property "PartNum" "PCA6408APW,118"
			(at -0.762 -20.574 0)
		)
		(property "VendorNum" "568-9910-1-ND"
			(at 0.762 -27.686 0)
		)
		(property "Subst" "No"
			(at -0.508 -22.606 0)
		)
		(property "Vendor" "Digikey"
			(at -0.254 -24.638 0)
		)
		(symbol "PCA6408A_1_0"
			(pin bidirectional line
				(at -12.7 8.89 0)
				(length 5.08)
				(name "VDDI")
				(number "1")
			)
			(pin bidirectional line
				(at 12.7 -6.35 180)
				(length 5.08)
				(name "P5")
				(number "10")
			)
			(pin bidirectional line
				(at 12.7 -3.81 180)
				(length 5.08)
				(name "P6")
				(number "11")
			)
			(pin bidirectional line
				(at 12.7 -1.27 180)
				(length 5.08)
				(name "P7")
				(number "12")
			)
			(pin bidirectional line
				(at 12.7 1.27 180)
				(length 5.08)
				(name "~{INT}")
				(number "13")
			)
			(pin bidirectional line
				(at 12.7 3.81 180)
				(length 5.08)
				(name "SCL")
				(number "14")
			)
			(pin bidirectional line
				(at 12.7 6.35 180)
				(length 5.08)
				(name "SDA")
				(number "15")
			)
			(pin bidirectional line
				(at 12.7 8.89 180)
				(length 5.08)
				(name "VDDP")
				(number "16")
			)
			(pin bidirectional line
				(at -12.7 6.35 0)
				(length 5.08)
				(name "ADDR")
				(number "2")
			)
			(pin bidirectional line
				(at -12.7 3.81 0)
				(length 5.08)
				(name "~{RST}")
				(number "3")
			)
			(pin bidirectional line
				(at -12.7 1.27 0)
				(length 5.08)
				(name "P0")
				(number "4")
			)
			(pin bidirectional line
				(at -12.7 -1.27 0)
				(length 5.08)
				(name "P1")
				(number "5")
			)
			(pin bidirectional line
				(at -12.7 -3.81 0)
				(length 5.08)
				(name "P2")
				(number "6")
			)
			(pin bidirectional line
				(at -12.7 -6.35 0)
				(length 5.08)
				(name "P3")
				(number "7")
			)
			(pin bidirectional line
				(at -12.7 -8.89 0)
				(length 5.08)
				(name "GND")
				(number "8")
			)
			(pin bidirectional line
				(at 12.7 -8.89 180)
				(length 5.08)
				(name "P4")
				(number "9")
			)
		)
		(symbol "PCA6408A_1_1")
	)
	(symbol "PEP1-S5-D9-M"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "PS"
			(at -10.16 8.89 0)
		)
		(property "Value" "PEP1-S5-D9-M"
			(at -10.16 -8.89 0)
		)
		(property "Footprint" "ProjectDevices:CONV_PEP1-S5-D9-M"
			(at -2.54 -15.24 0)
		)
		(property "Datasheet" "https://www.cui.com/product/dc-dc-converters/isolated/pep1-m-series/pep1-s5-d9-m"
			(at -2.54 -10.16 0)
		)
		(property "Description" "1 W, 1:1 Input Range, Single/Dual Unregulated Output, SMT, 3000 Vdc Isolation, Dc-Dc Converter"
			(at -2.54 -12.7 0)
		)
		(property "PartNum" "PEP1-S5-D9-M"
			(at -2.54 -17.78 0)
		)
		(property "VendorNum" ""
			(at 0 0 0)
		)
		(property "Vendor" ""
			(at 0 0 0)
		)
		(property "Subst" ""
			(at 0 0 0)
		)
		(symbol "PEP1-S5-D9-M_0_0"
			(pin power_in line
				(at -15.24 -5.08 0)
				(length 5.08)
				(name "GND")
				(number "1")
			)
			(pin input line
				(at -15.24 5.08 0)
				(length 5.08)
				(name "VIN")
				(number "2")
			)
			(pin output line
				(at 15.24 0 180)
				(length 5.08)
				(name "0V")
				(number "5")
			)
			(pin output line
				(at 15.24 -5.08 180)
				(length 5.08)
				(name "-VO")
				(number "6")
			)
			(pin output line
				(at 15.24 5.08 180)
				(length 5.08)
				(name "+VO")
				(number "8")
			)
		)
	)
	(symbol "Pololu-2137"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 -7.62 0)
		)
		(property "Value" "Pololu-2137"
			(at 0 17.78 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "Pololu-2137_0_1")
		(symbol "Pololu-2137_1_1"
			(pin passive line
				(at -10.16 13.97 0)
				(length 2.54)
				(name "EF1")
				(number "1")
			)
			(pin passive line
				(at 10.16 -1.27 180)
				(length 2.54)
				(name "VIN")
				(number "10")
			)
			(pin passive line
				(at 10.16 1.27 180)
				(length 2.54)
				(name "VBB")
				(number "11")
			)
			(pin passive line
				(at 10.16 3.81 180)
				(length 2.54)
				(name "GND")
				(number "12")
			)
			(pin passive line
				(at 10.16 6.35 180)
				(length 2.54)
				(name "OUT4")
				(number "13")
			)
			(pin passive line
				(at 10.16 8.89 180)
				(length 2.54)
				(name "OUT3")
				(number "14")
			)
			(pin passive line
				(at 10.16 11.43 180)
				(length 2.54)
				(name "OUT2")
				(number "15")
			)
			(pin passive line
				(at 10.16 13.97 180)
				(length 2.54)
				(name "OUT1")
				(number "16")
			)
			(pin passive line
				(at -10.16 11.43 0)
				(length 2.54)
				(name "EF2")
				(number "2")
			)
			(pin passive line
				(at -10.16 8.89 0)
				(length 2.54)
				(name "INH")
				(number "3")
			)
			(pin passive line
				(at -10.16 6.35 0)
				(length 2.54)
				(name "IN1")
				(number "4")
			)
			(pin passive line
				(at -10.16 3.81 0)
				(length 2.54)
				(name "IN2")
				(number "5")
			)
			(pin passive line
				(at -10.16 1.27 0)
				(length 2.54)
				(name "IN3")
				(number "6")
			)
			(pin passive line
				(at -10.16 -1.27 0)
				(length 2.54)
				(name "IN4")
				(number "7")
			)
			(pin passive line
				(at -10.16 -3.81 0)
				(length 2.54)
				(name "GND")
				(number "8")
			)
			(pin passive line
				(at 10.16 -3.81 180)
				(length 2.54)
				(name "GND")
				(number "9")
			)
		)
	)
	(symbol "R3117N"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 1.27 8.89 0)
		)
		(property "Value" "R3117N"
			(at 2.54 6.35 0)
		)
		(property "Footprint" ""
			(at 0 -10.16 0)
		)
		(property "Datasheet" ""
			(at 0 -10.16 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "R3117N_0_1")
		(symbol "R3117N_1_1"
			(pin output line
				(at -8.89 2.54 0)
				(length 2.54)
				(name "OUT")
				(number "1")
			)
			(pin power_in line
				(at -8.89 0 0)
				(length 2.54)
				(name "VDD")
				(number "2")
			)
			(pin power_in line
				(at -8.89 -2.54 0)
				(length 2.54)
				(name "GND")
				(number "3")
			)
			(pin no_connect line
				(at 8.89 -2.54 180)
				(length 2.54)
				(name "NC")
				(number "4")
			)
			(pin input line
				(at 8.89 2.54 180)
				(length 2.54)
				(name "SENSE")
				(number "5")
			)
		)
	)
	(symbol "R3118N"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 2.54 6.35 0)
		)
		(property "Value" "R3118N"
			(at -3.81 6.35 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "R3118N_0_1")
		(symbol "R3118N_1_1"
			(pin output line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "OUT")
				(number "1")
			)
			(pin power_in line
				(at -10.16 0 0)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin power_in line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "VDD")
				(number "3")
			)
			(pin bidirectional line
				(at 7.62 -2.54 180)
				(length 2.54)
				(name "CD")
				(number "4")
			)
			(pin input line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "SENSE")
				(number "5")
			)
		)
	)
	(symbol "REF6225"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -5.08 7.62 0)
		)
		(property "Value" "REF6225"
			(at 3.81 7.62 0)
		)
		(property "Footprint" "ProjectDevices:REF6241_SOP65P490X110-8N"
			(at 0 -10.16 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/ref6241.pdf"
			(at 0 -12.7 0)
		)
		(property "Description" "Voltage Reference Vref Fixed 2.5V V ±0.05% 4 mA 8-VSSOP"
			(at 0 0 0)
		)
		(property "PartNum" "REF6225IDGKT"
			(at 0 -7.62 0)
		)
		(property "VendorNum" "296-44922-1-ND"
			(at 1.27 -17.78 0)
		)
		(property "Vendor" "Digikey"
			(at 0 -15.24 0)
		)
		(property "Subst" "No"
			(at 6.35 -15.24 0)
		)
		(symbol "REF6225_1_1"
			(pin power_in line
				(at -10.16 3.81 0)
				(length 2.54)
				(name "VIN")
				(number "1")
			)
			(pin input line
				(at -10.16 1.27 0)
				(length 2.54)
				(name "EN")
				(number "2")
			)
			(pin bidirectional line
				(at -10.16 -1.27 0)
				(length 2.54)
				(name "SS")
				(number "3")
			)
			(pin bidirectional line
				(at -10.16 -3.81 0)
				(length 2.54)
				(name "FILT")
				(number "4")
			)
			(pin output line
				(at 11.43 -3.81 180)
				(length 2.54)
				(name "OUT_S")
				(number "5")
			)
			(pin output line
				(at 11.43 -1.27 180)
				(length 2.54)
				(name "OUT_F")
				(number "6")
			)
			(pin power_in line
				(at 11.43 1.27 180)
				(length 2.54)
				(name "GND_F")
				(number "7")
			)
			(pin power_in line
				(at 11.43 3.81 180)
				(length 2.54)
				(name "GND_S")
				(number "8")
			)
		)
	)
	(symbol "REF6241"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -3.81 8.89 0)
		)
		(property "Value" "REF6241"
			(at 0 -6.35 0)
		)
		(property "Footprint" "ProjectDevices:REF6241_SOP65P490X110-8N"
			(at 0 -13.97 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/ref6225.pdf"
			(at 0 -8.89 0)
		)
		(property "Description" " Voltage Reference Vref Fixed 4.096V V ±0.05% 4 mA 8-VSSOP"
			(at 0 0 0)
		)
		(property "PartNum" "REF6241IDGKT"
			(at 0 -11.43 0)
		)
		(property "VendorNum" ""
			(at 0 0 0)
		)
		(property "Vendor" ""
			(at 0 0 0)
		)
		(property "Subst" ""
			(at 0 0 0)
		)
		(symbol "REF6241_1_1"
			(pin power_in line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "VIN")
				(number "1")
			)
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "EN")
				(number "2")
			)
			(pin bidirectional line
				(at -10.16 0 0)
				(length 2.54)
				(name "SS")
				(number "3")
			)
			(pin bidirectional line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "FILT")
				(number "4")
			)
			(pin output line
				(at 11.43 -2.54 180)
				(length 2.54)
				(name "OUT_S")
				(number "5")
			)
			(pin output line
				(at 11.43 0 180)
				(length 2.54)
				(name "OUT_F")
				(number "6")
			)
			(pin power_in line
				(at 11.43 2.54 180)
				(length 2.54)
				(name "GND_F")
				(number "7")
			)
			(pin power_in line
				(at 11.43 5.08 180)
				(length 2.54)
				(name "GND_S")
				(number "8")
			)
		)
	)
	(symbol "RESET_R3111"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 5.08 0)
		)
		(property "Value" "RESET_R3111"
			(at 0 7.62 0)
		)
		(property "Footprint" ""
			(at -5.08 0 0)
		)
		(property "Datasheet" ""
			(at -5.08 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "RESET_R3111_0_1")
		(symbol "RESET_R3111_1_1"
			(pin output line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "OUT")
				(number "1")
			)
			(pin power_in line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin power_in line
				(at 6.35 0 180)
				(length 2.54)
				(name "VDD")
				(number "3")
			)
		)
	)
	(symbol "RESET_R3117"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 3.81 6.35 0)
		)
		(property "Value" "RESET_R3117"
			(at 0 -6.35 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "RESET_R3117_0_1")
		(symbol "RESET_R3117_1_1"
			(pin output line
				(at -8.89 2.54 0)
				(length 2.54)
				(name "OUT")
				(number "1")
			)
			(pin input line
				(at -8.89 -2.54 0)
				(length 2.54)
				(name "SENSE")
				(number "2")
			)
			(pin power_in line
				(at 8.89 -2.54 180)
				(length 2.54)
				(name "GND")
				(number "3")
			)
			(pin power_in line
				(at 8.89 2.54 180)
				(length 2.54)
				(name "VDD")
				(number "4")
			)
			(pin power_in line
				(at 0 7.62 270)
				(length 2.54)
				(name "PAD")
				(number "5")
			)
		)
	)
	(symbol "RNM-0505S/HP"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "ISO"
			(at -10.1639 8.8979 0)
		)
		(property "Value" "RNM-0505S{slash}HP"
			(at -10.1614 -10.1627 0)
		)
		(property "Footprint" "CONV_RNM-0505S/HP"
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(property "STANDARD" "Manufacturer Recommendations"
			(at 0 0 0)
		)
		(property "PARTREV" "1"
			(at 0 0 0)
		)
		(property "MANUFACTURER" "RECOM"
			(at 0 0 0)
		)
		(property "MAXIMUM_PACKAGE_HEIGHT" "6.80mm"
			(at 0 0 0)
		)
		(symbol "RNM-0505S/HP_0_0"
			(pin input line
				(at -11.43 -5.08 0)
				(length 5.08)
				(name "-VIN")
				(number "1")
			)
			(pin input line
				(at -11.43 5.08 0)
				(length 5.08)
				(name "+VIN")
				(number "3")
			)
			(pin output line
				(at 11.43 5.08 180)
				(length 5.08)
				(name "+VOUT")
				(number "4")
			)
			(pin output line
				(at 11.43 -5.08 180)
				(length 5.08)
				(name "-VOUT")
				(number "5")
			)
		)
		(symbol "RNM-0505S/HP_0_1")
	)
	(symbol "RTC-RV-3028-C7"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 6.35 8.89 0)
		)
		(property "Value" "RTC-RV-3028-C7"
			(at 0 -7.62 0)
		)
		(property "Footprint" ""
			(at 0 -2.54 0)
		)
		(property "Datasheet" ""
			(at 0 -2.54 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "RTC-RV-3028-C7_0_0"
			(pin output line
				(at -12.7 5.08 0)
				(length 5.08)
				(name "CLKOUT")
				(number "1")
			)
			(pin output line
				(at -12.7 2.54 0)
				(length 5.08)
				(name "~{INT}")
				(number "2")
			)
			(pin bidirectional line
				(at -12.7 0 0)
				(length 5.08)
				(name "SCL")
				(number "3")
			)
			(pin bidirectional line
				(at -12.7 -2.54 0)
				(length 5.08)
				(name "SDA")
				(number "4")
			)
			(pin power_in line
				(at 12.7 -2.54 180)
				(length 5.08)
				(name "GND")
				(number "5")
			)
			(pin power_in line
				(at 12.7 0 180)
				(length 5.08)
				(name "Vbackup")
				(number "6")
			)
			(pin power_in line
				(at 12.7 2.54 180)
				(length 5.08)
				(name "VDD")
				(number "7")
			)
			(pin input line
				(at 12.7 5.08 180)
				(length 5.08)
				(name "EVI")
				(number "8")
			)
		)
		(symbol "RTC-RV-3028-C7_0_1")
	)
	(symbol "RTC-RV-3032"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 3.81 7.62 0)
		)
		(property "Value" "RTC-RV-3032"
			(at 0 -7.62 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "RTC-RV-3032_0_0"
			(pin bidirectional line
				(at -12.7 3.81 0)
				(length 5.08)
				(name "Vbackup")
				(number "1")
			)
			(pin bidirectional line
				(at -12.7 1.27 0)
				(length 5.08)
				(name "SDA")
				(number "2")
			)
			(pin output line
				(at -12.7 -1.27 0)
				(length 5.08)
				(name "~{INT}")
				(number "3")
			)
			(pin input line
				(at -12.7 -3.81 0)
				(length 5.08)
				(name "EVI")
				(number "4")
			)
			(pin power_in line
				(at 12.7 -3.81 180)
				(length 5.08)
				(name "GND")
				(number "5")
			)
			(pin power_in line
				(at 12.7 -1.27 180)
				(length 5.08)
				(name "VDD")
				(number "6")
			)
			(pin output line
				(at 12.7 1.27 180)
				(length 5.08)
				(name "CLKOUT")
				(number "7")
			)
			(pin bidirectional line
				(at 12.7 3.81 180)
				(length 5.08)
				(name "SCL")
				(number "8")
			)
		)
		(symbol "RTC-RV-3032_0_1")
	)
	(symbol "Resistor_Small"
		(pin_numbers hide)
		(pin_names
			(offset 0.254) hide)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "R"
			(at 0.762 0.508 0)
		)
		(property "Value" "Resistor_Small"
			(at 0.762 -1.016 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Resistor, small symbol"
			(at 0 0 0)
		)
		(property "ki_keywords" "r resistor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "R_*"
			(at 0 0 0)
		)
		(symbol "Resistor_Small_0_1")
		(symbol "Resistor_Small_1_1"
			(pin passive line
				(at 0 2.54 270)
				(length 0.762)
				(name "~")
				(number "1")
			)
			(pin passive line
				(at 0 -2.54 90)
				(length 0.762)
				(name "~")
				(number "2")
			)
		)
	)
	(symbol "S-1009C20I-M5T1U"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.35 5.08 0)
		)
		(property "Value" "S-1009C20I-M5T1U"
			(at -10.16 -7.62 0)
		)
		(property "Footprint" "ProjectFootprints:S-1009_SOT95P280X130-5N"
			(at 3.81 0 0)
		)
		(property "Datasheet" "https://www.ablic.com/en/doc/datasheet/voltage_detector/S1009_E.pdf"
			(at 3.81 0 0)
		)
		(property "Description" "IC SUPERVISOR 1 CHANNEL SOT23-5"
			(at 3.81 0 0)
		)
		(symbol "S-1009C20I-M5T1U_0_0"
			(pin output line
				(at -11.43 2.54 0)
				(length 5.08)
				(name "OUT")
				(number "1")
			)
			(pin power_in line
				(at -11.43 0 0)
				(length 5.08)
				(name "VDD")
				(number "2")
			)
			(pin power_in line
				(at -11.43 -2.54 0)
				(length 5.08)
				(name "VSS")
				(number "3")
			)
			(pin no_connect line
				(at 11.43 -2.54 180)
				(length 5.08)
				(name "NC")
				(number "4")
			)
			(pin passive line
				(at 11.43 2.54 180)
				(length 5.08)
				(name "CD")
				(number "5")
			)
		)
	)
	(symbol "S18V20F12"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 15.24 10.16 0)
		)
		(property "Value" "S18V20F12"
			(at -11.43 10.16 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "S18V20F12_0_1")
		(symbol "S18V20F12_1_1"
			(pin bidirectional line
				(at -19.05 0 0)
				(length 2.54)
				(name "GND")
				(number "1")
			)
			(pin bidirectional line
				(at -19.05 6.35 0)
				(length 2.54)
				(name "Vin")
				(number "2")
			)
			(pin bidirectional line
				(at -19.05 -5.08 0)
				(length 2.54)
				(name "ENABLE")
				(number "3")
			)
			(pin bidirectional line
				(at 19.05 6.35 180)
				(length 2.54)
				(name "Vout")
				(number "4")
			)
			(pin bidirectional line
				(at 19.05 0 180)
				(length 2.54)
				(name "GND")
				(number "5")
			)
		)
	)
	(symbol "SA72SB0"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 -3.81 0)
		)
		(property "Value" "SA72SB0"
			(at 0 3.81 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "SA72SB0_0_0"
			(text "72 deg. C"
				(at 0 -1.27 0)
			)
		)
		(symbol "SA72SB0_0_1")
		(symbol "SA72SB0_1_1"
			(pin output line
				(at -6.35 1.27 0)
				(length 2.54)
				(name "~")
				(number "1")
			)
			(pin output line
				(at -6.35 -1.27 0)
				(length 2.54)
				(name "~")
				(number "2")
			)
			(pin output line
				(at 6.35 -1.27 180)
				(length 2.54)
				(name "~")
				(number "3")
			)
			(pin output line
				(at 6.35 1.27 180)
				(length 2.54)
				(name "~")
				(number "4")
			)
		)
	)
	(symbol "SN65HVD77"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 0 0)
		)
		(property "Value" "SN65HVD77"
			(at 0 0 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
	)
	(symbol "SN65HVD77DR"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.35 10.16 0)
		)
		(property "Value" "SN65HVD77DR"
			(at -7.62 7.62 0)
		)
		(property "Footprint" "SOIC127P599X175-8N"
			(at -10.16 -8.89 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(symbol "SN65HVD77DR_0_0"
			(pin power_in line
				(at -11.43 3.81 0)
				(length 5.08)
				(name "VCC")
				(number "1")
			)
			(pin output line
				(at -11.43 1.27 0)
				(length 5.08)
				(name "R")
				(number "2")
			)
			(pin input line
				(at -11.43 -1.27 0)
				(length 5.08)
				(name "D")
				(number "3")
			)
			(pin power_in line
				(at -11.43 -3.81 0)
				(length 5.08)
				(name "GND")
				(number "4")
			)
			(pin output line
				(at 11.43 -3.81 180)
				(length 5.08)
				(name "Y")
				(number "5")
			)
			(pin output line
				(at 11.43 -1.27 180)
				(length 5.08)
				(name "Z")
				(number "6")
			)
			(pin input line
				(at 11.43 1.27 180)
				(length 5.08)
				(name "B")
				(number "7")
			)
			(pin input line
				(at 11.43 3.81 180)
				(length 5.08)
				(name "A")
				(number "8")
			)
		)
		(symbol "SN65HVD77DR_1_1")
	)
	(symbol "SN74AUP2G07DSFR"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -5.08 7.62 0)
		)
		(property "Value" "SN74AUP2G07DSFR"
			(at -7.62 -7.62 0)
		)
		(property "Footprint" "ProjectFootprints:SN74AUP2G07_SON35P100X100X40-6N"
			(at 2.54 -12.7 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/sn74aup2g07.pdf"
			(at 2.54 -10.16 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "SN74AUP2G07DSFR_0_0"
			(pin input line
				(at -10.16 2.54 0)
				(length 5.08)
				(name "1A")
				(number "1")
			)
			(pin passive line
				(at -10.16 0 0)
				(length 5.08)
				(name "GND")
				(number "2")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 5.08)
				(name "2A")
				(number "3")
			)
			(pin output line
				(at 10.16 -2.54 180)
				(length 5.08)
				(name "2Y")
				(number "4")
			)
			(pin power_in line
				(at 10.16 0 180)
				(length 5.08)
				(name "VCC")
				(number "5")
			)
			(pin output line
				(at 10.16 2.54 180)
				(length 5.08)
				(name "1Y")
				(number "6")
			)
		)
		(symbol "SN74AUP2G07DSFR_1_1")
	)
	(symbol "STM32F413RHTx-tm"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -2.54 10.16 0)
		)
		(property "Value" "STM32F413RHTx-tm"
			(at 0 7.62 0)
		)
		(property "Footprint" ""
			(at -8.89 -1.27 0)
		)
		(property "Datasheet" ""
			(at -8.89 -1.27 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "STM32F413RHTx-tm_0_1")
		(symbol "STM32F413RHTx-tm_1_1"
			(pin input line
				(at -35.56 17.78 0)
				(length 2.54)
				(name "Vbat")
				(number "1")
			)
			(pin input line
				(at -35.56 -5.08 0)
				(length 2.54)
				(name "SPI2_CIPO")
				(number "10")
			)
			(pin output line
				(at -35.56 -7.62 0)
				(length 2.54)
				(name "SPI2_COPI")
				(number "11")
			)
			(pin power_in line
				(at -35.56 -10.16 0)
				(length 2.54)
				(name "VSSA")
				(number "12")
			)
			(pin power_in line
				(at -35.56 -12.7 0)
				(length 2.54)
				(name "VDDA")
				(number "13")
			)
			(pin output line
				(at -35.56 -15.24 0)
				(length 2.54)
				(name "UART4_TX")
				(number "14")
			)
			(pin input line
				(at -35.56 -17.78 0)
				(length 2.54)
				(name "UART4_RX")
				(number "15")
			)
			(pin output line
				(at -35.56 -20.32 0)
				(length 2.54)
				(name "USART2_TX")
				(number "16")
			)
			(pin input line
				(at -19.05 -34.29 90)
				(length 2.54)
				(name "USART2_RX")
				(number "17")
			)
			(pin power_in line
				(at -16.51 -34.29 90)
				(length 2.54)
				(name "VSS")
				(number "18")
			)
			(pin power_in line
				(at -13.97 -34.29 90)
				(length 2.54)
				(name "VDD")
				(number "19")
			)
			(pin input line
				(at -35.56 15.24 0)
				(length 2.54)
				(name "RTC_AF1")
				(number "2")
			)
			(pin input line
				(at -11.43 -34.29 90)
				(length 2.54)
				(name "SPI1_NSS")
				(number "20")
			)
			(pin input line
				(at -8.89 -34.29 90)
				(length 2.54)
				(name "SPI1_SCK")
				(number "21")
			)
			(pin input line
				(at -6.35 -34.29 90)
				(length 2.54)
				(name "SPI1_CIPO")
				(number "22")
			)
			(pin input line
				(at -3.81 -34.29 90)
				(length 2.54)
				(name "SPI1_COPI")
				(number "23")
			)
			(pin input line
				(at -1.27 -34.29 90)
				(length 2.54)
				(name "ADC1_IN14")
				(number "24")
			)
			(pin input line
				(at 1.27 -34.29 90)
				(length 2.54)
				(name "ADC1_IN15")
				(number "25")
			)
			(pin input line
				(at 3.81 -34.29 90)
				(length 2.54)
				(name "GPIO_Input")
				(number "26")
			)
			(pin input line
				(at 6.35 -34.29 90)
				(length 2.54)
				(name "GPIO_Output")
				(number "27")
			)
			(pin input line
				(at 8.89 -34.29 90)
				(length 2.54)
				(name "LPTIM1_OUT")
				(number "28")
			)
			(pin input line
				(at 11.43 -34.29 90)
				(length 2.54)
				(name "SPI2_SCK")
				(number "29")
			)
			(pin input line
				(at -35.56 12.7 0)
				(length 2.54)
				(name "RCC_OSC32_IN")
				(number "3")
			)
			(pin power_out line
				(at 13.97 -34.29 90)
				(length 2.54)
				(name "VCAP")
				(number "30")
			)
			(pin power_in line
				(at 16.51 -34.29 90)
				(length 2.54)
				(name "VSS")
				(number "31")
			)
			(pin power_in line
				(at 19.05 -34.29 90)
				(length 2.54)
				(name "VDD")
				(number "32")
			)
			(pin bidirectional line
				(at 33.02 -20.32 180)
				(length 2.54)
				(name "SPI2_NSS")
				(number "33")
			)
			(pin output line
				(at 33.02 -17.78 180)
				(length 2.54)
				(name "UART5_TX")
				(number "34")
			)
			(pin bidirectional line
				(at 33.02 -15.24 180)
				(length 2.54)
				(name "FMPI2C1_SDA")
				(number "35")
			)
			(pin bidirectional line
				(at 33.02 -12.7 180)
				(length 2.54)
				(name "FMPI2C1_SCL")
				(number "36")
			)
			(pin output line
				(at 33.02 -10.16 180)
				(length 2.54)
				(name "USART6_TX")
				(number "37")
			)
			(pin input line
				(at 33.02 -7.62 180)
				(length 2.54)
				(name "USART6_RX")
				(number "38")
			)
			(pin input line
				(at 33.02 -5.08 180)
				(length 2.54)
				(name "GPIO_PC8")
				(number "39")
			)
			(pin output line
				(at -35.56 10.16 0)
				(length 2.54)
				(name "RCC_OSC32_OUT")
				(number "4")
			)
			(pin bidirectional line
				(at 33.02 -2.54 180)
				(length 2.54)
				(name "GPIO_PC9")
				(number "40")
			)
			(pin bidirectional line
				(at 33.02 0 180)
				(length 2.54)
				(name "USART1_CK")
				(number "41")
			)
			(pin input line
				(at 33.02 2.54 180)
				(length 2.54)
				(name "USB_VBUS")
				(number "42")
			)
			(pin input line
				(at 33.02 5.08 180)
				(length 2.54)
				(name "GPIO_PA10")
				(number "43")
			)
			(pin input line
				(at 33.02 7.62 180)
				(length 2.54)
				(name "USB_OTG_FS_DM")
				(number "44")
			)
			(pin input line
				(at 33.02 10.16 180)
				(length 2.54)
				(name "USB_OTG_FS_DP")
				(number "45")
			)
			(pin bidirectional line
				(at 33.02 12.7 180)
				(length 2.54)
				(name "SYS_JTMS-SWDIO")
				(number "46")
			)
			(pin power_in line
				(at 33.02 15.24 180)
				(length 2.54)
				(name "VSS")
				(number "47")
			)
			(pin power_in line
				(at 33.02 17.78 180)
				(length 2.54)
				(name "VDD")
				(number "48")
			)
			(pin bidirectional line
				(at 19.05 35.56 270)
				(length 2.54)
				(name "SYS_SWCLK")
				(number "49")
			)
			(pin input line
				(at -35.56 7.62 0)
				(length 2.54)
				(name "RCC_OSC_IN")
				(number "5")
			)
			(pin bidirectional line
				(at 16.51 35.56 270)
				(length 2.54)
				(name "SYS_JTDI")
				(number "50")
			)
			(pin output line
				(at 13.97 35.56 270)
				(length 2.54)
				(name "USART3_TX")
				(number "51")
			)
			(pin input line
				(at 11.43 35.56 270)
				(length 2.54)
				(name "USART3_RX")
				(number "52")
			)
			(pin bidirectional line
				(at 8.89 35.56 270)
				(length 2.54)
				(name "USART3_CK")
				(number "53")
			)
			(pin input line
				(at 6.35 35.56 270)
				(length 2.54)
				(name "UART5_RX")
				(number "54")
			)
			(pin input line
				(at 3.81 35.56 270)
				(length 2.54)
				(name "UART7_RX")
				(number "55")
			)
			(pin output line
				(at 1.27 35.56 270)
				(length 2.54)
				(name "UART7_TX")
				(number "56")
			)
			(pin input line
				(at -1.27 35.56 270)
				(length 2.54)
				(name "I2C1_SMBA")
				(number "57")
			)
			(pin output line
				(at -3.81 35.56 270)
				(length 2.54)
				(name "USART1_TX")
				(number "58")
			)
			(pin input line
				(at -6.35 35.56 270)
				(length 2.54)
				(name "USART1_RX")
				(number "59")
			)
			(pin output line
				(at -35.56 5.08 0)
				(length 2.54)
				(name "RCC_OSC_OUT")
				(number "6")
			)
			(pin input line
				(at -8.89 35.56 270)
				(length 2.54)
				(name "BOOT0")
				(number "60")
			)
			(pin bidirectional line
				(at -11.43 35.56 270)
				(length 2.54)
				(name "I2C1_SCL")
				(number "61")
			)
			(pin bidirectional line
				(at -13.97 35.56 270)
				(length 2.54)
				(name "I2C1_SDA")
				(number "62")
			)
			(pin power_in line
				(at -16.51 35.56 270)
				(length 2.54)
				(name "VSS")
				(number "63")
			)
			(pin power_in line
				(at -19.05 35.56 270)
				(length 2.54)
				(name "VDD")
				(number "64")
			)
			(pin input line
				(at -35.56 2.54 0)
				(length 2.54)
				(name "RESET_N")
				(number "7")
			)
			(pin input line
				(at -35.56 0 0)
				(length 2.54)
				(name "SYS_WKUP2_PC0")
				(number "8")
			)
			(pin bidirectional line
				(at -35.56 -2.54 0)
				(length 2.54)
				(name "GPIO_PC1")
				(number "9")
			)
		)
	)
	(symbol "STM32G431KBU6"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 1.27 2.54 0)
		)
		(property "Value" ""
			(at -3.81 -2.54 0)
		)
		(property "Footprint" ""
			(at -3.81 -2.54 0)
		)
		(property "Datasheet" ""
			(at -3.81 -2.54 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "STM32G431KBU6_1_1"
			(pin power_in line
				(at -22.86 10.16 0)
				(length 2.54)
				(name "VDD")
				(number "1")
			)
			(pin bidirectional line
				(at -7.62 -20.32 90)
				(length 2.54)
				(name "PA5")
				(number "10")
			)
			(pin bidirectional line
				(at -5.08 -20.32 90)
				(length 2.54)
				(name "PA6")
				(number "11")
			)
			(pin bidirectional line
				(at -2.54 -20.32 90)
				(length 2.54)
				(name "PA7")
				(number "12")
			)
			(pin bidirectional line
				(at 0 -20.32 90)
				(length 2.54)
				(name "PB0")
				(number "13")
			)
			(pin power_out line
				(at 2.54 -20.32 90)
				(length 2.54)
				(name "VSSA")
				(number "14")
			)
			(pin bidirectional line
				(at -7.62 24.13 270)
				(length 2.54)
				(name "BOOT0")
				(number "15")
			)
			(pin bidirectional line
				(at 5.08 -20.32 90)
				(length 2.54)
				(name "VDDA")
				(number "15")
			)
			(pin power_in line
				(at 7.62 -20.32 90)
				(length 2.54)
				(name "VSS")
				(number "16")
			)
			(pin power_in line
				(at 21.59 -7.62 180)
				(length 2.54)
				(name "VDD")
				(number "17")
			)
			(pin input line
				(at 21.59 -5.08 180)
				(length 2.54)
				(name "PA8")
				(number "18")
			)
			(pin bidirectional line
				(at 21.59 -2.54 180)
				(length 2.54)
				(name "PA9")
				(number "19")
			)
			(pin input line
				(at -22.86 7.62 0)
				(length 2.54)
				(name "RCC_OSC_IN")
				(number "2")
			)
			(pin bidirectional line
				(at 21.59 0 180)
				(length 2.54)
				(name "PA10")
				(number "20")
			)
			(pin bidirectional line
				(at 21.59 2.54 180)
				(length 2.54)
				(name "PA11")
				(number "21")
			)
			(pin bidirectional line
				(at 21.59 5.08 180)
				(length 2.54)
				(name "PA12")
				(number "22")
			)
			(pin bidirectional line
				(at 21.59 7.62 180)
				(length 2.54)
				(name "SWDIO")
				(number "23")
			)
			(pin bidirectional line
				(at 21.59 10.16 180)
				(length 2.54)
				(name "SWCLK")
				(number "24")
			)
			(pin bidirectional line
				(at 7.62 24.13 270)
				(length 2.54)
				(name "PA15")
				(number "25")
			)
			(pin bidirectional line
				(at 5.08 24.13 270)
				(length 2.54)
				(name "PB3")
				(number "26")
			)
			(pin bidirectional line
				(at 2.54 24.13 270)
				(length 2.54)
				(name "PB4")
				(number "27")
			)
			(pin bidirectional line
				(at 0 24.13 270)
				(length 2.54)
				(name "PB5")
				(number "28")
			)
			(pin bidirectional line
				(at -2.54 24.13 270)
				(length 2.54)
				(name "PB6")
				(number "29")
			)
			(pin output line
				(at -22.86 5.08 0)
				(length 2.54)
				(name "RCC_OSC_OUT")
				(number "3")
			)
			(pin bidirectional line
				(at -5.08 24.13 270)
				(length 2.54)
				(name "PB7")
				(number "30")
			)
			(pin power_in line
				(at -10.16 24.13 270)
				(length 2.54)
				(name "VSS")
				(number "32")
			)
			(pin input line
				(at -22.86 2.54 0)
				(length 2.54)
				(name "nRST")
				(number "4")
			)
			(pin bidirectional line
				(at -22.86 0 0)
				(length 2.54)
				(name "PA0")
				(number "5")
			)
			(pin bidirectional line
				(at -22.86 -2.54 0)
				(length 2.54)
				(name "PA1")
				(number "6")
			)
			(pin bidirectional line
				(at -22.86 -5.08 0)
				(length 2.54)
				(name "PA2")
				(number "7")
			)
			(pin bidirectional line
				(at -22.86 -7.62 0)
				(length 2.54)
				(name "PA3")
				(number "8")
			)
			(pin bidirectional line
				(at -10.16 -20.32 90)
				(length 2.54)
				(name "PA4")
				(number "9")
			)
		)
	)
	(symbol "STM32H7A3"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 0 0)
		)
		(property "Value" "STM32H7A3"
			(at 0 0 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "STM32H7A3_0_1")
		(symbol "STM32H7A3_1_1"
			(pin bidirectional line
				(at -49.53 31.75 0)
				(length 2.54)
				(name "PE2_RX10")
				(number "1")
			)
			(pin power_in line
				(at -49.53 8.89 0)
				(length 2.54)
				(name "VSS")
				(number "10")
			)
			(pin bidirectional line
				(at -29.21 50.8 270)
				(length 2.54)
				(name "VDD")
				(number "100")
			)
			(pin power_in line
				(at -49.53 6.35 0)
				(length 2.54)
				(name "VDD")
				(number "11")
			)
			(pin bidirectional line
				(at -49.53 3.81 0)
				(length 2.54)
				(name "PH0_OSC_IN")
				(number "12")
			)
			(pin bidirectional line
				(at -49.53 1.27 0)
				(length 2.54)
				(name "PH1_OSC_OUT")
				(number "13")
			)
			(pin bidirectional line
				(at -49.53 -1.27 0)
				(length 2.54)
				(name "~{RST}")
				(number "14")
			)
			(pin bidirectional line
				(at -49.53 -3.81 0)
				(length 2.54)
				(name "PC0_USB_STP")
				(number "15")
			)
			(pin bidirectional line
				(at -49.53 -6.35 0)
				(length 2.54)
				(name "PC1_SDMMC2_CK")
				(number "16")
			)
			(pin bidirectional line
				(at -49.53 -8.89 0)
				(length 2.54)
				(name "PC2_C_GPIO")
				(number "17")
			)
			(pin bidirectional line
				(at -49.53 -11.43 0)
				(length 2.54)
				(name "PC3_C_ADC2_IN1")
				(number "18")
			)
			(pin power_in line
				(at -49.53 -13.97 0)
				(length 2.54)
				(name "VSSA")
				(number "19")
			)
			(pin bidirectional line
				(at -49.53 29.21 0)
				(length 2.54)
				(name "PE3_TX10")
				(number "2")
			)
			(pin bidirectional line
				(at -49.53 -16.51 0)
				(length 2.54)
				(name "VREF_OUT")
				(number "20")
			)
			(pin power_in line
				(at -49.53 -19.05 0)
				(length 2.54)
				(name "VDDA")
				(number "21")
			)
			(pin bidirectional line
				(at -49.53 -21.59 0)
				(length 2.54)
				(name "PA0_SDMMC2_CMD")
				(number "22")
			)
			(pin bidirectional line
				(at -49.53 -24.13 0)
				(length 2.54)
				(name "PA1_GPIO")
				(number "23")
			)
			(pin bidirectional line
				(at -49.53 -26.67 0)
				(length 2.54)
				(name "PA2_WKUP2")
				(number "24")
			)
			(pin bidirectional line
				(at -49.53 -29.21 0)
				(length 2.54)
				(name "PA3_ADC1_IN15")
				(number "25")
			)
			(pin power_in line
				(at -29.21 -49.53 90)
				(length 2.54)
				(name "VSS")
				(number "26")
			)
			(pin power_in line
				(at -26.67 -49.53 90)
				(length 2.54)
				(name "VDD")
				(number "27")
			)
			(pin bidirectional line
				(at -24.13 -49.53 90)
				(length 2.54)
				(name "PA4_I2S1_WS")
				(number "28")
			)
			(pin bidirectional line
				(at -21.59 -49.53 90)
				(length 2.54)
				(name "PA5_DAC1_OUT2")
				(number "29")
			)
			(pin bidirectional line
				(at -49.53 26.67 0)
				(length 2.54)
				(name "PE4_SPI4_NSS")
				(number "3")
			)
			(pin bidirectional line
				(at -19.05 -49.53 90)
				(length 2.54)
				(name "PA6_I2S1_SDI")
				(number "30")
			)
			(pin bidirectional line
				(at -16.51 -49.53 90)
				(length 2.54)
				(name "PA7_I2S1_SDO")
				(number "31")
			)
			(pin bidirectional line
				(at -13.97 -49.53 90)
				(length 2.54)
				(name "PC4_I2S1_MCK")
				(number "32")
			)
			(pin bidirectional line
				(at -11.43 -49.53 90)
				(length 2.54)
				(name "PC5_ADC2_IN8")
				(number "33")
			)
			(pin bidirectional line
				(at -8.89 -49.53 90)
				(length 2.54)
				(name "PB0_GPIO")
				(number "34")
			)
			(pin bidirectional line
				(at -6.35 -49.53 90)
				(length 2.54)
				(name "PB1_ADC1_IN5")
				(number "35")
			)
			(pin bidirectional line
				(at -3.81 -49.53 90)
				(length 2.54)
				(name "PB2_SPI3_COPI")
				(number "36")
			)
			(pin bidirectional line
				(at -1.27 -49.53 90)
				(length 2.54)
				(name "PE7_RX7")
				(number "37")
			)
			(pin bidirectional line
				(at 1.27 -49.53 90)
				(length 2.54)
				(name "PE8_TX7")
				(number "38")
			)
			(pin bidirectional line
				(at 3.81 -49.53 90)
				(length 2.54)
				(name "PE9_GPIO")
				(number "39")
			)
			(pin bidirectional line
				(at -49.53 24.13 0)
				(length 2.54)
				(name "PE5_SPI4_CIPO")
				(number "4")
			)
			(pin bidirectional line
				(at 6.35 -49.53 90)
				(length 2.54)
				(name "PE10_GPIO")
				(number "40")
			)
			(pin bidirectional line
				(at 8.89 -49.53 90)
				(length 2.54)
				(name "PE11_GPIO")
				(number "41")
			)
			(pin bidirectional line
				(at 11.43 -49.53 90)
				(length 2.54)
				(name "PE12_SPI4_SCK")
				(number "42")
			)
			(pin bidirectional line
				(at 13.97 -49.53 90)
				(length 2.54)
				(name "PE13_GPIO_~{SLEEP}")
				(number "43")
			)
			(pin bidirectional line
				(at 16.51 -49.53 90)
				(length 2.54)
				(name "PE14_GPIO")
				(number "44")
			)
			(pin bidirectional line
				(at 19.05 -49.53 90)
				(length 2.54)
				(name "PE15_GPIO")
				(number "45")
			)
			(pin bidirectional line
				(at 21.59 -49.53 90)
				(length 2.54)
				(name "PB10_GPIO")
				(number "46")
			)
			(pin bidirectional line
				(at 24.13 -49.53 90)
				(length 2.54)
				(name "PB11_GPIO")
				(number "47")
			)
			(pin power_out line
				(at 26.67 -49.53 90)
				(length 2.54)
				(name "VCAP")
				(number "48")
			)
			(pin power_in line
				(at 29.21 -49.53 90)
				(length 2.54)
				(name "VSS")
				(number "49")
			)
			(pin bidirectional line
				(at -49.53 21.59 0)
				(length 2.54)
				(name "PE6_SPI4_COPI")
				(number "5")
			)
			(pin power_in line
				(at 31.75 -49.53 90)
				(length 2.54)
				(name "VDD")
				(number "50")
			)
			(pin bidirectional line
				(at 50.8 -29.21 180)
				(length 2.54)
				(name "PB12_GPIO")
				(number "51")
			)
			(pin bidirectional line
				(at 50.8 -26.67 180)
				(length 2.54)
				(name "PB13_GPIO")
				(number "52")
			)
			(pin bidirectional line
				(at 50.8 -24.13 180)
				(length 2.54)
				(name "PB14_SDMMC2_D0")
				(number "53")
			)
			(pin bidirectional line
				(at 50.8 -21.59 180)
				(length 2.54)
				(name "PB15_GPIO")
				(number "54")
			)
			(pin bidirectional line
				(at 50.8 -19.05 180)
				(length 2.54)
				(name "PD8_TX3")
				(number "55")
			)
			(pin bidirectional line
				(at 50.8 -16.51 180)
				(length 2.54)
				(name "PD9_RX3")
				(number "56")
			)
			(pin bidirectional line
				(at 50.8 -13.97 180)
				(length 2.54)
				(name "PD10_GPIO")
				(number "57")
			)
			(pin bidirectional line
				(at 50.8 -11.43 180)
				(length 2.54)
				(name "PD11_SMBA")
				(number "58")
			)
			(pin bidirectional line
				(at 50.8 -8.89 180)
				(length 2.54)
				(name "PD12_I2C4_SCL")
				(number "59")
			)
			(pin bidirectional line
				(at -49.53 19.05 0)
				(length 2.54)
				(name "VBAT")
				(number "6")
			)
			(pin bidirectional line
				(at 50.8 -6.35 180)
				(length 2.54)
				(name "PD13_I2C4_SDA")
				(number "60")
			)
			(pin bidirectional line
				(at 50.8 -3.81 180)
				(length 2.54)
				(name "PD14_RX9")
				(number "61")
			)
			(pin bidirectional line
				(at 50.8 -1.27 180)
				(length 2.54)
				(name "PD15_TX9")
				(number "62")
			)
			(pin bidirectional line
				(at 50.8 1.27 180)
				(length 2.54)
				(name "PC6_TX6")
				(number "63")
			)
			(pin bidirectional line
				(at 50.8 3.81 180)
				(length 2.54)
				(name "PC7_RX6")
				(number "64")
			)
			(pin bidirectional line
				(at 50.8 6.35 180)
				(length 2.54)
				(name "PC8_GPIO_CK6")
				(number "65")
			)
			(pin bidirectional line
				(at 50.8 8.89 180)
				(length 2.54)
				(name "PC9_I2C3_SDA")
				(number "66")
			)
			(pin bidirectional line
				(at 50.8 11.43 180)
				(length 2.54)
				(name "PA8_I2C3_SCL")
				(number "67")
			)
			(pin bidirectional line
				(at 50.8 13.97 180)
				(length 2.54)
				(name "PA9_TX1")
				(number "68")
			)
			(pin bidirectional line
				(at 50.8 16.51 180)
				(length 2.54)
				(name "PA10_RX1")
				(number "69")
			)
			(pin bidirectional line
				(at -49.53 16.51 0)
				(length 2.54)
				(name "PC13_WKUP4")
				(number "7")
			)
			(pin bidirectional line
				(at 50.8 19.05 180)
				(length 2.54)
				(name "PA11_USB_DM")
				(number "70")
			)
			(pin bidirectional line
				(at 50.8 21.59 180)
				(length 2.54)
				(name "PA12_USB_DP")
				(number "71")
			)
			(pin bidirectional line
				(at 50.8 24.13 180)
				(length 2.54)
				(name "PA13_SWDIO")
				(number "72")
			)
			(pin power_out line
				(at 50.8 26.67 180)
				(length 2.54)
				(name "VCAP")
				(number "73")
			)
			(pin power_in line
				(at 50.8 29.21 180)
				(length 2.54)
				(name "VSS")
				(number "74")
			)
			(pin power_in line
				(at 50.8 31.75 180)
				(length 2.54)
				(name "VDD")
				(number "75")
			)
			(pin bidirectional line
				(at 31.75 50.8 270)
				(length 2.54)
				(name "PA14_SWCLK")
				(number "76")
			)
			(pin bidirectional line
				(at 29.21 50.8 270)
				(length 2.54)
				(name "PA15_SPI3_NSS")
				(number "77")
			)
			(pin bidirectional line
				(at 26.67 50.8 270)
				(length 2.54)
				(name "PC10_SPI3_SCK")
				(number "78")
			)
			(pin bidirectional line
				(at 24.13 50.8 270)
				(length 2.54)
				(name "PC11_SPI3_CIPO")
				(number "79")
			)
			(pin bidirectional line
				(at -49.53 13.97 0)
				(length 2.54)
				(name "PC14_OSC32_IN")
				(number "8")
			)
			(pin bidirectional line
				(at 21.59 50.8 270)
				(length 2.54)
				(name "PC12_TX5")
				(number "80")
			)
			(pin bidirectional line
				(at 19.05 50.8 270)
				(length 2.54)
				(name "PD0_RX4")
				(number "81")
			)
			(pin bidirectional line
				(at 16.51 50.8 270)
				(length 2.54)
				(name "PD1_TX4")
				(number "82")
			)
			(pin bidirectional line
				(at 13.97 50.8 270)
				(length 2.54)
				(name "PD2_RX5")
				(number "83")
			)
			(pin bidirectional line
				(at 11.43 50.8 270)
				(length 2.54)
				(name "PD3_CTS2")
				(number "84")
			)
			(pin bidirectional line
				(at 8.89 50.8 270)
				(length 2.54)
				(name "PD4_RTS2")
				(number "85")
			)
			(pin bidirectional line
				(at 6.35 50.8 270)
				(length 2.54)
				(name "PD5_TX2")
				(number "86")
			)
			(pin bidirectional line
				(at 3.81 50.8 270)
				(length 2.54)
				(name "PD6_RX2")
				(number "87")
			)
			(pin bidirectional line
				(at 1.27 50.8 270)
				(length 2.54)
				(name "PD7_GPIO_CK2")
				(number "88")
			)
			(pin bidirectional line
				(at -1.27 50.8 270)
				(length 2.54)
				(name "PB3_I2S1_CK")
				(number "89")
			)
			(pin bidirectional line
				(at -49.53 11.43 0)
				(length 2.54)
				(name "PC15_OSC32_OUT")
				(number "9")
			)
			(pin bidirectional line
				(at -3.81 50.8 270)
				(length 2.54)
				(name "PB4_GPIO")
				(number "90")
			)
			(pin bidirectional line
				(at -6.35 50.8 270)
				(length 2.54)
				(name "PB5_I2C1_SMBA")
				(number "91")
			)
			(pin bidirectional line
				(at -8.89 50.8 270)
				(length 2.54)
				(name "PB6_LP_TX1")
				(number "92")
			)
			(pin bidirectional line
				(at -11.43 50.8 270)
				(length 2.54)
				(name "PB7_LP_RX1")
				(number "93")
			)
			(pin bidirectional line
				(at -13.97 50.8 270)
				(length 2.54)
				(name "BOOT0")
				(number "94")
			)
			(pin bidirectional line
				(at -16.51 50.8 270)
				(length 2.54)
				(name "PB8_I2C1_SCL")
				(number "95")
			)
			(pin bidirectional line
				(at -19.05 50.8 270)
				(length 2.54)
				(name "PB9_I2C1_SDA")
				(number "96")
			)
			(pin bidirectional line
				(at -21.59 50.8 270)
				(length 2.54)
				(name "PE0_RX8")
				(number "97")
			)
			(pin bidirectional line
				(at -24.13 50.8 270)
				(length 2.54)
				(name "PE1_TX8")
				(number "98")
			)
			(pin bidirectional line
				(at -26.67 50.8 270)
				(length 2.54)
				(name "VSS")
				(number "99")
			)
		)
	)
	(symbol "STWD100PYW83F"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.35 6.5786 0)
		)
		(property "Value" "STWD100NYWY3F"
			(at -7.62 -7.62 0)
		)
		(property "Footprint" "ProjectFootprints:STWD100_5-TSSOP_SC-70-5_SOT-353-5"
			(at 0 -12.7 0)
		)
		(property "Datasheet" "https://www.st.com/content/ccc/resource/technical/document/datasheet/06/6a/b3/83/9a/c7/4f/22/CD00176077.pdf/files/CD00176077.pdf/jcr:content/translations/en.CD00176077.pdf"
			(at 0 -10.16 0)
		)
		(property "Description" "Watchdog Timer 1.6s Open Drain"
			(at 0 0 0)
		)
		(symbol "STWD100PYW83F_0_0"
			(pin bidirectional line
				(at -12.7 2.54 0)
				(length 5.08)
				(name "~{WDO}")
				(number "1")
			)
			(pin bidirectional line
				(at -12.7 0 0)
				(length 5.08)
				(name "GND")
				(number "2")
			)
			(pin bidirectional line
				(at -12.7 -2.54 0)
				(length 5.08)
				(name "~{EN}")
				(number "3")
			)
			(pin bidirectional line
				(at 12.7 -2.54 180)
				(length 5.08)
				(name "WDI")
				(number "4")
			)
			(pin bidirectional line
				(at 12.7 2.54 180)
				(length 5.08)
				(name "VCC")
				(number "5")
			)
		)
	)
	(symbol "SerLog_CF3"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "M"
			(at -5.08 45.72 0)
		)
		(property "Value" ""
			(at 71.12 -99.06 0)
		)
		(property "Footprint" ""
			(at 71.12 -99.06 0)
		)
		(property "Datasheet" ""
			(at 71.12 -99.06 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "SerLog_CF3_1_1"
			(pin passive line
				(at -55.88 30.48 0)
				(length 2.54)
				(name "GND")
				(number "1")
			)
			(pin no_connect line
				(at -27.94 20.32 180)
				(length 2.54)
				(name "TBD")
				(number "10")
			)
			(pin passive line
				(at -55.88 17.78 0)
				(length 2.54)
				(name "I2C1_SCL")
				(number "11")
			)
			(pin passive line
				(at -27.94 17.78 180)
				(length 2.54)
				(name "I2C1_SDA")
				(number "12")
			)
			(pin passive line
				(at -55.88 15.24 0)
				(length 2.54)
				(name "I2C0_SCL")
				(number "13")
			)
			(pin passive line
				(at -27.94 15.24 180)
				(length 2.54)
				(name "I2C0_SDA")
				(number "14")
			)
			(pin passive line
				(at -55.88 12.7 0)
				(length 2.54)
				(name "SPI1_CS")
				(number "15")
			)
			(pin passive line
				(at -27.94 12.7 180)
				(length 2.54)
				(name "SPI1_SCK")
				(number "16")
			)
			(pin passive line
				(at -55.88 10.16 0)
				(length 2.54)
				(name "SPI1_COPI")
				(number "17")
			)
			(pin passive line
				(at -27.94 10.16 180)
				(length 2.54)
				(name "SPI1_CIPO")
				(number "18")
			)
			(pin passive line
				(at -55.88 7.62 0)
				(length 2.54)
				(name "SPI2_CS")
				(number "19")
			)
			(pin passive line
				(at -27.94 30.48 180)
				(length 2.54)
				(name "VIN")
				(number "2")
			)
			(pin passive line
				(at -27.94 7.62 180)
				(length 2.54)
				(name "SPI2_SCK")
				(number "20")
			)
			(pin passive line
				(at -55.88 5.08 0)
				(length 2.54)
				(name "SPI2_COPI")
				(number "21")
			)
			(pin passive line
				(at -27.94 5.08 180)
				(length 2.54)
				(name "SPI2_CIPO")
				(number "22")
			)
			(pin passive line
				(at -55.88 2.54 0)
				(length 2.54)
				(name "SPI3_CS")
				(number "23")
			)
			(pin passive line
				(at -27.94 2.54 180)
				(length 2.54)
				(name "SPI3_SCK")
				(number "24")
			)
			(pin passive line
				(at -55.88 0 0)
				(length 2.54)
				(name "SPI3_COPI")
				(number "25")
			)
			(pin passive line
				(at -27.94 0 180)
				(length 2.54)
				(name "SPI3_CIPO")
				(number "26")
			)
			(pin passive line
				(at -55.88 -2.54 0)
				(length 2.54)
				(name "GPIOA_27")
				(number "27")
			)
			(pin passive line
				(at -27.94 -2.54 180)
				(length 2.54)
				(name "GPIOA_28")
				(number "28")
			)
			(pin passive line
				(at -55.88 -5.08 0)
				(length 2.54)
				(name "CAN1_TX")
				(number "29")
			)
			(pin passive line
				(at -55.88 27.94 0)
				(length 2.54)
				(name "VO_3V6")
				(number "3")
			)
			(pin passive line
				(at -27.94 -5.08 180)
				(length 2.54)
				(name "CAN1_RX")
				(number "30")
			)
			(pin passive line
				(at -55.88 -7.62 0)
				(length 2.54)
				(name "UART7_TX")
				(number "31")
			)
			(pin passive line
				(at -27.94 -7.62 180)
				(length 2.54)
				(name "UART7_RX")
				(number "32")
			)
			(pin passive line
				(at -55.88 -10.16 0)
				(length 2.54)
				(name "UART6_TX")
				(number "33")
			)
			(pin passive line
				(at -27.94 -10.16 180)
				(length 2.54)
				(name "UART6_RX")
				(number "34")
			)
			(pin passive line
				(at -55.88 -12.7 0)
				(length 2.54)
				(name "UART5_TX")
				(number "35")
			)
			(pin passive line
				(at -27.94 -12.7 180)
				(length 2.54)
				(name "UART5_RX")
				(number "36")
			)
			(pin passive line
				(at -55.88 -15.24 0)
				(length 2.54)
				(name "UART4_TX")
				(number "37")
			)
			(pin passive line
				(at -27.94 -15.24 180)
				(length 2.54)
				(name "UART4_TX")
				(number "38")
			)
			(pin passive line
				(at -55.88 -17.78 0)
				(length 2.54)
				(name "UART3_TX")
				(number "39")
			)
			(pin passive line
				(at -27.94 27.94 180)
				(length 2.54)
				(name "~{RST}")
				(number "4")
			)
			(pin passive line
				(at -27.94 -17.78 180)
				(length 2.54)
				(name "UART3_RX")
				(number "40")
			)
			(pin passive line
				(at -55.88 -20.32 0)
				(length 2.54)
				(name "UART2_TX")
				(number "41")
			)
			(pin passive line
				(at -27.94 -20.32 180)
				(length 2.54)
				(name "UART2_RX")
				(number "42")
			)
			(pin passive line
				(at -55.88 -22.86 0)
				(length 2.54)
				(name "SER1_TX")
				(number "43")
			)
			(pin passive line
				(at -27.94 -22.86 180)
				(length 2.54)
				(name "SER1_RX")
				(number "44")
			)
			(pin passive line
				(at -55.88 -25.4 0)
				(length 2.54)
				(name "SER0_TX")
				(number "45")
			)
			(pin passive line
				(at -27.94 -25.4 180)
				(length 2.54)
				(name "SER0_TX")
				(number "46")
			)
			(pin passive line
				(at -55.88 -27.94 0)
				(length 2.54)
				(name "GPIOA_47")
				(number "47")
			)
			(pin passive line
				(at -27.94 -27.94 180)
				(length 2.54)
				(name "GPIOA_48")
				(number "48")
			)
			(pin passive line
				(at -55.88 -30.48 0)
				(length 2.54)
				(name "GPIOA_49")
				(number "49")
			)
			(pin passive line
				(at -55.88 25.4 0)
				(length 2.54)
				(name "VO_3V3")
				(number "5")
			)
			(pin passive line
				(at -27.94 -30.48 180)
				(length 2.54)
				(name "GPIOA_50")
				(number "50")
			)
			(pin passive line
				(at 22.86 22.86 90)
				(length 2.54)
				(name "GND")
				(number "51")
			)
			(pin passive line
				(at 22.86 45.72 270)
				(length 2.54)
				(name "VIN_5Y")
				(number "52")
			)
			(pin passive line
				(at 25.4 22.86 90)
				(length 2.54)
				(name "VO_3V6")
				(number "53")
			)
			(pin passive line
				(at 25.4 45.72 270)
				(length 2.54)
				(name "VO_LOG")
				(number "54")
			)
			(pin no_connect line
				(at 27.94 22.86 90)
				(length 2.54)
				(name "TBD")
				(number "55")
			)
			(pin passive line
				(at 27.94 45.72 270)
				(length 2.54)
				(name "GPIO_56")
				(number "56")
			)
			(pin passive line
				(at 30.48 22.86 90)
				(length 2.54)
				(name "CAN0_TX")
				(number "57")
			)
			(pin passive line
				(at 30.48 45.72 270)
				(length 2.54)
				(name "CAN0_RX")
				(number "58")
			)
			(pin no_connect line
				(at 33.02 22.86 90)
				(length 2.54)
				(name "TBD")
				(number "59")
			)
			(pin passive line
				(at -27.94 25.4 180)
				(length 2.54)
				(name "~{SHDN}")
				(number "6")
			)
			(pin no_connect line
				(at 33.02 45.72 270)
				(length 2.54)
				(name "TBD")
				(number "60")
			)
			(pin no_connect line
				(at 35.56 22.86 90)
				(length 2.54)
				(name "TBD")
				(number "61")
			)
			(pin passive line
				(at 35.56 45.72 270)
				(length 2.54)
				(name "GPIO_62")
				(number "62")
			)
			(pin passive line
				(at 38.1 22.86 90)
				(length 2.54)
				(name "GPIO_63")
				(number "63")
			)
			(pin passive line
				(at 38.1 45.72 270)
				(length 2.54)
				(name "GPIO_64")
				(number "64")
			)
			(pin passive line
				(at 40.64 22.86 90)
				(length 2.54)
				(name "GPIO_65")
				(number "65")
			)
			(pin passive line
				(at 40.64 45.72 270)
				(length 2.54)
				(name "GPIO_66")
				(number "66")
			)
			(pin passive line
				(at 43.18 22.86 90)
				(length 2.54)
				(name "GPIO_67")
				(number "67")
			)
			(pin passive line
				(at 43.18 45.72 270)
				(length 2.54)
				(name "GPIO_68")
				(number "68")
			)
			(pin passive line
				(at 45.72 22.86 90)
				(length 2.54)
				(name "GPIO_69")
				(number "69")
			)
			(pin passive line
				(at -55.88 22.86 0)
				(length 2.54)
				(name "VbuBAT")
				(number "7")
			)
			(pin passive line
				(at 45.72 45.72 270)
				(length 2.54)
				(name "GPIO_70")
				(number "70")
			)
			(pin passive line
				(at 22.86 -45.72 90)
				(length 2.54)
				(name "GND")
				(number "71")
			)
			(pin passive line
				(at 22.86 -20.32 270)
				(length 2.54)
				(name "VIN_5X")
				(number "72")
			)
			(pin passive line
				(at 25.4 -45.72 90)
				(length 2.54)
				(name "VO_3V6")
				(number "73")
			)
			(pin passive line
				(at 25.4 -20.32 270)
				(length 2.54)
				(name "VO_EXT_3V3")
				(number "74")
			)
			(pin passive line
				(at 27.94 -45.72 90)
				(length 2.54)
				(name "GPIOA_75")
				(number "75")
			)
			(pin no_connect line
				(at 27.94 -20.32 270)
				(length 2.54)
				(name "TBD")
				(number "76")
			)
			(pin passive line
				(at 30.48 -45.72 90)
				(length 2.54)
				(name "GPIOA_77")
				(number "77")
			)
			(pin no_connect line
				(at 30.48 -20.32 270)
				(length 2.54)
				(name "TBD")
				(number "78")
			)
			(pin passive line
				(at 33.02 -45.72 90)
				(length 2.54)
				(name "GPIOA_79")
				(number "79")
			)
			(pin passive line
				(at -27.94 22.86 180)
				(length 2.54)
				(name "~{WAKE}")
				(number "8")
			)
			(pin no_connect line
				(at 33.02 -20.32 270)
				(length 2.54)
				(name "TBD")
				(number "80")
			)
			(pin passive line
				(at 35.56 -45.72 90)
				(length 2.54)
				(name "GPIOA_81")
				(number "81")
			)
			(pin no_connect line
				(at 35.56 -20.32 270)
				(length 2.54)
				(name "TBD")
				(number "82")
			)
			(pin passive line
				(at 38.1 -45.72 90)
				(length 2.54)
				(name "GPIOA_83")
				(number "83")
			)
			(pin no_connect line
				(at 38.1 -20.32 270)
				(length 2.54)
				(name "TBD")
				(number "84")
			)
			(pin passive line
				(at 40.64 -45.72 90)
				(length 2.54)
				(name "GPIOA_85")
				(number "85")
			)
			(pin passive line
				(at 40.64 -20.32 270)
				(length 2.54)
				(name "GPIOA_86")
				(number "86")
			)
			(pin no_connect line
				(at 43.18 -45.72 90)
				(length 2.54)
				(name "TBD")
				(number "87")
			)
			(pin no_connect line
				(at 43.18 -20.32 270)
				(length 2.54)
				(name "TBD")
				(number "88")
			)
			(pin no_connect line
				(at 45.72 -45.72 90)
				(length 2.54)
				(name "TBD")
				(number "89")
			)
			(pin passive line
				(at -55.88 20.32 0)
				(length 2.54)
				(name "VrtcBAT")
				(number "9")
			)
			(pin no_connect line
				(at 45.72 -20.32 270)
				(length 2.54)
				(name "TBD")
				(number "90")
			)
		)
	)
	(symbol "SerMonK_v3"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -13.97 53.34 0)
		)
		(property "Value" "SerMonK_v3"
			(at 8.89 53.34 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "SerMonK_v3_0_0"
			(text " rtc i2c3 addr 0x68"
				(at 0 -22.86 0)
			)
			(text "bme i2c3 addr 0x77"
				(at 0 -25.4 0)
			)
			(text "fram i2c3 addr 0x50"
				(at 0 -27.94 0)
			)
			(pin power_in line
				(at -33.02 24.13 0)
				(length 5.08)
				(name "GND")
				(number "1")
			)
			(pin bidirectional line
				(at -33.02 1.27 0)
				(length 5.08)
				(name "PE6_SPI4_COPI")
				(number "10")
			)
			(pin bidirectional line
				(at -33.02 -1.27 0)
				(length 5.08)
				(name "PA5_GPIO_DAC1_O2")
				(number "11")
			)
			(pin bidirectional line
				(at -33.02 -3.81 0)
				(length 5.08)
				(name "PA4_I2S1_WS")
				(number "12")
			)
			(pin bidirectional line
				(at -33.02 -6.35 0)
				(length 5.08)
				(name "PA6_I2S1_SDI_ADC3")
				(number "13")
			)
			(pin bidirectional line
				(at -33.02 -8.89 0)
				(length 5.08)
				(name "PB3_I2S1_CK_SD2_D2")
				(number "14")
			)
			(pin bidirectional line
				(at -33.02 -11.43 0)
				(length 5.08)
				(name "PA7_I2S1_SDO_ADC7")
				(number "15")
			)
			(pin bidirectional line
				(at -33.02 -13.97 0)
				(length 5.08)
				(name "PC4_I2S1_MCK_ADC4")
				(number "16")
			)
			(pin bidirectional line
				(at -33.02 -16.51 0)
				(length 5.08)
				(name "PC8_I2C3_SCL")
				(number "17")
			)
			(pin bidirectional line
				(at -33.02 -19.05 0)
				(length 5.08)
				(name "PC9_I2C3_SDA")
				(number "18")
			)
			(pin bidirectional line
				(at -33.02 -21.59 0)
				(length 5.08)
				(name "PD14_RX9")
				(number "19")
			)
			(pin bidirectional line
				(at -33.02 21.59 0)
				(length 5.08)
				(name "~{RST}")
				(number "2")
			)
			(pin bidirectional line
				(at -33.02 -24.13 0)
				(length 5.08)
				(name "PD15_TX9")
				(number "20")
			)
			(pin bidirectional line
				(at 33.02 -24.13 180)
				(length 5.08)
				(name "PC6_TX6")
				(number "21")
			)
			(pin bidirectional line
				(at 33.02 -21.59 180)
				(length 5.08)
				(name "PC7_RX6")
				(number "22")
			)
			(pin bidirectional line
				(at 33.02 -19.05 180)
				(length 5.08)
				(name "PC8_GPIO_CK6")
				(number "23")
			)
			(pin bidirectional line
				(at 33.02 -16.51 180)
				(length 5.08)
				(name "PA9_TX1")
				(number "24")
			)
			(pin bidirectional line
				(at 33.02 -13.97 180)
				(length 5.08)
				(name "PA10_RX1")
				(number "25")
			)
			(pin bidirectional line
				(at 33.02 -11.43 180)
				(length 5.08)
				(name "PA12_TX4")
				(number "26")
			)
			(pin bidirectional line
				(at 33.02 -8.89 180)
				(length 5.08)
				(name "PA11_RX4")
				(number "27")
			)
			(pin bidirectional line
				(at 33.02 -6.35 180)
				(length 5.08)
				(name "PB6_LP_TX1")
				(number "28")
			)
			(pin bidirectional line
				(at 33.02 -3.81 180)
				(length 5.08)
				(name "PB7_LP_RX1")
				(number "29")
			)
			(pin bidirectional line
				(at -33.02 19.05 0)
				(length 5.08)
				(name "PA2_WKUP2")
				(number "3")
			)
			(pin bidirectional line
				(at 33.02 -1.27 180)
				(length 5.08)
				(name "PD5_TX2")
				(number "30")
			)
			(pin bidirectional line
				(at 33.02 1.27 180)
				(length 5.08)
				(name "PD6_RX2")
				(number "31")
			)
			(pin bidirectional line
				(at 33.02 3.81 180)
				(length 5.08)
				(name "PE10_GPIO")
				(number "32")
			)
			(pin bidirectional line
				(at 33.02 6.35 180)
				(length 5.08)
				(name "PB2_SPI3_COPI")
				(number "33")
			)
			(pin bidirectional line
				(at 33.02 8.89 180)
				(length 5.08)
				(name "PC10_SPI3_SCK")
				(number "34")
			)
			(pin bidirectional line
				(at 33.02 11.43 180)
				(length 5.08)
				(name "PC11_SPI3_CIPO")
				(number "35")
			)
			(pin bidirectional line
				(at 33.02 13.97 180)
				(length 5.08)
				(name "PB9_I2C1_SDA")
				(number "36")
			)
			(pin bidirectional line
				(at 33.02 16.51 180)
				(length 5.08)
				(name "PB8_I2C1_SCL")
				(number "37")
			)
			(pin power_out line
				(at 33.02 19.05 180)
				(length 5.08)
				(name "+3V3")
				(number "38")
			)
			(pin power_in line
				(at 33.02 21.59 180)
				(length 5.08)
				(name "VIN_5V_15V")
				(number "39")
			)
			(pin bidirectional line
				(at -33.02 16.51 0)
				(length 5.08)
				(name "PE7_RX7")
				(number "4")
			)
			(pin power_in line
				(at 33.02 24.13 180)
				(length 5.08)
				(name "GND")
				(number "40")
			)
			(pin bidirectional line
				(at -22.86 46.99 0)
				(length 5.08)
				(name "~{BRD_WAKE}")
				(number "41")
			)
			(pin bidirectional line
				(at -22.86 44.45 0)
				(length 5.08)
				(name "PE15_GPIO")
				(number "42")
			)
			(pin bidirectional line
				(at -22.86 41.91 0)
				(length 5.08)
				(name "PE14_GPIO")
				(number "43")
			)
			(pin bidirectional line
				(at -22.86 39.37 0)
				(length 5.08)
				(name "PD2_RX5")
				(number "44")
			)
			(pin bidirectional line
				(at -22.86 36.83 0)
				(length 5.08)
				(name "PC12_TX5")
				(number "45")
			)
			(pin bidirectional line
				(at -22.86 34.29 0)
				(length 5.08)
				(name "PE2_RX10")
				(number "46")
			)
			(pin bidirectional line
				(at -22.86 31.75 0)
				(length 5.08)
				(name "PE3_TX10")
				(number "47")
			)
			(pin bidirectional line
				(at -22.86 29.21 0)
				(length 5.08)
				(name "PE4_SPI4_NSS")
				(number "48")
			)
			(pin bidirectional line
				(at 22.86 29.21 180)
				(length 5.08)
				(name "PA15_SPI3_NSS")
				(number "49")
			)
			(pin bidirectional line
				(at -33.02 13.97 0)
				(length 5.08)
				(name "PE8_TX7")
				(number "5")
			)
			(pin bidirectional line
				(at 22.86 31.75 180)
				(length 5.08)
				(name "PE1_TX8")
				(number "50")
			)
			(pin bidirectional line
				(at 22.86 34.29 180)
				(length 5.08)
				(name "PE0_RX8")
				(number "51")
			)
			(pin bidirectional line
				(at 22.86 36.83 180)
				(length 5.08)
				(name "PD3_CTS2")
				(number "52")
			)
			(pin bidirectional line
				(at 22.86 39.37 180)
				(length 5.08)
				(name "PD4_RTS2")
				(number "53")
			)
			(pin bidirectional line
				(at 22.86 41.91 180)
				(length 5.08)
				(name "PD7_GPIO_CK2")
				(number "54")
			)
			(pin output line
				(at 22.86 44.45 180)
				(length 5.08)
				(name "VREG_5V")
				(number "55")
			)
			(pin input line
				(at 22.86 46.99 180)
				(length 5.08)
				(name "VIN_6V_36V")
				(number "56")
			)
			(pin bidirectional line
				(at -33.02 11.43 0)
				(length 5.08)
				(name "PD9_RX3")
				(number "6")
			)
			(pin bidirectional line
				(at -33.02 8.89 0)
				(length 5.08)
				(name "PD8_TX3")
				(number "7")
			)
			(pin bidirectional line
				(at -33.02 6.35 0)
				(length 5.08)
				(name "PE5_SPI4_CIPO")
				(number "8")
			)
			(pin bidirectional line
				(at -33.02 3.81 0)
				(length 5.08)
				(name "PE12_SPI4_SCK")
				(number "9")
			)
		)
		(symbol "SerMonK_v3_0_1")
	)
	(symbol "SerialMonster_I2C_SPI"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 19.05 26.67 0)
		)
		(property "Value" "SerialMonster_I2C_SPI"
			(at 3.81 26.67 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "SerialMonster_I2C_SPI_0_1")
		(symbol "SerialMonster_I2C_SPI_1_1"
			(pin power_in line
				(at -25.4 20.32 0)
				(length 2.54)
				(name "GND")
				(number "1")
			)
			(pin input line
				(at -25.4 -5.08 0)
				(length 2.54)
				(name "~{SPI_B_CS}")
				(number "10")
			)
			(pin output line
				(at -25.4 -7.62 0)
				(length 2.54)
				(name "SPI_B_COPI")
				(number "11")
			)
			(pin output line
				(at -25.4 -10.16 0)
				(length 2.54)
				(name "SPI_B_SCLK")
				(number "12")
			)
			(pin power_in line
				(at -25.4 -15.24 0)
				(length 2.54)
				(name "GND")
				(number "13")
			)
			(pin power_in line
				(at -25.4 -17.78 0)
				(length 2.54)
				(name "SPI_A_VOUT")
				(number "14")
			)
			(pin input line
				(at -25.4 -20.32 0)
				(length 2.54)
				(name "SPI_A_CIPO")
				(number "15")
			)
			(pin input line
				(at -25.4 -22.86 0)
				(length 2.54)
				(name "~{SPI_A_CS}")
				(number "16")
			)
			(pin output line
				(at -25.4 -25.4 0)
				(length 2.54)
				(name "SPI_A_COPI")
				(number "17")
			)
			(pin output line
				(at -25.4 -27.94 0)
				(length 2.54)
				(name "SPI_A_SCLK")
				(number "18")
			)
			(pin power_in line
				(at 30.48 20.32 180)
				(length 2.54)
				(name "GND")
				(number "19")
			)
			(pin power_in line
				(at -25.4 17.78 0)
				(length 2.54)
				(name "SPI_C_VOUT")
				(number "2")
			)
			(pin output line
				(at 30.48 17.78 180)
				(length 2.54)
				(name "+3V3")
				(number "20")
			)
			(pin bidirectional line
				(at 30.48 15.24 180)
				(length 2.54)
				(name "I2C_A_SCL")
				(number "21")
			)
			(pin bidirectional line
				(at 30.48 12.7 180)
				(length 2.54)
				(name "I2C_C_SCL")
				(number "22")
			)
			(pin bidirectional line
				(at 30.48 10.16 180)
				(length 2.54)
				(name "I2C_A_SDA")
				(number "23")
			)
			(pin bidirectional line
				(at 30.48 7.62 180)
				(length 2.54)
				(name "I2C_C_SDA")
				(number "24")
			)
			(pin power_in line
				(at -17.78 -44.45 90)
				(length 2.54)
				(name "GND")
				(number "25")
			)
			(pin power_out line
				(at -15.24 -44.45 90)
				(length 2.54)
				(name "VOUT_21")
				(number "26")
			)
			(pin power_in line
				(at -12.7 -44.45 90)
				(length 2.54)
				(name "GND")
				(number "27")
			)
			(pin power_out line
				(at -10.16 -44.45 90)
				(length 2.54)
				(name "VOUT_22")
				(number "28")
			)
			(pin power_in line
				(at -7.62 -44.45 90)
				(length 2.54)
				(name "GND")
				(number "29")
			)
			(pin input line
				(at -25.4 15.24 0)
				(length 2.54)
				(name "SPI_C_CIPO")
				(number "3")
			)
			(pin power_out line
				(at -5.08 -44.45 90)
				(length 2.54)
				(name "VOUT_23")
				(number "30")
			)
			(pin power_in line
				(at -2.54 -44.45 90)
				(length 2.54)
				(name "GND")
				(number "31")
			)
			(pin power_out line
				(at 0 -44.45 90)
				(length 2.54)
				(name "VOUT_24")
				(number "32")
			)
			(pin power_in line
				(at 5.08 -44.45 90)
				(length 2.54)
				(name "GND")
				(number "33")
			)
			(pin power_out line
				(at 7.62 -44.45 90)
				(length 2.54)
				(name "VOUT_OPTO_21")
				(number "34")
			)
			(pin power_in line
				(at 10.16 -44.45 90)
				(length 2.54)
				(name "GND")
				(number "35")
			)
			(pin power_out line
				(at 12.7 -44.45 90)
				(length 2.54)
				(name "VOUT_OPTO_22")
				(number "36")
			)
			(pin power_in line
				(at 15.24 -44.45 90)
				(length 2.54)
				(name "GND")
				(number "37")
			)
			(pin power_out line
				(at 17.78 -44.45 90)
				(length 2.54)
				(name "VOUT_OPTO_23")
				(number "38")
			)
			(pin power_in line
				(at 20.32 -44.45 90)
				(length 2.54)
				(name "GND")
				(number "39")
			)
			(pin input line
				(at -25.4 12.7 0)
				(length 2.54)
				(name "~{SPI_C_CS}")
				(number "4")
			)
			(pin power_out line
				(at 22.86 -44.45 90)
				(length 2.54)
				(name "VOUT_OPTO_24")
				(number "40")
			)
			(pin output line
				(at -25.4 10.16 0)
				(length 2.54)
				(name "SPI_C_COPI")
				(number "5")
			)
			(pin output line
				(at -25.4 7.62 0)
				(length 2.54)
				(name "SPI_C_SCLK")
				(number "6")
			)
			(pin power_in line
				(at -25.4 2.54 0)
				(length 2.54)
				(name "GND")
				(number "7")
			)
			(pin power_in line
				(at -25.4 0 0)
				(length 2.54)
				(name "SPI_B_VOUT")
				(number "8")
			)
			(pin input line
				(at -25.4 -2.54 0)
				(length 2.54)
				(name "SPI_B_CIPO")
				(number "9")
			)
		)
	)
	(symbol "Serial_Monster_mod_02x34_02x16"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 -10.16 0)
		)
		(property "Value" "Serial_Monster_mod_02x34_02x16"
			(at -5.08 -6.35 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "Serial_Monster_mod_02x34_02x16_0_1")
		(symbol "Serial_Monster_mod_02x34_02x16_1_1"
			(text "Boot: USART2, SPI1, USB"
				(at -3.81 34.29 0)
			)
			(pin passive line
				(at -35.56 43.18 0)
				(length 3.81)
				(name "AVCC")
				(number "1")
			)
			(pin passive line
				(at -35.56 20.32 0)
				(length 3.81)
				(name "I2C_A_SDA")
				(number "10")
			)
			(pin input line
				(at 25.4 -48.26 180)
				(length 2.54)
				(name "UART16_RX")
				(number "100")
			)
			(pin passive line
				(at -35.56 17.78 0)
				(length 3.81)
				(name "I2C_A_SCL")
				(number "11")
			)
			(pin passive line
				(at -35.56 15.24 0)
				(length 3.81)
				(name "SPI_A_COPI")
				(number "12")
			)
			(pin passive line
				(at -35.56 12.7 0)
				(length 3.81)
				(name "SPI_A_CIPO")
				(number "13")
			)
			(pin passive line
				(at -35.56 10.16 0)
				(length 3.81)
				(name "SPI_A_SCLK")
				(number "14")
			)
			(pin passive line
				(at -35.56 7.62 0)
				(length 3.81)
				(name "SPI_A_CS")
				(number "15")
			)
			(pin passive line
				(at -35.56 5.08 0)
				(length 3.81)
				(name "SPI_A_NSS")
				(number "16")
			)
			(pin passive line
				(at -35.56 2.54 0)
				(length 3.81)
				(name "GND")
				(number "17")
			)
			(pin passive line
				(at -35.56 0 0)
				(length 3.81)
				(name "GPIO_B")
				(number "18")
			)
			(pin passive line
				(at -35.56 -2.54 0)
				(length 3.81)
				(name "GPIO_C")
				(number "19")
			)
			(pin passive line
				(at -35.56 40.64 0)
				(length 3.81)
				(name "ADC_A")
				(number "2")
			)
			(pin passive line
				(at -35.56 -5.08 0)
				(length 3.81)
				(name "GPIO_D")
				(number "20")
			)
			(pin passive line
				(at -35.56 -7.62 0)
				(length 3.81)
				(name "USART1_RX")
				(number "21")
			)
			(pin passive line
				(at -35.56 -10.16 0)
				(length 3.81)
				(name "USART1_TX")
				(number "22")
			)
			(pin passive line
				(at -35.56 -12.7 0)
				(length 3.81)
				(name "USART1_CK")
				(number "23")
			)
			(pin passive line
				(at -35.56 -15.24 0)
				(length 3.81)
				(name "USART2_RX")
				(number "24")
			)
			(pin passive line
				(at -35.56 -17.78 0)
				(length 3.81)
				(name "USART2_TX")
				(number "25")
			)
			(pin passive line
				(at -35.56 -20.32 0)
				(length 3.81)
				(name "USART2_CTS")
				(number "26")
			)
			(pin passive line
				(at -35.56 -22.86 0)
				(length 3.81)
				(name "USART2_RTS")
				(number "27")
			)
			(pin passive line
				(at -35.56 -25.4 0)
				(length 3.81)
				(name "USART3_RX")
				(number "28")
			)
			(pin passive line
				(at -35.56 -27.94 0)
				(length 3.81)
				(name "USART3_TX")
				(number "29")
			)
			(pin passive line
				(at -35.56 38.1 0)
				(length 3.81)
				(name "ADC_B")
				(number "3")
			)
			(pin passive line
				(at -35.56 -30.48 0)
				(length 3.81)
				(name "USART3_CK")
				(number "30")
			)
			(pin passive line
				(at -35.56 -33.02 0)
				(length 3.81)
				(name "UART4_RX")
				(number "31")
			)
			(pin passive line
				(at -35.56 -35.56 0)
				(length 3.81)
				(name "UART4_TX")
				(number "32")
			)
			(pin passive line
				(at -35.56 -38.1 0)
				(length 3.81)
				(name "UART5_RX")
				(number "33")
			)
			(pin passive line
				(at -35.56 -40.64 0)
				(length 3.81)
				(name "UART5_TX")
				(number "34")
			)
			(pin passive line
				(at 35.56 -40.64 180)
				(length 3.81)
				(name "SPARE1_TX")
				(number "35")
			)
			(pin passive line
				(at 35.56 -38.1 180)
				(length 3.81)
				(name "SPARE1_RX")
				(number "36")
			)
			(pin passive line
				(at 35.56 -35.56 180)
				(length 3.81)
				(name "UART10_TX")
				(number "37")
			)
			(pin passive line
				(at 35.56 -33.02 180)
				(length 3.81)
				(name "UART10_RX")
				(number "38")
			)
			(pin passive line
				(at 35.56 -30.48 180)
				(length 3.81)
				(name "UART9_TX")
				(number "39")
			)
			(pin passive line
				(at -35.56 35.56 0)
				(length 3.81)
				(name "ADC_C")
				(number "4")
			)
			(pin passive line
				(at 35.56 -27.94 180)
				(length 3.81)
				(name "UART9_RX")
				(number "40")
			)
			(pin passive line
				(at 35.56 -25.4 180)
				(length 3.81)
				(name "UART8_TX")
				(number "41")
			)
			(pin passive line
				(at 35.56 -22.86 180)
				(length 3.81)
				(name "UART8_RX")
				(number "42")
			)
			(pin passive line
				(at 35.56 -20.32 180)
				(length 3.81)
				(name "USART7_TX")
				(number "43")
			)
			(pin passive line
				(at 35.56 -17.78 180)
				(length 3.81)
				(name "USART7_RX")
				(number "44")
			)
			(pin passive line
				(at 35.56 -15.24 180)
				(length 3.81)
				(name "USART6_TX")
				(number "45")
			)
			(pin passive line
				(at 35.56 -12.7 180)
				(length 3.81)
				(name "USART6_RX")
				(number "46")
			)
			(pin passive line
				(at 35.56 -10.16 180)
				(length 3.81)
				(name "SPI_C_CS")
				(number "47")
			)
			(pin passive line
				(at 35.56 -7.62 180)
				(length 3.81)
				(name "SPI_C_SCLK")
				(number "48")
			)
			(pin passive line
				(at 35.56 -5.08 180)
				(length 3.81)
				(name "SPI_C_CIPO")
				(number "49")
			)
			(pin passive line
				(at -35.56 33.02 0)
				(length 3.81)
				(name "AGND")
				(number "5")
			)
			(pin passive line
				(at 35.56 -2.54 180)
				(length 3.81)
				(name "SPI_C_COPI")
				(number "50")
			)
			(pin passive line
				(at 35.56 0 180)
				(length 3.81)
				(name "GPIO_G")
				(number "51")
			)
			(pin passive line
				(at 35.56 2.54 180)
				(length 3.81)
				(name "SPARE_CS_NSS")
				(number "52")
			)
			(pin passive line
				(at 35.56 5.08 180)
				(length 3.81)
				(name "SPI_B_CS")
				(number "53")
			)
			(pin passive line
				(at 35.56 7.62 180)
				(length 3.81)
				(name "SPI_B_SCLK")
				(number "54")
			)
			(pin passive line
				(at 35.56 10.16 180)
				(length 3.81)
				(name "SPI_B_CIPO")
				(number "55")
			)
			(pin passive line
				(at 35.56 12.7 180)
				(length 3.81)
				(name "SPI_B_COPI")
				(number "56")
			)
			(pin passive line
				(at 35.56 15.24 180)
				(length 3.81)
				(name "I2C_C_SCL")
				(number "57")
			)
			(pin passive line
				(at 35.56 17.78 180)
				(length 3.81)
				(name "I2C_C_SDA")
				(number "58")
			)
			(pin passive line
				(at 35.56 20.32 180)
				(length 3.81)
				(name "I2C_B_SCL")
				(number "59")
			)
			(pin passive line
				(at -35.56 30.48 0)
				(length 3.81)
				(name "PWM_A")
				(number "6")
			)
			(pin passive line
				(at 35.56 22.86 180)
				(length 3.81)
				(name "I2C_B_SDA")
				(number "60")
			)
			(pin passive line
				(at 35.56 25.4 180)
				(length 3.81)
				(name "GPIO_F")
				(number "61")
			)
			(pin passive line
				(at 35.56 27.94 180)
				(length 3.81)
				(name "GPIO_E")
				(number "62")
			)
			(pin passive line
				(at 35.56 30.48 180)
				(length 3.81)
				(name "~{WAKE_IN}")
				(number "63")
			)
			(pin passive line
				(at 35.56 33.02 180)
				(length 3.81)
				(name "~{SLEEP_OUT}")
				(number "64")
			)
			(pin passive line
				(at 35.56 35.56 180)
				(length 3.81)
				(name "GND")
				(number "65")
			)
			(pin passive line
				(at 35.56 38.1 180)
				(length 3.81)
				(name "+3V_COIN")
				(number "66")
			)
			(pin passive line
				(at 35.56 40.64 180)
				(length 3.81)
				(name "+5V_USB_OUT")
				(number "67")
			)
			(pin passive line
				(at 35.56 43.18 180)
				(length 3.81)
				(name "+3V3_IN")
				(number "68")
			)
			(pin input line
				(at -25.4 -48.26 0)
				(length 2.54)
				(name "USART11_RX")
				(number "69")
			)
			(pin passive line
				(at -35.56 27.94 0)
				(length 3.81)
				(name "PWM_B")
				(number "7")
			)
			(pin input line
				(at -25.4 -50.8 0)
				(length 2.54)
				(name "USART11_TX")
				(number "70")
			)
			(pin input line
				(at -25.4 -53.34 0)
				(length 2.54)
				(name "USART11_CK")
				(number "71")
			)
			(pin input line
				(at -25.4 -55.88 0)
				(length 2.54)
				(name "USART12_RX")
				(number "72")
			)
			(pin input line
				(at -25.4 -58.42 0)
				(length 2.54)
				(name "USART12_TX")
				(number "73")
			)
			(pin input line
				(at -25.4 -60.96 0)
				(length 2.54)
				(name "USART12_CTS")
				(number "74")
			)
			(pin input line
				(at -25.4 -63.5 0)
				(length 2.54)
				(name "USART12_RTS")
				(number "75")
			)
			(pin input line
				(at -25.4 -66.04 0)
				(length 2.54)
				(name "USART13_RX")
				(number "76")
			)
			(pin input line
				(at -25.4 -68.58 0)
				(length 2.54)
				(name "USART13_TX")
				(number "77")
			)
			(pin input line
				(at -25.4 -71.12 0)
				(length 2.54)
				(name "USART13_CK")
				(number "78")
			)
			(pin input line
				(at -25.4 -73.66 0)
				(length 2.54)
				(name "UART14_RX")
				(number "79")
			)
			(pin passive line
				(at -35.56 25.4 0)
				(length 3.81)
				(name "PWM_C")
				(number "8")
			)
			(pin input line
				(at -25.4 -76.2 0)
				(length 2.54)
				(name "UART14_TX")
				(number "80")
			)
			(pin input line
				(at -25.4 -78.74 0)
				(length 2.54)
				(name "UART15_RX")
				(number "81")
			)
			(pin input line
				(at -25.4 -81.28 0)
				(length 2.54)
				(name "UART15_TX")
				(number "82")
			)
			(pin input line
				(at -25.4 -83.82 0)
				(length 2.54)
				(name "SPARE_83")
				(number "83")
			)
			(pin input line
				(at -25.4 -86.36 0)
				(length 2.54)
				(name "SPARE_84")
				(number "84")
			)
			(pin input line
				(at 25.4 -86.36 180)
				(length 2.54)
				(name "SPARE_85")
				(number "85")
			)
			(pin input line
				(at 25.4 -83.82 180)
				(length 2.54)
				(name "SPARE_86")
				(number "86")
			)
			(pin input line
				(at 25.4 -81.28 180)
				(length 2.54)
				(name "SPARE_87")
				(number "87")
			)
			(pin input line
				(at 25.4 -78.74 180)
				(length 2.54)
				(name "SPARE_88")
				(number "88")
			)
			(pin input line
				(at 25.4 -76.2 180)
				(length 2.54)
				(name "SPARE_89")
				(number "89")
			)
			(pin passive line
				(at -35.56 22.86 0)
				(length 3.81)
				(name "GPIO_A")
				(number "9")
			)
			(pin input line
				(at 25.4 -73.66 180)
				(length 2.54)
				(name "SPARE_90")
				(number "90")
			)
			(pin input line
				(at 25.4 -71.12 180)
				(length 2.54)
				(name "UART20_TX")
				(number "91")
			)
			(pin input line
				(at 25.4 -68.58 180)
				(length 2.54)
				(name "UART20_RX")
				(number "92")
			)
			(pin input line
				(at 25.4 -66.04 180)
				(length 2.54)
				(name "UART19_TX")
				(number "93")
			)
			(pin input line
				(at 25.4 -63.5 180)
				(length 2.54)
				(name "UART19_RX")
				(number "94")
			)
			(pin input line
				(at 25.4 -60.96 180)
				(length 2.54)
				(name "UART18_TX")
				(number "95")
			)
			(pin input line
				(at 25.4 -58.42 180)
				(length 2.54)
				(name "UART18_RX")
				(number "96")
			)
			(pin input line
				(at 25.4 -55.88 180)
				(length 2.54)
				(name "UART17_TX")
				(number "97")
			)
			(pin input line
				(at 25.4 -53.34 180)
				(length 2.54)
				(name "UART17_RX")
				(number "98")
			)
			(pin input line
				(at 25.4 -50.8 180)
				(length 2.54)
				(name "UART16_TX")
				(number "99")
			)
		)
	)
	(symbol "Si7113DN"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "Q"
			(at 6.35 1.27 0)
		)
		(property "Value" "Si7113DN"
			(at 10.16 -1.27 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "Si7113DN_1_1"
			(pin bidirectional line
				(at 3.81 -3.81 90)
				(length 1.27)
				(name "S")
				(number "1")
			)
			(pin bidirectional line
				(at 1.27 -3.81 90)
				(length 1.27)
				(name "S")
				(number "2")
			)
			(pin bidirectional line
				(at 2.54 -3.81 90)
				(length 1.27)
				(name "S")
				(number "3")
			)
			(pin bidirectional line
				(at -3.81 0 0)
				(length 1.27)
				(name "G")
				(number "4")
			)
			(pin bidirectional line
				(at 0 6.35 270)
				(length 1.27)
				(name "D")
				(number "5")
			)
			(pin bidirectional line
				(at 1.27 6.35 270)
				(length 1.27)
				(name "D")
				(number "5")
			)
			(pin bidirectional line
				(at 2.54 6.35 270)
				(length 1.27)
				(name "D")
				(number "5")
			)
			(pin bidirectional line
				(at 3.81 6.35 270)
				(length 1.27)
				(name "D")
				(number "5")
			)
		)
	)
	(symbol "Si7137DP"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 -12.7 0)
		)
		(property "Value" "Si7137DP"
			(at 0 -10.16 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "Si7137DP_1_1"
			(pin passive line
				(at -1.27 5.08 270)
				(length 1.27)
				(name "S")
				(number "1")
			)
			(pin bidirectional line
				(at 0 5.08 270)
				(length 1.27)
				(name "S")
				(number "2")
			)
			(pin power_in line
				(at 1.27 5.08 270)
				(length 1.27)
				(name "S")
				(number "3")
			)
			(pin passive line
				(at -6.35 1.27 0)
				(length 1.27)
				(name "G")
				(number "4")
			)
			(pin passive line
				(at -2.54 -5.08 90)
				(length 1.27)
				(name "D")
				(number "5")
			)
			(pin power_in line
				(at -1.27 -5.08 90)
				(length 1.27)
				(name "D")
				(number "6")
			)
			(pin power_in line
				(at 0 -5.08 90)
				(length 1.27)
				(name "D")
				(number "7")
			)
			(pin power_in line
				(at 1.27 -5.08 90)
				(length 1.27)
				(name "D")
				(number "8")
			)
		)
	)
	(symbol "Si7463DP"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "Q"
			(at 2.54 0 0)
		)
		(property "Value" "Si7463DP"
			(at 6.35 3.81 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "Si7463DP_1_1"
			(pin power_out line
				(at -1.27 5.08 270)
				(length 1.27)
				(name "S")
				(number "1")
			)
			(pin power_out line
				(at 0 5.08 270)
				(length 1.27)
				(name "S")
				(number "2")
			)
			(pin power_out line
				(at 1.27 5.08 270)
				(length 1.27)
				(name "S")
				(number "3")
			)
			(pin passive line
				(at -6.35 1.27 0)
				(length 1.27)
				(name "G")
				(number "4")
			)
			(pin power_in line
				(at -2.54 -5.08 90)
				(length 1.27)
				(name "D")
				(number "5")
			)
			(pin power_in line
				(at -1.27 -5.08 90)
				(length 1.27)
				(name "D")
				(number "5")
			)
			(pin power_in line
				(at 0 -5.08 90)
				(length 1.27)
				(name "D")
				(number "5")
			)
			(pin power_in line
				(at 1.27 -5.08 90)
				(length 1.27)
				(name "D")
				(number "5")
			)
		)
	)
	(symbol "SiSA72DN"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "Q"
			(at 3.81 1.27 0)
		)
		(property "Value" "SiSA72DN"
			(at -15.24 6.35 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "SiSA72DN_1_1"
			(pin power_in line
				(at 1.27 -5.08 90)
				(length 1.27)
				(name "S")
				(number "1")
			)
			(pin bidirectional line
				(at -1.27 -5.08 90)
				(length 1.27)
				(name "S")
				(number "2")
			)
			(pin bidirectional line
				(at 0 -5.08 90)
				(length 1.27)
				(name "S")
				(number "3")
			)
			(pin passive line
				(at -6.35 -1.27 0)
				(length 1.27)
				(name "G")
				(number "4")
			)
			(pin passive line
				(at -2.54 5.08 270)
				(length 1.27)
				(name "D")
				(number "5")
			)
			(pin power_in line
				(at -1.27 5.08 270)
				(length 1.27)
				(name "D")
				(number "5")
			)
			(pin power_in line
				(at 0 5.08 270)
				(length 1.27)
				(name "D")
				(number "5")
			)
			(pin power_in line
				(at 1.27 5.08 270)
				(length 1.27)
				(name "D")
				(number "5")
			)
		)
	)
	(symbol "SparkFun_MAX3232"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 1.27 -15.24 0)
		)
		(property "Value" "SparkFun_MAX3232"
			(at 0 15.24 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "SparkFun_MAX3232_0_1")
		(symbol "SparkFun_MAX3232_1_1"
			(pin bidirectional line
				(at 7.62 11.43 180)
				(length 2.54)
				(name "T1_OUT")
				(number "1")
			)
			(pin bidirectional line
				(at 7.62 -11.43 180)
				(length 2.54)
				(name "R2_OUT")
				(number "10")
			)
			(pin bidirectional line
				(at 7.62 8.89 180)
				(length 2.54)
				(name "T2_OUT")
				(number "2")
			)
			(pin bidirectional line
				(at 7.62 6.35 180)
				(length 2.54)
				(name "R1_IN")
				(number "3")
			)
			(pin bidirectional line
				(at 7.62 3.81 180)
				(length 2.54)
				(name "R2_IN")
				(number "4")
			)
			(pin bidirectional line
				(at 7.62 1.27 180)
				(length 2.54)
				(name "3-5.5V")
				(number "5")
			)
			(pin bidirectional line
				(at 7.62 -1.27 180)
				(length 2.54)
				(name "GND")
				(number "6")
			)
			(pin bidirectional line
				(at 7.62 -3.81 180)
				(length 2.54)
				(name "T1_IN")
				(number "7")
			)
			(pin bidirectional line
				(at 7.62 -6.35 180)
				(length 2.54)
				(name "T2_IN")
				(number "8")
			)
			(pin bidirectional line
				(at 7.62 -8.89 180)
				(length 2.54)
				(name "R1_OUT")
				(number "9")
			)
		)
	)
	(symbol "TC59"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 5.08 0)
		)
		(property "Value" "TC595002"
			(at 6.35 5.08 0)
		)
		(property "Footprint" "ProjectDevices:TC59_SOT95P237X112-3N"
			(at -1.27 -8.89 0)
		)
		(property "Datasheet" "https://ww1.microchip.com/downloads/aemDocuments/documents/APID/ProductDocuments/DataSheets/21438C.pdf"
			(at 1.27 -6.35 0)
		)
		(property "Description" "Low Dropout, Negative Output Voltage Regulator, Iq=3.5uA, Vdrop 0.12 @50mA, 0.38 @100mA"
			(at -1.27 -11.43 0)
		)
		(property "PartNum" "TC595002ECBTR"
			(at -1.27 -12.7 0)
		)
		(property "VendorNum" "TC595002ECBCT-ND"
			(at 0 -13.97 0)
		)
		(property "Vendor" "Digikey"
			(at -3.81 -13.97 0)
		)
		(property "Subst" "No"
			(at 5.08 -15.24 0)
		)
		(symbol "TC59_1_1"
			(pin output line
				(at -8.89 2.54 0)
				(length 2.54)
				(name "-Vout")
				(number "1")
			)
			(pin input line
				(at -8.89 -2.54 0)
				(length 2.54)
				(name "-Vin")
				(number "2")
			)
			(pin input line
				(at 8.89 0 180)
				(length 2.54)
				(name "Vss")
				(number "3")
			)
		)
	)
	(symbol "TCA9543A"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -5.08 12.7 0)
		)
		(property "Value" "TCA9543A"
			(at 2.54 12.7 0)
		)
		(property "Footprint" "ProjectFootprints:tca9543a_SOP65P640X120-14N"
			(at 2.54 -11.43 0)
		)
		(property "Datasheet" ""
			(at 8.89 -7.62 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "TCA9543A_0_1")
		(symbol "TCA9543A_1_1"
			(pin input line
				(at -10.16 8.89 0)
				(length 2.54)
				(name "A0")
				(number "1")
			)
			(pin bidirectional line
				(at 10.16 -1.27 180)
				(length 2.54)
				(name "SC1")
				(number "10")
			)
			(pin output line
				(at 10.16 1.27 180)
				(length 2.54)
				(name "~{INT}")
				(number "11")
			)
			(pin bidirectional line
				(at 10.16 3.81 180)
				(length 2.54)
				(name "SCL")
				(number "12")
			)
			(pin bidirectional line
				(at 10.16 6.35 180)
				(length 2.54)
				(name "SDA")
				(number "13")
			)
			(pin power_in line
				(at 10.16 8.89 180)
				(length 2.54)
				(name "VCC")
				(number "14")
			)
			(pin input line
				(at -10.16 6.35 0)
				(length 2.54)
				(name "A1")
				(number "2")
			)
			(pin input line
				(at -10.16 3.81 0)
				(length 2.54)
				(name "~{RST}")
				(number "3")
			)
			(pin input line
				(at -10.16 1.27 0)
				(length 2.54)
				(name "~{INT0}")
				(number "4")
			)
			(pin bidirectional line
				(at -10.16 -1.27 0)
				(length 2.54)
				(name "SD0")
				(number "5")
			)
			(pin bidirectional line
				(at -10.16 -3.81 0)
				(length 2.54)
				(name "SC0")
				(number "6")
			)
			(pin power_in line
				(at -10.16 -6.35 0)
				(length 2.54)
				(name "GND")
				(number "7")
			)
			(pin input line
				(at 10.16 -6.35 180)
				(length 2.54)
				(name "~{INT1}")
				(number "8")
			)
			(pin bidirectional line
				(at 10.16 -3.81 180)
				(length 2.54)
				(name "SD1")
				(number "9")
			)
		)
	)
	(symbol "TEENSY3.6_Min"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 20.32 57.15 0)
		)
		(property "Value" "TEENSY3.6_Min"
			(at -10.16 57.15 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "TEENSY3.6_Min_1_1"
			(pin power_in line
				(at -24.13 53.34 0)
				(length 5.08)
				(name "GND")
				(number "1")
			)
			(pin bidirectional line
				(at -24.13 30.48 0)
				(length 5.08)
				(name "8_TX3_miso0_sda0")
				(number "10")
			)
			(pin bidirectional line
				(at -24.13 27.94 0)
				(length 5.08)
				(name "9_PWM_RX2_CS0")
				(number "11")
			)
			(pin bidirectional line
				(at -24.13 25.4 0)
				(length 5.08)
				(name "10_PWM_TX2_CS0")
				(number "12")
			)
			(pin bidirectional line
				(at -24.13 22.86 0)
				(length 5.08)
				(name "11_MOSI0")
				(number "13")
			)
			(pin bidirectional line
				(at -24.13 20.32 0)
				(length 5.08)
				(name "12_MISO0")
				(number "14")
			)
			(pin power_in line
				(at -24.13 17.78 0)
				(length 5.08)
				(name "3.3V")
				(number "15")
			)
			(pin bidirectional line
				(at -24.13 15.24 0)
				(length 5.08)
				(name "24")
				(number "16")
			)
			(pin bidirectional line
				(at -24.13 12.7 0)
				(length 5.08)
				(name "25")
				(number "17")
			)
			(pin bidirectional line
				(at -24.13 10.16 0)
				(length 5.08)
				(name "26_tx1")
				(number "18")
			)
			(pin bidirectional line
				(at -24.13 7.62 0)
				(length 5.08)
				(name "27_rx1")
				(number "19")
			)
			(pin bidirectional line
				(at -24.13 50.8 0)
				(length 5.08)
				(name "0_RX1_MOSI1_Touch")
				(number "2")
			)
			(pin bidirectional line
				(at -24.13 5.08 0)
				(length 5.08)
				(name "28")
				(number "20")
			)
			(pin bidirectional line
				(at -24.13 2.54 0)
				(length 5.08)
				(name "29_PWM_can0tx_Touch")
				(number "21")
			)
			(pin bidirectional line
				(at -24.13 0 0)
				(length 5.08)
				(name "30_PWM_can0rx_Touch")
				(number "22")
			)
			(pin bidirectional line
				(at -24.13 -2.54 0)
				(length 5.08)
				(name "31_A12_RX4_CS1")
				(number "23")
			)
			(pin bidirectional line
				(at -24.13 -5.08 0)
				(length 5.08)
				(name "32_A13_TX4_SCK1")
				(number "24")
			)
			(pin power_in line
				(at -24.13 -7.62 0)
				(length 5.08)
				(name "VBat")
				(number "25")
			)
			(pin power_in line
				(at -24.13 -10.16 0)
				(length 5.08)
				(name "3.3V")
				(number "26")
			)
			(pin power_in line
				(at -24.13 -12.7 0)
				(length 5.08)
				(name "GND")
				(number "27")
			)
			(pin input line
				(at -24.13 -15.24 0)
				(length 5.08)
				(name "Program")
				(number "28")
			)
			(pin input line
				(at -24.13 -17.78 0)
				(length 5.08)
				(name "Reset")
				(number "29")
			)
			(pin bidirectional line
				(at -24.13 48.26 0)
				(length 5.08)
				(name "1_TX1_MISO1_Touch")
				(number "3")
			)
			(pin bidirectional line
				(at -24.13 -20.32 0)
				(length 5.08)
				(name "33_A14_CAN1TX_scl0")
				(number "30")
			)
			(pin bidirectional line
				(at -24.13 -22.86 0)
				(length 5.08)
				(name "34_A15_CAN1TX_sda0")
				(number "31")
			)
			(pin bidirectional line
				(at -24.13 -25.4 0)
				(length 5.08)
				(name "35_A16_PWM")
				(number "32")
			)
			(pin bidirectional line
				(at -24.13 -27.94 0)
				(length 5.08)
				(name "36_A17_PWM")
				(number "33")
			)
			(pin bidirectional line
				(at -24.13 -30.48 0)
				(length 5.08)
				(name "37_A18_PWM_SCL1")
				(number "34")
			)
			(pin bidirectional line
				(at -24.13 -33.02 0)
				(length 5.08)
				(name "38_A19_PWM_SDA1")
				(number "35")
			)
			(pin bidirectional line
				(at -24.13 -35.56 0)
				(length 5.08)
				(name "39_A20")
				(number "36")
			)
			(pin bidirectional line
				(at -24.13 -38.1 0)
				(length 5.08)
				(name "A21_DAC0")
				(number "37")
			)
			(pin bidirectional line
				(at -24.13 -40.64 0)
				(length 5.08)
				(name "A22_DAC1")
				(number "38")
			)
			(pin power_in line
				(at -24.13 -43.18 0)
				(length 5.08)
				(name "GND")
				(number "39")
			)
			(pin bidirectional line
				(at -24.13 45.72 0)
				(length 5.08)
				(name "2_PWM")
				(number "4")
			)
			(pin bidirectional line
				(at -24.13 -45.72 0)
				(length 5.08)
				(name "13_SCK0_LED")
				(number "40")
			)
			(pin bidirectional line
				(at -24.13 -48.26 0)
				(length 5.08)
				(name "14_A0_PWM_sck0")
				(number "41")
			)
			(pin bidirectional line
				(at -24.13 -50.8 0)
				(length 5.08)
				(name "15_A1_CS0_Touch")
				(number "42")
			)
			(pin bidirectional line
				(at -24.13 -53.34 0)
				(length 5.08)
				(name "16_A2_scl0_Touch")
				(number "43")
			)
			(pin bidirectional line
				(at 26.67 -53.34 180)
				(length 5.08)
				(name "17_A3_sda0_Touch")
				(number "44")
			)
			(pin bidirectional line
				(at 26.67 -50.8 180)
				(length 5.08)
				(name "18_A4_SDA0_Touch")
				(number "45")
			)
			(pin bidirectional line
				(at 26.67 -48.26 180)
				(length 5.08)
				(name "19_A5_SCL0_Touch")
				(number "46")
			)
			(pin bidirectional line
				(at 26.67 -45.72 180)
				(length 5.08)
				(name "20_A6_PWM_CS0_sck1")
				(number "47")
			)
			(pin bidirectional line
				(at 26.67 -43.18 180)
				(length 5.08)
				(name "21_A7_PWM_CS0_sck1")
				(number "48")
			)
			(pin bidirectional line
				(at 26.67 -40.64 180)
				(length 5.08)
				(name "22_A8_PWM_Touch")
				(number "49")
			)
			(pin bidirectional line
				(at -24.13 43.18 0)
				(length 5.08)
				(name "3_PWM_CAN0TX_SCL2")
				(number "5")
			)
			(pin bidirectional line
				(at 26.67 -38.1 180)
				(length 5.08)
				(name "23_A9_PWM_Touch")
				(number "50")
			)
			(pin power_out line
				(at 26.67 -35.56 180)
				(length 5.08)
				(name "3.3V_max250mA")
				(number "51")
			)
			(pin power_out line
				(at 26.67 -33.02 180)
				(length 5.08)
				(name "AGND")
				(number "52")
			)
			(pin power_in line
				(at 26.67 -30.48 180)
				(length 5.08)
				(name "Vin")
				(number "53")
			)
			(pin bidirectional line
				(at -24.13 40.64 0)
				(length 5.08)
				(name "4_PWM_CAN0RX_SDA2")
				(number "6")
			)
			(pin bidirectional line
				(at -24.13 38.1 0)
				(length 5.08)
				(name "5_PWM_tx1_miso1")
				(number "7")
			)
			(pin bidirectional line
				(at -24.13 35.56 0)
				(length 5.08)
				(name "6_PWM")
				(number "8")
			)
			(pin bidirectional line
				(at -24.13 33.02 0)
				(length 5.08)
				(name "7_RX3_miso0_scl0")
				(number "9")
			)
		)
	)
	(symbol "TLV803EC29DCKR"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 10.16 0)
		)
		(property "Value" "TLV803EC"
			(at 0 7.62 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-323_SC-70"
			(at 0 -7.62 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/tlv803e.pdf"
			(at 0 -10.16 0)
		)
		(property "Description" "Voltage Sup, 10ms reset lo, 2.93v"
			(at 0 0 0)
		)
		(symbol "TLV803EC29DCKR_1_1"
			(pin power_in line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "GND")
				(number "1")
			)
			(pin output line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "~{RST}")
				(number "2")
			)
			(pin output line
				(at 7.62 0 180)
				(length 2.54)
				(name "VDD")
				(number "3")
			)
		)
	)
	(symbol "TLV809EC"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -2.54 8.89 0)
		)
		(property "Value" "TLV809EC"
			(at 0 6.35 0)
		)
		(property "Footprint" ""
			(at 1.27 0 0)
		)
		(property "Datasheet" ""
			(at 1.27 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "TLV809EC_0_1")
		(symbol "TLV809EC_1_1"
			(pin output line
				(at -8.89 2.54 0)
				(length 2.54)
				(name "~{RESET}")
				(number "1")
			)
			(pin power_in line
				(at -8.89 0 0)
				(length 2.54)
				(name "VDD")
				(number "2")
			)
			(pin power_in line
				(at -8.89 -2.54 0)
				(length 2.54)
				(name "GND")
				(number "3")
			)
			(pin input line
				(at 8.89 -2.54 180)
				(length 2.54)
				(name "~{MR}")
				(number "4")
			)
			(pin bidirectional line
				(at 8.89 2.54 180)
				(length 2.54)
				(name "CT")
				(number "5")
			)
		)
	)
	(symbol "TLV840"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -1.27 8.89 0)
		)
		(property "Value" "TLV840"
			(at -1.27 6.35 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "TLV840_0_1")
		(symbol "TLV840_1_1"
			(pin output line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "~{RESET}")
				(number "1")
			)
			(pin power_in line
				(at -7.62 0 0)
				(length 2.54)
				(name "VDD")
				(number "2")
			)
			(pin power_in line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "GND")
				(number "3")
			)
			(pin input line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "CT")
				(number "4")
			)
			(pin input line
				(at 7.62 -2.54 180)
				(length 2.54)
				(name "~{MR}")
				(number "5")
			)
		)
	)
	(symbol "TLVM23615RDNR"
		(pin_names
			(offset 0.254)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 10.16 0)
		)
		(property "Value" "TLVM23615RDNR"
			(at -19.05 12.7 0)
		)
		(property "Footprint" "ProjectFootprints:TLVM23615_QFN-FCMOD11_RDN_TEX"
			(at -16.51 5.08 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/tlvm23615.pdf"
			(at -16.51 5.08 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "TLVM23615RDNR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN-FCMOD11_RDN_TEX"
			(at 0 0 0)
		)
		(symbol "TLVM23615RDNR_0_1"
			(pin unspecified line
				(at -11.43 2.54 0)
				(length 2.54)
				(name "PGOOD")
				(number "1")
			)
			(pin power_out line
				(at 0 8.89 270)
				(length 2.54)
				(name "GND")
				(number "10")
			)
			(pin unspecified line
				(at -3.81 8.89 270)
				(length 2.54)
				(name "RT")
				(number "11")
			)
			(pin unspecified line
				(at -11.43 0 0)
				(length 2.54)
				(name "EN")
				(number "2")
			)
			(pin power_in line
				(at -11.43 -2.54 0)
				(length 2.54)
				(name "VIN")
				(number "3")
			)
			(pin power_in line
				(at -11.43 -6.35 0)
				(length 2.54)
				(name "VOUT")
				(number "4")
			)
			(pin no_connect line
				(at 11.43 -6.35 180)
				(length 2.54)
				(name "SW")
				(number "5")
			)
			(pin no_connect line
				(at 11.43 -2.54 180)
				(length 2.54)
				(name "SW")
				(number "6")
			)
			(pin power_in line
				(at 11.43 0 180)
				(length 2.54)
				(name "BOOT")
				(number "7")
			)
			(pin power_in line
				(at 11.43 2.54 180)
				(length 2.54)
				(name "VCC")
				(number "8")
			)
			(pin unspecified line
				(at 3.81 8.89 270)
				(length 2.54)
				(name "FB")
				(number "9")
			)
		)
		(symbol "TLVM23615RDNR_1_1")
	)
	(symbol "TM4C123GH6PM"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 29.21 38.1 0)
		)
		(property "Value" "TM4C123GH6PM"
			(at 29.21 35.56 0)
		)
		(property "Footprint" ""
			(at -16.51 -13.97 0)
		)
		(property "Datasheet" ""
			(at -16.51 -13.97 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "TM4C123GH6PM_0_1")
		(symbol "TM4C123GH6PM_1_1"
			(pin bidirectional line
				(at -39.37 19.05 0)
				(length 3.81)
				(name "PB6_M0PWM0")
				(number "1")
			)
			(pin bidirectional line
				(at -39.37 -3.81 0)
				(length 3.81)
				(name "PD7_UART2_TX")
				(number "10")
			)
			(pin power_in line
				(at -39.37 -6.35 0)
				(length 3.81)
				(name "VDD")
				(number "11")
			)
			(pin power_in line
				(at -39.37 -8.89 0)
				(length 3.81)
				(name "GND")
				(number "12")
			)
			(pin bidirectional line
				(at -39.37 -11.43 0)
				(length 3.81)
				(name "PC7_UART3_TX")
				(number "13")
			)
			(pin bidirectional line
				(at -39.37 -13.97 0)
				(length 3.81)
				(name "PC6_UART3_RX")
				(number "14")
			)
			(pin bidirectional line
				(at -39.37 -16.51 0)
				(length 3.81)
				(name "PC5_UART1_TX")
				(number "15")
			)
			(pin bidirectional line
				(at -39.37 -19.05 0)
				(length 3.81)
				(name "PC4_UART1_RX")
				(number "16")
			)
			(pin bidirectional line
				(at -19.05 -36.83 90)
				(length 3.81)
				(name "PA0_UART0_RX")
				(number "17")
			)
			(pin bidirectional line
				(at -16.51 -36.83 90)
				(length 3.81)
				(name "PA1_UART0_TX")
				(number "18")
			)
			(pin bidirectional line
				(at -13.97 -36.83 90)
				(length 3.81)
				(name "PA2_SSI0CLK")
				(number "19")
			)
			(pin power_in line
				(at -39.37 16.51 0)
				(length 3.81)
				(name "VDDA")
				(number "2")
			)
			(pin bidirectional line
				(at -11.43 -36.83 90)
				(length 3.81)
				(name "PA3_SSI0FSS")
				(number "20")
			)
			(pin bidirectional line
				(at -8.89 -36.83 90)
				(length 3.81)
				(name "PA4_SSI0RX")
				(number "21")
			)
			(pin bidirectional line
				(at -6.35 -36.83 90)
				(length 3.81)
				(name "PA5_SSI0TX")
				(number "22")
			)
			(pin bidirectional line
				(at -3.81 -36.83 90)
				(length 3.81)
				(name "PA6_I2C1_SCL")
				(number "23")
			)
			(pin bidirectional line
				(at -1.27 -36.83 90)
				(length 3.81)
				(name "PA7_I2C1_SDA")
				(number "24")
			)
			(pin power_in line
				(at 1.27 -36.83 90)
				(length 3.81)
				(name "VDDC")
				(number "25")
			)
			(pin power_in line
				(at 3.81 -36.83 90)
				(length 3.81)
				(name "VDD")
				(number "26")
			)
			(pin power_in line
				(at 6.35 -36.83 90)
				(length 3.81)
				(name "GND")
				(number "27")
			)
			(pin bidirectional line
				(at 8.89 -36.83 90)
				(length 3.81)
				(name "PF0_UART1_RTS")
				(number "28")
			)
			(pin bidirectional line
				(at 11.43 -36.83 90)
				(length 3.81)
				(name "PF1_UART1_CTS")
				(number "29")
			)
			(pin power_in line
				(at -39.37 13.97 0)
				(length 3.81)
				(name "GNDA")
				(number "3")
			)
			(pin bidirectional line
				(at 13.97 -36.83 90)
				(length 3.81)
				(name "PF2_SSI1CLK")
				(number "30")
			)
			(pin bidirectional line
				(at 16.51 -36.83 90)
				(length 3.81)
				(name "PF3_SSI1FSS")
				(number "31")
			)
			(pin input line
				(at 19.05 -36.83 90)
				(length 3.81)
				(name "~{WAKE}")
				(number "32")
			)
			(pin open_collector line
				(at 40.64 -19.05 180)
				(length 3.81)
				(name "~{HIB}")
				(number "33")
			)
			(pin passive line
				(at 40.64 -16.51 180)
				(length 3.81)
				(name "XOSC0")
				(number "34")
			)
			(pin power_in line
				(at 40.64 -13.97 180)
				(length 3.81)
				(name "GNDX")
				(number "35")
			)
			(pin passive line
				(at 40.64 -11.43 180)
				(length 3.81)
				(name "XOSC1")
				(number "36")
			)
			(pin passive line
				(at 40.64 -8.89 180)
				(length 3.81)
				(name "VBAT")
				(number "37")
			)
			(pin input line
				(at 40.64 -6.35 180)
				(length 3.81)
				(name "~{RST}")
				(number "38")
			)
			(pin bidirectional line
				(at 40.64 -3.81 180)
				(length 3.81)
				(name "GND")
				(number "39")
			)
			(pin bidirectional line
				(at -39.37 11.43 0)
				(length 3.81)
				(name "PB7_M0PWM1")
				(number "4")
			)
			(pin passive line
				(at 40.64 -1.27 180)
				(length 3.81)
				(name "OSC0")
				(number "40")
			)
			(pin passive line
				(at 40.64 1.27 180)
				(length 3.81)
				(name "OSC1")
				(number "41")
			)
			(pin power_in line
				(at 40.64 3.81 180)
				(length 3.81)
				(name "VDD")
				(number "42")
			)
			(pin bidirectional line
				(at 40.64 6.35 180)
				(length 3.81)
				(name "PD4_USB0DM")
				(number "43")
			)
			(pin bidirectional line
				(at 40.64 8.89 180)
				(length 3.81)
				(name "PD5_USB0DP")
				(number "44")
			)
			(pin bidirectional line
				(at 40.64 11.43 180)
				(length 3.81)
				(name "PB0_USB0ID")
				(number "45")
			)
			(pin bidirectional line
				(at 40.64 13.97 180)
				(length 3.81)
				(name "PB1_USB0VBUS")
				(number "46")
			)
			(pin bidirectional line
				(at 40.64 16.51 180)
				(length 3.81)
				(name "PB2_I2C0SCL")
				(number "47")
			)
			(pin bidirectional line
				(at 40.64 19.05 180)
				(length 3.81)
				(name "PB3_I2C0SDA")
				(number "48")
			)
			(pin bidirectional line
				(at 19.05 38.1 270)
				(length 3.81)
				(name "PC3_JTAG_TDO")
				(number "49")
			)
			(pin bidirectional line
				(at -39.37 8.89 0)
				(length 3.81)
				(name "PF4_T2CCP0")
				(number "5")
			)
			(pin bidirectional line
				(at 16.51 38.1 270)
				(length 3.81)
				(name "PC2_JTAG_TDI")
				(number "50")
			)
			(pin bidirectional line
				(at 13.97 38.1 270)
				(length 3.81)
				(name "PC1_TMS_SWDIO")
				(number "51")
			)
			(pin bidirectional line
				(at 11.43 38.1 270)
				(length 3.81)
				(name "PC0_TCK_SWCLK")
				(number "52")
			)
			(pin bidirectional line
				(at 8.89 38.1 270)
				(length 3.81)
				(name "PD6_UART2_RX")
				(number "53")
			)
			(pin power_in line
				(at 6.35 38.1 270)
				(length 3.81)
				(name "VDD")
				(number "54")
			)
			(pin power_in line
				(at 3.81 38.1 270)
				(length 3.81)
				(name "GND")
				(number "55")
			)
			(pin power_in line
				(at 1.27 38.1 270)
				(length 3.81)
				(name "VDDC")
				(number "56")
			)
			(pin bidirectional line
				(at -1.27 38.1 270)
				(length 3.81)
				(name "PB5_CAN0_TX")
				(number "57")
			)
			(pin bidirectional line
				(at -3.81 38.1 270)
				(length 3.81)
				(name "PB4_CAN0_RX")
				(number "58")
			)
			(pin bidirectional line
				(at -6.35 38.1 270)
				(length 3.81)
				(name "PE4_UART5_RX")
				(number "59")
			)
			(pin bidirectional line
				(at -39.37 6.35 0)
				(length 3.81)
				(name "PE3_AIN0")
				(number "6")
			)
			(pin bidirectional line
				(at -8.89 38.1 270)
				(length 3.81)
				(name "PE5_UART5_TX")
				(number "60")
			)
			(pin bidirectional line
				(at -11.43 38.1 270)
				(length 3.81)
				(name "PD0_AIN7_SSI3CLK")
				(number "61")
			)
			(pin bidirectional line
				(at -13.97 38.1 270)
				(length 3.81)
				(name "PD1_AIN6_SSI3FSS")
				(number "62")
			)
			(pin bidirectional line
				(at -16.51 38.1 270)
				(length 3.81)
				(name "PD2_SSI1RX")
				(number "63")
			)
			(pin bidirectional line
				(at -19.05 38.1 270)
				(length 3.81)
				(name "PD3_SSI1TX")
				(number "64")
			)
			(pin bidirectional line
				(at -39.37 3.81 0)
				(length 3.81)
				(name "PE2_AIN1")
				(number "7")
			)
			(pin bidirectional line
				(at -39.37 1.27 0)
				(length 3.81)
				(name "PE1_UART7_TX")
				(number "8")
			)
			(pin bidirectional line
				(at -39.37 -1.27 0)
				(length 3.81)
				(name "PE0_UART7_RX")
				(number "9")
			)
		)
	)
	(symbol "TM4C123GH6PZ"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 36.83 40.64 0)
		)
		(property "Value" "TM4C123GH6PZ"
			(at 0 -2.54 0)
		)
		(property "Footprint" "ProjectFootprints:TM4C123g_TIVA_QFP50P1600X1600X160-100N"
			(at 3.556 -20.32 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/tm4c1231h6pz.pdf"
			(at -1.27 -5.08 0)
		)
		(property "Description" "Tiva 100pin Cortex M4F 80MHz"
			(at 0 0 0)
		)
		(symbol "TM4C123GH6PZ_1_1"
			(pin bidirectional line
				(at -44.45 29.21 0)
				(length 3.81)
				(name "PD0_AIN15")
				(number "1")
			)
			(pin power_in line
				(at -44.45 6.35 0)
				(length 3.81)
				(name "GNDA")
				(number "10")
			)
			(pin bidirectional line
				(at -29.21 43.18 270)
				(length 3.81)
				(name "PD7_AIN4")
				(number "100")
			)
			(pin bidirectional line
				(at -44.45 3.81 0)
				(length 3.81)
				(name "PJ2_U5RX")
				(number "11")
			)
			(pin bidirectional line
				(at -44.45 1.27 0)
				(length 3.81)
				(name "PE3_GP_AIN0")
				(number "12")
			)
			(pin bidirectional line
				(at -44.45 -1.27 0)
				(length 3.81)
				(name "PE2_GP_AIN1")
				(number "13")
			)
			(pin bidirectional line
				(at -44.45 -3.81 0)
				(length 3.81)
				(name "PE1_U7TX")
				(number "14")
			)
			(pin bidirectional line
				(at -44.45 -6.35 0)
				(length 3.81)
				(name "PE0_U7RX")
				(number "15")
			)
			(pin bidirectional line
				(at -44.45 -8.89 0)
				(length 3.81)
				(name "PH0_GP_AIN16")
				(number "16")
			)
			(pin bidirectional line
				(at -44.45 -11.43 0)
				(length 3.81)
				(name "PH1_GP_AIN17")
				(number "17")
			)
			(pin bidirectional line
				(at -44.45 -13.97 0)
				(length 3.81)
				(name "PH2_GP_AIN18")
				(number "18")
			)
			(pin bidirectional line
				(at -44.45 -16.51 0)
				(length 3.81)
				(name "PH3_GP_AIN19")
				(number "19")
			)
			(pin bidirectional line
				(at -44.45 26.67 0)
				(length 3.81)
				(name "PD1_GP_AIN14")
				(number "2")
			)
			(pin power_in line
				(at -44.45 -19.05 0)
				(length 3.81)
				(name "VDD")
				(number "20")
			)
			(pin power_in line
				(at -44.45 -21.59 0)
				(length 3.81)
				(name "GND")
				(number "21")
			)
			(pin bidirectional line
				(at -44.45 -24.13 0)
				(length 3.81)
				(name "PC7_U3TX")
				(number "22")
			)
			(pin bidirectional line
				(at -44.45 -26.67 0)
				(length 3.81)
				(name "PC6_U3RX")
				(number "23")
			)
			(pin bidirectional line
				(at -44.45 -29.21 0)
				(length 3.81)
				(name "PC5_U4TX")
				(number "24")
			)
			(pin bidirectional line
				(at -44.45 -31.75 0)
				(length 3.81)
				(name "PC4_U4RX")
				(number "25")
			)
			(pin bidirectional line
				(at -29.21 -46.99 90)
				(length 3.81)
				(name "PA0_U0RX")
				(number "26")
			)
			(pin bidirectional line
				(at -26.67 -46.99 90)
				(length 3.81)
				(name "PA1_U0TX")
				(number "27")
			)
			(pin bidirectional line
				(at -24.13 -46.99 90)
				(length 3.81)
				(name "PA2_SSI0CLK")
				(number "28")
			)
			(pin bidirectional line
				(at -21.59 -46.99 90)
				(length 3.81)
				(name "PA3_SSI0FSS")
				(number "29")
			)
			(pin bidirectional line
				(at -44.45 24.13 0)
				(length 3.81)
				(name "PD2_GP_AIN13")
				(number "3")
			)
			(pin bidirectional line
				(at -19.05 -46.99 90)
				(length 3.81)
				(name "PA4_SSI0RX")
				(number "30")
			)
			(pin bidirectional line
				(at -16.51 -46.99 90)
				(length 3.81)
				(name "PA5_SSI0TX")
				(number "31")
			)
			(pin power_in line
				(at -13.97 -46.99 90)
				(length 3.81)
				(name "VDD")
				(number "32")
			)
			(pin power_in line
				(at -11.43 -46.99 90)
				(length 3.81)
				(name "GND")
				(number "33")
			)
			(pin bidirectional line
				(at -8.89 -46.99 90)
				(length 3.81)
				(name "PA6_I2C1SCL")
				(number "34")
			)
			(pin bidirectional line
				(at -6.35 -46.99 90)
				(length 3.81)
				(name "PA7_I2C1SDA")
				(number "35")
			)
			(pin bidirectional line
				(at -3.81 -46.99 90)
				(length 3.81)
				(name "PF6_GP_PF6")
				(number "36")
			)
			(pin bidirectional line
				(at -1.27 -46.99 90)
				(length 3.81)
				(name "PF5_GP_USB0PFLT")
				(number "37")
			)
			(pin power_in line
				(at 1.27 -46.99 90)
				(length 3.81)
				(name "VDD")
				(number "38")
			)
			(pin bidirectional line
				(at 3.81 -46.99 90)
				(length 3.81)
				(name "PF4_GP_USB0EPEN")
				(number "39")
			)
			(pin bidirectional line
				(at -44.45 21.59 0)
				(length 3.81)
				(name "PD3_GP_AIN12")
				(number "4")
			)
			(pin bidirectional line
				(at 6.35 -46.99 90)
				(length 3.81)
				(name "PF0_SSI1RX")
				(number "40")
			)
			(pin bidirectional line
				(at 8.89 -46.99 90)
				(length 3.81)
				(name "PF1_SSI1TX")
				(number "41")
			)
			(pin bidirectional line
				(at 11.43 -46.99 90)
				(length 3.81)
				(name "PF2_SSI1CLK")
				(number "42")
			)
			(pin bidirectional line
				(at 13.97 -46.99 90)
				(length 3.81)
				(name "PF3_SSI1FSS")
				(number "43")
			)
			(pin power_in line
				(at 16.51 -46.99 90)
				(length 3.81)
				(name "VDD")
				(number "44")
			)
			(pin power_in line
				(at 19.05 -46.99 90)
				(length 3.81)
				(name "GND")
				(number "45")
			)
			(pin bidirectional line
				(at 21.59 -46.99 90)
				(length 3.81)
				(name "PK3_SSI3TX")
				(number "46")
			)
			(pin bidirectional line
				(at 24.13 -46.99 90)
				(length 3.81)
				(name "PK2_SSI3RX")
				(number "47")
			)
			(pin bidirectional line
				(at 26.67 -46.99 90)
				(length 3.81)
				(name "PK1_SSI3FSS")
				(number "48")
			)
			(pin bidirectional line
				(at 29.21 -46.99 90)
				(length 3.81)
				(name "PK0_SSI3CLK")
				(number "49")
			)
			(pin power_in line
				(at -44.45 19.05 0)
				(length 3.81)
				(name "VDD")
				(number "5")
			)
			(pin input line
				(at 46.99 -34.29 180)
				(length 3.81)
				(name "~{WAKE}")
				(number "50")
			)
			(pin output line
				(at 46.99 -31.75 180)
				(length 3.81)
				(name "~{HIB}")
				(number "51")
			)
			(pin input line
				(at 46.99 -29.21 180)
				(length 3.81)
				(name "XOSC0")
				(number "52")
			)
			(pin power_in line
				(at 46.99 -26.67 180)
				(length 3.81)
				(name "GNDX")
				(number "53")
			)
			(pin output line
				(at 46.99 -24.13 180)
				(length 3.81)
				(name "XOSC1")
				(number "54")
			)
			(pin power_in line
				(at 46.99 -21.59 180)
				(length 3.81)
				(name "VBAT")
				(number "55")
			)
			(pin power_in line
				(at 46.99 -19.05 180)
				(length 3.81)
				(name "VDD")
				(number "56")
			)
			(pin power_in line
				(at 46.99 -16.51 180)
				(length 3.81)
				(name "GND")
				(number "57")
			)
			(pin bidirectional line
				(at 46.99 -13.97 180)
				(length 3.81)
				(name "PF7_GP")
				(number "58")
			)
			(pin bidirectional line
				(at 46.99 -11.43 180)
				(length 3.81)
				(name "PG3_GP")
				(number "59")
			)
			(pin power_in line
				(at -44.45 16.51 0)
				(length 3.81)
				(name "GND")
				(number "6")
			)
			(pin bidirectional line
				(at 46.99 -8.89 180)
				(length 3.81)
				(name "PG2_GP")
				(number "60")
			)
			(pin bidirectional line
				(at 46.99 -6.35 180)
				(length 3.81)
				(name "PG1_GP")
				(number "61")
			)
			(pin bidirectional line
				(at 46.99 -3.81 180)
				(length 3.81)
				(name "PG0_GP")
				(number "62")
			)
			(pin input line
				(at 46.99 -1.27 180)
				(length 3.81)
				(name "~{RST}")
				(number "63")
			)
			(pin power_in line
				(at 46.99 1.27 180)
				(length 3.81)
				(name "GND")
				(number "64")
			)
			(pin input line
				(at 46.99 3.81 180)
				(length 3.81)
				(name "OSC0")
				(number "65")
			)
			(pin output line
				(at 46.99 6.35 180)
				(length 3.81)
				(name "OSC1")
				(number "66")
			)
			(pin power_in line
				(at 46.99 8.89 180)
				(length 3.81)
				(name "VDD")
				(number "67")
			)
			(pin bidirectional line
				(at 46.99 11.43 180)
				(length 3.81)
				(name "PJ0_GP_USB0DM")
				(number "68")
			)
			(pin bidirectional line
				(at 46.99 13.97 180)
				(length 3.81)
				(name "PJ1_GP_USB0DP")
				(number "69")
			)
			(pin power_in line
				(at -44.45 13.97 0)
				(length 3.81)
				(name "VDDA")
				(number "7")
			)
			(pin bidirectional line
				(at 46.99 16.51 180)
				(length 3.81)
				(name "PB0_U1RX")
				(number "70")
			)
			(pin bidirectional line
				(at 46.99 19.05 180)
				(length 3.81)
				(name "PB1_U1TX")
				(number "71")
			)
			(pin bidirectional line
				(at 46.99 21.59 180)
				(length 3.81)
				(name "PB2_I2C0SCL")
				(number "72")
			)
			(pin bidirectional line
				(at 46.99 24.13 180)
				(length 3.81)
				(name "PB3_I2C0SDA")
				(number "73")
			)
			(pin bidirectional line
				(at 46.99 26.67 180)
				(length 3.81)
				(name "PG4_U2RX")
				(number "74")
			)
			(pin bidirectional line
				(at 46.99 29.21 180)
				(length 3.81)
				(name "PG5_U2TX")
				(number "75")
			)
			(pin bidirectional line
				(at 31.75 43.18 270)
				(length 3.81)
				(name "PH7_SSI2TX")
				(number "76")
			)
			(pin bidirectional line
				(at 29.21 43.18 270)
				(length 3.81)
				(name "PH6_SSI2RX")
				(number "77")
			)
			(pin bidirectional line
				(at 26.67 43.18 270)
				(length 3.81)
				(name "PH5_SSI2FSS")
				(number "78")
			)
			(pin bidirectional line
				(at 24.13 43.18 270)
				(length 3.81)
				(name "PH4_SSI2CLK")
				(number "79")
			)
			(pin power_in line
				(at -44.45 11.43 0)
				(length 3.81)
				(name "VREF+")
				(number "8")
			)
			(pin power_in line
				(at 21.59 43.18 270)
				(length 3.81)
				(name "VDD")
				(number "80")
			)
			(pin power_in line
				(at 19.05 43.18 270)
				(length 3.81)
				(name "GND")
				(number "81")
			)
			(pin bidirectional line
				(at 16.51 43.18 270)
				(length 3.81)
				(name "PC3_TDO")
				(number "82")
			)
			(pin bidirectional line
				(at 13.97 43.18 270)
				(length 3.81)
				(name "PC2_TDI")
				(number "83")
			)
			(pin bidirectional line
				(at 11.43 43.18 270)
				(length 3.81)
				(name "PC1_SWDIO")
				(number "84")
			)
			(pin bidirectional line
				(at 8.89 43.18 270)
				(length 3.81)
				(name "PC0_SWCLK")
				(number "85")
			)
			(pin output line
				(at 6.35 43.18 270)
				(length 3.81)
				(name "VDDC")
				(number "86")
			)
			(pin bidirectional line
				(at 3.81 43.18 270)
				(length 3.81)
				(name "PG6_GP")
				(number "87")
			)
			(pin bidirectional line
				(at 1.27 43.18 270)
				(length 3.81)
				(name "PG7_GP")
				(number "88")
			)
			(pin bidirectional line
				(at -1.27 43.18 270)
				(length 3.81)
				(name "PE6_GP_AIN21")
				(number "89")
			)
			(pin power_in line
				(at -44.45 8.89 0)
				(length 3.81)
				(name "VREF-")
				(number "9")
			)
			(pin bidirectional line
				(at -3.81 43.18 270)
				(length 3.81)
				(name "PE7_GP_AIN20")
				(number "90")
			)
			(pin bidirectional line
				(at -6.35 43.18 270)
				(length 3.81)
				(name "PB5_GP_AIN11")
				(number "91")
			)
			(pin bidirectional line
				(at -8.89 43.18 270)
				(length 3.81)
				(name "PB4_GP_AIN10")
				(number "92")
			)
			(pin power_in line
				(at -11.43 43.18 270)
				(length 3.81)
				(name "VDD")
				(number "93")
			)
			(pin power_in line
				(at -13.97 43.18 270)
				(length 3.81)
				(name "GND")
				(number "94")
			)
			(pin bidirectional line
				(at -16.51 43.18 270)
				(length 3.81)
				(name "PE4_GP_AIN9")
				(number "95")
			)
			(pin bidirectional line
				(at -19.05 43.18 270)
				(length 3.81)
				(name "PE5_U5TX")
				(number "96")
			)
			(pin bidirectional line
				(at -21.59 43.18 270)
				(length 3.81)
				(name "PD4_U6RX")
				(number "97")
			)
			(pin bidirectional line
				(at -24.13 43.18 270)
				(length 3.81)
				(name "PD5_U6TX")
				(number "98")
			)
			(pin bidirectional line
				(at -26.67 43.18 270)
				(length 3.81)
				(name "PD6_AIN5")
				(number "99")
			)
		)
	)
	(symbol "TM4C123GH6ZXRI7"
		(pin_names
			(offset 0.254)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 2.54 0)
		)
		(property "Value" "TM4C123GH6ZXRI7"
			(at 0 0 0)
		)
		(property "Footprint" "ZXR0168A"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/tm4c123gh6zxr.pdf"
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(property "PartNum" "TM4C123GH6ZXRI7"
			(at 0 0 0)
		)
		(property "VendorNum" "TM4C123GH6ZXRI7-ND"
			(at 0 0 0)
		)
		(property "Vendor" "Digikey"
			(at 0 0 0)
		)
		(property "Subst" "No"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "TM4C123GH6ZXRI7"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "ZXR0168A"
			(at 0 0 0)
		)
		(symbol "TM4C123GH6ZXRI7_1_1"
			(pin bidirectional line
				(at -27.94 -38.1 0)
				(length 7.62)
				(name "PD5")
				(number "A1")
			)
			(pin bidirectional line
				(at -27.94 -35.56 0)
				(length 7.62)
				(name "PD4")
				(number "A2")
			)
			(pin bidirectional line
				(at 27.94 30.48 180)
				(length 7.62)
				(name "PE5")
				(number "A3")
			)
			(pin bidirectional line
				(at -27.94 10.16 0)
				(length 7.62)
				(name "PB4")
				(number "A4")
			)
			(pin bidirectional line
				(at -27.94 -25.4 0)
				(length 7.62)
				(name "PD0")
				(number "B1")
			)
			(pin bidirectional line
				(at -27.94 -7.62 0)
				(length 7.62)
				(name "PC2_TDI")
				(number "B10")
			)
			(pin bidirectional line
				(at 27.94 33.02 180)
				(length 7.62)
				(name "PE4")
				(number "B3")
			)
			(pin bidirectional line
				(at -27.94 7.62 0)
				(length 7.62)
				(name "PB5")
				(number "B4")
			)
			(pin bidirectional line
				(at -27.94 -2.54 0)
				(length 7.62)
				(name "PC0_TCK_SWCLK")
				(number "B9")
			)
			(pin bidirectional line
				(at -27.94 -27.94 0)
				(length 7.62)
				(name "PD1")
				(number "C1")
			)
			(pin bidirectional line
				(at -27.94 -10.16 0)
				(length 7.62)
				(name "PC3_TDO_SWO")
				(number "C10")
			)
			(pin bidirectional line
				(at -27.94 -43.18 0)
				(length 7.62)
				(name "PD7")
				(number "C2")
			)
			(pin bidirectional line
				(at -27.94 -40.64 0)
				(length 7.62)
				(name "PD6")
				(number "C3")
			)
			(pin bidirectional line
				(at 27.94 25.4 180)
				(length 7.62)
				(name "PE7")
				(number "C4")
			)
			(pin bidirectional line
				(at 27.94 27.94 180)
				(length 7.62)
				(name "PE6")
				(number "C5")
			)
			(pin bidirectional line
				(at -27.94 -5.08 0)
				(length 7.62)
				(name "PC1_TMS_SWDIO")
				(number "C9")
			)
			(pin bidirectional line
				(at -27.94 17.78 0)
				(length 7.62)
				(name "PB1_USB0VBUS")
				(number "D11")
			)
			(pin bidirectional line
				(at -27.94 12.7 0)
				(length 7.62)
				(name "PB3_I2C0SDA")
				(number "D12")
			)
			(pin bidirectional line
				(at -27.94 15.24 0)
				(length 7.62)
				(name "PB2_I2C0SCL")
				(number "D13")
			)
			(pin bidirectional line
				(at -27.94 -30.48 0)
				(length 7.62)
				(name "PD2")
				(number "D3")
			)
			(pin bidirectional line
				(at -27.94 -33.02 0)
				(length 7.62)
				(name "PD3")
				(number "D4")
			)
			(pin bidirectional line
				(at -27.94 20.32 0)
				(length 7.62)
				(name "PB0_USB0ID")
				(number "E11")
			)
			(pin bidirectional line
				(at -27.94 5.08 0)
				(length 7.62)
				(name "PB6")
				(number "E3")
			)
			(pin bidirectional line
				(at -27.94 2.54 0)
				(length 7.62)
				(name "PB7")
				(number "E4")
			)
			(pin bidirectional line
				(at 27.94 43.18 180)
				(length 7.62)
				(name "PE0")
				(number "G1")
			)
			(pin bidirectional line
				(at 27.94 40.64 180)
				(length 7.62)
				(name "PE1")
				(number "G2")
			)
			(pin bidirectional line
				(at 27.94 38.1 180)
				(length 7.62)
				(name "PE2")
				(number "G3")
			)
			(pin bidirectional line
				(at 27.94 35.56 180)
				(length 7.62)
				(name "PE3")
				(number "G4")
			)
			(pin bidirectional line
				(at 27.94 -40.64 180)
				(length 7.62)
				(name "PH6")
				(number "J2")
			)
			(pin bidirectional line
				(at 27.94 -38.1 180)
				(length 7.62)
				(name "PH5")
				(number "J3")
			)
			(pin bidirectional line
				(at 27.94 -43.18 180)
				(length 7.62)
				(name "PH7")
				(number "J4")
			)
			(pin bidirectional line
				(at 27.94 -35.56 180)
				(length 7.62)
				(name "PH4")
				(number "K1")
			)
			(pin bidirectional line
				(at 27.94 10.16 180)
				(length 7.62)
				(name "PF4")
				(number "K10")
			)
			(pin bidirectional line
				(at 27.94 -33.02 180)
				(length 7.62)
				(name "PH3")
				(number "K2")
			)
			(pin bidirectional line
				(at 27.94 -30.48 180)
				(length 7.62)
				(name "PH2")
				(number "K3")
			)
			(pin bidirectional line
				(at -27.94 40.64 0)
				(length 7.62)
				(name "PA1_U0Tx")
				(number "K5")
			)
			(pin bidirectional line
				(at 27.94 2.54 180)
				(length 7.62)
				(name "PF7")
				(number "K8")
			)
			(pin bidirectional line
				(at 27.94 -27.94 180)
				(length 7.62)
				(name "PH1")
				(number "L1")
			)
			(pin bidirectional line
				(at 27.94 20.32 180)
				(length 7.62)
				(name "PF0")
				(number "L10")
			)
			(pin bidirectional line
				(at 27.94 -25.4 180)
				(length 7.62)
				(name "PH0")
				(number "L2")
			)
			(pin bidirectional line
				(at -27.94 43.18 0)
				(length 7.62)
				(name "PA0_U0Rx")
				(number "L3")
			)
			(pin bidirectional line
				(at -27.94 33.02 0)
				(length 7.62)
				(name "PA4_SSI0Rx")
				(number "L4")
			)
			(pin bidirectional line
				(at -27.94 25.4 0)
				(length 7.62)
				(name "PA7")
				(number "L5")
			)
			(pin bidirectional line
				(at 27.94 -10.16 180)
				(length 7.62)
				(name "PG3")
				(number "L8")
			)
			(pin bidirectional line
				(at 27.94 -7.62 180)
				(length 7.62)
				(name "PG2")
				(number "L9")
			)
			(pin bidirectional line
				(at -27.94 -20.32 0)
				(length 7.62)
				(name "PC7")
				(number "M1")
			)
			(pin bidirectional line
				(at 27.94 7.62 180)
				(length 7.62)
				(name "PF5")
				(number "M10")
			)
			(pin bidirectional line
				(at 27.94 12.7 180)
				(length 7.62)
				(name "PF3")
				(number "M11")
			)
			(pin bidirectional line
				(at -27.94 -15.24 0)
				(length 7.62)
				(name "PC5")
				(number "M2")
			)
			(pin bidirectional line
				(at -27.94 -12.7 0)
				(length 7.62)
				(name "PC4")
				(number "M3")
			)
			(pin bidirectional line
				(at -27.94 30.48 0)
				(length 7.62)
				(name "PA5_SSI0Tx")
				(number "M4")
			)
			(pin bidirectional line
				(at 27.94 -20.32 180)
				(length 7.62)
				(name "PG7")
				(number "M5")
			)
			(pin bidirectional line
				(at 27.94 -12.7 180)
				(length 7.62)
				(name "PG4")
				(number "M8")
			)
			(pin bidirectional line
				(at 27.94 -5.08 180)
				(length 7.62)
				(name "PG1")
				(number "M9")
			)
			(pin bidirectional line
				(at -27.94 -17.78 0)
				(length 7.62)
				(name "PC6")
				(number "N1")
			)
			(pin bidirectional line
				(at 27.94 5.08 180)
				(length 7.62)
				(name "PF6")
				(number "N10")
			)
			(pin bidirectional line
				(at 27.94 17.78 180)
				(length 7.62)
				(name "PF1")
				(number "N11")
			)
			(pin bidirectional line
				(at 27.94 15.24 180)
				(length 7.62)
				(name "PF2")
				(number "N12")
			)
			(pin bidirectional line
				(at -27.94 38.1 0)
				(length 7.62)
				(name "PA2_SSI0Clk")
				(number "N2")
			)
			(pin bidirectional line
				(at -27.94 35.56 0)
				(length 7.62)
				(name "PA3_SSI0Fss")
				(number "N3")
			)
			(pin bidirectional line
				(at -27.94 27.94 0)
				(length 7.62)
				(name "PA6")
				(number "N4")
			)
			(pin bidirectional line
				(at 27.94 -17.78 180)
				(length 7.62)
				(name "PG6")
				(number "N5")
			)
			(pin bidirectional line
				(at 27.94 -15.24 180)
				(length 7.62)
				(name "PG5")
				(number "N8")
			)
			(pin bidirectional line
				(at 27.94 -2.54 180)
				(length 7.62)
				(name "PG0")
				(number "N9")
			)
		)
		(symbol "TM4C123GH6ZXRI7_2_1"
			(pin bidirectional line
				(at -22.86 10.16 0)
				(length 7.62)
				(name "PK4")
				(number "A11")
			)
			(pin bidirectional line
				(at -22.86 5.08 0)
				(length 7.62)
				(name "PK6")
				(number "A12")
			)
			(pin bidirectional line
				(at -22.86 -2.54 0)
				(length 7.62)
				(name "PL0")
				(number "A13")
			)
			(pin bidirectional line
				(at 22.86 43.18 180)
				(length 7.62)
				(name "PN0")
				(number "A5")
			)
			(pin bidirectional line
				(at -22.86 33.02 0)
				(length 7.62)
				(name "PJ4")
				(number "A6")
			)
			(pin bidirectional line
				(at 22.86 5.08 180)
				(length 7.62)
				(name "PP6")
				(number "A7")
			)
			(pin bidirectional line
				(at -22.86 40.64 0)
				(length 7.62)
				(name "PJ1")
				(number "A8")
			)
			(pin bidirectional line
				(at 22.86 35.56 180)
				(length 7.62)
				(name "PN3")
				(number "A9")
			)
			(pin bidirectional line
				(at -22.86 7.62 0)
				(length 7.62)
				(name "PK5")
				(number "B11")
			)
			(pin bidirectional line
				(at -22.86 2.54 0)
				(length 7.62)
				(name "PK7")
				(number "B12")
			)
			(pin bidirectional line
				(at -22.86 -7.62 0)
				(length 7.62)
				(name "PL2")
				(number "B13")
			)
			(pin bidirectional line
				(at 22.86 40.64 180)
				(length 7.62)
				(name "PN1")
				(number "B5")
			)
			(pin bidirectional line
				(at -22.86 30.48 0)
				(length 7.62)
				(name "PJ5")
				(number "B6")
			)
			(pin bidirectional line
				(at -22.86 38.1 0)
				(length 7.62)
				(name "PJ2")
				(number "B8")
			)
			(pin bidirectional line
				(at -22.86 -5.08 0)
				(length 7.62)
				(name "PL1")
				(number "C11")
			)
			(pin bidirectional line
				(at -22.86 -12.7 0)
				(length 7.62)
				(name "PL4")
				(number "C12")
			)
			(pin bidirectional line
				(at -22.86 -15.24 0)
				(length 7.62)
				(name "PL5")
				(number "C13")
			)
			(pin bidirectional line
				(at -22.86 25.4 0)
				(length 7.62)
				(name "PJ7")
				(number "C6")
			)
			(pin bidirectional line
				(at -22.86 27.94 0)
				(length 7.62)
				(name "PJ6")
				(number "C7")
			)
			(pin bidirectional line
				(at -22.86 35.56 0)
				(length 7.62)
				(name "PJ3")
				(number "C8")
			)
			(pin bidirectional line
				(at 22.86 -5.08 180)
				(length 7.62)
				(name "PQ1")
				(number "D1")
			)
			(pin bidirectional line
				(at -22.86 -10.16 0)
				(length 7.62)
				(name "PL3")
				(number "D10")
			)
			(pin bidirectional line
				(at 22.86 -2.54 180)
				(length 7.62)
				(name "PQ0")
				(number "D2")
			)
			(pin bidirectional line
				(at -22.86 43.18 0)
				(length 7.62)
				(name "PJ0")
				(number "D8")
			)
			(pin bidirectional line
				(at -22.86 -17.78 0)
				(length 7.62)
				(name "PL6")
				(number "E12")
			)
			(pin bidirectional line
				(at -22.86 -20.32 0)
				(length 7.62)
				(name "PL7")
				(number "E13")
			)
			(pin bidirectional line
				(at 22.86 -7.62 180)
				(length 7.62)
				(name "PQ2")
				(number "F1")
			)
			(pin bidirectional line
				(at -22.86 -25.4 0)
				(length 7.62)
				(name "PM0")
				(number "F10")
			)
			(pin bidirectional line
				(at -22.86 -35.56 0)
				(length 7.62)
				(name "PM4")
				(number "G10")
			)
			(pin bidirectional line
				(at -22.86 -30.48 0)
				(length 7.62)
				(name "PM2")
				(number "G11")
			)
			(pin bidirectional line
				(at -22.86 -27.94 0)
				(length 7.62)
				(name "PM1")
				(number "G12")
			)
			(pin bidirectional line
				(at -22.86 -33.02 0)
				(length 7.62)
				(name "PM3")
				(number "G13")
			)
			(pin bidirectional line
				(at -22.86 15.24 0)
				(length 7.62)
				(name "PK2")
				(number "H1")
			)
			(pin bidirectional line
				(at -22.86 -38.1 0)
				(length 7.62)
				(name "PM5")
				(number "H10")
			)
			(pin bidirectional line
				(at -22.86 -43.18 0)
				(length 7.62)
				(name "PM7")
				(number "H11")
			)
			(pin bidirectional line
				(at 22.86 17.78 180)
				(length 7.62)
				(name "PP1")
				(number "H12")
			)
			(pin bidirectional line
				(at -22.86 -40.64 0)
				(length 7.62)
				(name "PM6")
				(number "H13")
			)
			(pin bidirectional line
				(at -22.86 12.7 0)
				(length 7.62)
				(name "PK3")
				(number "H2")
			)
			(pin bidirectional line
				(at -22.86 17.78 0)
				(length 7.62)
				(name "PK1")
				(number "H3")
			)
			(pin bidirectional line
				(at -22.86 20.32 0)
				(length 7.62)
				(name "PK0")
				(number "H4")
			)
			(pin bidirectional line
				(at 22.86 20.32 180)
				(length 7.62)
				(name "PP0")
				(number "J10")
			)
			(pin bidirectional line
				(at 22.86 12.7 180)
				(length 7.62)
				(name "PP3")
				(number "J11")
			)
			(pin bidirectional line
				(at 22.86 10.16 180)
				(length 7.62)
				(name "PP4")
				(number "J12")
			)
			(pin bidirectional line
				(at 22.86 38.1 180)
				(length 7.62)
				(name "PN2")
				(number "K4")
			)
			(pin bidirectional line
				(at 22.86 15.24 180)
				(length 7.62)
				(name "PP2")
				(number "K6")
			)
			(pin bidirectional line
				(at 22.86 7.62 180)
				(length 7.62)
				(name "PP5")
				(number "K7")
			)
			(pin bidirectional line
				(at 22.86 25.4 180)
				(length 7.62)
				(name "PN7")
				(number "L11")
			)
			(pin bidirectional line
				(at 22.86 33.02 180)
				(length 7.62)
				(name "PN4")
				(number "L12")
			)
			(pin bidirectional line
				(at 22.86 2.54 180)
				(length 7.62)
				(name "PP7")
				(number "L6")
			)
			(pin bidirectional line
				(at 22.86 -15.24 180)
				(length 7.62)
				(name "PQ5")
				(number "L7")
			)
			(pin bidirectional line
				(at 22.86 30.48 180)
				(length 7.62)
				(name "PN5")
				(number "M12")
			)
			(pin bidirectional line
				(at 22.86 -10.16 180)
				(length 7.62)
				(name "PQ3")
				(number "M6")
			)
			(pin bidirectional line
				(at 22.86 -17.78 180)
				(length 7.62)
				(name "PQ6")
				(number "M7")
			)
			(pin bidirectional line
				(at 22.86 27.94 180)
				(length 7.62)
				(name "PN6")
				(number "N13")
			)
			(pin bidirectional line
				(at 22.86 -12.7 180)
				(length 7.62)
				(name "PQ4")
				(number "N6")
			)
			(pin bidirectional line
				(at 22.86 -20.32 180)
				(length 7.62)
				(name "PQ7")
				(number "N7")
			)
		)
		(symbol "TM4C123GH6ZXRI7_3_1"
			(pin unspecified line
				(at 22.86 2.54 180)
				(length 7.62)
				(name "NC")
				(number "B7")
			)
			(pin input line
				(at -22.86 2.54 0)
				(length 7.62)
				(name "RST_N")
				(number "F11")
			)
			(pin output line
				(at -22.86 -7.62 0)
				(length 7.62)
				(name "OSC1")
				(number "F12")
			)
			(pin input line
				(at -22.86 -2.54 0)
				(length 7.62)
				(name "OSC0")
				(number "F13")
			)
			(pin input line
				(at 22.86 -2.54 180)
				(length 7.62)
				(name "XOSC0")
				(number "K11")
			)
			(pin output line
				(at 22.86 -7.62 180)
				(length 7.62)
				(name "XOSC1")
				(number "K12")
			)
			(pin output line
				(at 22.86 7.62 180)
				(length 7.62)
				(name "HIB_N")
				(number "L13")
			)
			(pin input line
				(at -22.86 7.62 0)
				(length 7.62)
				(name "WAKE_N")
				(number "M13")
			)
		)
		(symbol "TM4C123GH6ZXRI7_4_1"
			(pin power_in line
				(at 22.86 27.94 180)
				(length 7.62)
				(name "GND")
				(number "A10")
			)
			(pin power_in line
				(at 22.86 25.4 180)
				(length 7.62)
				(name "GND")
				(number "D5")
			)
			(pin power_in line
				(at 22.86 22.86 180)
				(length 7.62)
				(name "GND")
				(number "D6")
			)
			(pin power_in line
				(at -22.86 -5.08 0)
				(length 7.62)
				(name "VDDC")
				(number "D7")
			)
			(pin power_in line
				(at 22.86 20.32 180)
				(length 7.62)
				(name "GND")
				(number "D9")
			)
			(pin power_in line
				(at -22.86 -25.4 0)
				(length 7.62)
				(name "VREFA+")
				(number "E1")
			)
			(pin power_in line
				(at 22.86 10.16 180)
				(length 7.62)
				(name "GND")
				(number "E10")
			)
			(pin power_in line
				(at -22.86 -27.94 0)
				(length 7.62)
				(name "VREFA-")
				(number "E2")
			)
			(pin power_in line
				(at 22.86 17.78 180)
				(length 7.62)
				(name "GND")
				(number "E5")
			)
			(pin power_in line
				(at -22.86 27.94 0)
				(length 7.62)
				(name "VDD")
				(number "E6")
			)
			(pin power_in line
				(at -22.86 25.4 0)
				(length 7.62)
				(name "VDD")
				(number "E7")
			)
			(pin power_in line
				(at 22.86 15.24 180)
				(length 7.62)
				(name "GND")
				(number "E8")
			)
			(pin power_in line
				(at 22.86 12.7 180)
				(length 7.62)
				(name "GND")
				(number "E9")
			)
			(pin power_in line
				(at 22.86 -25.4 180)
				(length 7.62)
				(name "GNDA")
				(number "F2")
			)
			(pin power_in line
				(at -22.86 0 0)
				(length 7.62)
				(name "VDDA")
				(number "F3")
			)
			(pin power_in line
				(at 22.86 -27.94 180)
				(length 7.62)
				(name "GNDA")
				(number "F4")
			)
			(pin power_in line
				(at 22.86 7.62 180)
				(length 7.62)
				(name "GND")
				(number "F5")
			)
			(pin power_in line
				(at -22.86 22.86 0)
				(length 7.62)
				(name "VDD")
				(number "F6")
			)
			(pin power_in line
				(at -22.86 20.32 0)
				(length 7.62)
				(name "VDD")
				(number "F7")
			)
			(pin power_in line
				(at -22.86 17.78 0)
				(length 7.62)
				(name "VDD")
				(number "F8")
			)
			(pin power_in line
				(at 22.86 5.08 180)
				(length 7.62)
				(name "GND")
				(number "F9")
			)
			(pin power_in line
				(at 22.86 2.54 180)
				(length 7.62)
				(name "GND")
				(number "G5")
			)
			(pin power_in line
				(at -22.86 15.24 0)
				(length 7.62)
				(name "VDD")
				(number "G6")
			)
			(pin power_in line
				(at -22.86 12.7 0)
				(length 7.62)
				(name "VDD")
				(number "G7")
			)
			(pin power_in line
				(at -22.86 10.16 0)
				(length 7.62)
				(name "VDD")
				(number "G8")
			)
			(pin power_in line
				(at 22.86 0 180)
				(length 7.62)
				(name "GND")
				(number "G9")
			)
			(pin power_in line
				(at 22.86 -2.54 180)
				(length 7.62)
				(name "GND")
				(number "H5")
			)
			(pin power_in line
				(at -22.86 7.62 0)
				(length 7.62)
				(name "VDD")
				(number "H6")
			)
			(pin power_in line
				(at -22.86 5.08 0)
				(length 7.62)
				(name "VDD")
				(number "H7")
			)
			(pin power_in line
				(at 22.86 -5.08 180)
				(length 7.62)
				(name "GND")
				(number "H8")
			)
			(pin power_in line
				(at -22.86 -7.62 0)
				(length 7.62)
				(name "VDDC")
				(number "H9")
			)
			(pin power_in line
				(at -22.86 -10.16 0)
				(length 7.62)
				(name "VDDC")
				(number "J1")
			)
			(pin power_in line
				(at -22.86 -15.24 0)
				(length 7.62)
				(name "VDDC")
				(number "J13")
			)
			(pin power_in line
				(at 22.86 -7.62 180)
				(length 7.62)
				(name "GND")
				(number "J5")
			)
			(pin power_in line
				(at 22.86 -10.16 180)
				(length 7.62)
				(name "GND")
				(number "J6")
			)
			(pin power_in line
				(at 22.86 -12.7 180)
				(length 7.62)
				(name "GND")
				(number "J7")
			)
			(pin power_in line
				(at 22.86 -15.24 180)
				(length 7.62)
				(name "GND")
				(number "J8")
			)
			(pin power_in line
				(at -22.86 -12.7 0)
				(length 7.62)
				(name "VDDC")
				(number "J9")
			)
			(pin power_in line
				(at -22.86 -20.32 0)
				(length 7.62)
				(name "VBAT")
				(number "K13")
			)
			(pin power_in line
				(at 22.86 -17.78 180)
				(length 7.62)
				(name "GND")
				(number "K9")
			)
		)
	)
	(symbol "TM4C1290NCPDT"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 25.4 69.85 0)
		)
		(property "Value" "TM4C1290NCPDT"
			(at -19.05 -39.37 0)
		)
		(property "Footprint" "ProjectFootprints:TM4C1290N_128N"
			(at -6.35 1.27 0)
		)
		(property "Datasheet" ""
			(at -6.35 1.27 0)
		)
		(property "Description" ""
			(at -6.35 1.27 0)
		)
		(property "PartNum" "TM4C1290NCPDTI3R"
			(at -6.35 1.27 0)
		)
		(property "VendorNum" ""
			(at -6.35 1.27 0)
		)
		(property "Vendor" ""
			(at -6.35 1.27 0)
		)
		(property "Subst" ""
			(at -6.35 1.27 0)
		)
		(symbol "TM4C1290NCPDT_1_0"
			(pin bidirectional line
				(at -55.88 38.1 0)
				(length 5.08)
				(name "PD0")
				(number "1")
			)
			(pin bidirectional line
				(at -55.88 15.24 0)
				(length 5.08)
				(name "PD3")
				(number "10")
			)
			(pin bidirectional line
				(at 30.48 50.8 270)
				(length 5.08)
				(name "huh")
				(number "100")
			)
			(pin bidirectional line
				(at 27.94 50.8 270)
				(length 5.08)
				(name "PD3")
				(number "101")
			)
			(pin bidirectional line
				(at 25.4 50.8 270)
				(length 5.08)
				(name "PD3")
				(number "102")
			)
			(pin bidirectional line
				(at 22.86 50.8 270)
				(length 5.08)
				(name "PD3")
				(number "103")
			)
			(pin bidirectional line
				(at 20.32 50.8 270)
				(length 5.08)
				(name "PD3")
				(number "104")
			)
			(pin bidirectional line
				(at 17.78 50.8 270)
				(length 5.08)
				(name "PD3")
				(number "105")
			)
			(pin bidirectional line
				(at 15.24 50.8 270)
				(length 5.08)
				(name "PD3")
				(number "106")
			)
			(pin bidirectional line
				(at 12.7 50.8 270)
				(length 5.08)
				(name "PD3")
				(number "107")
			)
			(pin bidirectional line
				(at 10.16 50.8 270)
				(length 5.08)
				(name "PE3")
				(number "108")
			)
			(pin bidirectional line
				(at 7.62 50.8 270)
				(length 5.08)
				(name "PE2")
				(number "109")
			)
			(pin bidirectional line
				(at -55.88 12.7 0)
				(length 5.08)
				(name "PD3")
				(number "11")
			)
			(pin bidirectional line
				(at 5.08 50.8 270)
				(length 5.08)
				(name "huh")
				(number "110")
			)
			(pin bidirectional line
				(at 2.54 50.8 270)
				(length 5.08)
				(name "PE0")
				(number "111")
			)
			(pin bidirectional line
				(at 0 50.8 270)
				(length 5.08)
				(name "PE0")
				(number "112")
			)
			(pin bidirectional line
				(at -2.54 50.8 270)
				(length 5.08)
				(name "PE0")
				(number "113")
			)
			(pin bidirectional line
				(at -5.08 50.8 270)
				(length 5.08)
				(name "PE0")
				(number "114")
			)
			(pin bidirectional line
				(at -7.62 50.8 270)
				(length 5.08)
				(name "PE0")
				(number "115")
			)
			(pin bidirectional line
				(at -10.16 50.8 270)
				(length 5.08)
				(name "PJ0")
				(number "116")
			)
			(pin bidirectional line
				(at -12.7 50.8 270)
				(length 5.08)
				(name "PJ1")
				(number "117")
			)
			(pin bidirectional line
				(at -15.24 50.8 270)
				(length 5.08)
				(name "PC7")
				(number "118")
			)
			(pin bidirectional line
				(at -17.78 50.8 270)
				(length 5.08)
				(name "PC6")
				(number "119")
			)
			(pin bidirectional line
				(at -55.88 10.16 0)
				(length 5.08)
				(name "PE3")
				(number "12")
			)
			(pin bidirectional line
				(at -20.32 50.8 270)
				(length 5.08)
				(name "PB5")
				(number "120")
			)
			(pin bidirectional line
				(at -22.86 50.8 270)
				(length 5.08)
				(name "PB4")
				(number "121")
			)
			(pin bidirectional line
				(at -25.4 50.8 270)
				(length 5.08)
				(name "PE0")
				(number "122")
			)
			(pin bidirectional line
				(at -27.94 50.8 270)
				(length 5.08)
				(name "PE4")
				(number "123")
			)
			(pin bidirectional line
				(at -30.48 50.8 270)
				(length 5.08)
				(name "PE5")
				(number "124")
			)
			(pin bidirectional line
				(at -33.02 50.8 270)
				(length 5.08)
				(name "PD4")
				(number "125")
			)
			(pin bidirectional line
				(at -35.56 50.8 270)
				(length 5.08)
				(name "PD5")
				(number "126")
			)
			(pin bidirectional line
				(at -38.1 50.8 270)
				(length 5.08)
				(name "PD6")
				(number "127")
			)
			(pin bidirectional line
				(at -40.64 50.8 270)
				(length 5.08)
				(name "PD7")
				(number "128")
			)
			(pin bidirectional line
				(at -55.88 7.62 0)
				(length 5.08)
				(name "PE2")
				(number "13")
			)
			(pin bidirectional line
				(at -55.88 5.08 0)
				(length 5.08)
				(name "PE1")
				(number "14")
			)
			(pin bidirectional line
				(at -55.88 2.54 0)
				(length 5.08)
				(name "PE0")
				(number "15")
			)
			(pin bidirectional line
				(at -55.88 0 0)
				(length 5.08)
				(name "PE0")
				(number "16")
			)
			(pin bidirectional line
				(at -55.88 -2.54 0)
				(length 5.08)
				(name "PE0")
				(number "17")
			)
			(pin bidirectional line
				(at -55.88 -5.08 0)
				(length 5.08)
				(name "PE0")
				(number "18")
			)
			(pin bidirectional line
				(at -55.88 -7.62 0)
				(length 5.08)
				(name "PE0")
				(number "19")
			)
			(pin bidirectional line
				(at -55.88 35.56 0)
				(length 5.08)
				(name "PD1")
				(number "2")
			)
			(pin bidirectional line
				(at -55.88 -10.16 0)
				(length 5.08)
				(name "PE0")
				(number "20")
			)
			(pin bidirectional line
				(at -55.88 -12.7 0)
				(length 5.08)
				(name "PE0")
				(number "21")
			)
			(pin bidirectional line
				(at -55.88 -15.24 0)
				(length 5.08)
				(name "PC7")
				(number "22")
			)
			(pin bidirectional line
				(at -55.88 -17.78 0)
				(length 5.08)
				(name "PC6")
				(number "23")
			)
			(pin bidirectional line
				(at -55.88 -20.32 0)
				(length 5.08)
				(name "PC5")
				(number "24")
			)
			(pin bidirectional line
				(at -55.88 -22.86 0)
				(length 5.08)
				(name "PC4")
				(number "25")
			)
			(pin bidirectional line
				(at -55.88 -25.4 0)
				(length 5.08)
				(name "PE0")
				(number "26")
			)
			(pin bidirectional line
				(at -55.88 -27.94 0)
				(length 5.08)
				(name "PE0")
				(number "27")
			)
			(pin bidirectional line
				(at -55.88 -30.48 0)
				(length 5.08)
				(name "PE0")
				(number "28")
			)
			(pin bidirectional line
				(at -55.88 -33.02 0)
				(length 5.08)
				(name "PH0")
				(number "29")
			)
			(pin bidirectional line
				(at -55.88 33.02 0)
				(length 5.08)
				(name "PD2")
				(number "3")
			)
			(pin bidirectional line
				(at -55.88 -35.56 0)
				(length 5.08)
				(name "PH1")
				(number "30")
			)
			(pin bidirectional line
				(at -55.88 -38.1 0)
				(length 5.08)
				(name "PH2")
				(number "31")
			)
			(pin bidirectional line
				(at -55.88 -40.64 0)
				(length 5.08)
				(name "PH3")
				(number "32")
			)
			(pin bidirectional line
				(at -38.1 -52.07 90)
				(length 5.08)
				(name "PA0_U0RX")
				(number "33")
			)
			(pin bidirectional line
				(at -35.56 -52.07 90)
				(length 5.08)
				(name "PA1_U0TX")
				(number "34")
			)
			(pin bidirectional line
				(at -33.02 -52.07 90)
				(length 5.08)
				(name "PA2_SSI0CLK")
				(number "35")
			)
			(pin bidirectional line
				(at -30.48 -52.07 90)
				(length 5.08)
				(name "PA3_SSI0FSS")
				(number "36")
			)
			(pin bidirectional line
				(at -27.94 -52.07 90)
				(length 5.08)
				(name "PA4")
				(number "37")
			)
			(pin bidirectional line
				(at -25.4 -52.07 90)
				(length 5.08)
				(name "PA5")
				(number "38")
			)
			(pin bidirectional line
				(at -22.86 -52.07 90)
				(length 5.08)
				(name "PA5")
				(number "39")
			)
			(pin bidirectional line
				(at -55.88 30.48 0)
				(length 5.08)
				(name "PD3")
				(number "4")
			)
			(pin bidirectional line
				(at -20.32 -52.07 90)
				(length 5.08)
				(name "PA6")
				(number "40")
			)
			(pin bidirectional line
				(at -17.78 -52.07 90)
				(length 5.08)
				(name "PA7")
				(number "41")
			)
			(pin bidirectional line
				(at -15.24 -52.07 90)
				(length 5.08)
				(name "PF0")
				(number "42")
			)
			(pin bidirectional line
				(at -12.7 -52.07 90)
				(length 5.08)
				(name "PF1")
				(number "43")
			)
			(pin bidirectional line
				(at -10.16 -52.07 90)
				(length 5.08)
				(name "PF2")
				(number "44")
			)
			(pin bidirectional line
				(at -7.62 -52.07 90)
				(length 5.08)
				(name "PF3")
				(number "45")
			)
			(pin bidirectional line
				(at -5.08 -52.07 90)
				(length 5.08)
				(name "PF4")
				(number "46")
			)
			(pin bidirectional line
				(at -2.54 -52.07 90)
				(length 5.08)
				(name "PE1")
				(number "47")
			)
			(pin bidirectional line
				(at 0 -52.07 90)
				(length 5.08)
				(name "PE0")
				(number "48")
			)
			(pin bidirectional line
				(at 2.54 -52.07 90)
				(length 5.08)
				(name "PG0")
				(number "49")
			)
			(pin bidirectional line
				(at -55.88 27.94 0)
				(length 5.08)
				(name "PD3")
				(number "5")
			)
			(pin bidirectional line
				(at 5.08 -52.07 90)
				(length 5.08)
				(name "PG1")
				(number "50")
			)
			(pin bidirectional line
				(at 7.62 -52.07 90)
				(length 5.08)
				(name "PG2")
				(number "51")
			)
			(pin bidirectional line
				(at 10.16 -52.07 90)
				(length 5.08)
				(name "PG3")
				(number "52")
			)
			(pin bidirectional line
				(at 12.7 -52.07 90)
				(length 5.08)
				(name "PG4")
				(number "53")
			)
			(pin bidirectional line
				(at 15.24 -52.07 90)
				(length 5.08)
				(name "PG5")
				(number "54")
			)
			(pin bidirectional line
				(at 17.78 -52.07 90)
				(length 5.08)
				(name "PG6")
				(number "55")
			)
			(pin bidirectional line
				(at 20.32 -52.07 90)
				(length 5.08)
				(name "PG7")
				(number "56")
			)
			(pin bidirectional line
				(at 22.86 -52.07 90)
				(length 5.08)
				(name "PC5")
				(number "57")
			)
			(pin bidirectional line
				(at 25.4 -52.07 90)
				(length 5.08)
				(name "PC4")
				(number "58")
			)
			(pin bidirectional line
				(at 27.94 -52.07 90)
				(length 5.08)
				(name "PE0")
				(number "59")
			)
			(pin bidirectional line
				(at -55.88 25.4 0)
				(length 5.08)
				(name "PD3")
				(number "6")
			)
			(pin bidirectional line
				(at 30.48 -52.07 90)
				(length 5.08)
				(name "PE0")
				(number "60")
			)
			(pin bidirectional line
				(at 33.02 -52.07 90)
				(length 5.08)
				(name "PE0")
				(number "61")
			)
			(pin bidirectional line
				(at 35.56 -52.07 90)
				(length 5.08)
				(name "PH0")
				(number "62")
			)
			(pin bidirectional line
				(at 38.1 -52.07 90)
				(length 5.08)
				(name "PH1")
				(number "63")
			)
			(pin bidirectional line
				(at 40.64 -52.07 90)
				(length 5.08)
				(name "PH2")
				(number "64")
			)
			(pin bidirectional line
				(at 53.34 -38.1 180)
				(length 5.08)
				(name "PD0")
				(number "65")
			)
			(pin bidirectional line
				(at 53.34 -35.56 180)
				(length 5.08)
				(name "PD1")
				(number "66")
			)
			(pin bidirectional line
				(at 53.34 -33.02 180)
				(length 5.08)
				(name "PD2")
				(number "67")
			)
			(pin bidirectional line
				(at 53.34 -30.48 180)
				(length 5.08)
				(name "PD3")
				(number "68")
			)
			(pin bidirectional line
				(at 53.34 -27.94 180)
				(length 5.08)
				(name "PD3")
				(number "69")
			)
			(pin bidirectional line
				(at -55.88 22.86 0)
				(length 5.08)
				(name "PD3")
				(number "7")
			)
			(pin bidirectional line
				(at 53.34 -25.4 180)
				(length 5.08)
				(name "PD3")
				(number "70")
			)
			(pin bidirectional line
				(at 53.34 -22.86 180)
				(length 5.08)
				(name "PD3")
				(number "71")
			)
			(pin bidirectional line
				(at 53.34 -20.32 180)
				(length 5.08)
				(name "PD3")
				(number "72")
			)
			(pin bidirectional line
				(at 53.34 -17.78 180)
				(length 5.08)
				(name "PD3")
				(number "73")
			)
			(pin bidirectional line
				(at 53.34 -15.24 180)
				(length 5.08)
				(name "PD3")
				(number "74")
			)
			(pin bidirectional line
				(at 53.34 -12.7 180)
				(length 5.08)
				(name "PD3")
				(number "75")
			)
			(pin bidirectional line
				(at 53.34 -10.16 180)
				(length 5.08)
				(name "PE3")
				(number "76")
			)
			(pin bidirectional line
				(at 53.34 -7.62 180)
				(length 5.08)
				(name "PE2")
				(number "77")
			)
			(pin bidirectional line
				(at 53.34 -5.08 180)
				(length 5.08)
				(name "PE1")
				(number "78")
			)
			(pin bidirectional line
				(at 53.34 -2.54 180)
				(length 5.08)
				(name "PE0")
				(number "79")
			)
			(pin bidirectional line
				(at -55.88 20.32 0)
				(length 5.08)
				(name "PD3")
				(number "8")
			)
			(pin bidirectional line
				(at 53.34 0 180)
				(length 5.08)
				(name "PE0")
				(number "80")
			)
			(pin bidirectional line
				(at 53.34 2.54 180)
				(length 5.08)
				(name "PE0")
				(number "81")
			)
			(pin bidirectional line
				(at 53.34 5.08 180)
				(length 5.08)
				(name "PE0")
				(number "82")
			)
			(pin bidirectional line
				(at 53.34 7.62 180)
				(length 5.08)
				(name "PE0")
				(number "83")
			)
			(pin bidirectional line
				(at 53.34 10.16 180)
				(length 5.08)
				(name "PE0")
				(number "84")
			)
			(pin bidirectional line
				(at 53.34 12.7 180)
				(length 5.08)
				(name "PE0")
				(number "85")
			)
			(pin bidirectional line
				(at 53.34 15.24 180)
				(length 5.08)
				(name "PC7")
				(number "86")
			)
			(pin bidirectional line
				(at 53.34 17.78 180)
				(length 5.08)
				(name "PC6")
				(number "87")
			)
			(pin bidirectional line
				(at 53.34 20.32 180)
				(length 5.08)
				(name "PC5")
				(number "88")
			)
			(pin bidirectional line
				(at 53.34 22.86 180)
				(length 5.08)
				(name "PC4")
				(number "89")
			)
			(pin bidirectional line
				(at -55.88 17.78 0)
				(length 5.08)
				(name "PD3")
				(number "9")
			)
			(pin bidirectional line
				(at 53.34 25.4 180)
				(length 5.08)
				(name "PE0")
				(number "90")
			)
			(pin bidirectional line
				(at 53.34 27.94 180)
				(length 5.08)
				(name "PB2")
				(number "91")
			)
			(pin bidirectional line
				(at 53.34 30.48 180)
				(length 5.08)
				(name "PB3")
				(number "92")
			)
			(pin bidirectional line
				(at 53.34 33.02 180)
				(length 5.08)
				(name "PH0")
				(number "93")
			)
			(pin bidirectional line
				(at 53.34 35.56 180)
				(length 5.08)
				(name "PH1")
				(number "94")
			)
			(pin bidirectional line
				(at 53.34 38.1 180)
				(length 5.08)
				(name "PB0")
				(number "95")
			)
			(pin bidirectional line
				(at 53.34 40.64 180)
				(length 5.08)
				(name "PB1")
				(number "96")
			)
			(pin bidirectional line
				(at 38.1 50.8 270)
				(length 5.08)
				(name "huh")
				(number "97")
			)
			(pin bidirectional line
				(at 35.56 50.8 270)
				(length 5.08)
				(name "PD1")
				(number "98")
			)
			(pin bidirectional line
				(at 33.02 50.8 270)
				(length 5.08)
				(name "PD2")
				(number "99")
			)
		)
		(symbol "TM4C1290NCPDT_2_0"
			(pin bidirectional line
				(at 17.78 20.32 180)
				(length 5.08)
				(name "PQ4")
				(number "102")
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 5.08)
				(name "PP2")
				(number "103")
			)
			(pin bidirectional line
				(at 17.78 0 180)
				(length 5.08)
				(name "PP3")
				(number "104")
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 5.08)
				(name "PP4")
				(number "105")
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 5.08)
				(name "PP5")
				(number "106")
			)
			(pin bidirectional line
				(at 17.78 -25.4 180)
				(length 5.08)
				(name "PN0")
				(number "107")
			)
			(pin bidirectional line
				(at 17.78 -22.86 180)
				(length 5.08)
				(name "PN1")
				(number "108")
			)
			(pin bidirectional line
				(at 17.78 -20.32 180)
				(length 5.08)
				(name "PN2")
				(number "109")
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 5.08)
				(name "PQ2")
				(number "11")
			)
			(pin bidirectional line
				(at 17.78 -17.78 180)
				(length 5.08)
				(name "PN3")
				(number "110")
			)
			(pin bidirectional line
				(at 17.78 -15.24 180)
				(length 5.08)
				(name "PN4")
				(number "111")
			)
			(pin bidirectional line
				(at 17.78 -12.7 180)
				(length 5.08)
				(name "PN5")
				(number "112")
			)
			(pin bidirectional line
				(at 17.78 -7.62 180)
				(length 5.08)
				(name "PP0")
				(number "118")
			)
			(pin bidirectional line
				(at 17.78 -5.08 180)
				(length 5.08)
				(name "PP1")
				(number "119")
			)
			(pin bidirectional line
				(at -17.78 30.48 0)
				(length 5.08)
				(name "PK0")
				(number "18")
			)
			(pin bidirectional line
				(at -17.78 27.94 0)
				(length 5.08)
				(name "PK1")
				(number "19")
			)
			(pin bidirectional line
				(at -17.78 25.4 0)
				(length 5.08)
				(name "PK2")
				(number "20")
			)
			(pin bidirectional line
				(at -17.78 22.86 0)
				(length 5.08)
				(name "PK3")
				(number "21")
			)
			(pin bidirectional line
				(at 17.78 17.78 180)
				(length 5.08)
				(name "PQ3")
				(number "27")
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 5.08)
				(name "PQ0")
				(number "5")
			)
			(pin bidirectional line
				(at 17.78 22.86 180)
				(length 5.08)
				(name "PQ5")
				(number "57")
			)
			(pin bidirectional line
				(at 17.78 25.4 180)
				(length 5.08)
				(name "PQ6")
				(number "58")
			)
			(pin bidirectional line
				(at -17.78 12.7 0)
				(length 5.08)
				(name "PK7")
				(number "59")
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 5.08)
				(name "PQ1")
				(number "6")
			)
			(pin bidirectional line
				(at -17.78 15.24 0)
				(length 5.08)
				(name "PK6")
				(number "60")
			)
			(pin bidirectional line
				(at -17.78 17.78 0)
				(length 5.08)
				(name "PK5")
				(number "61")
			)
			(pin bidirectional line
				(at -17.78 20.32 0)
				(length 5.08)
				(name "PK4")
				(number "62")
			)
			(pin bidirectional line
				(at -17.78 -33.02 0)
				(length 5.08)
				(name "PM7")
				(number "71")
			)
			(pin bidirectional line
				(at -17.78 -30.48 0)
				(length 5.08)
				(name "PM6")
				(number "72")
			)
			(pin bidirectional line
				(at -17.78 -27.94 0)
				(length 5.08)
				(name "PM5")
				(number "73")
			)
			(pin bidirectional line
				(at -17.78 -25.4 0)
				(length 5.08)
				(name "PM4")
				(number "74")
			)
			(pin bidirectional line
				(at -17.78 -22.86 0)
				(length 5.08)
				(name "PM3")
				(number "75")
			)
			(pin bidirectional line
				(at -17.78 -20.32 0)
				(length 5.08)
				(name "PM2")
				(number "76")
			)
			(pin bidirectional line
				(at -17.78 -17.78 0)
				(length 5.08)
				(name "PM1")
				(number "77")
			)
			(pin bidirectional line
				(at -17.78 -15.24 0)
				(length 5.08)
				(name "PM0")
				(number "78")
			)
			(pin bidirectional line
				(at -17.78 7.62 0)
				(length 5.08)
				(name "PL0")
				(number "81")
			)
			(pin bidirectional line
				(at -17.78 5.08 0)
				(length 5.08)
				(name "PL1")
				(number "82")
			)
			(pin bidirectional line
				(at -17.78 2.54 0)
				(length 5.08)
				(name "PL2")
				(number "83")
			)
			(pin bidirectional line
				(at -17.78 0 0)
				(length 5.08)
				(name "PL3")
				(number "84")
			)
			(pin bidirectional line
				(at -17.78 -2.54 0)
				(length 5.08)
				(name "PL4")
				(number "85")
			)
			(pin bidirectional line
				(at -17.78 -5.08 0)
				(length 5.08)
				(name "PL5")
				(number "86")
			)
			(pin bidirectional line
				(at -17.78 -10.16 0)
				(length 5.08)
				(name "PL7")
				(number "93")
			)
			(pin bidirectional line
				(at -17.78 -7.62 0)
				(length 5.08)
				(name "PL6")
				(number "94")
			)
		)
		(symbol "TM4C1290NCPDT_3_0"
			(pin bidirectional line
				(at 22.86 5.08 180)
				(length 5.08)
				(name "TCK/PC0/SWCLK")
				(number "100")
			)
			(pin input line
				(at -22.86 7.62 0)
				(length 5.08)
				(name "~{WAKE}")
				(number "64")
			)
			(pin output line
				(at -22.86 5.08 0)
				(length 5.08)
				(name "~{HIB}")
				(number "65")
			)
			(pin input line
				(at -22.86 0 0)
				(length 5.08)
				(name "XOSC0")
				(number "66")
			)
			(pin output line
				(at -22.86 -2.54 0)
				(length 5.08)
				(name "XOSC1")
				(number "67")
			)
			(pin input line
				(at -22.86 -7.62 0)
				(length 5.08)
				(name "~{RST}")
				(number "70")
			)
			(pin input line
				(at -22.86 -12.7 0)
				(length 5.08)
				(name "OSC0")
				(number "88")
			)
			(pin output line
				(at -22.86 -15.24 0)
				(length 5.08)
				(name "OSC1")
				(number "89")
			)
			(pin input line
				(at -22.86 12.7 0)
				(length 5.08)
				(name "VREFA+")
				(number "9")
			)
			(pin bidirectional line
				(at 22.86 12.7 180)
				(length 5.08)
				(name "TDO/PC3/SWO")
				(number "97")
			)
			(pin bidirectional line
				(at 22.86 10.16 180)
				(length 5.08)
				(name "TDI/PC2")
				(number "98")
			)
			(pin bidirectional line
				(at 22.86 7.62 180)
				(length 5.08)
				(name "TMS/PC1/SWDIO")
				(number "99")
			)
		)
		(symbol "TM4C1290NCPDT_4_0"
			(pin power_in line
				(at 20.32 -27.94 180)
				(length 5.08)
				(name "GNDA")
				(number "10")
			)
			(pin power_in line
				(at -20.32 2.54 0)
				(length 5.08)
				(name "VDD_101")
				(number "101")
			)
			(pin power_in line
				(at -20.32 0 0)
				(length 5.08)
				(name "VDD_113")
				(number "113")
			)
			(pin power_in line
				(at 20.32 -25.4 180)
				(length 5.08)
				(name "GND_114")
				(number "114")
			)
			(pin power_in line
				(at -20.32 -10.16 0)
				(length 5.08)
				(name "VDDC_115")
				(number "115")
			)
			(pin power_in line
				(at -20.32 -2.54 0)
				(length 5.08)
				(name "VDD_122")
				(number "122")
			)
			(pin power_in line
				(at -20.32 25.4 0)
				(length 5.08)
				(name "VDD_16")
				(number "16")
			)
			(pin power_in line
				(at 20.32 -17.78 180)
				(length 5.08)
				(name "GND_17")
				(number "17")
			)
			(pin power_in line
				(at -20.32 22.86 0)
				(length 5.08)
				(name "VDD_26")
				(number "26")
			)
			(pin power_in line
				(at -20.32 20.32 0)
				(length 5.08)
				(name "VDD_28")
				(number "28")
			)
			(pin power_in line
				(at -20.32 17.78 0)
				(length 5.08)
				(name "VDD_39")
				(number "39")
			)
			(pin power_in line
				(at -20.32 15.24 0)
				(length 5.08)
				(name "VDD_47")
				(number "47")
			)
			(pin power_in line
				(at 20.32 -20.32 180)
				(length 5.08)
				(name "GND_48")
				(number "48")
			)
			(pin power_in line
				(at -20.32 12.7 0)
				(length 5.08)
				(name "VDD_63")
				(number "63")
			)
			(pin power_in line
				(at 20.32 27.94 180)
				(length 5.08)
				(name "VBAT")
				(number "68")
			)
			(pin power_in line
				(at -20.32 10.16 0)
				(length 5.08)
				(name "VDD_69")
				(number "69")
			)
			(pin power_in line
				(at -20.32 27.94 0)
				(length 5.08)
				(name "VDD_7")
				(number "7")
			)
			(pin power_in line
				(at -20.32 7.62 0)
				(length 5.08)
				(name "VDD_79")
				(number "79")
			)
			(pin power_in line
				(at -20.32 -5.08 0)
				(length 5.08)
				(name "VDDA")
				(number "8")
			)
			(pin power_in line
				(at 20.32 -22.86 180)
				(length 5.08)
				(name "GND_80")
				(number "80")
			)
			(pin power_in line
				(at -20.32 -7.62 0)
				(length 5.08)
				(name "VDDC_87")
				(number "87")
			)
			(pin power_in line
				(at -20.32 5.08 0)
				(length 5.08)
				(name "VDD_90")
				(number "90")
			)
		)
	)
	(symbol "TM4C1290NCPDTI3R"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -12.7 39.37 0)
		)
		(property "Value" "TM4C1290NCPDTI3R"
			(at -12.7 -40.64 0)
		)
		(property "Footprint" "ProjectFootprints:TM4C1290N_128N"
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(property "PartNum" "TM4C1290NCPDTI3R"
			(at 0 0 0)
		)
		(property "VendorNum" ""
			(at 0 0 0)
		)
		(property "Vendor" ""
			(at 0 0 0)
		)
		(property "Subst" ""
			(at 0 0 0)
		)
		(symbol "TM4C1290NCPDTI3R_1_0"
			(pin bidirectional line
				(at -17.78 -17.78 0)
				(length 5.08)
				(name "PD0")
				(number "1")
			)
			(pin bidirectional line
				(at 17.78 33.02 180)
				(length 5.08)
				(name "PJ0")
				(number "116")
			)
			(pin bidirectional line
				(at 17.78 35.56 180)
				(length 5.08)
				(name "PJ1")
				(number "117")
			)
			(pin bidirectional line
				(at 17.78 -27.94 180)
				(length 5.08)
				(name "PE3")
				(number "12")
			)
			(pin bidirectional line
				(at -17.78 0 0)
				(length 5.08)
				(name "PB5")
				(number "120")
			)
			(pin bidirectional line
				(at -17.78 2.54 0)
				(length 5.08)
				(name "PB4")
				(number "121")
			)
			(pin bidirectional line
				(at 17.78 -25.4 180)
				(length 5.08)
				(name "PE4")
				(number "123")
			)
			(pin bidirectional line
				(at 17.78 -22.86 180)
				(length 5.08)
				(name "PE5")
				(number "124")
			)
			(pin bidirectional line
				(at -17.78 -27.94 0)
				(length 5.08)
				(name "PD4")
				(number "125")
			)
			(pin bidirectional line
				(at -17.78 -30.48 0)
				(length 5.08)
				(name "PD5")
				(number "126")
			)
			(pin bidirectional line
				(at -17.78 -33.02 0)
				(length 5.08)
				(name "PD6")
				(number "127")
			)
			(pin bidirectional line
				(at -17.78 -35.56 0)
				(length 5.08)
				(name "PD7")
				(number "128")
			)
			(pin bidirectional line
				(at 17.78 -30.48 180)
				(length 5.08)
				(name "PE2")
				(number "13")
			)
			(pin bidirectional line
				(at 17.78 -33.02 180)
				(length 5.08)
				(name "PE1")
				(number "14")
			)
			(pin bidirectional line
				(at 17.78 -35.56 180)
				(length 5.08)
				(name "PE0")
				(number "15")
			)
			(pin bidirectional line
				(at -17.78 -20.32 0)
				(length 5.08)
				(name "PD1")
				(number "2")
			)
			(pin bidirectional line
				(at -17.78 -12.7 0)
				(length 5.08)
				(name "PC7")
				(number "22")
			)
			(pin bidirectional line
				(at -17.78 -10.16 0)
				(length 5.08)
				(name "PC6")
				(number "23")
			)
			(pin bidirectional line
				(at -17.78 -7.62 0)
				(length 5.08)
				(name "PC5")
				(number "24")
			)
			(pin bidirectional line
				(at -17.78 -5.08 0)
				(length 5.08)
				(name "PC4")
				(number "25")
			)
			(pin bidirectional line
				(at 17.78 20.32 180)
				(length 5.08)
				(name "PH0")
				(number "29")
			)
			(pin bidirectional line
				(at -17.78 -22.86 0)
				(length 5.08)
				(name "PD2")
				(number "3")
			)
			(pin bidirectional line
				(at 17.78 22.86 180)
				(length 5.08)
				(name "PH1")
				(number "30")
			)
			(pin bidirectional line
				(at 17.78 25.4 180)
				(length 5.08)
				(name "PH2")
				(number "31")
			)
			(pin bidirectional line
				(at 17.78 27.94 180)
				(length 5.08)
				(name "PH3")
				(number "32")
			)
			(pin bidirectional line
				(at -17.78 35.56 0)
				(length 5.08)
				(name "PA0")
				(number "33")
			)
			(pin bidirectional line
				(at -17.78 33.02 0)
				(length 5.08)
				(name "PA1")
				(number "34")
			)
			(pin bidirectional line
				(at -17.78 30.48 0)
				(length 5.08)
				(name "PA2")
				(number "35")
			)
			(pin bidirectional line
				(at -17.78 27.94 0)
				(length 5.08)
				(name "PA3")
				(number "36")
			)
			(pin bidirectional line
				(at -17.78 25.4 0)
				(length 5.08)
				(name "PA4")
				(number "37")
			)
			(pin bidirectional line
				(at -17.78 22.86 0)
				(length 5.08)
				(name "PA5")
				(number "38")
			)
			(pin bidirectional line
				(at -17.78 -25.4 0)
				(length 5.08)
				(name "PD3")
				(number "4")
			)
			(pin bidirectional line
				(at -17.78 20.32 0)
				(length 5.08)
				(name "PA6")
				(number "40")
			)
			(pin bidirectional line
				(at -17.78 17.78 0)
				(length 5.08)
				(name "PA7")
				(number "41")
			)
			(pin bidirectional line
				(at 17.78 -17.78 180)
				(length 5.08)
				(name "PF0")
				(number "42")
			)
			(pin bidirectional line
				(at 17.78 -15.24 180)
				(length 5.08)
				(name "PF1")
				(number "43")
			)
			(pin bidirectional line
				(at 17.78 -12.7 180)
				(length 5.08)
				(name "PF2")
				(number "44")
			)
			(pin bidirectional line
				(at 17.78 -10.16 180)
				(length 5.08)
				(name "PF3")
				(number "45")
			)
			(pin bidirectional line
				(at 17.78 -7.62 180)
				(length 5.08)
				(name "PF4")
				(number "46")
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 5.08)
				(name "PG0")
				(number "49")
			)
			(pin bidirectional line
				(at 17.78 0 180)
				(length 5.08)
				(name "PG1")
				(number "50")
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 5.08)
				(name "PG2")
				(number "51")
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 5.08)
				(name "PG3")
				(number "52")
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 5.08)
				(name "PG4")
				(number "53")
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 5.08)
				(name "PG5")
				(number "54")
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 5.08)
				(name "PG6")
				(number "55")
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 5.08)
				(name "PG7")
				(number "56")
			)
			(pin bidirectional line
				(at -17.78 7.62 0)
				(length 5.08)
				(name "PB2")
				(number "91")
			)
			(pin bidirectional line
				(at -17.78 5.08 0)
				(length 5.08)
				(name "PB3")
				(number "92")
			)
			(pin bidirectional line
				(at -17.78 12.7 0)
				(length 5.08)
				(name "PB0")
				(number "95")
			)
			(pin bidirectional line
				(at -17.78 10.16 0)
				(length 5.08)
				(name "PB1")
				(number "96")
			)
		)
		(symbol "TM4C1290NCPDTI3R_2_0"
			(pin bidirectional line
				(at 17.78 20.32 180)
				(length 5.08)
				(name "PQ4")
				(number "102")
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 5.08)
				(name "PP2")
				(number "103")
			)
			(pin bidirectional line
				(at 17.78 0 180)
				(length 5.08)
				(name "PP3")
				(number "104")
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 5.08)
				(name "PP4")
				(number "105")
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 5.08)
				(name "PP5")
				(number "106")
			)
			(pin bidirectional line
				(at 17.78 -25.4 180)
				(length 5.08)
				(name "PN0")
				(number "107")
			)
			(pin bidirectional line
				(at 17.78 -22.86 180)
				(length 5.08)
				(name "PN1")
				(number "108")
			)
			(pin bidirectional line
				(at 17.78 -20.32 180)
				(length 5.08)
				(name "PN2")
				(number "109")
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 5.08)
				(name "PQ2")
				(number "11")
			)
			(pin bidirectional line
				(at 17.78 -17.78 180)
				(length 5.08)
				(name "PN3")
				(number "110")
			)
			(pin bidirectional line
				(at 17.78 -15.24 180)
				(length 5.08)
				(name "PN4")
				(number "111")
			)
			(pin bidirectional line
				(at 17.78 -12.7 180)
				(length 5.08)
				(name "PN5")
				(number "112")
			)
			(pin bidirectional line
				(at 17.78 -7.62 180)
				(length 5.08)
				(name "PP0")
				(number "118")
			)
			(pin bidirectional line
				(at 17.78 -5.08 180)
				(length 5.08)
				(name "PP1")
				(number "119")
			)
			(pin bidirectional line
				(at -17.78 30.48 0)
				(length 5.08)
				(name "PK0")
				(number "18")
			)
			(pin bidirectional line
				(at -17.78 27.94 0)
				(length 5.08)
				(name "PK1")
				(number "19")
			)
			(pin bidirectional line
				(at -17.78 25.4 0)
				(length 5.08)
				(name "PK2")
				(number "20")
			)
			(pin bidirectional line
				(at -17.78 22.86 0)
				(length 5.08)
				(name "PK3")
				(number "21")
			)
			(pin bidirectional line
				(at 17.78 17.78 180)
				(length 5.08)
				(name "PQ3")
				(number "27")
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 5.08)
				(name "PQ0")
				(number "5")
			)
			(pin bidirectional line
				(at 17.78 22.86 180)
				(length 5.08)
				(name "PQ5")
				(number "57")
			)
			(pin bidirectional line
				(at 17.78 25.4 180)
				(length 5.08)
				(name "PQ6")
				(number "58")
			)
			(pin bidirectional line
				(at -17.78 12.7 0)
				(length 5.08)
				(name "PK7")
				(number "59")
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 5.08)
				(name "PQ1")
				(number "6")
			)
			(pin bidirectional line
				(at -17.78 15.24 0)
				(length 5.08)
				(name "PK6")
				(number "60")
			)
			(pin bidirectional line
				(at -17.78 17.78 0)
				(length 5.08)
				(name "PK5")
				(number "61")
			)
			(pin bidirectional line
				(at -17.78 20.32 0)
				(length 5.08)
				(name "PK4")
				(number "62")
			)
			(pin bidirectional line
				(at -17.78 -33.02 0)
				(length 5.08)
				(name "PM7")
				(number "71")
			)
			(pin bidirectional line
				(at -17.78 -30.48 0)
				(length 5.08)
				(name "PM6")
				(number "72")
			)
			(pin bidirectional line
				(at -17.78 -27.94 0)
				(length 5.08)
				(name "PM5")
				(number "73")
			)
			(pin bidirectional line
				(at -17.78 -25.4 0)
				(length 5.08)
				(name "PM4")
				(number "74")
			)
			(pin bidirectional line
				(at -17.78 -22.86 0)
				(length 5.08)
				(name "PM3")
				(number "75")
			)
			(pin bidirectional line
				(at -17.78 -20.32 0)
				(length 5.08)
				(name "PM2")
				(number "76")
			)
			(pin bidirectional line
				(at -17.78 -17.78 0)
				(length 5.08)
				(name "PM1")
				(number "77")
			)
			(pin bidirectional line
				(at -17.78 -15.24 0)
				(length 5.08)
				(name "PM0")
				(number "78")
			)
			(pin bidirectional line
				(at -17.78 7.62 0)
				(length 5.08)
				(name "PL0")
				(number "81")
			)
			(pin bidirectional line
				(at -17.78 5.08 0)
				(length 5.08)
				(name "PL1")
				(number "82")
			)
			(pin bidirectional line
				(at -17.78 2.54 0)
				(length 5.08)
				(name "PL2")
				(number "83")
			)
			(pin bidirectional line
				(at -17.78 0 0)
				(length 5.08)
				(name "PL3")
				(number "84")
			)
			(pin bidirectional line
				(at -17.78 -2.54 0)
				(length 5.08)
				(name "PL4")
				(number "85")
			)
			(pin bidirectional line
				(at -17.78 -5.08 0)
				(length 5.08)
				(name "PL5")
				(number "86")
			)
			(pin bidirectional line
				(at -17.78 -10.16 0)
				(length 5.08)
				(name "PL7")
				(number "93")
			)
			(pin bidirectional line
				(at -17.78 -7.62 0)
				(length 5.08)
				(name "PL6")
				(number "94")
			)
		)
		(symbol "TM4C1290NCPDTI3R_3_0"
			(pin bidirectional line
				(at 22.86 5.08 180)
				(length 5.08)
				(name "TCK/PC0/SWCLK")
				(number "100")
			)
			(pin input line
				(at -22.86 7.62 0)
				(length 5.08)
				(name "~{WAKE}")
				(number "64")
			)
			(pin output line
				(at -22.86 5.08 0)
				(length 5.08)
				(name "~{HIB}")
				(number "65")
			)
			(pin input line
				(at -22.86 0 0)
				(length 5.08)
				(name "XOSC0")
				(number "66")
			)
			(pin output line
				(at -22.86 -2.54 0)
				(length 5.08)
				(name "XOSC1")
				(number "67")
			)
			(pin input line
				(at -22.86 -7.62 0)
				(length 5.08)
				(name "~{RST}")
				(number "70")
			)
			(pin input line
				(at -22.86 -12.7 0)
				(length 5.08)
				(name "OSC0")
				(number "88")
			)
			(pin output line
				(at -22.86 -15.24 0)
				(length 5.08)
				(name "OSC1")
				(number "89")
			)
			(pin input line
				(at -22.86 12.7 0)
				(length 5.08)
				(name "VREFA+")
				(number "9")
			)
			(pin bidirectional line
				(at 22.86 12.7 180)
				(length 5.08)
				(name "TDO/PC3/SWO")
				(number "97")
			)
			(pin bidirectional line
				(at 22.86 10.16 180)
				(length 5.08)
				(name "TDI/PC2")
				(number "98")
			)
			(pin bidirectional line
				(at 22.86 7.62 180)
				(length 5.08)
				(name "TMS/PC1/SWDIO")
				(number "99")
			)
		)
		(symbol "TM4C1290NCPDTI3R_4_0"
			(pin power_in line
				(at 20.32 -27.94 180)
				(length 5.08)
				(name "GNDA")
				(number "10")
			)
			(pin power_in line
				(at -20.32 2.54 0)
				(length 5.08)
				(name "VDD_101")
				(number "101")
			)
			(pin power_in line
				(at -20.32 0 0)
				(length 5.08)
				(name "VDD_113")
				(number "113")
			)
			(pin power_in line
				(at 20.32 -25.4 180)
				(length 5.08)
				(name "GND_114")
				(number "114")
			)
			(pin power_in line
				(at -20.32 -10.16 0)
				(length 5.08)
				(name "VDDC_115")
				(number "115")
			)
			(pin power_in line
				(at -20.32 -2.54 0)
				(length 5.08)
				(name "VDD_122")
				(number "122")
			)
			(pin power_in line
				(at -20.32 25.4 0)
				(length 5.08)
				(name "VDD_16")
				(number "16")
			)
			(pin power_in line
				(at 20.32 -17.78 180)
				(length 5.08)
				(name "GND_17")
				(number "17")
			)
			(pin power_in line
				(at -20.32 22.86 0)
				(length 5.08)
				(name "VDD_26")
				(number "26")
			)
			(pin power_in line
				(at -20.32 20.32 0)
				(length 5.08)
				(name "VDD_28")
				(number "28")
			)
			(pin power_in line
				(at -20.32 17.78 0)
				(length 5.08)
				(name "VDD_39")
				(number "39")
			)
			(pin power_in line
				(at -20.32 15.24 0)
				(length 5.08)
				(name "VDD_47")
				(number "47")
			)
			(pin power_in line
				(at 20.32 -20.32 180)
				(length 5.08)
				(name "GND_48")
				(number "48")
			)
			(pin power_in line
				(at -20.32 12.7 0)
				(length 5.08)
				(name "VDD_63")
				(number "63")
			)
			(pin power_in line
				(at 20.32 27.94 180)
				(length 5.08)
				(name "VBAT")
				(number "68")
			)
			(pin power_in line
				(at -20.32 10.16 0)
				(length 5.08)
				(name "VDD_69")
				(number "69")
			)
			(pin power_in line
				(at -20.32 27.94 0)
				(length 5.08)
				(name "VDD_7")
				(number "7")
			)
			(pin power_in line
				(at -20.32 7.62 0)
				(length 5.08)
				(name "VDD_79")
				(number "79")
			)
			(pin power_in line
				(at -20.32 -5.08 0)
				(length 5.08)
				(name "VDDA")
				(number "8")
			)
			(pin power_in line
				(at 20.32 -22.86 180)
				(length 5.08)
				(name "GND_80")
				(number "80")
			)
			(pin power_in line
				(at -20.32 -7.62 0)
				(length 5.08)
				(name "VDDC_87")
				(number "87")
			)
			(pin power_in line
				(at -20.32 5.08 0)
				(length 5.08)
				(name "VDD_90")
				(number "90")
			)
		)
	)
	(symbol "TPH1R306P1_L1Q"
		(pin_names
			(offset 0.254)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 22.86 7.62 0)
		)
		(property "Value" "TPH1R306P1_L1Q"
			(at 22.86 5.08 0)
		)
		(property "Footprint" "IC8_TPH1R306P1_TOS"
			(at 22.86 3.556 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_fp_filters" "IC8_TPH1R306P1_TOS IC8_TPH1R306P1_TOS-M IC8_TPH1R306P1_TOS-L"
			(at 0 0 0)
		)
		(symbol "TPH1R306P1_L1Q_1_1"
			(pin unspecified line
				(at 0 0 0)
				(length 7.62)
				(name "Source")
				(number "1")
			)
			(pin unspecified line
				(at 0 -5.08 0)
				(length 7.62)
				(name "Source")
				(number "2")
			)
			(pin unspecified line
				(at 0 -10.16 0)
				(length 7.62)
				(name "Source")
				(number "3")
			)
			(pin unspecified line
				(at 0 -15.24 0)
				(length 7.62)
				(name "Gate")
				(number "4")
			)
			(pin unspecified line
				(at 45.72 -15.24 180)
				(length 7.62)
				(name "Drain")
				(number "5")
			)
			(pin unspecified line
				(at 45.72 -10.16 180)
				(length 7.62)
				(name "Drain")
				(number "6")
			)
			(pin unspecified line
				(at 45.72 -5.08 180)
				(length 7.62)
				(name "Drain")
				(number "7")
			)
			(pin unspecified line
				(at 45.72 0 180)
				(length 7.62)
				(name "Drain")
				(number "8")
			)
		)
	)
	(symbol "TPH1R306PL"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "Q"
			(at 10.16 1.27 0)
		)
		(property "Value" "TPH1R306PL"
			(at 10.16 -1.27 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "TPH1R306PL_1_1"
			(pin power_in line
				(at 2.54 -5.08 90)
				(length 1.27)
				(name "S")
				(number "1")
			)
			(pin bidirectional line
				(at 1.27 -5.08 90)
				(length 1.27)
				(name "S")
				(number "2")
			)
			(pin bidirectional line
				(at 0 -5.08 90)
				(length 1.27)
				(name "S")
				(number "3")
			)
			(pin passive line
				(at -5.08 -1.27 0)
				(length 1.27)
				(name "G")
				(number "4")
			)
			(pin passive line
				(at -1.27 5.08 270)
				(length 1.27)
				(name "D")
				(number "5")
			)
			(pin power_in line
				(at 0 5.08 270)
				(length 1.27)
				(name "D")
				(number "6")
			)
			(pin power_in line
				(at 1.27 5.08 270)
				(length 1.27)
				(name "D")
				(number "7")
			)
			(pin power_in line
				(at 2.54 5.08 270)
				(length 1.27)
				(name "D")
				(number "8")
			)
		)
	)
	(symbol "TPH1R306PL,L1Q"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "Q"
			(at 10.16 1.27 0)
		)
		(property "Value" "TPH1R306PL,L1Q"
			(at 11.43 -1.27 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "TPH1R306PL,L1Q_0_1")
		(symbol "TPH1R306PL,L1Q_1_1"
			(pin power_in line
				(at 3.81 -6.35 90)
				(length 1.27)
				(name "S")
				(number "1")
			)
			(pin bidirectional line
				(at 2.54 -6.35 90)
				(length 1.27)
				(name "S")
				(number "2")
			)
			(pin bidirectional line
				(at 1.27 -6.35 90)
				(length 1.27)
				(name "S")
				(number "3")
			)
			(pin passive line
				(at -5.08 -1.27 0)
				(length 1.27)
				(name "G")
				(number "4")
			)
			(pin power_in line
				(at 1.27 5.08 270)
				(length 1.27)
				(name "D")
				(number "5")
			)
		)
	)
	(symbol "TPL5010"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 2.54 7.62 0)
		)
		(property "Value" "TPL5010"
			(at 0 0 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-6"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tpl5010.pdf"
			(at 0 0 0)
		)
		(property "Description" "IC OSC PROG TIMER TSOT23-6"
			(at 0 0 0)
		)
		(symbol "TPL5010_1_1"
			(pin power_in line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "VDD")
				(number "1")
			)
			(pin power_in line
				(at -10.16 0 0)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "M_RST")
				(number "3")
			)
			(pin input line
				(at 10.16 0 180)
				(length 2.54)
				(name "DONE")
				(number "4")
			)
			(pin output line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "WAKE")
				(number "5")
			)
			(pin open_collector line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "~{RST}")
				(number "6")
			)
		)
	)
	(symbol "TPS3435CAKAGDDFR"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 10.16 0)
		)
		(property "Value" "TPS3435CAKAGDDFR"
			(at -10.16 -7.62 0)
		)
		(property "Footprint" "ProjectFootprints:TPS3435_SOP65P280X110-8N"
			(at 0 -20.32 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/tps3435.pdf"
			(at 0 -17.78 0)
		)
		(property "Description" "TPS3435CAKAGDDFR"
			(at 0 0 0)
		)
		(symbol "TPS3435CAKAGDDFR_0_0"
			(pin input line
				(at -12.7 5.08 0)
				(length 5.08)
				(name "SET0")
				(number "1")
			)
			(pin input line
				(at -12.7 2.54 0)
				(length 5.08)
				(name "~{MR}")
				(number "2")
			)
			(pin input line
				(at -12.7 0 0)
				(length 5.08)
				(name "WDI")
				(number "3")
			)
			(pin power_in line
				(at -12.7 -2.54 0)
				(length 5.08)
				(name "GND")
				(number "4")
			)
			(pin input line
				(at 10.16 -2.54 180)
				(length 5.08)
				(name "SET1")
				(number "5")
			)
			(pin input line
				(at 10.16 0 180)
				(length 5.08)
				(name "WD-EN")
				(number "6")
			)
			(pin output line
				(at 10.16 2.54 180)
				(length 5.08)
				(name "~{WDO}")
				(number "7")
			)
			(pin power_in line
				(at 10.16 5.08 180)
				(length 5.08)
				(name "VDD")
				(number "8")
			)
		)
		(symbol "TPS3435CAKAGDDFR_1_1")
	)
	(symbol "TPS552892"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -12.7 30.48 0)
		)
		(property "Value" "TPS552892"
			(at -12.7 -30.48 0)
		)
		(property "Footprint" "ProjectFootprints:CONV_TPS552892RYQR"
			(at 0.254 -40.894 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/tps55289.pdf"
			(at 1.016 -33.528 0)
		)
		(property "Description" "36-V 8-A fully-integrated buck-boost converter"
			(at 0.508 -37.846 0)
		)
		(property "PartNum" "TPS552892RYQR"
			(at 1.27 28.956 0)
		)
		(property "VendorNum" "296-TPS55289RYQRCT-ND"
			(at 0.762 -31.75 0)
		)
		(property "Vendor" "Digikey"
			(at -6.35 -35.814 0)
		)
		(property "Subst" "No"
			(at 0.508 -35.814 0)
		)
		(symbol "TPS552892_0_0"
			(pin input line
				(at -17.78 5.08 0)
				(length 5.08)
				(name "EN/UVLO")
				(number "1")
			)
			(pin power_in line
				(at 17.78 10.16 180)
				(length 5.08)
				(name "SW2")
				(number "10")
			)
			(pin power_in line
				(at 17.78 17.78 180)
				(length 5.08)
				(name "VOUT")
				(number "11")
			)
			(pin input line
				(at -17.78 -15.24 0)
				(length 5.08)
				(name "ISP")
				(number "12")
			)
			(pin input line
				(at -17.78 -17.78 0)
				(length 5.08)
				(name "ISN")
				(number "13")
			)
			(pin input line
				(at -17.78 -2.54 0)
				(length 5.08)
				(name "FB")
				(number "14")
			)
			(pin output line
				(at 17.78 -12.7 180)
				(length 5.08)
				(name "COMP")
				(number "15")
			)
			(pin output line
				(at 17.78 -10.16 180)
				(length 5.08)
				(name "CDC")
				(number "16")
			)
			(pin power_in line
				(at 17.78 -25.4 180)
				(length 5.08)
				(name "AGND")
				(number "17")
			)
			(pin power_in line
				(at 17.78 22.86 180)
				(length 5.08)
				(name "VCC")
				(number "18")
			)
			(pin output line
				(at 17.78 -5.08 180)
				(length 5.08)
				(name "BOOT2")
				(number "19")
			)
			(pin input line
				(at -17.78 2.54 0)
				(length 5.08)
				(name "MODE")
				(number "2")
			)
			(pin output line
				(at 17.78 -2.54 180)
				(length 5.08)
				(name "BOOT1")
				(number "20")
			)
			(pin power_in line
				(at 17.78 25.4 180)
				(length 5.08)
				(name "EXTVCC")
				(number "21")
			)
			(pin output line
				(at 17.78 5.08 180)
				(length 5.08)
				(name "PG")
				(number "3")
			)
			(pin output line
				(at 17.78 2.54 180)
				(length 5.08)
				(name "~{CC}")
				(number "4")
			)
			(pin input line
				(at -17.78 -7.62 0)
				(length 5.08)
				(name "DITH/SYNC")
				(number "5")
			)
			(pin input line
				(at -17.78 -10.16 0)
				(length 5.08)
				(name "FSW")
				(number "6")
			)
			(pin power_in line
				(at 17.78 20.32 180)
				(length 5.08)
				(name "VIN")
				(number "7")
			)
			(pin power_in line
				(at 17.78 12.7 180)
				(length 5.08)
				(name "SW1")
				(number "8")
			)
			(pin power_in line
				(at 17.78 -22.86 180)
				(length 5.08)
				(name "PGND")
				(number "9")
			)
		)
	)
	(symbol "TPS70933DBVR"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -12.7 5.08 0)
		)
		(property "Value" "TPS70933DBVR"
			(at -12.7 -7.62 0)
		)
		(property "Footprint" "SOT95P280X145-5N"
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "TPS70933DBVR_0_0"
			(pin input line
				(at -17.78 2.54 0)
				(length 5.08)
				(name "IN")
				(number "1")
			)
			(pin power_in line
				(at -17.78 0 0)
				(length 5.08)
				(name "GND")
				(number "2")
			)
			(pin bidirectional line
				(at -17.78 -2.54 0)
				(length 5.08)
				(name "EN")
				(number "3")
			)
			(pin no_connect line
				(at 1.27 -2.54 180)
				(length 5.08)
				(name "NC")
				(number "4")
			)
			(pin output line
				(at 1.27 2.54 180)
				(length 5.08)
				(name "OUT")
				(number "5")
			)
		)
	)
	(symbol "TPS7A0233PDBVR"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 2.54 7.62 0)
		)
		(property "Value" "TPS7A0233PDBVR"
			(at -7.62 -7.62 0)
		)
		(property "Footprint" "TPS7A0233PDBVR:SOT95P280X145-5N"
			(at 2.54 -15.24 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" "\n200mA, nanopower-IQ (25 nA), low-dropout (LDO) voltage regulator with enable\n"
			(at 2.54 -10.16 0)
		)
		(property "Package" "SOT-23-5 Texas Instruments"
			(at 0 -12.7 0)
		)
		(symbol "TPS7A0233PDBVR_0_0"
			(pin input line
				(at -12.7 2.54 0)
				(length 5.08)
				(name "IN")
				(number "1")
			)
			(pin power_in line
				(at -12.7 0 0)
				(length 5.08)
				(name "GND")
				(number "2")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 5.08)
				(name "EN")
				(number "3")
			)
			(pin output line
				(at 12.7 2.54 180)
				(length 5.08)
				(name "OUT")
				(number "5")
			)
		)
		(symbol "TPS7A0233PDBVR_1_0"
			(pin no_connect line
				(at 12.7 -2.54 180)
				(length 5.08)
				(name "NC")
				(number "4")
			)
		)
		(symbol "TPS7A0233PDBVR_1_1")
	)
	(symbol "TPS7A2633DRVR"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -1.27 6.35 0)
		)
		(property "Value" "TPS7A2633DRVR"
			(at -7.62 3.81 0)
		)
		(property "Footprint" "TPS7A2633DRVR:SON65P200X200X80-7N"
			(at 0 -19.05 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" "\n500-mA, 18-V, ultra-low-IQ, high-accuracy, adjustable low-dropout voltage regulator with power good\n"
			(at 0 0 0)
		)
		(property "MF" ""
			(at 17.78 26.67 0)
		)
		(property "PACKAGE" ""
			(at 0 22.86 0)
		)
		(property "PRICE" ""
			(at -1.27 29.21 0)
		)
		(property "Package" "WSON-6 Texas Instruments"
			(at -1.27 -24.13 0)
		)
		(property "Check_prices" ""
			(at 5.08 -19.05 0)
		)
		(property "Price" ""
			(at 11.43 33.02 0)
		)
		(property "SnapEDA_Link" ""
			(at 5.08 -16.51 0)
		)
		(property "MP" ""
			(at 1.27 15.24 0)
		)
		(property "Purchase-URL" "https://www.snapeda.com/api/url_track_click_mouser/?unipart_id=4639091&manufacturer=Texas Instruments&part_name=TPS7A2633DRVR&search_term=	 tps7a2633drvr"
			(at 6.35 -21.59 0)
		)
		(property "Availability" ""
			(at -1.27 33.02 0)
		)
		(property "AVAILABILITY" "Warning"
			(at 15.24 -12.7 0)
		)
		(property "PURCHASE-URL" ""
			(at 1.27 13.97 0)
		)
		(symbol "TPS7A2633DRVR_0_0"
			(pin output line
				(at -11.43 0 0)
				(length 5.08)
				(name "OUT")
				(number "1")
			)
			(pin passive line
				(at -11.43 -3.81 0)
				(length 5.08)
				(name "NC/FB")
				(number "2")
			)
			(pin output line
				(at -11.43 -7.62 0)
				(length 5.08)
				(name "PG")
				(number "3")
			)
			(pin input line
				(at 11.43 -7.62 180)
				(length 5.08)
				(name "EN")
				(number "4")
			)
			(pin power_in line
				(at 11.43 -3.81 180)
				(length 5.08)
				(name "GND")
				(number "5")
			)
			(pin input line
				(at 11.43 0 180)
				(length 5.08)
				(name "IN")
				(number "6")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(name "EXP")
				(number "7")
			)
		)
	)
	(symbol "TPWR8004PL"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "Q"
			(at 8.89 1.27 0)
		)
		(property "Value" "TPWR8004PL"
			(at 8.89 -1.27 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "TPWR8004PL_0_1")
		(symbol "TPWR8004PL_1_1"
			(pin power_in line
				(at 3.81 -7.62 90)
				(length 1.27)
				(name "S")
				(number "1")
			)
			(pin bidirectional line
				(at 2.54 -7.62 90)
				(length 1.27)
				(name "S")
				(number "2")
			)
			(pin bidirectional line
				(at 1.27 -7.62 90)
				(length 1.27)
				(name "S")
				(number "3")
			)
			(pin passive line
				(at -5.08 -1.27 0)
				(length 1.27)
				(name "G")
				(number "4")
			)
			(pin power_in line
				(at 1.27 5.08 270)
				(length 1.27)
				(name "D")
				(number "5")
			)
		)
	)
	(symbol "Wakestr_Slim_v1"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 1.27 13.97 0)
		)
		(property "Value" "Wakestr_Slim_v1"
			(at 16.51 13.97 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "Wakestr_Slim_v1_0_0"
			(text "(3.3v to 5v)"
				(at 6.35 -5.08 0)
			)
			(text "(Max 55v)"
				(at 2.54 -7.62 0)
			)
		)
		(symbol "Wakestr_Slim_v1_0_1")
		(symbol "Wakestr_Slim_v1_1_1"
			(pin input line
				(at -8.89 -10.16 0)
				(length 2.54)
				(name "Gnd")
				(number "1")
			)
			(pin input line
				(at 27.94 5.08 180)
				(length 2.54)
				(name "Ser_RX")
				(number "10")
			)
			(pin input line
				(at 27.94 2.54 180)
				(length 2.54)
				(name "~{SPI_CS}")
				(number "11")
			)
			(pin input line
				(at 27.94 0 180)
				(length 2.54)
				(name "Wake_P")
				(number "12")
			)
			(pin output line
				(at 27.94 -2.54 180)
				(length 2.54)
				(name "~{Vreg_EN}")
				(number "13")
			)
			(pin output line
				(at 27.94 -5.08 180)
				(length 2.54)
				(name "~{Alarm}")
				(number "14")
			)
			(pin output line
				(at 27.94 -7.62 180)
				(length 2.54)
				(name "+Vreg_ON")
				(number "15")
			)
			(pin input line
				(at 27.94 -10.16 180)
				(length 2.54)
				(name "Gnd")
				(number "16")
			)
			(pin input line
				(at -8.89 -7.62 0)
				(length 2.54)
				(name "Vin")
				(number "2")
			)
			(pin output line
				(at -8.89 -5.08 0)
				(length 2.54)
				(name "+Vreg")
				(number "3")
			)
			(pin output line
				(at -8.89 -2.54 0)
				(length 2.54)
				(name "+3V_Coin")
				(number "4")
			)
			(pin output line
				(at -8.89 0 0)
				(length 2.54)
				(name "Vreg_EN")
				(number "5")
			)
			(pin input line
				(at -8.89 2.54 0)
				(length 2.54)
				(name "~{Wake}")
				(number "6")
			)
			(pin input line
				(at -8.89 5.08 0)
				(length 2.54)
				(name "~{Proc_Sleep}")
				(number "7")
			)
			(pin bidirectional line
				(at -8.89 7.62 0)
				(length 2.54)
				(name "I2C_SDA")
				(number "8")
			)
			(pin bidirectional line
				(at -8.89 10.16 0)
				(length 2.54)
				(name "I2C_SCL")
				(number "9")
			)
		)
	)
	(symbol "XAL6060-103MEC"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "L"
			(at -10.16 7.62 0)
		)
		(property "Value" "10uH"
			(at -10.16 5.08 0)
		)
		(property "Footprint" "ProjectFootprints:IND_XAL6060-103MEC"
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(property "PartNum" "XGL6060-103MEB"
			(at 0 0 0)
		)
		(property "VendorNum" ""
			(at 0 0 0)
		)
		(property "Vendor" "Coiltronics"
			(at 0 0 0)
		)
		(property "Subst" "No"
			(at 0 0 0)
		)
		(symbol "XAL6060-103MEC_0_0"
			(pin passive line
				(at -12.7 0 0)
				(length 5.08)
				(name "~")
				(number "1")
			)
			(pin passive line
				(at 12.7 0 180)
				(length 5.08)
				(name "~")
				(number "2")
			)
		)
	)
	(symbol "XMC1302T038"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 7.62 26.67 0)
		)
		(property "Value" "XMC1302T038"
			(at -6.35 26.67 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "XMC1302T038_0_0"
			(pin bidirectional line
				(at -15.24 22.86 0)
				(length 2.54)
				(name "P2.4")
				(number "1")
			)
			(pin power_in line
				(at -15.24 0 0)
				(length 2.54)
				(name "Vddp/Vdd")
				(number "10")
			)
			(pin bidirectional line
				(at -15.24 -2.54 0)
				(length 2.54)
				(name "P1.5")
				(number "11")
			)
			(pin bidirectional line
				(at -15.24 -5.08 0)
				(length 2.54)
				(name "P1.4")
				(number "12")
			)
			(pin bidirectional line
				(at -15.24 -7.62 0)
				(length 2.54)
				(name "P1.3")
				(number "13")
			)
			(pin bidirectional line
				(at -15.24 -10.16 0)
				(length 2.54)
				(name "P1.2")
				(number "14")
			)
			(pin bidirectional line
				(at -15.24 -12.7 0)
				(length 2.54)
				(name "P1.1")
				(number "15")
			)
			(pin bidirectional line
				(at -15.24 -15.24 0)
				(length 2.54)
				(name "P1.0")
				(number "16")
			)
			(pin bidirectional line
				(at -15.24 -17.78 0)
				(length 2.54)
				(name "P0.0")
				(number "17")
			)
			(pin bidirectional line
				(at -15.24 -20.32 0)
				(length 2.54)
				(name "P0.1")
				(number "18")
			)
			(pin bidirectional line
				(at -15.24 -22.86 0)
				(length 2.54)
				(name "P0.2")
				(number "19")
			)
			(pin bidirectional line
				(at -15.24 20.32 0)
				(length 2.54)
				(name "P2.5")
				(number "2")
			)
			(pin bidirectional line
				(at 15.24 -22.86 180)
				(length 2.54)
				(name "P0.3")
				(number "20")
			)
			(pin bidirectional line
				(at 15.24 -20.32 180)
				(length 2.54)
				(name "P0.4")
				(number "21")
			)
			(pin bidirectional line
				(at 15.24 -17.78 180)
				(length 2.54)
				(name "P0.5")
				(number "22")
			)
			(pin bidirectional line
				(at 15.24 -15.24 180)
				(length 2.54)
				(name "P0.6")
				(number "23")
			)
			(pin bidirectional line
				(at 15.24 -12.7 180)
				(length 2.54)
				(name "P0.7")
				(number "24")
			)
			(pin power_in line
				(at 15.24 -10.16 180)
				(length 2.54)
				(name "Vssp")
				(number "25")
			)
			(pin power_in line
				(at 15.24 -7.62 180)
				(length 2.54)
				(name "Vddp")
				(number "26")
			)
			(pin bidirectional line
				(at 15.24 -5.08 180)
				(length 2.54)
				(name "P0.8")
				(number "27")
			)
			(pin bidirectional line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "P0.9")
				(number "28")
			)
			(pin bidirectional line
				(at 15.24 0 180)
				(length 2.54)
				(name "P0.10")
				(number "29")
			)
			(pin bidirectional line
				(at -15.24 17.78 0)
				(length 2.54)
				(name "P2.6")
				(number "3")
			)
			(pin bidirectional line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "P0.11")
				(number "30")
			)
			(pin bidirectional line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "P0.12")
				(number "31")
			)
			(pin bidirectional line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "P0.13")
				(number "32")
			)
			(pin bidirectional line
				(at 15.24 10.16 180)
				(length 2.54)
				(name "P0.14")
				(number "33")
			)
			(pin bidirectional line
				(at 15.24 12.7 180)
				(length 2.54)
				(name "P0.15")
				(number "34")
			)
			(pin bidirectional line
				(at 15.24 15.24 180)
				(length 2.54)
				(name "P2.0")
				(number "35")
			)
			(pin bidirectional line
				(at 15.24 17.78 180)
				(length 2.54)
				(name "P2.1")
				(number "36")
			)
			(pin bidirectional line
				(at 15.24 20.32 180)
				(length 2.54)
				(name "P2.2")
				(number "37")
			)
			(pin bidirectional line
				(at 15.24 22.86 180)
				(length 2.54)
				(name "P2.3")
				(number "38")
			)
			(pin bidirectional line
				(at -15.24 15.24 0)
				(length 2.54)
				(name "P2.7")
				(number "4")
			)
			(pin bidirectional line
				(at -15.24 12.7 0)
				(length 2.54)
				(name "P2.8")
				(number "5")
			)
			(pin bidirectional line
				(at -15.24 10.16 0)
				(length 2.54)
				(name "P2.9")
				(number "6")
			)
			(pin bidirectional line
				(at -15.24 7.62 0)
				(length 2.54)
				(name "P2.10")
				(number "7")
			)
			(pin bidirectional line
				(at -15.24 5.08 0)
				(length 2.54)
				(name "P2.11")
				(number "8")
			)
			(pin power_in line
				(at -15.24 2.54 0)
				(length 2.54)
				(name "Vssp/Vss")
				(number "9")
			)
		)
		(symbol "XMC1302T038_0_1")
	)
	(symbol "boostr_v1_0"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 0 0)
		)
		(property "Value" "boostr_v1_0"
			(at 0 0 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "boostr_v1_0_0_1")
		(symbol "boostr_v1_0_1_1"
			(pin input line
				(at -12.7 -22.86 90)
				(length 2.54)
				(name "GND")
				(number "1")
			)
			(pin output line
				(at 10.16 -22.86 90)
				(length 2.54)
				(name "ISMON")
				(number "10")
			)
			(pin input line
				(at -10.16 22.86 270)
				(length 2.54)
				(name "GND")
				(number "11")
			)
			(pin input line
				(at -7.62 22.86 270)
				(length 2.54)
				(name "GND")
				(number "12")
			)
			(pin input line
				(at -5.08 22.86 270)
				(length 2.54)
				(name "GND")
				(number "13")
			)
			(pin input line
				(at -2.54 22.86 270)
				(length 2.54)
				(name "GND")
				(number "14")
			)
			(pin output line
				(at 0 22.86 270)
				(length 2.54)
				(name "VOUT")
				(number "15")
			)
			(pin output line
				(at 2.54 22.86 270)
				(length 2.54)
				(name "VOUT")
				(number "16")
			)
			(pin output line
				(at 5.08 22.86 270)
				(length 2.54)
				(name "VOUT")
				(number "17")
			)
			(pin output line
				(at 7.62 22.86 270)
				(length 2.54)
				(name "VOUT")
				(number "18")
			)
			(pin output line
				(at 10.16 22.86 270)
				(length 2.54)
				(name "~{PGOOD}")
				(number "19")
			)
			(pin input line
				(at -10.16 -22.86 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin input line
				(at -7.62 -22.86 90)
				(length 2.54)
				(name "GND")
				(number "3")
			)
			(pin input line
				(at -5.08 -22.86 90)
				(length 2.54)
				(name "GND")
				(number "4")
			)
			(pin input line
				(at -2.54 -22.86 90)
				(length 2.54)
				(name "VIN")
				(number "5")
			)
			(pin input line
				(at 0 -22.86 90)
				(length 2.54)
				(name "VIN")
				(number "6")
			)
			(pin input line
				(at 2.54 -22.86 90)
				(length 2.54)
				(name "VIN")
				(number "7")
			)
			(pin input line
				(at 5.08 -22.86 90)
				(length 2.54)
				(name "VIN")
				(number "8")
			)
			(pin input line
				(at 7.62 -22.86 90)
				(length 2.54)
				(name "EN")
				(number "9")
			)
		)
	)
	(symbol "iC-HG"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 36.83 0)
		)
		(property "Value" "iC-HG"
			(at 13.97 36.83 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "iC-HG_0_0"
			(text "+"
				(at -7.239 -25.527 0)
			)
			(text "+"
				(at -7.239 -2.667 0)
			)
			(text "+"
				(at -7.239 20.193 0)
			)
			(text "-"
				(at -7.239 -26.67 0)
			)
			(text "-"
				(at -7.239 -3.81 0)
			)
			(text "-"
				(at -7.239 19.05 0)
			)
			(text "Pwr Temp Mon"
				(at -8.763 -52.578 0)
			)
			(text "S"
				(at -7.112 -34.163 0)
			)
			(text "S"
				(at -7.112 -22.606 0)
			)
			(text "S"
				(at -7.112 -11.303 0)
			)
			(text "S"
				(at -7.112 0.254 0)
			)
			(text "S"
				(at -7.112 11.557 0)
			)
			(text "S"
				(at -7.112 23.114 0)
			)
			(text "TTL/LVDS"
				(at -5.969 -44.704 0)
			)
		)
		(symbol "iC-HG_0_1")
		(symbol "iC-HG_1_1"
			(pin passive line
				(at -21.59 26.67 0)
				(length 5.08)
				(name "CI1")
				(number "1")
			)
			(pin passive line
				(at 21.59 -24.13 180)
				(length 5.08)
				(name "AGND5")
				(number "10")
			)
			(pin passive line
				(at 21.59 -17.78 180)
				(length 5.08)
				(name "LDK5")
				(number "11")
			)
			(pin passive line
				(at 21.59 -12.7 180)
				(length 5.08)
				(name "AGND4")
				(number "12")
			)
			(pin passive line
				(at 21.59 -6.35 180)
				(length 5.08)
				(name "LDK4")
				(number "13")
			)
			(pin passive line
				(at -21.59 -34.29 0)
				(length 5.08)
				(name "EN6")
				(number "14")
			)
			(pin passive line
				(at -21.59 -22.86 0)
				(length 5.08)
				(name "EN5")
				(number "15")
			)
			(pin passive line
				(at -21.59 -11.43 0)
				(length 5.08)
				(name "EN4")
				(number "16")
			)
			(pin passive line
				(at -21.59 0 0)
				(length 5.08)
				(name "EN3")
				(number "17")
			)
			(pin passive line
				(at 0 40.64 270)
				(length 5.08)
				(name "VDD")
				(number "18")
			)
			(pin passive line
				(at -21.59 -44.45 0)
				(length 5.08)
				(name "ELVDS")
				(number "19")
			)
			(pin passive line
				(at -21.59 15.24 0)
				(length 5.08)
				(name "CI2")
				(number "2")
			)
			(pin passive line
				(at -21.59 11.43 0)
				(length 5.08)
				(name "EN2")
				(number "20")
			)
			(pin passive line
				(at -21.59 22.86 0)
				(length 5.08)
				(name "EN1")
				(number "21")
			)
			(pin passive line
				(at 21.59 -44.45 180)
				(length 5.08)
				(name "NER")
				(number "22")
			)
			(pin passive line
				(at 21.59 5.08 180)
				(length 5.08)
				(name "LDK3")
				(number "23")
			)
			(pin passive line
				(at 21.59 -1.27 180)
				(length 5.08)
				(name "AGND3")
				(number "24")
			)
			(pin passive line
				(at 21.59 16.51 180)
				(length 5.08)
				(name "LDK2")
				(number "25")
			)
			(pin passive line
				(at 21.59 10.16 180)
				(length 5.08)
				(name "AGND2")
				(number "26")
			)
			(pin passive line
				(at 21.59 27.94 180)
				(length 5.08)
				(name "LDK1")
				(number "27")
			)
			(pin passive line
				(at 21.59 21.59 180)
				(length 5.08)
				(name "AGND1")
				(number "28")
			)
			(pin passive line
				(at 0 -66.04 90)
				(length 5.08)
				(name "GND_PAD")
				(number "29")
			)
			(pin passive line
				(at -21.59 3.81 0)
				(length 5.08)
				(name "CI3")
				(number "3")
			)
			(pin passive line
				(at 2.54 -66.04 90)
				(length 5.08)
				(name "GND")
				(number "4")
			)
			(pin passive line
				(at -21.59 -7.62 0)
				(length 5.08)
				(name "CI4")
				(number "5")
			)
			(pin passive line
				(at -21.59 -19.05 0)
				(length 5.08)
				(name "CI5")
				(number "6")
			)
			(pin passive line
				(at -21.59 -30.48 0)
				(length 5.08)
				(name "CI6")
				(number "7")
			)
			(pin passive line
				(at 21.59 -35.56 180)
				(length 5.08)
				(name "AGND6")
				(number "8")
			)
			(pin passive line
				(at 21.59 -29.21 180)
				(length 5.08)
				(name "LDK6")
				(number "9")
			)
		)
	)
	(symbol "max3323e"
		(pin_names
			(offset 0.254)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 30.48 3.81 0)
		)
		(property "Value" "max3323e"
			(at 38.1 -21.59 0)
		)
		(property "Footprint" "21-0066J_16_MXM"
			(at 38.1 1.27 0)
		)
		(property "Datasheet" ""
			(at 17.78 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_fp_filters" "21-0066J_16_MXM 21-0066J_16_MXM-M 21-0066J_16_MXM-L"
			(at 0 0 0)
		)
		(symbol "max3323e_1_1"
			(pin unspecified line
				(at 17.78 0 0)
				(length 7.62)
				(name "C1+")
				(number "1")
			)
			(pin input line
				(at 58.42 -15.24 180)
				(length 7.62)
				(name "TIN1")
				(number "10")
			)
			(pin input line
				(at 58.42 -12.7 180)
				(length 7.62)
				(name "TXENABLE")
				(number "11")
			)
			(pin input line
				(at 58.42 -10.16 180)
				(length 7.62)
				(name "RENABLE")
				(number "12")
			)
			(pin power_in line
				(at 58.42 -7.62 180)
				(length 7.62)
				(name "VL")
				(number "13")
			)
			(pin input line
				(at 58.42 -5.08 180)
				(length 7.62)
				(name "*SHDN")
				(number "14")
			)
			(pin power_in line
				(at 58.42 -2.54 180)
				(length 7.62)
				(name "GND")
				(number "15")
			)
			(pin power_in line
				(at 58.42 0 180)
				(length 7.62)
				(name "VCC")
				(number "16")
			)
			(pin power_in line
				(at 17.78 -2.54 0)
				(length 7.62)
				(name "V+")
				(number "2")
			)
			(pin unspecified line
				(at 17.78 -5.08 0)
				(length 7.62)
				(name "C1-")
				(number "3")
			)
			(pin unspecified line
				(at 17.78 -7.62 0)
				(length 7.62)
				(name "C2+")
				(number "4")
			)
			(pin unspecified line
				(at 17.78 -10.16 0)
				(length 7.62)
				(name "C2-")
				(number "5")
			)
			(pin power_in line
				(at 17.78 -12.7 0)
				(length 7.62)
				(name "V-")
				(number "6")
			)
			(pin output line
				(at 17.78 -15.24 0)
				(length 7.62)
				(name "TOUT1")
				(number "7")
			)
			(pin input line
				(at 17.78 -17.78 0)
				(length 7.62)
				(name "RIN1")
				(number "8")
			)
			(pin output line
				(at 58.42 -17.78 180)
				(length 7.62)
				(name "ROUT1")
				(number "9")
			)
		)
	)
	(symbol "rPi_Zero_2W"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 30.48 0)
		)
		(property "Value" "rPi_Zero_2W"
			(at -6.35 27.94 0)
		)
		(property "Footprint" ""
			(at -7.62 11.43 0)
		)
		(property "Datasheet" ""
			(at -7.62 11.43 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "rPi_Zero_2W_0_1")
		(symbol "rPi_Zero_2W_1_1"
			(pin power_out line
				(at -15.24 24.13 0)
				(length 2.54)
				(name "3v3")
				(number "1")
			)
			(pin passive line
				(at 13.97 13.97 180)
				(length 2.54)
				(name "RXD0")
				(number "10")
			)
			(pin passive line
				(at -15.24 11.43 0)
				(length 2.54)
				(name "SPI1_CE1")
				(number "11")
			)
			(pin passive line
				(at 13.97 11.43 180)
				(length 2.54)
				(name "SPI1_CE0")
				(number "12")
			)
			(pin passive line
				(at -15.24 8.89 0)
				(length 2.54)
				(name "GPIO27")
				(number "13")
			)
			(pin passive line
				(at 13.97 8.89 180)
				(length 2.54)
				(name "GND")
				(number "14")
			)
			(pin passive line
				(at -15.24 6.35 0)
				(length 2.54)
				(name "GPIO22")
				(number "15")
			)
			(pin passive line
				(at 13.97 6.35 180)
				(length 2.54)
				(name "GPIO23")
				(number "16")
			)
			(pin power_out line
				(at -15.24 3.81 0)
				(length 2.54)
				(name "3v3")
				(number "17")
			)
			(pin passive line
				(at 13.97 3.81 180)
				(length 2.54)
				(name "GPIO24")
				(number "18")
			)
			(pin passive line
				(at -15.24 1.27 0)
				(length 2.54)
				(name "SPI0_COPI")
				(number "19")
			)
			(pin passive line
				(at 13.97 24.13 180)
				(length 2.54)
				(name "5v")
				(number "2")
			)
			(pin passive line
				(at 13.97 1.27 180)
				(length 2.54)
				(name "GND")
				(number "20")
			)
			(pin passive line
				(at -15.24 -1.27 0)
				(length 2.54)
				(name "SPI0_CIPO")
				(number "21")
			)
			(pin passive line
				(at 13.97 -1.27 180)
				(length 2.54)
				(name "GPIO25")
				(number "22")
			)
			(pin passive line
				(at -15.24 -3.81 0)
				(length 2.54)
				(name "SPI0_SCLK")
				(number "23")
			)
			(pin passive line
				(at 13.97 -3.81 180)
				(length 2.54)
				(name "SPI0_CE0")
				(number "24")
			)
			(pin passive line
				(at -15.24 -6.35 0)
				(length 2.54)
				(name "GND")
				(number "25")
			)
			(pin passive line
				(at 13.97 -6.35 180)
				(length 2.54)
				(name "SPI0_CE1")
				(number "26")
			)
			(pin passive line
				(at -15.24 -8.89 0)
				(length 2.54)
				(name "ID_SD")
				(number "27")
			)
			(pin passive line
				(at 13.97 -8.89 180)
				(length 2.54)
				(name "ID_SC")
				(number "28")
			)
			(pin passive line
				(at -15.24 -11.43 0)
				(length 2.54)
				(name "GPIO5")
				(number "29")
			)
			(pin passive line
				(at -15.24 21.59 0)
				(length 2.54)
				(name "SDA1")
				(number "3")
			)
			(pin passive line
				(at 13.97 -11.43 180)
				(length 2.54)
				(name "GND")
				(number "30")
			)
			(pin passive line
				(at -15.24 -13.97 0)
				(length 2.54)
				(name "GPIO6")
				(number "31")
			)
			(pin passive line
				(at 13.97 -13.97 180)
				(length 2.54)
				(name "GPIO12")
				(number "32")
			)
			(pin passive line
				(at -15.24 -16.51 0)
				(length 2.54)
				(name "GPIO13")
				(number "33")
			)
			(pin passive line
				(at 13.97 -16.51 180)
				(length 2.54)
				(name "GND")
				(number "34")
			)
			(pin passive line
				(at -15.24 -19.05 0)
				(length 2.54)
				(name "SPI1_CIPO")
				(number "35")
			)
			(pin passive line
				(at 13.97 -19.05 180)
				(length 2.54)
				(name "SPI1_CE2")
				(number "36")
			)
			(pin passive line
				(at -15.24 -21.59 0)
				(length 2.54)
				(name "GPIO26")
				(number "37")
			)
			(pin passive line
				(at 13.97 -21.59 180)
				(length 2.54)
				(name "SPI1_COPI")
				(number "38")
			)
			(pin passive line
				(at -15.24 -24.13 0)
				(length 2.54)
				(name "GND")
				(number "39")
			)
			(pin passive line
				(at 13.97 21.59 180)
				(length 2.54)
				(name "5v")
				(number "4")
			)
			(pin passive line
				(at 13.97 -24.13 180)
				(length 2.54)
				(name "SPI1_SCLK")
				(number "40")
			)
			(pin passive line
				(at -15.24 19.05 0)
				(length 2.54)
				(name "SCL1")
				(number "5")
			)
			(pin passive line
				(at 13.97 19.05 180)
				(length 2.54)
				(name "GND")
				(number "6")
			)
			(pin passive line
				(at -15.24 16.51 0)
				(length 2.54)
				(name "GPIO4")
				(number "7")
			)
			(pin passive line
				(at 13.97 16.51 180)
				(length 2.54)
				(name "TXD0")
				(number "8")
			)
			(pin passive line
				(at -15.24 13.97 0)
				(length 2.54)
				(name "GND")
				(number "9")
			)
		)
	)
	(symbol "LTC4440IS6"
		(extends "LTC4440-5ES6")
		(property "Reference" "U"
			(at -7.62 8.89 0)
		)
		(property "Value" "LTC4440IS6"
			(at -1.27 8.89 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-6"
			(at 0 -10.16 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/4440fb.pdf"
			(at -2.54 11.43 0)
		)
		(property "Description" "High-side, N-Channel, Mosfet driver, 80V input, -40°C to +85°C, SOT23-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "high-side mosfet-driver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
)
