(kicad_symbol_lib (version 20211014) (generator kicad_symbol_editor)
  (symbol "ADM7160AUJZ-3.3" (pin_names (offset 1.016)) (in_bom yes) (on_board yes)
    (property "Reference" "U" (id 0) (at 3.81 6.35 0))
    (property "Value" "ADM7160AUJZ-3.3" (id 1) (at 0 8.89 0))
    (property "Footprint" "Package_TO_SOT_SMD:TSOT-23-5_HandSoldering" (id 2) (at 0 0 0))
    (property "Datasheet" "" (id 3) (at 0 0 0))
    (symbol "ADM7160AUJZ-3.3_0_1")
    (symbol "ADM7160AUJZ-3.3_1_1"
      (pin power_in line (at -7.62 3.81 0) (length 2.54)
        (name "Vin")
        (number "1")
      )
      (pin power_in line (at -7.62 1.27 0) (length 2.54)
        (name "GND")
        (number "2")
      )
      (pin input line (at -7.62 -1.27 0) (length 2.54)
        (name "EN")
        (number "3")
      )
      (pin input line (at 7.62 -1.27 180) (length 2.54)
        (name "NC")
        (number "4")
      )
      (pin power_out line (at 7.62 3.81 180) (length 2.54)
        (name "Vout")
        (number "5")
      )
    )
  )
  (symbol "MP7720" (pin_names (offset 1.016)) (in_bom yes) (on_board yes)
    (property "Reference" "U" (id 0) (at 0 0 0))
    (property "Value" "MP7720" (id 1) (at 0 0 0))
    (property "Footprint" "Package_SO:SOIC-8-1EP_3.9x4.9mm_P1.27mm_EP2.29x3mm_ThermalVias" (id 2) (at 0 0 0))
    (property "Datasheet" "https://www.monolithicpower.com/en/documentview/productdocument/index/version/2/document_type/Datasheet/lang/en/sku/MP7720/document_id/136" (id 3) (at 0 0 0))
    (symbol "MP7720_0_1")
    (symbol "MP7720_1_1"
      (pin input line (at -8.89 3.81 0) (length 2.54)
        (name "PIN")
        (number "1")
      )
      (pin input line (at -8.89 1.27 0) (length 2.54)
        (name "NIN")
        (number "2")
      )
      (pin power_in line (at -8.89 -1.27 0) (length 2.54)
        (name "AGND")
        (number "3")
      )
      (pin input line (at -8.89 -3.81 0) (length 2.54)
        (name "EN")
        (number "4")
      )
      (pin power_out line (at 8.89 -3.81 180) (length 2.54)
        (name "BS")
        (number "5")
      )
      (pin power_out line (at 8.89 -1.27 180) (length 2.54)
        (name "VDD")
        (number "6")
      )
      (pin power_out line (at 8.89 1.27 180) (length 2.54)
        (name "SW")
        (number "7")
      )
      (pin power_in line (at 8.89 3.81 180) (length 2.54)
        (name "PGND")
        (number "8")
      )
    )
  )
  (symbol "S-1155B" (pin_names (offset 1.016)) (in_bom yes) (on_board yes)
    (property "Reference" "U" (id 0) (at 0 7.62 0))
    (property "Value" "S-1155B" (id 1) (at 0 5.08 0))
    (property "Footprint" "" (id 2) (at 0 0 0))
    (property "Datasheet" "" (id 3) (at 0 0 0))
    (symbol "S-1155B_0_1")
    (symbol "S-1155B_1_1"
      (pin input line (at -7.62 2.54 0) (length 2.54)
        (name "EN")
        (number "1")
      )
      (pin power_in line (at -7.62 0 0) (length 2.54)
        (name "GND")
        (number "2")
      )
      (pin input line (at -7.62 -2.54 0) (length 2.54)
        (name "NC")
        (number "3")
      )
      (pin power_in line (at 7.62 -2.54 180) (length 2.54)
        (name "VIN")
        (number "4")
      )
      (pin power_out line (at 7.62 2.54 180) (length 2.54)
        (name "VOUT")
        (number "5")
      )
    )
  )
  (symbol "VN5E160S-E" (pin_names (offset 1.016)) (in_bom yes) (on_board yes)
    (property "Reference" "U" (id 0) (at 2.54 12.7 0))
    (property "Value" "VN5E160S-E" (id 1) (at 1.27 8.89 0))
    (property "Footprint" "Package_SO:SO-8_3.9x4.9mm_P1.27mm" (id 2) (at 1.27 0 0))
    (property "Datasheet" "" (id 3) (at 1.27 0 0))
    (symbol "VN5E160S-E_0_1")
    (symbol "VN5E160S-E_1_1"
      (pin power_in line (at -10.16 3.81 0) (length 2.54)
        (name "GND")
        (number "1")
      )
      (pin output line (at -10.16 1.27 0) (length 2.54)
        (name "IN")
        (number "2")
      )
      (pin output line (at -10.16 -1.27 0) (length 2.54)
        (name "STAT")
        (number "3")
      )
      (pin input line (at -10.16 -3.81 0) (length 2.54)
        (name "STAT_DIS")
        (number "4")
      )
      (pin power_in line (at 10.16 -3.81 180) (length 2.54)
        (name "VCC")
        (number "5")
      )
      (pin output line (at 10.16 -1.27 180) (length 2.54)
        (name "OUT")
        (number "6")
      )
      (pin output line (at 10.16 1.27 180) (length 2.54)
        (name "OUT")
        (number "7")
      )
      (pin output line (at 10.16 3.81 180) (length 2.54)
        (name "VCC")
        (number "8")
      )
    )
  )
)
