(kicad_sch (version 20230121) (generator eeschema)
  (paper "A4")
  (lib_symbols
    (symbol "Device:C" (pin_numbers hide) (pin_names (offset 0.254)) (in_bom yes) (on_board yes)
      (property "Reference" "C" (at 0.635 2.54 0))
      (property "Value" "C" (at 0.635 -2.54 0))
      (property "Footprint" "" (at 0.9652 -3.81 0))
      (property "Datasheet" "~" (at 0 0 0))
      (property "ki_keywords" "cap capacitor" (at 0 0 0))
      (property "ki_description" "Unpolarized capacitor" (at 0 0 0))
      (property "ki_fp_filters" "C_*" (at 0 0 0))
      (symbol "C_0_1"
        (polyline
          (pts
            (xy -2.032 -0.762)
            (xy 2.032 -0.762)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -2.032 0.762)
            (xy 2.032 0.762)
          )
          (fill (type none))
        )
      )
      (symbol "C_1_1"
        (pin passive line (at 0 3.81 270) (length 2.794)
          (name "~")
          (number "1")
        )
        (pin passive line (at 0 -3.81 90) (length 2.794)
          (name "~")
          (number "2")
        )
      )
    )
    (symbol "Device:L_Iron" (pin_numbers hide) (pin_names (offset 1.016) hide) (in_bom yes) (on_board yes)
      (property "Reference" "L" (at -1.27 0 90))
      (property "Value" "L_Iron" (at 2.794 0 90))
      (property "Footprint" "" (at 0 0 0))
      (property "Datasheet" "~" (at 0 0 0))
      (property "ki_keywords" "inductor choke coil reactor magnetic" (at 0 0 0))
      (property "ki_description" "Inductor with iron core" (at 0 0 0))
      (property "ki_fp_filters" "Choke_* *Coil* Inductor_* L_*" (at 0 0 0))
      (symbol "L_Iron_0_1"
        (arc (start 0 -2.54) (mid 0.6323 -1.905) (end 0 -1.27)
          (fill (type none))
        )
        (arc (start 0 -1.27) (mid 0.6323 -0.635) (end 0 0)
          (fill (type none))
        )
        (polyline
          (pts
            (xy 1.016 2.54)
            (xy 1.016 -2.54)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 1.524 -2.54)
            (xy 1.524 2.54)
          )
          (fill (type none))
        )
        (arc (start 0 0) (mid 0.6323 0.635) (end 0 1.27)
          (fill (type none))
        )
        (arc (start 0 1.27) (mid 0.6323 1.905) (end 0 2.54)
          (fill (type none))
        )
      )
      (symbol "L_Iron_1_1"
        (pin passive line (at 0 3.81 270) (length 1.27)
          (name "1")
          (number "1")
        )
        (pin passive line (at 0 -3.81 90) (length 1.27)
          (name "2")
          (number "2")
        )
      )
    )
    (symbol "Device:Polyfuse" (pin_numbers hide) (pin_names (offset 0)) (in_bom yes) (on_board yes)
      (property "Reference" "F" (at -2.54 0 90))
      (property "Value" "Polyfuse" (at 2.54 0 90))
      (property "Footprint" "" (at 1.27 -5.08 0))
      (property "Datasheet" "~" (at 0 0 0))
      (property "ki_keywords" "resettable fuse PTC PPTC polyfuse polyswitch" (at 0 0 0))
      (property "ki_description" "Resettable fuse, polymeric positive temperature coefficient" (at 0 0 0))
      (property "ki_fp_filters" "*polyfuse* *PTC*" (at 0 0 0))
      (symbol "Polyfuse_0_1"
        (rectangle (start -0.762 2.54) (end 0.762 -2.54)
          (fill (type none))
        )
        (polyline
          (pts
            (xy 0 2.54)
            (xy 0 -2.54)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -1.524 2.54)
            (xy -1.524 1.524)
            (xy 1.524 -1.524)
            (xy 1.524 -2.54)
          )
          (fill (type none))
        )
      )
      (symbol "Polyfuse_1_1"
        (pin passive line (at 0 3.81 270) (length 1.27)
          (name "~")
          (number "1")
        )
        (pin passive line (at 0 -3.81 90) (length 1.27)
          (name "~")
          (number "2")
        )
      )
    )
    (symbol "Device:R" (pin_numbers hide) (pin_names (offset 0)) (in_bom yes) (on_board yes)
      (property "Reference" "R" (at 2.032 0 90))
      (property "Value" "R" (at 0 0 90))
      (property "Footprint" "" (at -1.778 0 90))
      (property "Datasheet" "~" (at 0 0 0))
      (property "ki_keywords" "R res resistor" (at 0 0 0))
      (property "ki_description" "Resistor" (at 0 0 0))
      (property "ki_fp_filters" "R_*" (at 0 0 0))
      (symbol "R_0_1"
        (rectangle (start -1.016 -2.54) (end 1.016 2.54)
          (fill (type none))
        )
      )
      (symbol "R_1_1"
        (pin passive line (at 0 3.81 270) (length 1.27)
          (name "~")
          (number "1")
        )
        (pin passive line (at 0 -3.81 90) (length 1.27)
          (name "~")
          (number "2")
        )
      )
    )
    (symbol "Diode:SMAJ26A" (pin_numbers hide) (pin_names (offset 1.016) hide) (in_bom yes) (on_board yes)
      (property "Reference" "D" (at 0 2.54 0))
      (property "Value" "SMAJ26A" (at 0 -2.54 0))
      (property "Footprint" "Diode_SMD:D_SMA" (at 0 -5.08 0))
      (property "Datasheet" "https://www.littelfuse.com/media?resourcetype=datasheets&itemid=75e32973-b177-4ee3-a0ff-cedaf1abdb93&filename=smaj-datasheet" (at -1.27 0 0))
      (property "ki_keywords" "unidirectional diode TVS voltage suppressor" (at 0 0 0))
      (property "ki_description" "400W unidirectional Transient Voltage Suppressor, 26.0Vr, SMA(DO-214AC)" (at 0 0 0))
      (property "ki_fp_filters" "D*SMA*" (at 0 0 0))
      (symbol "SMAJ26A_0_1"
        (polyline
          (pts
            (xy -0.762 1.27)
            (xy -1.27 1.27)
            (xy -1.27 -1.27)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 1.27 1.27)
            (xy 1.27 -1.27)
            (xy -1.27 0)
            (xy 1.27 1.27)
          )
          (fill (type none))
        )
      )
      (symbol "SMAJ26A_1_1"
        (pin passive line (at -3.81 0 0) (length 2.54)
          (name "A1")
          (number "1")
        )
        (pin passive line (at 3.81 0 180) (length 2.54)
          (name "A2")
          (number "2")
        )
      )
    )
    (symbol "Isolator:SFH617A-1X007T" (pin_names (offset 1.016)) (in_bom yes) (on_board yes)
      (property "Reference" "U" (at -5.08 6.35 0))
      (property "Value" "SFH617A-1X007T" (at -5.08 -6.35 0))
      (property "Footprint" "Package_DIP:SMDIP-4_W9.53mm_Clearance8mm" (at 0 -8.89 0))
      (property "Datasheet" "http://www.vishay.com/docs/83740/sfh617a.pdf" (at 0 -1.27 0))
      (property "ki_keywords" "Optocoupler, Phototransistor Output, 5300 VRMS, VCEO 70V, CTR% 40-80" (at 0 0 0))
      (property "ki_description" "Optocoupler, Phototransistor Output, 5300 VRMS, VCEO 70V, CTR% 40-80, -55 to +110 degree Celsius, UL, BSI, FIMKO, cUL, 8mm clearence SMD PDIP-4" (at 0 0 0))
      (property "ki_fp_filters" "SMDIP*W9.53mm*Clearance8mm*" (at 0 0 0))
      (symbol "SFH617A-1X007T_0_1"
        (rectangle (start -5.08 3.81) (end 5.08 -3.81)
          (fill (type background))
        )
        (polyline
          (pts
            (xy -3.175 -0.635)
            (xy -1.905 -0.635)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 2.54 0.635)
            (xy 4.445 2.54)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 4.445 -2.54)
            (xy 2.54 -0.635)
          )
          (fill (type outline))
        )
        (polyline
          (pts
            (xy 4.445 -2.54)
            (xy 5.08 -2.54)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 4.445 2.54)
            (xy 5.08 2.54)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -2.54 -0.635)
            (xy -2.54 -2.54)
            (xy -5.08 -2.54)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 2.54 1.905)
            (xy 2.54 -1.905)
            (xy 2.54 -1.905)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -5.08 2.54)
            (xy -2.54 2.54)
            (xy -2.54 -1.27)
            (xy -2.54 0.635)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -2.54 -0.635)
            (xy -3.175 0.635)
            (xy -1.905 0.635)
            (xy -2.54 -0.635)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -0.508 -0.508)
            (xy 0.762 -0.508)
            (xy 0.381 -0.635)
            (xy 0.381 -0.381)
            (xy 0.762 -0.508)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -0.508 0.508)
            (xy 0.762 0.508)
            (xy 0.381 0.381)
            (xy 0.381 0.635)
            (xy 0.762 0.508)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 3.048 -1.651)
            (xy 3.556 -1.143)
            (xy 4.064 -2.159)
            (xy 3.048 -1.651)
            (xy 3.048 -1.651)
          )
          (fill (type outline))
        )
      )
      (symbol "SFH617A-1X007T_1_1"
        (pin passive line (at -7.62 2.54 0) (length 2.54)
          (name "~")
          (number "1")
        )
        (pin passive line (at -7.62 -2.54 0) (length 2.54)
          (name "~")
          (number "2")
        )
        (pin passive line (at 7.62 -2.54 180) (length 2.54)
          (name "~")
          (number "3")
        )
        (pin passive line (at 7.62 2.54 180) (length 2.54)
          (name "~")
          (number "4")
        )
      )
    )
    (symbol "PDQE15-Q24-S12-D:PDQE15-Q24-S12-D" (pin_names (offset 1.016)) (in_bom yes) (on_board yes)
      (property "Reference" "PS" (at -10.16 8.382 0))
      (property "Value" "PDQE15-Q24-S12-D" (at -10.16 -10.16 0))
      (property "Footprint" "CONV_PDQE15-Q24-S12-D" (at 0 0 0))
      (property "Datasheet" "" (at 0 0 0))
      (property "PARTREV" "1.0" (at 0 0 0))
      (property "MANUFACTURER" "CUI Inc." (at 0 0 0))
      (property "MAXIMUM_PACKAGE_HEIGHT" "11.70mm" (at 0 0 0))
      (property "STANDARD" "Manufacturer Recommendations" (at 0 0 0))
      (property "ki_locked" "" (at 0 0 0))
      (symbol "PDQE15-Q24-S12-D_0_0"
        (rectangle (start -10.16 -7.62) (end 10.16 7.62)
          (fill (type background))
        )
        (pin input line (at -15.24 0 0) (length 5.08)
          (name "CTRL")
          (number "1")
        )
        (pin power_in line (at -15.24 -5.08 0) (length 5.08)
          (name "GND")
          (number "2")
        )
        (pin input line (at -15.24 5.08 0) (length 5.08)
          (name "VIN")
          (number "3")
        )
        (pin output line (at 15.24 5.08 180) (length 5.08)
          (name "+VO")
          (number "4")
        )
        (pin passive line (at 15.24 0 180) (length 5.08)
          (name "TRIM")
          (number "5")
        )
        (pin output line (at 15.24 -5.08 180) (length 5.08)
          (name "0V")
          (number "6")
        )
      )
    )
    (symbol "flexLinkLibrary:PJT7603_R1_00001" (pin_names hide) (in_bom yes) (on_board yes)
      (property "Reference" "U14" (at 8.128 -22.098 0))
      (property "Value" "~" (at 0 0 0))
      (property "Footprint" "" (at 0 0 0))
      (property "Datasheet" "" (at 0 0 0))
      (symbol "PJT7603_R1_00001_0_1"
        (polyline
          (pts
            (xy 3.048 -17.272)
            (xy 5.207 -17.272)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 3.048 -11.43)
            (xy 6.096 -11.43)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 3.048 -6.096)
            (xy 5.334 -6.096)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 3.8891 -8.5089)
            (xy 3.7621 -8.7629)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 3.8891 -8.5089)
            (xy 4.6511 -8.5089)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 4.318 -7.874)
            (xy 4.318 -6.096)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 4.699 -8.509)
            (xy 3.937 -8.509)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 4.7781 -8.5089)
            (xy 4.9051 -8.2549)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 5.207 -17.272)
            (xy 5.969 -17.272)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 5.207 -6.096)
            (xy 5.969 -6.096)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 5.461 -15.494)
            (xy 6.477 -15.494)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 5.461 -7.874)
            (xy 6.477 -7.874)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 5.842 -14.986)
            (xy 9.652 -14.986)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 5.842 -8.382)
            (xy 9.652 -8.382)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 7.239 -15.494)
            (xy 8.255 -15.494)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 7.239 -7.874)
            (xy 8.255 -7.874)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 7.747 -10.414)
            (xy 7.747 -8.382)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 8.128 -18.415)
            (xy 8.128 -17.653)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 8.128 -5.715)
            (xy 8.128 -4.953)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 9.017 -15.494)
            (xy 10.033 -15.494)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 9.017 -7.874)
            (xy 10.033 -7.874)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 10.16 -6.096)
            (xy 11.303 -6.096)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 10.287 -17.272)
            (xy 11.176 -17.272)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 10.414 -11.43)
            (xy 11.176 -11.43)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 11.176 -17.272)
            (xy 11.684 -17.272)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 11.176 -11.43)
            (xy 11.684 -11.43)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 11.303 -6.096)
            (xy 11.811 -6.096)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 4.318 -9.144)
            (xy 4.318 -10.414)
            (xy 7.747 -10.414)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 6.096 -11.43)
            (xy 7.747 -11.43)
            (xy 7.747 -10.287)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 10.287 -17.272)
            (xy 7.747 -17.272)
            (xy 7.747 -15.494)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 10.287 -6.096)
            (xy 7.747 -6.096)
            (xy 7.747 -7.874)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 10.414 -11.43)
            (xy 8.255 -11.43)
            (xy 8.255 -14.986)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 4.2701 -8.5089)
            (xy 3.8891 -7.8739)
            (xy 4.6511 -7.8739)
            (xy 4.2701 -8.5089)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 4.318 -8.509)
            (xy 4.699 -9.144)
            (xy 3.937 -9.144)
            (xy 4.318 -8.509)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 5.969 -15.494)
            (xy 5.969 -18.034)
            (xy 9.525 -18.034)
            (xy 9.525 -15.494)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 5.969 -7.874)
            (xy 5.969 -5.334)
            (xy 9.525 -5.334)
            (xy 9.525 -7.874)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 7.747 -17.018)
            (xy 7.366 -16.002)
            (xy 8.128 -16.002)
            (xy 7.747 -17.018)
          )
          (fill (type outline))
        )
        (polyline
          (pts
            (xy 7.747 -7.366)
            (xy 7.366 -6.35)
            (xy 8.128 -6.35)
            (xy 7.747 -7.366)
          )
          (fill (type outline))
        )
        (polyline
          (pts
            (xy 8.128 -18.034)
            (xy 7.493 -17.653)
            (xy 7.493 -18.415)
            (xy 8.128 -18.034)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 8.128 -5.334)
            (xy 7.493 -5.715)
            (xy 7.493 -4.953)
            (xy 8.128 -5.334)
          )
          (fill (type none))
        )
        (rectangle (start 2.413 -3.429) (end 12.319 -20.32)
          (fill (type none))
        )
        (circle (center 5.969 -17.272) (radius 0.254)
          (fill (type outline))
        )
        (circle (center 5.969 -6.096) (radius 0.254)
          (fill (type outline))
        )
        (circle (center 7.747 -16.383) (radius 2.794)
          (fill (type none))
        )
        (circle (center 7.747 -7.112) (radius 2.794)
          (fill (type none))
        )
        (circle (center 9.525 -17.272) (radius 0.254)
          (fill (type outline))
        )
        (circle (center 9.525 -6.096) (radius 0.254)
          (fill (type outline))
        )
      )
      (symbol "PJT7603_R1_00001_1_1"
        (pin input line (at 0.508 -6.096 0) (length 2.54)
          (name "S1")
          (number "1")
        )
        (pin passive line (at 0.508 -11.43 0) (length 2.54)
          (name "G1")
          (number "2")
        )
        (pin passive line (at 0.508 -17.272 0) (length 2.54)
          (name "D2")
          (number "3")
        )
        (pin passive line (at 14.224 -17.272 180) (length 2.54)
          (name "S2")
          (number "4")
        )
        (pin passive line (at 14.224 -11.43 180) (length 2.54)
          (name "G2")
          (number "5")
        )
        (pin input line (at 14.224 -6.096 180) (length 2.54)
          (name "D1")
          (number "6")
        )
      )
    )
  )
  (junction (at 113.03 60.96) (diameter 0) (color 0 0 0 0))
  (junction (at 113.03 106.68) (diameter 0) (color 0 0 0 0))
  (junction (at 229.87 71.12) (diameter 0) (color 0 0 0 0))
  (junction (at 40.64 63.5) (diameter 0) (color 0 0 0 0))
  (junction (at 91.44 106.68) (diameter 0) (color 0 0 0 0))
  (junction (at 60.96 60.96) (diameter 0) (color 0 0 0 0))
  (junction (at 119.38 106.68) (diameter 0) (color 0 0 0 0))
  (junction (at 167.767 60.96) (diameter 0) (color 0 0 0 0))
  (junction (at 40.64 60.96) (diameter 0) (color 0 0 0 0))
  (junction (at 26.67 60.96) (diameter 0) (color 0 0 0 0))
  (junction (at 242.57 71.12) (diameter 0) (color 0 0 0 0))
  (junction (at 229.87 106.553) (diameter 0) (color 0 0 0 0))
  (junction (at 153.162 106.68) (diameter 0) (color 0 0 0 0))
  (junction (at 195.58 60.96) (diameter 0) (color 0 0 0 0))
  (junction (at 195.58 106.68) (diameter 0) (color 0 0 0 0))
  (junction (at 91.44 60.96) (diameter 0) (color 0 0 0 0))
  (junction (at 26.67 106.68) (diameter 0) (color 0 0 0 0))
  (junction (at 144.78 106.68) (diameter 0) (color 0 0 0 0))
  (junction (at 60.96 81.28) (diameter 0) (color 0 0 0 0))
  (junction (at 242.57 60.96) (diameter 0) (color 0 0 0 0))
  (junction (at 167.894 83.439) (diameter 0) (color 0 0 0 0))
  (junction (at 171.45 106.68) (diameter 0) (color 0 0 0 0))
  (junction (at 119.38 60.96) (diameter 0) (color 0 0 0 0))
  (junction (at 181.737 60.96) (diameter 0) (color 0 0 0 0))
  (junction (at 171.45 93.98) (diameter 0) (color 0 0 0 0))
  (junction (at 85.09 60.96) (diameter 0) (color 0 0 0 0))
  (junction (at 144.78 95.25) (diameter 0) (color 0 0 0 0))
  (junction (at 195.58 106.553) (diameter 0) (color 0 0 0 0))
  (junction (at 85.09 106.68) (diameter 0) (color 0 0 0 0))
  (junction (at 229.87 60.96) (diameter 0) (color 0 0 0 0))
  (junction (at 60.96 106.68) (diameter 0) (color 0 0 0 0))
  (wire (pts (xy 44.45 78.74) (xy 40.64 78.74)))
  (wire (pts (xy 26.67 60.96) (xy 26.67 76.2)))
  (wire (pts (xy 52.07 63.5) (xy 55.88 63.5)))
  (wire (pts (xy 167.894 83.439) (xy 167.894 88.773)))
  (wire (pts (xy 144.78 95.25) (xy 144.78 83.439)))
  (wire (pts (xy 171.45 93.98) (xy 193.04 93.98)))
  (wire (pts (xy 149.352 93.98) (xy 171.45 93.98)))
  (wire (pts (xy 181.737 60.96) (xy 195.58 60.96)))
  (wire (pts (xy 62.23 81.28) (xy 60.96 81.28)))
  (wire (pts (xy 113.03 106.68) (xy 119.38 106.68)))
  (wire (pts (xy 171.45 93.98) (xy 171.45 96.52)))
  (wire (pts (xy 167.767 64.643) (xy 167.767 60.96)))
  (wire (pts (xy 113.03 81.28) (xy 113.03 60.96)))
  (wire (pts (xy 91.44 88.9) (xy 91.44 106.68)))
  (wire (pts (xy 181.737 72.517) (xy 181.737 83.439)))
  (wire (pts (xy 181.737 83.439) (xy 167.894 83.439)))
  (wire (pts (xy 144.78 95.25) (xy 144.78 96.52)))
  (wire (pts (xy 171.45 104.14) (xy 171.45 106.68)))
  (wire (pts (xy 144.78 83.439) (xy 154.051 83.439)))
  (wire (pts (xy 195.58 71.12) (xy 195.58 106.553)))
  (wire (pts (xy 21.59 106.68) (xy 26.67 106.68)))
  (wire (pts (xy 119.38 106.68) (xy 144.78 106.68)))
  (wire (pts (xy 195.58 121.92) (xy 195.58 106.68)))
  (wire (pts (xy 153.162 106.68) (xy 171.45 106.68)))
  (wire (pts (xy 60.96 63.5) (xy 60.96 60.96)))
  (wire (pts (xy 153.162 88.773) (xy 153.162 106.68)))
  (wire (pts (xy 52.07 78.74) (xy 55.88 78.74)))
  (wire (pts (xy 193.04 66.04) (xy 193.04 93.98)))
  (wire (pts (xy 26.67 60.96) (xy 40.64 60.96)))
  (wire (pts (xy 181.737 64.897) (xy 181.737 60.96)))
  (wire (pts (xy 119.38 60.96) (xy 119.38 81.28)))
  (wire (pts (xy 119.38 88.9) (xy 119.38 106.68)))
  (wire (pts (xy 26.67 106.68) (xy 60.96 106.68)))
  (wire (pts (xy 154.051 77.597) (xy 149.352 77.597)))
  (wire (pts (xy 21.59 60.96) (xy 26.67 60.96)))
  (wire (pts (xy 58.42 60.96) (xy 60.96 60.96)))
  (wire (pts (xy 171.45 106.68) (xy 195.58 106.68)))
  (wire (pts (xy 167.894 88.773) (xy 167.767 88.773)))
  (wire (pts (xy 91.44 81.28) (xy 91.44 60.96)))
  (wire (pts (xy 154.051 88.773) (xy 153.162 88.773)))
  (wire (pts (xy 105.41 60.96) (xy 113.03 60.96)))
  (wire (pts (xy 242.57 71.12) (xy 248.92 71.12)))
  (wire (pts (xy 91.44 60.96) (xy 97.79 60.96)))
  (wire (pts (xy 40.64 63.5) (xy 40.64 60.96)))
  (wire (pts (xy 40.64 63.5) (xy 40.64 78.74)))
  (wire (pts (xy 195.58 106.553) (xy 195.58 106.68)))
  (wire (pts (xy 139.7 95.25) (xy 144.78 95.25)))
  (wire (pts (xy 195.58 39.37) (xy 195.58 60.96)))
  (wire (pts (xy 119.38 60.96) (xy 167.767 60.96)))
  (wire (pts (xy 113.03 60.96) (xy 119.38 60.96)))
  (wire (pts (xy 167.767 60.96) (xy 181.737 60.96)))
  (wire (pts (xy 113.03 88.9) (xy 113.03 106.68)))
  (wire (pts (xy 229.87 71.12) (xy 229.87 106.553)))
  (wire (pts (xy 242.57 71.12) (xy 229.87 71.12)))
  (wire (pts (xy 91.44 106.68) (xy 113.03 106.68)))
  (wire (pts (xy 149.352 77.597) (xy 149.352 93.98)))
  (wire (pts (xy 214.884 106.553) (xy 229.87 106.553)))
  (wire (pts (xy 193.04 66.04) (xy 195.58 66.04)))
  (wire (pts (xy 195.58 121.92) (xy 207.01 121.92)))
  (wire (pts (xy 214.63 121.92) (xy 229.87 121.92)))
  (wire (pts (xy 229.87 39.37) (xy 229.87 60.96)))
  (wire (pts (xy 242.57 60.96) (xy 248.92 60.96)))
  (wire (pts (xy 242.57 60.96) (xy 242.57 62.23)))
  (wire (pts (xy 85.09 81.28) (xy 85.09 60.96)))
  (polyline (pts (xy 211.074 18.542) (xy 211.074 145.542)))
  (wire (pts (xy 214.757 39.37) (xy 229.87 39.37)))
  (wire (pts (xy 226.06 71.12) (xy 229.87 71.12)))
  (wire (pts (xy 85.09 106.68) (xy 91.44 106.68)))
  (wire (pts (xy 167.767 83.439) (xy 167.894 83.439)))
  (wire (pts (xy 60.96 60.96) (xy 85.09 60.96)))
  (wire (pts (xy 60.96 106.68) (xy 85.09 106.68)))
  (wire (pts (xy 229.87 106.553) (xy 229.87 121.92)))
  (wire (pts (xy 60.96 81.28) (xy 60.96 82.55)))
  (wire (pts (xy 85.09 60.96) (xy 91.44 60.96)))
  (wire (pts (xy 167.767 72.263) (xy 167.767 77.597)))
  (wire (pts (xy 242.57 69.85) (xy 242.57 71.12)))
  (wire (pts (xy 195.58 106.553) (xy 207.264 106.553)))
  (wire (pts (xy 207.137 39.37) (xy 195.58 39.37)))
  (wire (pts (xy 40.64 60.96) (xy 50.8 60.96)))
  (wire (pts (xy 226.06 60.96) (xy 229.87 60.96)))
  (wire (pts (xy 60.96 90.17) (xy 60.96 106.68)))
  (wire (pts (xy 60.96 81.28) (xy 60.96 78.74)))
  (wire (pts (xy 85.09 88.9) (xy 85.09 106.68)))
  (wire (pts (xy 26.67 106.68) (xy 26.67 83.82)))
  (wire (pts (xy 144.78 104.14) (xy 144.78 106.68)))
  (wire (pts (xy 229.87 60.96) (xy 242.57 60.96)))
  (wire (pts (xy 40.64 63.5) (xy 44.45 63.5)))
  (wire (pts (xy 144.78 106.68) (xy 153.162 106.68)))
  (text "Isolation Boundary\n" (at 210.185 97.79 90))
  (text "Note: R10 is included to bypass isolation if desired.\n"
    (at 226.06 162.56 0)
  )
  (hierarchical_label "GND" (shape input) (at 248.92 71.12 0) (fields_autoplaced))
  (hierarchical_label "GNDD" (shape input) (at 21.59 106.68 180) (fields_autoplaced))
  (hierarchical_label "VIN" (shape input) (at 21.59 60.96 180) (fields_autoplaced))
  (hierarchical_label "VOUT" (shape input) (at 248.92 60.96 0) (fields_autoplaced))
  (hierarchical_label "CTRL" (shape input) (at 139.7 95.25 180) (fields_autoplaced))
  (hierarchical_label "FuseDet" (shape input) (at 62.23 81.28 0) (fields_autoplaced))
  (symbol (lib_id "Device:C") (at 91.44 85.09 0) (unit 1)
    (in_bom yes) (on_board yes) (dnp no)
    (property "Reference" "C21" (at 93.98 82.55 0))
    (property "Value" "4.7uF" (at 93.98 85.09 0))
    (property "Footprint" "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder" (at 92.4052 88.9 0))
    (property "Datasheet" "~" (at 91.44 85.09 0))
    (property "Field4" "50V" (at 96.52 87.63 0))
    (pin "1")
    (pin "2")
    (instances
      (project "channelCard"
        (path
          (reference "C21") (unit 1)
        )
        (path
          (reference "C22") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "Device:L_Iron") (at 101.6 60.96 90) (unit 1)
    (in_bom yes) (on_board yes) (dnp no) (fields_autoplaced)
    (property "Reference" "L1" (at 101.6 54.61 90))
    (property "Value" "22uH 4 A" (at 101.6 57.15 90))
    (property "Footprint" "footprint_Library:SPM7054VC-220M-D" (at 101.6 60.96 0))
    (property "Datasheet" "https://product.tdk.com/system/files/dam/doc/product/inductor/inductor/smd/catalog/inductor_automotive_power_spm7054vc-d_en.pdf" (at 101.6 60.96 0))
    (property "Part Number" "SPM7054VC-220M-D" (at 101.6 60.96 90))
    (pin "1")
    (pin "2")
    (instances
      (project "channelCard"
        (path
          (reference "L1") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "Device:R") (at 167.767 68.453 0) (unit 1)
    (in_bom yes) (on_board yes) (dnp no) (fields_autoplaced)
    (property "Reference" "R8" (at 170.307 67.183 0))
    (property "Value" "22000" (at 170.307 69.723 0))
    (property "Footprint" "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (at 165.989 68.453 90))
    (property "Datasheet" "~" (at 167.767 68.453 0))
    (pin "1")
    (pin "2")
    (instances
      (project "channelCard"
        (path
          (reference "R8") (unit 1)
        )
        (path
          (reference "R18") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "Device:R") (at 48.26 78.74 90) (unit 1)
    (in_bom yes) (on_board yes) (dnp no)
    (property "Reference" "R29" (at 43.18 81.28 90))
    (property "Value" "39000" (at 48.26 81.28 90))
    (property "Footprint" "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (at 48.26 80.518 90))
    (property "Datasheet" "~" (at 48.26 78.74 0))
    (pin "1")
    (pin "2")
    (instances
      (project "channelCard"
        (path
          (reference "R29") (unit 1)
        )
        (path
          (reference "R28") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "Device:R") (at 181.737 68.707 180) (unit 1)
    (in_bom yes) (on_board yes) (dnp no) (fields_autoplaced)
    (property "Reference" "R8" (at 184.277 67.437 0))
    (property "Value" "22000" (at 184.277 69.977 0))
    (property "Footprint" "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (at 183.515 68.707 90))
    (property "Datasheet" "~" (at 181.737 68.707 0))
    (pin "1")
    (pin "2")
    (instances
      (project "channelCard"
        (path
          (reference "R8") (unit 1)
        )
        (path
          (reference "R21") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "Device:Polyfuse") (at 54.61 60.96 90) (unit 1)
    (in_bom yes) (on_board yes) (dnp no)
    (property "Reference" "F1" (at 54.61 54.61 90))
    (property "Value" "2920L075/60MR\n" (at 54.61 57.15 90))
    (property "Footprint" "ptcfootprints:2920L075&slash_60MR_LTF-M" (at 59.69 59.69 0))
    (property "Datasheet" "~" (at 54.61 60.96 0))
    (pin "1")
    (pin "2")
    (instances
      (project "channelCard"
        (path
          (reference "F1") (unit 1)
        )
        (path
          (reference "F1") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "Device:C") (at 211.074 106.553 90) (unit 1)
    (in_bom yes) (on_board yes) (dnp no)
    (property "Reference" "C21" (at 208.534 109.093 90))
    (property "Value" "1nF" (at 217.424 109.093 90))
    (property "Footprint" "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder" (at 214.884 105.5878 0))
    (property "Datasheet" "~" (at 211.074 106.553 0))
    (property "Field4" "2kV Y rated" (at 211.074 111.633 90))
    (pin "1")
    (pin "2")
    (instances
      (project "channelCard"
        (path
          (reference "C21") (unit 1)
        )
        (path
          (reference "C25") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "Device:C") (at 119.38 85.09 0) (unit 1)
    (in_bom yes) (on_board yes) (dnp no)
    (property "Reference" "C21" (at 123.19 82.55 0))
    (property "Value" "330uF" (at 123.19 85.09 0))
    (property "Footprint" "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder" (at 120.3452 88.9 0))
    (property "Datasheet" "~" (at 119.38 85.09 0))
    (property "Field4" "50V" (at 124.46 87.63 0))
    (pin "1")
    (pin "2")
    (instances
      (project "channelCard"
        (path
          (reference "C21") (unit 1)
        )
        (path
          (reference "C20") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "Device:R") (at 48.26 63.5 90) (unit 1)
    (in_bom yes) (on_board yes) (dnp no)
    (property "Reference" "R27" (at 43.18 66.04 90))
    (property "Value" "4.7k" (at 48.26 66.04 90))
    (property "Footprint" "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (at 48.26 65.278 90))
    (property "Datasheet" "~" (at 48.26 63.5 0))
    (pin "1")
    (pin "2")
    (instances
      (project "channelCard"
        (path
          (reference "R27") (unit 1)
        )
        (path
          (reference "R27") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "Diode:SMAJ26A") (at 26.67 80.01 270) (unit 1)
    (in_bom yes) (on_board yes) (dnp no)
    (property "Reference" "D7" (at 29.21 78.74 90))
    (property "Value" "SMAJ26A" (at 29.21 81.28 90))
    (property "Footprint" "Diode_SMD:D_SMA" (at 21.59 80.01 0))
    (property "Datasheet" "https://www.littelfuse.com/media?resourcetype=datasheets&itemid=75e32973-b177-4ee3-a0ff-cedaf1abdb93&filename=smaj-datasheet" (at 26.67 78.74 0))
    (pin "1")
    (pin "2")
    (instances
      (project "channelCard"
        (path
          (reference "D7") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "Device:R") (at 210.82 121.92 90) (unit 1)
    (in_bom yes) (on_board yes) (dnp no)
    (property "Reference" "R10" (at 210.82 119.38 90))
    (property "Value" "NP" (at 210.82 124.46 90))
    (property "Footprint" "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder" (at 210.82 123.698 90))
    (property "Datasheet" "~" (at 210.82 121.92 0))
    (pin "1")
    (pin "2")
    (instances
      (project "channelCard"
        (path
          (reference "R10") (unit 1)
        )
        (path
          (reference "R10") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "Device:R") (at 60.96 86.36 0) (unit 1)
    (in_bom yes) (on_board yes) (dnp no)
    (property "Reference" "R28" (at 57.15 83.82 0))
    (property "Value" "4.7k" (at 57.15 86.36 0))
    (property "Footprint" "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (at 59.182 86.36 90))
    (property "Datasheet" "~" (at 60.96 86.36 0))
    (pin "1")
    (pin "2")
    (instances
      (project "channelCard"
        (path
          (reference "R28") (unit 1)
        )
        (path
          (reference "R29") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "Device:C") (at 210.947 39.37 90) (unit 1)
    (in_bom yes) (on_board yes) (dnp no)
    (property "Reference" "C21" (at 208.407 41.91 90))
    (property "Value" "1nF" (at 217.297 41.91 90))
    (property "Footprint" "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder" (at 214.757 38.4048 0))
    (property "Datasheet" "2kV Y rated" (at 210.947 44.704 90))
    (pin "1")
    (pin "2")
    (instances
      (project "channelCard"
        (path
          (reference "C21") (unit 1)
        )
        (path
          (reference "C24") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "flexLinkLibrary:PJT7603_R1_00001") (at 153.543 94.869 0) (mirror x) (unit 1)
    (in_bom yes) (on_board yes) (dnp no)
    (property "Reference" "U14" (at 161.671 72.771 0))
    (property "Value" "~" (at 153.543 94.869 0))
    (property "Footprint" "Package_TO_SOT_SMD:SOT-363_SC-70-6_Handsoldering" (at 153.543 94.869 0))
    (property "Datasheet" "" (at 153.543 94.869 0))
    (pin "1")
    (pin "2")
    (pin "3")
    (pin "4")
    (pin "5")
    (pin "6")
    (instances
      (project "channelCard"
        (path
          (reference "U14") (unit 1)
        )
        (path
          (reference "U15") (unit 1)
        )
        (path
          (reference "U16") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "Device:R") (at 144.78 100.33 0) (unit 1)
    (in_bom yes) (on_board yes) (dnp no) (fields_autoplaced)
    (property "Reference" "R8" (at 147.32 99.06 0))
    (property "Value" "4.7k" (at 147.32 101.6 0))
    (property "Footprint" "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (at 143.002 100.33 90))
    (property "Datasheet" "~" (at 144.78 100.33 0))
    (pin "1")
    (pin "2")
    (instances
      (project "channelCard"
        (path
          (reference "R8") (unit 1)
        )
        (path
          (reference "R26") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "Isolator:SFH617A-1X007T") (at 58.42 71.12 90) (mirror x) (unit 1)
    (in_bom yes) (on_board yes) (dnp no) (fields_autoplaced)
    (property "Reference" "U12" (at 63.5 69.85 90))
    (property "Value" "SFH617A-1X007T" (at 63.5 72.39 90))
    (property "Footprint" "Package_DIP:SMDIP-4_W9.53mm_Clearance8mm" (at 67.31 71.12 0))
    (property "Datasheet" "http://www.vishay.com/docs/83740/sfh617a.pdf" (at 59.69 71.12 0))
    (pin "1")
    (pin "2")
    (pin "3")
    (pin "4")
    (instances
      (project "channelCard"
        (path
          (reference "U12") (unit 1)
        )
        (path
          (reference "U12") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "Device:C") (at 113.03 85.09 0) (unit 1)
    (in_bom yes) (on_board yes) (dnp no)
    (property "Reference" "C21" (at 106.68 82.55 0))
    (property "Value" "4.7uF" (at 105.41 85.09 0))
    (property "Footprint" "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder" (at 113.9952 88.9 0))
    (property "Datasheet" "~" (at 113.03 85.09 0))
    (property "Field4" "50V" (at 109.22 87.63 0))
    (pin "1")
    (pin "2")
    (instances
      (project "channelCard"
        (path
          (reference "C21") (unit 1)
        )
        (path
          (reference "C23") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "Device:C") (at 242.57 66.04 0) (unit 1)
    (in_bom yes) (on_board yes) (dnp no)
    (property "Reference" "C20" (at 245.11 63.5 0))
    (property "Value" "100uF" (at 245.11 66.04 0))
    (property "Footprint" "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder" (at 243.5352 69.85 0))
    (property "Datasheet" "~" (at 242.57 66.04 0))
    (property "Field4" "50V" (at 247.65 68.58 0))
    (pin "1")
    (pin "2")
    (instances
      (project "channelCard"
        (path
          (reference "C20") (unit 1)
        )
        (path
          (reference "C21") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "Device:R") (at 171.45 100.33 0) (unit 1)
    (in_bom yes) (on_board yes) (dnp no) (fields_autoplaced)
    (property "Reference" "R8" (at 173.99 99.06 0))
    (property "Value" "4.7k" (at 173.99 101.6 0))
    (property "Footprint" "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (at 169.672 100.33 90))
    (property "Datasheet" "~" (at 171.45 100.33 0))
    (pin "1")
    (pin "2")
    (instances
      (project "channelCard"
        (path
          (reference "R8") (unit 1)
        )
        (path
          (reference "R19") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "Device:C") (at 85.09 85.09 0) (unit 1)
    (in_bom yes) (on_board yes) (dnp no)
    (property "Reference" "C21" (at 78.74 82.55 0))
    (property "Value" "330uF" (at 76.2 85.09 0))
    (property "Footprint" "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder" (at 86.0552 88.9 0))
    (property "Datasheet" "~" (at 85.09 85.09 0))
    (pin "1")
    (pin "2")
    (instances
      (project "channelCard"
        (path
          (reference "C21") (unit 1)
        )
        (path
          (reference "C26") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "PDQE15-Q24-S12-D:PDQE15-Q24-S12-D") (at 210.82 66.04 0) (unit 1)
    (in_bom yes) (on_board yes) (dnp no) (fields_autoplaced)
    (property "Reference" "PS1" (at 210.82 53.34 0))
    (property "Value" "PDQE15-Q24-S12-D" (at 210.82 55.88 0))
    (property "Footprint" "CONV_PDQE15-Q24-S12-D" (at 210.82 66.04 0))
    (property "Datasheet" "" (at 210.82 66.04 0))
    (property "PARTREV" "1.0" (at 210.82 66.04 0))
    (property "MANUFACTURER" "CUI Inc." (at 210.82 66.04 0))
    (property "MAXIMUM_PACKAGE_HEIGHT" "11.70mm" (at 210.82 66.04 0))
    (property "STANDARD" "Manufacturer Recommendations" (at 210.82 66.04 0))
    (pin "1")
    (pin "2")
    (pin "3")
    (pin "4")
    (pin "5")
    (pin "6")
    (instances
      (project "channelCard"
        (path
          (reference "PS1") (unit 1)
        )
        (path
          (reference "PS1") (unit 1)
        )
      )
    )
  )
)
