(kicad_pcb (version 20221018) (generator pcbnew)
  (general
    (thickness 1.6)
  )
  (paper "A4")
  (layers
    (0 "F.Cu" signal)
    (31 "B.Cu" signal)
    (32 "B.Adhes" user "B.Adhesive")
    (33 "F.Adhes" user "F.Adhesive")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (43 "Eco2.User" user "User.Eco2")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
    (50 "User.1" user)
    (51 "User.2" user)
    (52 "User.3" user)
    (53 "User.4" user)
    (54 "User.5" user)
    (55 "User.6" user)
    (56 "User.7" user)
    (57 "User.8" user)
    (58 "User.9" user)
  )
  (setup
    (pad_to_mask_clearance 0)
    (pcbplotparams
      (layerselection 0x00010fc_ffffffff)
      (plot_on_all_layers_selection 0x0000000_00000000)
      (disableapertmacros false)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (dashed_line_dash_ratio 12.000000)
      (dashed_line_gap_ratio 3.000000)
      (svgprecision 4)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory "")
    )
  )
  (net 0 "")
  (net 1 "unconnected-(PS1-TRIM-Pad5)")
  (net 2 "unconnected-(U2-ALERT-Pad3)")
  (net 3 "unconnected-(U3-ALERT-Pad3)")
  (net 4 "unconnected-(U5-Pad3)")
  (net 5 "unconnected-(U5-Pad5)")
  (net 6 "unconnected-(U1-2Y4-Pad3)")
  (net 7 "unconnected-(U1-2Y3-Pad5)")
  (net 8 "unconnected-(U1-2Y2-Pad7)")
  (net 9 "unconnected-(U1-1Y4-Pad12)")
  (net 10 "unconnected-(U1-1Y3-Pad14)")
  (net 11 "unconnected-(U1-1Y2-Pad16)")
  (net 12 "unconnected-(U9-PA02-Pad3)")
  (net 13 "unconnected-(U9-PA03-Pad4)")
  (net 14 "unconnected-(U9-PB08-Pad7)")
  (net 15 "unconnected-(U9-PB09-Pad8)")
  (net 16 "unconnected-(U9-PA04-Pad9)")
  (net 17 "unconnected-(U9-PA05-Pad10)")
  (net 18 "unconnected-(U9-PB10-Pad19)")
  (net 19 "unconnected-(U9-PB11-Pad20)")
  (net 20 "unconnected-(U9-PB22-Pad37)")
  (net 21 "unconnected-(U9-PB23-Pad38)")
  (net 22 "unconnected-(U9-PA27-Pad39)")
  (net 23 "unconnected-(U9-PA28-Pad41)")
  (net 24 "unconnected-(U9-PB02-Pad47)")
  (net 25 "unconnected-(U9-PB03-Pad48)")
  (net 26 "unconnected-(J1-ID-Pad4)")
  (net 27 "unconnected-(J3-Pad3)")
  (net 28 "unconnected-(J3-Pad6)")
  (net 29 "GNDD")
  (net 30 "Net-(U9-PA00)")
  (net 31 "Net-(U9-PA01)")
  (net 32 "Net-(U9-VDDCORE)")
  (net 33 "/D+")
  (net 34 "/D-")
  (net 35 "/SDA")
  (net 36 "/SCL")
  (net 37 "GND")
  (net 38 "/IsoSCL")
  (net 39 "/IsoSDA")
  (net 40 "/Iso3.3V")
  (net 41 "/A")
  (net 42 "/B")
  (net 43 "GNDPWR")
  (net 44 "Net-(C22-Pad1)")
  (net 45 "Net-(R5-Pad2)")
  (net 46 "/+24V")
  (net 47 "Net-(D3-A)")
  (net 48 "Net-(D5-A)")
  (net 49 "Net-(D1-A)")
  (net 50 "/BrdAdd1")
  (net 51 "/BrdAdd3")
  (net 52 "/BrdAdd2")
  (net 53 "/BrdAdd4")
  (net 54 "Net-(U6-VREG)")
  (net 55 "Net-(D2-A)")
  (net 56 "Net-(U3-VBUS)")
  (net 57 "/Gnd Det/Seawater")
  (net 58 "Net-(U3-IN+)")
  (net 59 "Net-(U3-IN-)")
  (net 60 "/Power Monitor/VBUS")
  (net 61 "/Gnd Det/GND")
  (net 62 "Net-(U3-A0)")
  (net 63 "/+12V out")
  (net 64 "/Ctl B")
  (net 65 "/Ctl A")
  (net 66 "/UART TX")
  (net 67 "/UART RX")
  (net 68 "Net-(U1-~{1OE})")
  (net 69 "Net-(U1-1A1)")
  (net 70 "Net-(U1-2A1)")
  (net 71 "Net-(U1-~{2OE})")
  (net 72 "Net-(PS1-VIN)")
  (net 73 "/3v3LDO/VIN")
  (net 74 "Net-(PS1-CTRL)")
  (net 75 "/+3.3V")
  (net 76 "/3v3LDO1/VIN")
  (net 77 "Net-(D1-K)")
  (net 78 "Net-(U10-SS)")
  (net 79 "Net-(U11-SS)")
  (net 80 "/RelayOut")
  (net 81 "/GndDetEn")
  (net 82 "Net-(U16-S2)")
  (net 83 "Net-(U16-D1)")
  (net 84 "/10E'")
  (net 85 "Net-(U8-ANODE1)")
  (net 86 "/20E'")
  (net 87 "Net-(U8-ANODE2)")
  (net 88 "/1A1")
  (net 89 "Net-(U8-ANODE3)")
  (net 90 "/2A1")
  (net 91 "Net-(U8-ANODE4)")
  (net 92 "/PwrCTRL")
  (net 93 "Net-(R27-Pad2)")
  (net 94 "Net-(R28-Pad2)")
  (net 95 "/FuseDet")
  (net 96 "Net-(U15-D1)")
  (net 97 "/LeakSig")
  (net 98 "Net-(U13-N1G)")
  (net 99 "/RelayCtrl")
  (net 100 "Net-(U13-N2G)")
  (net 101 "/LeakCTRL")
  (net 102 "/LeakSIG")
  (net 103 "/Leak-")
  (net 104 "/Leak+")
  (net 105 "/SWD")
  (net 106 "/SWCLK")
  (net 107 "Net-(J4-Pin_6)")
  (net 108 "Net-(J4-Pin_7)")
  (net 109 "unconnected-(J4-Pin_8-Pad8)")
  (net 110 "/Reset_L")
  (net 111 "unconnected-(R20-Pad1)")
  (net 112 "unconnected-(R36-Pad1)")
  (footprint "datasheets:SON65P200X200X65-7N" (layer "F.Cu")
    (at 122.2625 119.78)
    (property "MF" "Analog Devices")
    (property "PARTREV" "E")
    (property "SNAPEDA_PACKAGE_ID" "19057")
    (property "STANDARD" "IPC-7351B")
    (property "Sheetfile" "3v3LDO.kicad_sch")
    (property "Sheetname" "3v3LDO")
    (attr smd)
    (fp_text reference "U10" (at 0.375 -2.215) (layer "F.SilkS"))
    (fp_text value "ADP7142ACPZN3.3-R7" (at 9.465 2.345) (layer "F.Fab"))
    (pad "1" smd oval (at -1.005 -0.65) (size 0.71 0.32) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 75 "/+3.3V") (pinfunction "VOUT") (pintype "output"))
    (pad "2" smd oval (at -1.005 0) (size 0.71 0.32) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 75 "/+3.3V") (pinfunction "SENSE/ADJ") (pintype "input"))
    (pad "3" smd oval (at -1.005 0.65) (size 0.71 0.32) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 29 "GNDD") (pinfunction "GND") (pintype "power_in"))
    (pad "4" smd oval (at 1.005 0.65 180) (size 0.71 0.32) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 73 "/3v3LDO/VIN") (pinfunction "EN") (pintype "input"))
    (pad "5" smd oval (at 1.005 0 180) (size 0.71 0.32) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 78 "Net-(U10-SS)") (pinfunction "SS") (pintype "passive"))
    (pad "6" smd oval (at 1.005 -0.65 180) (size 0.71 0.32) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 73 "/3v3LDO/VIN") (pinfunction "VIN") (pintype "input"))
    (pad "7" smd rect (at 0 0) (size 1 1.6) (layers "F.Cu" "F.Mask")
      (net 29 "GNDD") (pinfunction "EP") (pintype "power_in"))
  )
  (footprint "Package_TO_SOT_SMD:SOT-363_SC-70-6_Handsoldering" (layer "F.Cu")
    (at 159.42 123.54)
    (descr "SOT-363, SC-70-6, Handsoldering")
    (tags "SOT-363 SC-70-6 Handsoldering")
    (property "Sheetfile" "channelCard.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "U15" (at 0 -2) (layer "F.SilkS"))
    (fp_text value "PJT7603-R1-00001" (at 0 2 180) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd rect (at -1.33 -0.65) (size 1.5 0.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 29 "GNDD") (pinfunction "S1") (pintype "input"))
    (pad "2" smd rect (at -1.33 0) (size 1.5 0.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 99 "/RelayCtrl") (pinfunction "G1") (pintype "passive"))
    (pad "3" smd rect (at -1.33 0.65) (size 1.5 0.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 80 "/RelayOut") (pinfunction "D2") (pintype "passive"))
    (pad "4" smd rect (at 1.33 0.65) (size 1.5 0.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 46 "/+24V") (pinfunction "S2") (pintype "passive"))
    (pad "5" smd rect (at 1.33 0) (size 1.5 0.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 96 "Net-(U15-D1)") (pinfunction "G2") (pintype "passive"))
    (pad "6" smd rect (at 1.33 -0.65) (size 1.5 0.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 96 "Net-(U15-D1)") (pinfunction "D1") (pintype "input"))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-363_SC-70-6.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "PDQE15-Q24-S12-D:CONV_PDQE15-Q24-S12-D" (layer "F.Cu")
    (at 113.55 76.04 90)
    (property "MANUFACTURER" "CUI Inc.")
    (property "MAXIMUM_PACKAGE_HEIGHT" "11.70mm")
    (property "PARTREV" "1.0")
    (property "STANDARD" "Manufacturer Recommendations")
    (property "Sheetfile" "DC-DC.kicad_sch")
    (property "Sheetname" "DC-DC")
    (attr through_hole)
    (fp_text reference "PS1" (at -8.89 -13.97 90) (layer "F.SilkS"))
    (fp_text value "PDQE15-Q24-S12-D" (at 1.27 13.97 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at -10.16 -10.16 90) (size 2.25 2.25) (drill 1.5) (layers "*.Cu" "*.Mask")
      (net 74 "Net-(PS1-CTRL)") (pinfunction "CTRL") (pintype "input"))
    (pad "2" thru_hole circle (at -10.16 -2.54 90) (size 2.25 2.25) (drill 1.5) (layers "*.Cu" "*.Mask")
      (net 29 "GNDD") (pinfunction "GND") (pintype "power_in"))
    (pad "3" thru_hole circle (at -10.16 2.54 90) (size 2.25 2.25) (drill 1.5) (layers "*.Cu" "*.Mask")
      (net 72 "Net-(PS1-VIN)") (pinfunction "VIN") (pintype "input"))
    (pad "4" thru_hole circle (at 10.16 10.16 90) (size 2.25 2.25) (drill 1.5) (layers "*.Cu" "*.Mask")
      (net 76 "/3v3LDO1/VIN") (pinfunction "+VO") (pintype "output"))
    (pad "5" thru_hole circle (at 10.16 0 90) (size 2.25 2.25) (drill 1.5) (layers "*.Cu" "*.Mask")
      (net 1 "unconnected-(PS1-TRIM-Pad5)") (pinfunction "TRIM") (pintype "passive"))
    (pad "6" thru_hole circle (at 10.16 -10.16 90) (size 2.25 2.25) (drill 1.5) (layers "*.Cu" "*.Mask")
      (net 37 "GND") (pinfunction "0V") (pintype "output"))
    (model ":ATLAS:PDQE15-Q24-S12-D/PDQE15-Q24-S12-D.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 -90))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder" (layer "F.Cu")
    (at 118.13 119.97)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "3v3LDO.kicad_sch")
    (property "Sheetname" "3v3LDO")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C27" (at -3.07 0.08) (layer "F.SilkS"))
    (fp_text value "2.2uF" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.8625 0) (size 1.075 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 73 "/3v3LDO/VIN") (pintype "passive"))
    (pad "2" smd roundrect (at 0.8625 0) (size 1.075 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 29 "GNDD") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "F.Cu")
    (at 92.76 79.95)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "DC-DC.kicad_sch")
    (property "Sheetname" "DC-DC")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R19" (at 0 -1.43) (layer "F.SilkS"))
    (fp_text value "4.7k" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 74 "Net-(PS1-CTRL)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 29 "GNDD") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder" (layer "F.Cu")
    (at 124.51 60.1)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "channelCard.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C9" (at 2.56 -0.07) (layer "F.SilkS"))
    (fp_text value ".1u" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.8625 0) (size 1.075 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 37 "GND") (pintype "passive"))
    (pad "2" smd roundrect (at 0.8625 0) (size 1.075 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 40 "/Iso3.3V") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder" (layer "F.Cu")
    (at 110.78 53.57)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "3v3LDO.kicad_sch")
    (property "Sheetname" "3v3LDO1")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C14" (at 0 -1.43) (layer "F.SilkS"))
    (fp_text value "1nF" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.8625 0) (size 1.075 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 79 "Net-(U11-SS)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.8625 0) (size 1.075 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 37 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MountingHole:MountingHole_2.7mm_Pad_Via" locked (layer "F.Cu")
    (at 120 110.25)
    (descr "Mounting Hole 2.7mm")
    (tags "mounting hole 2.7mm")
    (property "Sheetfile" "channelCard.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Mounting Hole without connection")
    (property "ki_keywords" "mounting hole")
    (attr exclude_from_pos_files)
    (fp_text reference "H3" (at 0 -3.7) (layer "F.SilkS") hide)
    (fp_text value "MountingHole" (at 0 3.7) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab") hide)
    (pad "1" thru_hole circle locked (at -2.025 0) (size 0.8 0.8) (drill 0.5) (layers "*.Cu" "*.Mask"))
    (pad "1" thru_hole circle locked (at -1.431891 -1.431891) (size 0.8 0.8) (drill 0.5) (layers "*.Cu" "*.Mask"))
    (pad "1" thru_hole circle locked (at -1.431891 1.431891) (size 0.8 0.8) (drill 0.5) (layers "*.Cu" "*.Mask"))
    (pad "1" thru_hole circle locked (at 0 -2.025) (size 0.8 0.8) (drill 0.5) (layers "*.Cu" "*.Mask"))
    (pad "1" thru_hole circle locked (at 0 0) (size 5.4 5.4) (drill 2.7) (layers "*.Cu" "*.Mask"))
    (pad "1" thru_hole circle locked (at 0 2.025) (size 0.8 0.8) (drill 0.5) (layers "*.Cu" "*.Mask"))
    (pad "1" thru_hole circle locked (at 1.431891 -1.431891) (size 0.8 0.8) (drill 0.5) (layers "*.Cu" "*.Mask"))
    (pad "1" thru_hole circle locked (at 1.431891 1.431891) (size 0.8 0.8) (drill 0.5) (layers "*.Cu" "*.Mask"))
    (pad "1" thru_hole circle locked (at 2.025 0) (size 0.8 0.8) (drill 0.5) (layers "*.Cu" "*.Mask"))
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder" (layer "F.Cu")
    (at 110.78 56.08)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "3v3LDO.kicad_sch")
    (property "Sheetname" "3v3LDO1")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C28" (at 0 -1.43) (layer "F.SilkS"))
    (fp_text value "2.2uF" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.8625 0) (size 1.075 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 76 "/3v3LDO1/VIN") (pintype "passive"))
    (pad "2" smd roundrect (at 0.8625 0) (size 1.075 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 37 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "bme280:PSON65P250X250X100-8N" (layer "F.Cu")
    (at 146.41 87.37)
    (descr "2.5 mm x 2.5 mm x 0.93 mm metal lid LGA")
    (property "AVAILABILITY" "Good")
    (property "DESCRIPTION" "Integrated pressure, humidity and temperature sensor; 8-pin 2.5x2.5x0.93mm LGA")
    (property "MF" "Bosch")
    (property "MP" "BME280")
    (property "PACKAGE" "LGA-8 Bosch")
    (property "PRICE" "4.94 USD")
    (property "STANDARD" "IPC-7351B")
    (property "Sheetfile" "bme280.kicad_sch")
    (property "Sheetname" "BME280")
    (attr smd)
    (fp_text reference "U7" (at -0.235245 -1.866763) (layer "F.SilkS"))
    (fp_text value "BME280" (at 3.077771 1.80686) (layer "F.Fab"))
    (pad "1" smd roundrect (at 0.97 -0.975) (size 0.49 0.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.06)
      (net 29 "GNDD") (pinfunction "GND") (pintype "power_in"))
    (pad "2" smd roundrect (at 0.97 -0.325) (size 0.49 0.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.06)
      (net 75 "/+3.3V") (pinfunction "CSB") (pintype "input"))
    (pad "3" smd roundrect (at 0.97 0.325) (size 0.49 0.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.06)
      (net 35 "/SDA") (pinfunction "SDI") (pintype "bidirectional"))
    (pad "4" smd roundrect (at 0.97 0.975) (size 0.49 0.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.06)
      (net 36 "/SCL") (pinfunction "SCK") (pintype "input"))
    (pad "5" smd roundrect (at -0.97 0.975) (size 0.49 0.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.06)
      (net 29 "GNDD") (pinfunction "SDO") (pintype "bidirectional"))
    (pad "6" smd roundrect (at -0.97 0.325) (size 0.49 0.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.06)
      (net 75 "/+3.3V") (pinfunction "VDDIO") (pintype "power_in"))
    (pad "7" smd roundrect (at -0.97 -0.325) (size 0.49 0.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.06)
      (net 29 "GNDD") (pinfunction "GND__1") (pintype "power_in"))
    (pad "8" smd roundrect (at -0.97 -0.975) (size 0.49 0.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.06)
      (net 75 "/+3.3V") (pinfunction "VDD") (pintype "power_in"))
    (model ":ATLAS:bme280/BME280.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 -90))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder" (layer "F.Cu")
    (at 96.66 70.03)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Field4" "50V")
    (property "Sheetfile" "DC-DC.kicad_sch")
    (property "Sheetname" "DC-DC")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C21" (at 0 -1.43) (layer "F.SilkS"))
    (fp_text value "100uF" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.8625 0) (size 1.075 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 76 "/3v3LDO1/VIN") (pintype "passive"))
    (pad "2" smd roundrect (at 0.8625 0) (size 1.075 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 37 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_DIP:DIP-6_W7.62mm" (layer "F.Cu")
    (at 107.165 53.99 -90)
    (descr "6-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils)")
    (tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil")
    (property "Sheetfile" "channelCard.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Photo MOSFET optically coupled, ON 3.5A, 60mohm, OFF state 40V, Isolation 2500 VRMS, DIP-6")
    (property "ki_keywords" "photocouplers photorelay solidstate relay normally opened (1-Form-A)")
    (attr through_hole)
    (fp_text reference "U5" (at 3.96 2.995 90) (layer "F.SilkS"))
    (fp_text value "TLP3544" (at 3.81 7.41 90) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 3.81 2.54 90) (layer "F.Fab") hide)
    (pad "1" thru_hole rect (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 45 "Net-(R5-Pad2)") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 2.54 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 29 "GNDD") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 5.08 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 4 "unconnected-(U5-Pad3)") (pintype "no_connect"))
    (pad "4" thru_hole oval (at 7.62 5.08 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 43 "GNDPWR") (pintype "passive"))
    (pad "5" thru_hole oval (at 7.62 2.54 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 5 "unconnected-(U5-Pad5)") (pintype "passive"))
    (pad "6" thru_hole oval (at 7.62 0 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 57 "/Gnd Det/Seawater") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Package_DIP.3dshapes/DIP-6_W7.62mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "F.Cu")
    (at 132.36 67.6711 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Field4" "")
    (property "Sheetfile" "flexlinkTelemPM.kicad_sch")
    (property "Sheetname" "Power Monitor")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R17" (at 0.85 1.72) (layer "F.SilkS"))
    (fp_text value "0.1 Ohm" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 180) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 63 "/+12V out") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 180) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 76 "/3v3LDO1/VIN") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "F.Cu")
    (at 92.81 82.68)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "DC-DC.kicad_sch")
    (property "Sheetname" "DC-DC")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R18" (at 0 -1.43) (layer "F.SilkS"))
    (fp_text value "22000" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 72 "Net-(PS1-VIN)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 82 "Net-(U16-S2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "LED_SMD:LED_0603_1608Metric_Pad1.05x0.95mm_HandSolder" (layer "F.Cu")
    (at 115.175 53.61)
    (descr "LED SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "LED handsolder")
    (property "Sheetfile" "3v3LDO.kicad_sch")
    (property "Sheetname" "3v3LDO1")
    (property "ki_description" "Light emitting diode")
    (property "ki_keywords" "LED diode")
    (attr smd)
    (fp_text reference "D5" (at 0 -1.43) (layer "F.SilkS"))
    (fp_text value "LT Q39G-q100-25-1" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.875 0) (size 1.05 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 37 "GND") (pinfunction "K") (pintype "passive"))
    (pad "2" smd roundrect (at 0.875 0) (size 1.05 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 48 "Net-(D5-A)") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/LED_SMD.3dshapes/LED_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "8posMolex:CON_430450802_MOL" (layer "F.Cu")
    (at 112.609648 104.040001)
    (tags "430450802 ")
    (property "Sheetfile" "channelCard.kicad_sch")
    (property "Sheetname" "")
    (property "ki_keywords" "430450802")
    (attr through_hole)
    (fp_text reference "J2" (at -4.499999 -8.89 unlocked) (layer "F.SilkS"))
    (fp_text value "430450802" (at -4.499999 -8.89 unlocked) (layer "F.Fab"))
    (fp_text user "430450802" (at -4.499999 -13.71 unlocked) (layer "F.SilkS"))
    (fp_text user "NPTH_DRILL_SIZE:_3.0_MM,_TOLERANCE:_+0.05/-0.05" (at -4.499999 16.77 unlocked) (layer "Cmts.User"))
    (fp_text user "PTH_DRILL_SIZE:_1.02_MM,_TOLERANCE:_+0.05/-0.05" (at -4.499999 14.23 unlocked) (layer "Cmts.User"))
    (fp_text user "${REFERENCE}" (at -4.499999 -8.89 unlocked) (layer "F.Fab"))
    (fp_text user "430450802" (at -4.499999 -13.71 unlocked) (layer "F.Fab"))
    (pad "" np_thru_hole circle (at -6.839996 4.319999) (size 2.999999 2.999999) (drill 2.999999) (layers "*.Cu" "*.Mask"))
    (pad "" np_thru_hole circle (at -2.140006 4.319999) (size 2.999999 2.999999) (drill 2.999999) (layers "*.Cu" "*.Mask"))
    (pad "1" thru_hole rect (at 0 0) (size 1.52 1.52) (drill 1.02) (layers "*.Cu" "*.Mask")
      (net 41 "/A") (pinfunction "1") (pintype "unspecified"))
    (pad "2" thru_hole circle (at -2.999999 0) (size 1.52 1.52) (drill 1.02) (layers "*.Cu" "*.Mask")
      (net 41 "/A") (pinfunction "2") (pintype "unspecified"))
    (pad "3" thru_hole circle (at -5.999998 0) (size 1.52 1.52) (drill 1.02) (layers "*.Cu" "*.Mask")
      (net 46 "/+24V") (pinfunction "3") (pintype "unspecified"))
    (pad "4" thru_hole circle (at -8.999997 0) (size 1.52 1.52) (drill 1.02) (layers "*.Cu" "*.Mask")
      (net 29 "GNDD") (pinfunction "4") (pintype "unspecified"))
    (pad "5" thru_hole circle (at 0 -2.999999) (size 1.52 1.52) (drill 1.02) (layers "*.Cu" "*.Mask")
      (net 42 "/B") (pinfunction "5") (pintype "unspecified"))
    (pad "6" thru_hole circle (at -2.999999 -2.999999) (size 1.52 1.52) (drill 1.02) (layers "*.Cu" "*.Mask")
      (net 42 "/B") (pinfunction "6") (pintype "unspecified"))
    (pad "7" thru_hole circle (at -5.999998 -2.999999) (size 1.52 1.52) (drill 1.02) (layers "*.Cu" "*.Mask")
      (net 46 "/+24V") (pinfunction "7") (pintype "unspecified"))
    (pad "8" thru_hole circle (at -8.999997 -2.999999) (size 1.52 1.52) (drill 1.02) (layers "*.Cu" "*.Mask")
      (net 29 "GNDD") (pinfunction "8") (pintype "unspecified"))
    (model ":ATLAS:8posMolex/430450802.stp"
      (offset (xyz -4.5 -4 3.5))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )
  (footprint "MountingHole:MountingHole_2.7mm_Pad_Via" locked (layer "F.Cu")
    (at 134.5 81)
    (descr "Mounting Hole 2.7mm")
    (tags "mounting hole 2.7mm")
    (property "Sheetfile" "channelCard.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Mounting Hole without connection")
    (property "ki_keywords" "mounting hole")
    (attr exclude_from_pos_files)
    (fp_text reference "H2" (at 0 -3.7) (layer "F.SilkS") hide)
    (fp_text value "MountingHole" (at 0 3.7) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab") hide)
    (pad "1" thru_hole circle locked (at -2.025 0) (size 0.8 0.8) (drill 0.5) (layers "*.Cu" "*.Mask"))
    (pad "1" thru_hole circle locked (at -1.431891 -1.431891) (size 0.8 0.8) (drill 0.5) (layers "*.Cu" "*.Mask"))
    (pad "1" thru_hole circle locked (at -1.431891 1.431891) (size 0.8 0.8) (drill 0.5) (layers "*.Cu" "*.Mask"))
    (pad "1" thru_hole circle locked (at 0 -2.025) (size 0.8 0.8) (drill 0.5) (layers "*.Cu" "*.Mask"))
    (pad "1" thru_hole circle locked (at 0 0) (size 5.4 5.4) (drill 2.7) (layers "*.Cu" "*.Mask"))
    (pad "1" thru_hole circle locked (at 0 2.025) (size 0.8 0.8) (drill 0.5) (layers "*.Cu" "*.Mask"))
    (pad "1" thru_hole circle locked (at 1.431891 -1.431891) (size 0.8 0.8) (drill 0.5) (layers "*.Cu" "*.Mask"))
    (pad "1" thru_hole circle locked (at 1.431891 1.431891) (size 0.8 0.8) (drill 0.5) (layers "*.Cu" "*.Mask"))
    (pad "1" thru_hole circle locked (at 2.025 0) (size 0.8 0.8) (drill 0.5) (layers "*.Cu" "*.Mask"))
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder" (layer "F.Cu")
    (at 118.12 118.44)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "3v3LDO.kicad_sch")
    (property "Sheetname" "3v3LDO")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C10" (at 0 -1.43) (layer "F.SilkS"))
    (fp_text value "1nF" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.8625 0) (size 1.075 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 78 "Net-(U10-SS)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.8625 0) (size 1.075 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 29 "GNDD") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder" (layer "F.Cu")
    (at 96.66 72.54)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Field4" "50V")
    (property "Sheetfile" "DC-DC.kicad_sch")
    (property "Sheetname" "DC-DC")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C22" (at 0 -1.43) (layer "F.SilkS"))
    (fp_text value "4.7uF" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.8625 0) (size 1.075 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 44 "Net-(C22-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.8625 0) (size 1.075 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 29 "GNDD") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder" (layer "F.Cu")
    (at 96.66 77.56)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "DC-DC.kicad_sch")
    (property "Sheetname" "DC-DC")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C24" (at 0 -1.43) (layer "F.SilkS"))
    (fp_text value "1nF" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.8625 0) (size 1.075 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 72 "Net-(PS1-VIN)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.8625 0) (size 1.075 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 76 "/3v3LDO1/VIN") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "datasheets:SON65P200X200X65-7N" (layer "F.Cu")
    (at 114.37 57.28)
    (property "MF" "Analog Devices")
    (property "PARTREV" "E")
    (property "SNAPEDA_PACKAGE_ID" "19057")
    (property "STANDARD" "IPC-7351B")
    (property "Sheetfile" "3v3LDO.kicad_sch")
    (property "Sheetname" "3v3LDO1")
    (attr smd)
    (fp_text reference "U11" (at 0.375 -2.215) (layer "F.SilkS"))
    (fp_text value "ADP7142ACPZN3.3-R7" (at 9.465 2.345) (layer "F.Fab"))
    (pad "1" smd oval (at -1.005 -0.65) (size 0.71 0.32) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 40 "/Iso3.3V") (pinfunction "VOUT") (pintype "output"))
    (pad "2" smd oval (at -1.005 0) (size 0.71 0.32) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 40 "/Iso3.3V") (pinfunction "SENSE/ADJ") (pintype "input"))
    (pad "3" smd oval (at -1.005 0.65) (size 0.71 0.32) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 37 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "4" smd oval (at 1.005 0.65 180) (size 0.71 0.32) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 76 "/3v3LDO1/VIN") (pinfunction "EN") (pintype "input"))
    (pad "5" smd oval (at 1.005 0 180) (size 0.71 0.32) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 79 "Net-(U11-SS)") (pinfunction "SS") (pintype "passive"))
    (pad "6" smd oval (at 1.005 -0.65 180) (size 0.71 0.32) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 76 "/3v3LDO1/VIN") (pinfunction "VIN") (pintype "input"))
    (pad "7" smd rect (at 0 0) (size 1 1.6) (layers "F.Cu" "F.Mask")
      (net 37 "GND") (pinfunction "EP") (pintype "power_in"))
  )
  (footprint "Package_TO_SOT_SMD:SOT-363_SC-70-6_Handsoldering" (layer "F.Cu")
    (at 91.2 91.34)
    (descr "SOT-363, SC-70-6, Handsoldering")
    (tags "SOT-363 SC-70-6 Handsoldering")
    (property "Sheetfile" "DC-DC.kicad_sch")
    (property "Sheetname" "DC-DC")
    (attr smd)
    (fp_text reference "U16" (at 0 -2) (layer "F.SilkS"))
    (fp_text value "~" (at 0 2 180) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd rect (at -1.33 -0.65) (size 1.5 0.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 29 "GNDD") (pinfunction "S1") (pintype "input"))
    (pad "2" smd rect (at -1.33 0) (size 1.5 0.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 92 "/PwrCTRL") (pinfunction "G1") (pintype "passive"))
    (pad "3" smd rect (at -1.33 0.65) (size 1.5 0.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 74 "Net-(PS1-CTRL)") (pinfunction "D2") (pintype "passive"))
    (pad "4" smd rect (at 1.33 0.65) (size 1.5 0.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 82 "Net-(U16-S2)") (pinfunction "S2") (pintype "passive"))
    (pad "5" smd rect (at 1.33 0) (size 1.5 0.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 83 "Net-(U16-D1)") (pinfunction "G2") (pintype "passive"))
    (pad "6" smd rect (at 1.33 -0.65) (size 1.5 0.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 83 "Net-(U16-D1)") (pinfunction "D1") (pintype "input"))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-363_SC-70-6.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_DIP:SMDIP-4_W9.53mm_Clearance8mm" (layer "F.Cu")
    (at 84.42 84.14)
    (descr "4-lead surface-mounted (SMD) DIP package, row spacing 9.53 mm (375 mils), Clearance8mm")
    (tags "SMD DIP DIL PDIP SMDIP 2.54mm 9.53mm 375mil Clearance8mm")
    (property "Sheetfile" "DC-DC.kicad_sch")
    (property "Sheetname" "DC-DC")
    (property "ki_description" "Optocoupler, Phototransistor Output, 5300 VRMS, VCEO 70V, CTR% 40-80, -55 to +110 degree Celsius, UL, BSI, FIMKO, cUL, 8mm clearence SMD PDIP-4")
    (property "ki_keywords" "Optocoupler, Phototransistor Output, 5300 VRMS, VCEO 70V, CTR% 40-80")
    (attr smd)
    (fp_text reference "U12" (at 0 -3.6) (layer "F.SilkS"))
    (fp_text value "SFH617A-1X007T" (at 0 3.6) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd rect (at -4.765 -1.27) (size 1.5 1.78) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 93 "Net-(R27-Pad2)") (pintype "passive"))
    (pad "2" smd rect (at -4.765 1.27) (size 1.5 1.78) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 44 "Net-(C22-Pad1)") (pintype "passive"))
    (pad "3" smd rect (at 4.765 1.27) (size 1.5 1.78) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 95 "/FuseDet") (pintype "passive"))
    (pad "4" smd rect (at 4.765 -1.27) (size 1.5 1.78) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 94 "Net-(R28-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Package_DIP.3dshapes/SMDIP-4_W9.53mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "F.Cu")
    (at 81.218801 77.4276)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "DC-DC.kicad_sch")
    (property "Sheetname" "DC-DC")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R29" (at 0 -1.43) (layer "F.SilkS"))
    (fp_text value "4.7k" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 95 "/FuseDet") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 29 "GNDD") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "F.Cu")
    (at 164.32 125.94)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "channelCard.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R33" (at 0 -1.43) (layer "F.SilkS"))
    (fp_text value "4.7k" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 29 "GNDD") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 99 "/RelayCtrl") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "ptcfootprints:2920L075&slash_60MR_LTF-M" (layer "F.Cu")
    (at 105.51 94.22 90)
    (tags "2920L075/60MR ")
    (property "Sheetfile" "DC-DC.kicad_sch")
    (property "Sheetname" "DC-DC")
    (property "ki_description" "Resettable fuse, polymeric positive temperature coefficient")
    (property "ki_keywords" "resettable fuse PTC PPTC polyfuse polyswitch")
    (attr smd)
    (fp_text reference "F1" (at 0 0 90 unlocked) (layer "F.SilkS"))
    (fp_text value "2920L075/60MR\n" (at 0 0 90 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90 unlocked) (layer "F.Fab"))
    (pad "1" smd rect (at -3.0248 0 90) (size 3.048 5.4864) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 46 "/+24V") (pintype "passive"))
    (pad "2" smd rect (at 3.0248 0 90) (size 3.048 5.4864) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 44 "Net-(C22-Pad1)") (pintype "passive"))
    (zone (net 0) (net_name "") (layer "F.Cu") (hatch full 0.508)
      (connect_pads (clearance 0))
      (min_thickness 0.254) (filled_areas_thickness no)
      (keepout (tracks not_allowed) (vias not_allowed) (pads allowed) (copperpour not_allowed) (footprints allowed))
      (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
      (polygon
        (pts
          (xy 102.843 95.67)
          (xy 102.843 92.77)
          (xy 108.177 92.77)
          (xy 108.177 95.67)
        )
      )
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder" (layer "F.Cu")
    (at 113.13 61.23 90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "3v3LDO.kicad_sch")
    (property "Sheetname" "3v3LDO1")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C15" (at 0 -1.43 90) (layer "F.SilkS"))
    (fp_text value "2.2uF" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.8625 0 90) (size 1.075 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 40 "/Iso3.3V") (pintype "passive"))
    (pad "2" smd roundrect (at 0.8625 0 90) (size 1.075 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 37 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "rotary dip:220AMA16_CTS" (layer "F.Cu")
    (at 133.0409 94.7265 180)
    (tags "220AMA16R ")
    (property "Sheetfile" "channelCard.kicad_sch")
    (property "Sheetname" "")
    (property "ki_keywords" "220AMA16R")
    (attr smd)
    (fp_text reference "SW1" (at 0 0 180 unlocked) (layer "F.SilkS"))
    (fp_text value "220AMA16R" (at 0 0 180 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 180 unlocked) (layer "F.Fab"))
    (pad "1" smd rect (at -3.75 -2.54 180) (size 2.9972 0.9906) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 50 "/BrdAdd1") (pinfunction "1") (pintype "unspecified"))
    (pad "2" smd rect (at -3.75 0 180) (size 2.9972 0.9906) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 29 "GNDD") (pinfunction "C") (pintype "unspecified"))
    (pad "3" smd rect (at -3.75 2.54 180) (size 2.9972 0.9906) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 51 "/BrdAdd3") (pinfunction "4") (pintype "unspecified"))
    (pad "4" smd rect (at 3.75 2.54 180) (size 2.9972 0.9906) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 52 "/BrdAdd2") (pinfunction "2") (pintype "unspecified"))
    (pad "5" smd rect (at 3.75 0 180) (size 2.9972 0.9906) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 29 "GNDD") (pinfunction "C") (pintype "unspecified"))
    (pad "6" smd rect (at 3.75 -2.54 180) (size 2.9972 0.9906) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 53 "/BrdAdd4") (pinfunction "8") (pintype "unspecified"))
    (model ":ATLAS:220AMA16R/220AMA16R.STEP"
      (offset (xyz 0 0 0.19))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 -180))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder" (layer "F.Cu")
    (at 96.66 82.58)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "DC-DC.kicad_sch")
    (property "Sheetname" "DC-DC")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C26" (at 0 -1.43) (layer "F.SilkS"))
    (fp_text value "330uF" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.8625 0) (size 1.075 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 44 "Net-(C22-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.8625 0) (size 1.075 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 29 "GNDD") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MountingHole:MountingHole_2.7mm_Pad_Via" locked (layer "F.Cu")
    (at 120 53.5)
    (descr "Mounting Hole 2.7mm")
    (tags "mounting hole 2.7mm")
    (property "Sheetfile" "channelCard.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Mounting Hole without connection")
    (property "ki_keywords" "mounting hole")
    (attr exclude_from_pos_files)
    (fp_text reference "H1" (at 0 -3.7) (layer "F.SilkS") hide)
    (fp_text value "MountingHole" (at 0 3.7) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab") hide)
    (pad "1" thru_hole circle locked (at -2.025 0) (size 0.8 0.8) (drill 0.5) (layers "*.Cu" "*.Mask"))
    (pad "1" thru_hole circle locked (at -1.431891 -1.431891) (size 0.8 0.8) (drill 0.5) (layers "*.Cu" "*.Mask"))
    (pad "1" thru_hole circle locked (at -1.431891 1.431891) (size 0.8 0.8) (drill 0.5) (layers "*.Cu" "*.Mask"))
    (pad "1" thru_hole circle locked (at 0 -2.025) (size 0.8 0.8) (drill 0.5) (layers "*.Cu" "*.Mask"))
    (pad "1" thru_hole circle locked (at 0 0) (size 5.4 5.4) (drill 2.7) (layers "*.Cu" "*.Mask"))
    (pad "1" thru_hole circle locked (at 0 2.025) (size 0.8 0.8) (drill 0.5) (layers "*.Cu" "*.Mask"))
    (pad "1" thru_hole circle locked (at 1.431891 -1.431891) (size 0.8 0.8) (drill 0.5) (layers "*.Cu" "*.Mask"))
    (pad "1" thru_hole circle locked (at 1.431891 1.431891) (size 0.8 0.8) (drill 0.5) (layers "*.Cu" "*.Mask"))
    (pad "1" thru_hole circle locked (at 2.025 0) (size 0.8 0.8) (drill 0.5) (layers "*.Cu" "*.Mask"))
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder" (layer "F.Cu")
    (at 143.1125 88.56)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "bme280.kicad_sch")
    (property "Sheetname" "BME280")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C6" (at 0 -1.43) (layer "F.SilkS"))
    (fp_text value ".1u" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.8625 0) (size 1.075 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 29 "GNDD") (pintype "passive"))
    (pad "2" smd roundrect (at 0.8625 0) (size 1.075 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 75 "/+3.3V") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "footprints:VSSOP10_DGS_TEX" (layer "F.Cu")
    (at 133.61 71.71 90)
    (tags "INA228AIDGSR ")
    (property "Sheetfile" "flexlinkTelemPM.kicad_sch")
    (property "Sheetname" "Power Monitor")
    (property "ki_keywords" "INA228AIDGSR")
    (attr smd)
    (fp_text reference "U2" (at 0 0 90 unlocked) (layer "F.SilkS"))
    (fp_text value "INA228AIDGSR" (at 0 0 90 unlocked) (layer "F.Fab"))
    (fp_text user "*" (at -2.47015 -2.4224 90) (layer "F.SilkS"))
    (fp_text user "*" (at -2.47015 -2.4224 90 unlocked) (layer "F.SilkS"))
    (fp_text user "*" (at -1.1684 -1.4732 90 unlocked) (layer "F.Fab"))
    (fp_text user "*" (at -1.1684 -1.4732 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90 unlocked) (layer "F.Fab"))
    (pad "1" smd rect (at -2.21615 -1.000001 90) (size 1.3335 0.2794) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 37 "GND") (pinfunction "A1") (pintype "input"))
    (pad "2" smd rect (at -2.21615 -0.499999 90) (size 1.3335 0.2794) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 37 "GND") (pinfunction "A0") (pintype "input"))
    (pad "3" smd rect (at -2.21615 0 90) (size 1.3335 0.2794) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "unconnected-(U2-ALERT-Pad3)") (pinfunction "ALERT") (pintype "output"))
    (pad "4" smd rect (at -2.21615 0.499999 90) (size 1.3335 0.2794) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 39 "/IsoSDA") (pinfunction "SDA") (pintype "bidirectional"))
    (pad "5" smd rect (at -2.21615 1.000001 90) (size 1.3335 0.2794) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 38 "/IsoSCL") (pinfunction "SCL") (pintype "input"))
    (pad "6" smd rect (at 2.21615 1.000001 90) (size 1.3335 0.2794) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 40 "/Iso3.3V") (pinfunction "VS") (pintype "power_in"))
    (pad "7" smd rect (at 2.21615 0.499999 90) (size 1.3335 0.2794) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 37 "GND") (pinfunction "GND") (pintype "power_out"))
    (pad "8" smd rect (at 2.21615 0 90) (size 1.3335 0.2794) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 60 "/Power Monitor/VBUS") (pinfunction "VBUS") (pintype "power_in"))
    (pad "9" smd rect (at 2.21615 -0.499999 90) (size 1.3335 0.2794) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 63 "/+12V out") (pinfunction "IN-") (pintype "input"))
    (pad "10" smd rect (at 2.21615 -1.000001 90) (size 1.3335 0.2794) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 76 "/3v3LDO1/VIN") (pinfunction "IN+") (pintype "input"))
    (model ":ATLAS:ina228/INA219BIDR.STEP"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model ":ATLAS:ina228/INA228AIDGST.STEP"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )
  (footprint "footprint_Library:SPM7054VC-220M-D" (layer "F.Cu")
    (at 114.97 92.83 180)
    (property "Part Number" "SPM7054VC-220M-D")
    (property "Sheetfile" "DC-DC.kicad_sch")
    (property "Sheetname" "DC-DC")
    (property "ki_description" "Inductor with iron core")
    (property "ki_keywords" "inductor choke coil reactor magnetic")
    (attr smd)
    (fp_text reference "L1" (at 0 -0.5 180 unlocked) (layer "F.SilkS"))
    (fp_text value "22uH 4 A" (at 0 1 180 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 2.5 180 unlocked) (layer "F.Fab"))
    (pad "1" smd roundrect (at -4.4 0 180) (size 2.85 3.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 44 "Net-(C22-Pad1)") (pinfunction "1") (pintype "passive") (thermal_bridge_angle 45))
    (pad "2" smd roundrect (at 4.4 0 180) (size 2.85 3.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 72 "Net-(PS1-VIN)") (pinfunction "2") (pintype "passive") (thermal_bridge_angle 45))
    (model ":ATLAS:SPM7054VC-220M-D/spm7054vt.step"
      (offset (xyz 57 0 -38.5))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )
  (footprint "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder" (layer "F.Cu")
    (at 96.65 85.77)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "DC-DC.kicad_sch")
    (property "Sheetname" "DC-DC")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R10" (at 0 -1.82) (layer "F.SilkS"))
    (fp_text value "NP" (at 0 1.82) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.55 0) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.192308)
      (net 29 "GNDD") (pintype "passive"))
    (pad "2" smd roundrect (at 1.55 0) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.192308)
      (net 37 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder" (layer "F.Cu")
    (at 96.66 67.52)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Field4" "50V")
    (property "Sheetfile" "DC-DC.kicad_sch")
    (property "Sheetname" "DC-DC")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C20" (at 0 -1.43) (layer "F.SilkS"))
    (fp_text value "330uF" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.8625 0) (size 1.075 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 72 "Net-(PS1-VIN)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.8625 0) (size 1.075 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 29 "GNDD") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "F.Cu")
    (at 81.218801 72.4076)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "DC-DC.kicad_sch")
    (property "Sheetname" "DC-DC")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R27" (at 0 -1.43) (layer "F.SilkS"))
    (fp_text value "4.7k" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 46 "/+24V") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 93 "Net-(R27-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder" (layer "F.Cu")
    (at 96.66 80.07)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Field4" "2kV Y rated")
    (property "Sheetfile" "DC-DC.kicad_sch")
    (property "Sheetname" "DC-DC")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C25" (at 0 -1.43) (layer "F.SilkS"))
    (fp_text value "1nF" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.8625 0) (size 1.075 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 29 "GNDD") (pintype "passive"))
    (pad "2" smd roundrect (at 0.8625 0) (size 1.075 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 37 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "F.Cu")
    (at 81.218801 67.3876)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "DC-DC.kicad_sch")
    (property "Sheetname" "DC-DC")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R21" (at 0 -1.43) (layer "F.SilkS"))
    (fp_text value "22000" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 83 "Net-(U16-D1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 72 "Net-(PS1-VIN)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "F.Cu")
    (at 110.78 58.59)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "3v3LDO.kicad_sch")
    (property "Sheetname" "3v3LDO1")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R9" (at 0 -1.43) (layer "F.SilkS"))
    (fp_text value "90" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 40 "/Iso3.3V") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 48 "Net-(D5-A)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder" (layer "F.Cu")
    (at 143.1125 86.05)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "bme280.kicad_sch")
    (property "Sheetname" "BME280")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C5" (at 0 -1.43) (layer "F.SilkS"))
    (fp_text value ".1u" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.8625 0) (size 1.075 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 29 "GNDD") (pintype "passive"))
    (pad "2" smd roundrect (at 0.8625 0) (size 1.075 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 75 "/+3.3V") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder" (layer "F.Cu")
    (at 96.66 75.05)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Field4" "50V")
    (property "Sheetfile" "DC-DC.kicad_sch")
    (property "Sheetname" "DC-DC")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C23" (at 0 -1.43) (layer "F.SilkS"))
    (fp_text value "4.7uF" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.8625 0) (size 1.075 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 72 "Net-(PS1-VIN)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.8625 0) (size 1.075 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 29 "GNDD") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "6posMolexVert:MOLEX_0430450612" (layer "F.Cu")
    (at 133.21 54.8)
    (property "MANUFACTURER" "Molex")
    (property "MAXIMUM_PACKAGE_HEIGHT" "9.91 mm")
    (property "PARTREV" "G1")
    (property "SNAPEDA_PN" "0430450612")
    (property "STANDARD" "Manufacturer Recommendations")
    (property "Sheetfile" "channelCard.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J3" (at -3.523 -6.05) (layer "F.SilkS"))
    (fp_text value "0430450612" (at 3.335 5.347) (layer "F.Fab"))
    (pad "" np_thru_hole circle (at -6 -2.44) (size 1.07 1.07) (drill 1.07) (layers "*.Cu" "*.Mask"))
    (pad "" np_thru_hole circle (at 6 -2.44) (size 1.07 1.07) (drill 1.07) (layers "*.Cu" "*.Mask"))
    (pad "1" thru_hole rect (at 3 1.5) (size 1.605 1.605) (drill 1.07) (layers "*.Cu" "*.Mask")
      (net 37 "GND") (pinfunction "1") (pintype "passive"))
    (pad "2" thru_hole circle (at 0 1.5) (size 1.605 1.605) (drill 1.07) (layers "*.Cu" "*.Mask")
      (net 63 "/+12V out") (pinfunction "2") (pintype "passive"))
    (pad "3" thru_hole circle (at -3 1.5) (size 1.605 1.605) (drill 1.07) (layers "*.Cu" "*.Mask")
      (net 27 "unconnected-(J3-Pad3)") (pinfunction "3") (pintype "passive"))
    (pad "4" thru_hole circle (at 3 -1.5) (size 1.605 1.605) (drill 1.07) (layers "*.Cu" "*.Mask")
      (net 65 "/Ctl A") (pinfunction "4") (pintype "passive"))
    (pad "5" thru_hole circle (at 0 -1.5) (size 1.605 1.605) (drill 1.07) (layers "*.Cu" "*.Mask")
      (net 64 "/Ctl B") (pinfunction "5") (pintype "passive"))
    (pad "6" thru_hole circle (at -3 -1.5) (size 1.605 1.605) (drill 1.07) (layers "*.Cu" "*.Mask")
      (net 28 "unconnected-(J3-Pad6)") (pinfunction "6") (pintype "passive"))
  )
  (footprint "6posMolex:CON_430450602_MOL" (layer "F.Cu")
    (at 136.42 104.03)
    (tags "430450602 ")
    (property "Sheetfile" "channelCard.kicad_sch")
    (property "Sheetname" "")
    (property "ki_keywords" "430450602")
    (attr through_hole)
    (fp_text reference "J6" (at -3.000002 -8.89 unlocked) (layer "F.SilkS"))
    (fp_text value "430450602" (at -3.000002 -8.89 unlocked) (layer "F.Fab"))
    (fp_text user "430450602" (at -3.000002 -13.71 unlocked) (layer "F.SilkS"))
    (fp_text user "NPTH_DRILL_SIZE:_3.0_MM,_TOLERANCE:_+0.05/-0.05" (at -3.000002 16.77 unlocked) (layer "Cmts.User"))
    (fp_text user "PTH_DRILL_SIZE:_1.02_MM,_TOLERANCE:_+0.05/-0.05" (at -3.000002 14.23 unlocked) (layer "Cmts.User"))
    (fp_text user "${REFERENCE}" (at -3.000002 -8.89 unlocked) (layer "F.Fab"))
    (fp_text user "430450602" (at -3.000002 -13.71 unlocked) (layer "F.Fab"))
    (pad "" np_thru_hole circle (at -2.999999 4.319999) (size 2.999999 2.999999) (drill 2.999999) (layers "*.Cu" "*.Mask"))
    (pad "1" thru_hole rect (at 0 0) (size 1.52 1.52) (drill 1.02) (layers "*.Cu" "*.Mask")
      (net 43 "GNDPWR") (pinfunction "1") (pintype "unspecified"))
    (pad "2" thru_hole circle (at -2.999999 0) (size 1.52 1.52) (drill 1.02) (layers "*.Cu" "*.Mask")
      (net 103 "/Leak-") (pinfunction "2") (pintype "unspecified"))
    (pad "3" thru_hole circle (at -5.999998 0) (size 1.52 1.52) (drill 1.02) (layers "*.Cu" "*.Mask")
      (net 43 "GNDPWR") (pinfunction "3") (pintype "unspecified"))
    (pad "4" thru_hole circle (at 0 -2.999999) (size 1.52 1.52) (drill 1.02) (layers "*.Cu" "*.Mask")
      (net 104 "/Leak+") (pinfunction "4") (pintype "unspecified"))
    (pad "5" thru_hole circle (at -2.999999 -2.999999) (size 1.52 1.52) (drill 1.02) (layers "*.Cu" "*.Mask")
      (net 29 "GNDD") (pinfunction "5") (pintype "unspecified"))
    (pad "6" thru_hole circle (at -5.999998 -2.999999) (size 1.52 1.52) (drill 1.02) (layers "*.Cu" "*.Mask")
      (net 80 "/RelayOut") (pinfunction "6") (pintype "unspecified"))
    (model ":ATLAS:6posMolex/430450602.stp"
      (offset (xyz -3 -4 3.5))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "F.Cu")
    (at 81.218801 69.8976)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "DC-DC.kicad_sch")
    (property "Sheetname" "DC-DC")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R26" (at 0 -1.43) (layer "F.SilkS"))
    (fp_text value "4.7k" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 92 "/PwrCTRL") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 29 "GNDD") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "F.Cu")
    (at 118.15 121.53)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "3v3LDO.kicad_sch")
    (property "Sheetname" "3v3LDO")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R8" (at -3.11 -0.03) (layer "F.SilkS"))
    (fp_text value "90" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 75 "/+3.3V") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 47 "Net-(D3-A)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Diode_SMD:D_SMA" (layer "F.Cu")
    (at 87.463801 76.0576)
    (descr "Diode SMA (DO-214AC)")
    (tags "Diode SMA (DO-214AC)")
    (property "Sheetfile" "DC-DC.kicad_sch")
    (property "Sheetname" "DC-DC")
    (property "ki_description" "400W unidirectional Transient Voltage Suppressor, 26.0Vr, SMA(DO-214AC)")
    (property "ki_keywords" "unidirectional diode TVS voltage suppressor")
    (attr smd)
    (fp_text reference "D7" (at 0 -2.5) (layer "F.SilkS"))
    (fp_text value "SMAJ26A" (at 0 2.6) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -2.5) (layer "F.Fab"))
    (pad "1" smd roundrect (at -2 0) (size 2.5 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1388888889)
      (net 46 "/+24V") (pinfunction "A1") (pintype "passive"))
    (pad "2" smd roundrect (at 2 0) (size 2.5 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1388888889)
      (net 29 "GNDD") (pinfunction "A2") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Diode_SMD.3dshapes/D_SMA.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "F.Cu")
    (at 164.32 123.43)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "channelCard.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R30" (at 0 -1.43) (layer "F.SilkS"))
    (fp_text value "4.7k" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 96 "Net-(U15-D1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 46 "/+24V") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder" (layer "F.Cu")
    (at 121.99 121.87)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "3v3LDO.kicad_sch")
    (property "Sheetname" "3v3LDO")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C11" (at -0.175 1.46) (layer "F.SilkS"))
    (fp_text value "2.2uF" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.8625 0) (size 1.075 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 75 "/+3.3V") (pintype "passive"))
    (pad "2" smd roundrect (at 0.8625 0) (size 1.075 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 29 "GNDD") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "LED_SMD:LED_0603_1608Metric_Pad1.05x0.95mm_HandSolder" (layer "F.Cu")
    (at 122.5325 117.19)
    (descr "LED SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "LED handsolder")
    (property "Sheetfile" "3v3LDO.kicad_sch")
    (property "Sheetname" "3v3LDO")
    (property "ki_description" "Light emitting diode")
    (property "ki_keywords" "LED diode")
    (attr smd)
    (fp_text reference "D3" (at 0 -1.43) (layer "F.SilkS"))
    (fp_text value "LT Q39G-q100-25-1" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.875 0) (size 1.05 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 29 "GNDD") (pinfunction "K") (pintype "passive"))
    (pad "2" smd roundrect (at 0.875 0) (size 1.05 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 47 "Net-(D3-A)") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/LED_SMD.3dshapes/LED_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder" (layer "F.Cu")
    (at 124.59 58.69)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "channelCard.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C8" (at 2.7 0.04) (layer "F.SilkS"))
    (fp_text value ".1u" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.8625 0) (size 1.075 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 37 "GND") (pintype "passive"))
    (pad "2" smd roundrect (at 0.8625 0) (size 1.075 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 40 "/Iso3.3V") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "F.Cu")
    (at 81.218801 74.9176)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "DC-DC.kicad_sch")
    (property "Sheetname" "DC-DC")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R28" (at 0 -1.43) (layer "F.SilkS"))
    (fp_text value "39000" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 46 "/+24V") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 94 "Net-(R28-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder" (layer "F.Cu")
    (at 136.31 70.2311 -90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "flexlinkTelemPM.kicad_sch")
    (property "Sheetname" "Power Monitor")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C19" (at -2.96 -0.1 90) (layer "F.SilkS"))
    (fp_text value "0.1uF" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.8625 0 270) (size 1.075 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 40 "/Iso3.3V") (pintype "passive"))
    (pad "2" smd roundrect (at 0.8625 0 270) (size 1.075 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 37 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "B.Cu")
    (at 113.1 72.87 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "channelCard.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R20" (at 0 1.43) (layer "B.SilkS"))
    (fp_text value "1k" (at 0 -1.43) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 180) (size 0.975 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 111 "unconnected-(R20-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 180) (size 0.975 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 108 "Net-(J4-Pin_7)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "B.Cu")
    (at 161.759524 96.33 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "leakDet.kicad_sch")
    (property "Sheetname" "leakDet")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R37" (at 0 1.43) (layer "B.SilkS"))
    (fp_text value "4.7K" (at 0 -1.43) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 180) (size 0.975 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 97 "/LeakSig") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 180) (size 0.975 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 29 "GNDD") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "B.Cu")
    (at 113.9311 60.2 -90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "gndDet.kicad_sch")
    (property "Sheetname" "Gnd Det")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (property "power" "0.1 Watt")
    (attr smd)
    (fp_text reference "R13" (at -3.137466 -0.049196 90) (layer "B.SilkS"))
    (fp_text value "30 Ohm" (at 0 -1.43 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 270) (size 0.975 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 56 "Net-(U3-VBUS)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 270) (size 0.975 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 57 "/Gnd Det/Seawater") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "xtalFootprint:XTAL_ECS-.327-7-34B-TR" (layer "B.Cu")
    (at 131.14 85.81)
    (property "MANUFACTURER" "ECS Inc.")
    (property "STANDARD" "Manufacturer recommendations")
    (property "Sheetfile" "channelCard.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "Y1" (at -0.529588 1.708135 180) (layer "B.SilkS"))
    (fp_text value "ECS-.327-7-34B-TR" (at 3.757338 -1.666251 180) (layer "B.Fab"))
    (pad "1" smd rect (at -1.25 0 180) (size 1.1 1.9) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 31 "Net-(U9-PA01)") (pintype "passive"))
    (pad "2" smd rect (at 1.25 0 180) (size 1.1 1.9) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 30 "Net-(U9-PA00)") (pintype "passive"))
    (model ":ATLAS:xtal/footprints/ECS-.327-7-34B-TR.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder" (layer "B.Cu")
    (at 124.4275 94.61)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Rating" "50v")
    (property "Sheetfile" "rs485.kicad_sch")
    (property "Sheetname" "rs485")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C13" (at 0 1.43) (layer "B.SilkS"))
    (fp_text value "1.0uF" (at 0 -1.43) (layer "B.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab") hide)
    (pad "1" smd roundrect (at -0.8625 0) (size 1.075 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 54 "Net-(U6-VREG)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.8625 0) (size 1.075 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 29 "GNDD") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "B.Cu")
    (at 131.36 98.42)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "channelCard.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R2" (at -2.51 -0.75) (layer "B.SilkS"))
    (fp_text value "4.7k" (at 0 -1.43) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.9125 0) (size 0.975 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 75 "/+3.3V") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0) (size 0.975 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 35 "/SDA") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "ptcfootprints:2920L075&slash_60MR_LTF-M" (layer "B.Cu")
    (at 105.04 94.33 90)
    (tags "2920L075/60MR ")
    (property "Sheetfile" "channelCard.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resettable fuse, polymeric positive temperature coefficient")
    (property "ki_keywords" "resettable fuse PTC PPTC polyfuse polyswitch")
    (attr smd)
    (fp_text reference "F2" (at 0 0 270 unlocked) (layer "B.SilkS"))
    (fp_text value "2920L030DR" (at 0 0 270 unlocked) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 270 unlocked) (layer "B.Fab"))
    (pad "1" smd rect (at -3.0248 0 90) (size 3.048 5.4864) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 77 "Net-(D1-K)") (pintype "passive"))
    (pad "2" smd rect (at 3.0248 0 90) (size 3.048 5.4864) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 73 "/3v3LDO/VIN") (pintype "passive"))
    (zone (net 0) (net_name "") (layer "B.Cu") (hatch full 0.508)
      (connect_pads (clearance 0))
      (min_thickness 0.254) (filled_areas_thickness no)
      (keepout (tracks not_allowed) (vias not_allowed) (pads allowed) (copperpour not_allowed) (footprints allowed))
      (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
      (polygon
        (pts
          (xy 107.707 95.78)
          (xy 107.707 92.88)
          (xy 102.373 92.88)
          (xy 102.373 95.78)
        )
      )
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "B.Cu")
    (at 106.08 51.86 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "channelCard.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R5" (at -2.96 -0.01) (layer "B.SilkS"))
    (fp_text value "4.7k" (at 0 -1.43) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 180) (size 0.975 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 81 "/GndDetEn") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 180) (size 0.975 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 45 "Net-(R5-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "B.Cu")
    (at 125.93 80.08 -90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "channelCard.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R3" (at 0.97 1.89) (layer "B.SilkS"))
    (fp_text value "4.7k" (at 0 -1.43 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 270) (size 0.975 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 40 "/Iso3.3V") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 270) (size 0.975 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 39 "/IsoSDA") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "B.Cu")
    (at 122.71 63.18)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "gndDet.kicad_sch")
    (property "Sheetname" "Gnd Det")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R16" (at 0 1.43) (layer "B.SilkS"))
    (fp_text value " 0 Ohm" (at 0 -1.43) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.9125 0) (size 0.975 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 40 "/Iso3.3V") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0) (size 0.975 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 62 "Net-(U3-A0)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder" (layer "B.Cu")
    (at 125.97 85.24 90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "channelCard.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C7" (at 0 1.43 90) (layer "B.SilkS"))
    (fp_text value ".1u" (at 0 -1.43 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.8625 0 90) (size 1.075 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 29 "GNDD") (pintype "passive"))
    (pad "2" smd roundrect (at 0.8625 0 90) (size 1.075 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 75 "/+3.3V") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Diode_SMD:D_SOD-123F" (layer "B.Cu")
    (at 159.055 73 180)
    (descr "D_SOD-123F")
    (tags "D_SOD-123F")
    (property "Sheetfile" "channelCard.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Schottky diode")
    (property "ki_keywords" "diode Schottky")
    (attr smd)
    (fp_text reference "D6" (at -0.127 1.905) (layer "B.SilkS"))
    (fp_text value "PMEG6010CEH,115" (at 0 -2.1) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at -0.127 1.905) (layer "B.Fab"))
    (pad "1" smd roundrect (at -1.4 0 180) (size 1.1 1.1) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.2272727273)
      (net 77 "Net-(D1-K)") (pinfunction "K") (pintype "passive"))
    (pad "2" smd roundrect (at 1.4 0 180) (size 1.1 1.1) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.2272727273)
      (net 46 "/+24V") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Diode_SMD.3dshapes/D_SOD-123F.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder" (layer "B.Cu")
    (at 118.7411 60.16 -90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "gndDet.kicad_sch")
    (property "Sheetname" "Gnd Det")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C18" (at -3.237466 0.040804 90) (layer "B.SilkS"))
    (fp_text value "0.1uF" (at 0 -1.43 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.8625 0 270) (size 1.075 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 58 "Net-(U3-IN+)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.8625 0 270) (size 1.075 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 59 "Net-(U3-IN-)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "B.Cu")
    (at 161.759524 86.29 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "leakDet.kicad_sch")
    (property "Sheetname" "leakDet")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R31" (at 0 1.43) (layer "B.SilkS"))
    (fp_text value "33k" (at 0 -1.43) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 180) (size 0.975 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 46 "/+24V") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 180) (size 0.975 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 97 "/LeakSig") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "B.Cu")
    (at 124.4675 96.19)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "rs485.kicad_sch")
    (property "Sheetname" "rs485")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R7" (at 0 1.43) (layer "B.SilkS"))
    (fp_text value "3.3k" (at 0 -1.43) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.9125 0) (size 0.975 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 54 "Net-(U6-VREG)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0) (size 0.975 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 55 "Net-(D2-A)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "B.Cu")
    (at 164 74.25 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "channelCard.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R24" (at 0 1.43) (layer "B.SilkS"))
    (fp_text value "4.7k" (at 0 -1.43) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 180) (size 0.975 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 88 "/1A1") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 180) (size 0.975 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 89 "Net-(U8-ANODE3)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "B.Cu")
    (at 114.005 95.37 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "rs485.kicad_sch")
    (property "Sheetname" "rs485")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R6" (at 0 1.43 90) (layer "B.SilkS"))
    (fp_text value "120" (at 0 -1.43 90) (layer "B.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab") hide)
    (pad "1" smd roundrect (at -0.9125 0 90) (size 0.975 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 41 "/A") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 90) (size 0.975 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 42 "/B") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "B.Cu")
    (at 135.36 98.46)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "channelCard.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R1" (at 0 1.43) (layer "B.SilkS"))
    (fp_text value "4.7k" (at 0 -1.43) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.9125 0) (size 0.975 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 75 "/+3.3V") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0) (size 0.975 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 36 "/SCL") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder" (layer "B.Cu")
    (at 119.090296 63.172534 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "gndDet.kicad_sch")
    (property "Sheetname" "Gnd Det")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C17" (at 3.07 -0.06) (layer "B.SilkS"))
    (fp_text value "0.1uF" (at 0 -1.43) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0.23 0.09) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.8625 0 180) (size 1.075 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 40 "/Iso3.3V") (pintype "passive"))
    (pad "2" smd roundrect (at 0.8625 0 180) (size 1.075 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 37 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "B.Cu")
    (at 164 76.76 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "channelCard.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R25" (at 0 1.43) (layer "B.SilkS"))
    (fp_text value "4.7k" (at 0 -1.43) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 180) (size 0.975 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 90 "/2A1") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 180) (size 0.975 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 91 "Net-(U8-ANODE4)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder" (layer "B.Cu")
    (at 128.05 86.95 90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "channelCard.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C1" (at 2.86 0.03 90) (layer "B.SilkS"))
    (fp_text value "22pF" (at 0 -1.43 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.8625 0 90) (size 1.075 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 29 "GNDD") (pintype "passive"))
    (pad "2" smd roundrect (at 0.8625 0 90) (size 1.075 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 30 "Net-(U9-PA00)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "footprints:VSSOP10_DGS_TEX" (layer "B.Cu")
    (at 123.26 60.16 180)
    (tags "INA228AIDGSR ")
    (property "Sheetfile" "gndDet.kicad_sch")
    (property "Sheetname" "Gnd Det")
    (property "ki_keywords" "INA228AIDGSR")
    (attr smd)
    (fp_text reference "U3" (at 0 0 unlocked) (layer "B.SilkS"))
    (fp_text value "INA228AIDGSR" (at 0 0 unlocked) (layer "B.Fab"))
    (fp_text user "*" (at -2.47015 2.4224) (layer "B.SilkS"))
    (fp_text user "*" (at -2.47015 2.4224 unlocked) (layer "B.SilkS"))
    (fp_text user "*" (at -1.1684 1.4732 unlocked) (layer "B.Fab"))
    (fp_text user "*" (at -1.1684 1.4732) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 unlocked) (layer "B.Fab"))
    (pad "1" smd rect (at -2.21615 1.000001 180) (size 1.3335 0.2794) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 61 "/Gnd Det/GND") (pinfunction "A1") (pintype "input"))
    (pad "2" smd rect (at -2.21615 0.499999 180) (size 1.3335 0.2794) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 62 "Net-(U3-A0)") (pinfunction "A0") (pintype "input"))
    (pad "3" smd rect (at -2.21615 0 180) (size 1.3335 0.2794) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 3 "unconnected-(U3-ALERT-Pad3)") (pinfunction "ALERT") (pintype "output"))
    (pad "4" smd rect (at -2.21615 -0.499999 180) (size 1.3335 0.2794) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 39 "/IsoSDA") (pinfunction "SDA") (pintype "bidirectional"))
    (pad "5" smd rect (at -2.21615 -1.000001 180) (size 1.3335 0.2794) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 38 "/IsoSCL") (pinfunction "SCL") (pintype "input"))
    (pad "6" smd rect (at 2.21615 -1.000001 180) (size 1.3335 0.2794) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 40 "/Iso3.3V") (pinfunction "VS") (pintype "power_in"))
    (pad "7" smd rect (at 2.21615 -0.499999 180) (size 1.3335 0.2794) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 37 "GND") (pinfunction "GND") (pintype "power_out"))
    (pad "8" smd rect (at 2.21615 0 180) (size 1.3335 0.2794) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 56 "Net-(U3-VBUS)") (pinfunction "VBUS") (pintype "power_in"))
    (pad "9" smd rect (at 2.21615 0.499999 180) (size 1.3335 0.2794) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 59 "Net-(U3-IN-)") (pinfunction "IN-") (pintype "input"))
    (pad "10" smd rect (at 2.21615 1.000001 180) (size 1.3335 0.2794) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 58 "Net-(U3-IN+)") (pinfunction "IN+") (pintype "input"))
    (model ":ATLAS:ina228/INA219BIDR.STEP"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model ":ATLAS:ina228/INA228AIDGST.STEP"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "B.Cu")
    (at 113.1 75.38 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "channelCard.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R36" (at 0 1.43) (layer "B.SilkS"))
    (fp_text value "1k" (at 0 -1.43) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 180) (size 0.975 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 112 "unconnected-(R36-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 180) (size 0.975 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 107 "Net-(J4-Pin_6)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "footprint_Library:TC2050-IDC-NLFP" (layer "B.Cu")
    (at 113.72 77.95 180)
    (property "Sheetfile" "channelCard.kicad_sch")
    (property "Sheetname" "")
    (property "Sim.Enable" "0")
    (property "exclude_from_bom" "")
    (property "ki_description" "Generic connector, single row, 01x10, script generated")
    (property "ki_keywords" "connector")
    (attr smd exclude_from_bom)
    (fp_text reference "J4" (at 0 0.5 unlocked) (layer "B.SilkS"))
    (fp_text value "Conn_01x10_Pin" (at 0 -1 unlocked) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -2.5 unlocked) (layer "B.Fab"))
    (fp_circle (center -3.81 0) (end -3.3145 0)
      (fill none) (layer "Edge.Cuts"))
    (fp_circle (center 3.81 -1.015) (end 4.3055 -1.015)
      (fill none) (layer "Edge.Cuts"))
    (fp_circle (center 3.81 1.015) (end 4.3055 1.015)
      (fill none) (layer "Edge.Cuts"))
    (pad "1" smd circle (at -2.54 -0.635 180) (size 0.787 0.787) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 75 "/+3.3V") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" smd circle (at -1.27 -0.635 180) (size 0.787 0.787) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 105 "/SWD") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" smd circle (at 0 -0.635 180) (size 0.787 0.787) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 29 "GNDD") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" smd circle (at 1.27 -0.635 180) (size 0.787 0.787) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 106 "/SWCLK") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" smd circle (at 2.54 -0.635 180) (size 0.787 0.787) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 29 "GNDD") (pinfunction "Pin_5") (pintype "passive"))
    (pad "6" smd circle (at 2.54 0.635 180) (size 0.787 0.787) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 107 "Net-(J4-Pin_6)") (pinfunction "Pin_6") (pintype "passive"))
    (pad "7" smd circle (at 1.27 0.635 180) (size 0.787 0.787) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 108 "Net-(J4-Pin_7)") (pinfunction "Pin_7") (pintype "passive"))
    (pad "8" smd circle (at 0 0.635 180) (size 0.787 0.787) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 109 "unconnected-(J4-Pin_8-Pad8)") (pinfunction "Pin_8") (pintype "passive"))
    (pad "9" smd circle (at -1.27 0.635 180) (size 0.787 0.787) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 29 "GNDD") (pinfunction "Pin_9") (pintype "passive"))
    (pad "10" smd circle (at -2.54 0.635 180) (size 0.787 0.787) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 110 "/Reset_L") (pinfunction "Pin_10") (pintype "passive"))
  )
  (footprint "LED_SMD:LED_0603_1608Metric_Pad1.05x0.95mm_HandSolder" (layer "B.Cu")
    (at 124.54 97.81)
    (descr "LED SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "LED handsolder")
    (property "Sheetfile" "rs485.kicad_sch")
    (property "Sheetname" "rs485")
    (property "ki_description" "Light emitting diode")
    (property "ki_keywords" "LED diode")
    (attr smd)
    (fp_text reference "D2" (at 0 1.43) (layer "B.SilkS"))
    (fp_text value "LED" (at 0 -1.43) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.875 0) (size 1.05 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 66 "/UART TX") (pinfunction "K") (pintype "passive"))
    (pad "2" smd roundrect (at 0.875 0) (size 1.05 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 55 "Net-(D2-A)") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/LED_SMD.3dshapes/LED_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_SMD:SOT-363_SC-70-6_Handsoldering" (layer "B.Cu")
    (at 155.909524 93.26 180)
    (descr "SOT-363, SC-70-6, Handsoldering")
    (tags "SOT-363 SC-70-6 Handsoldering")
    (property "Sheetfile" "leakDet.kicad_sch")
    (property "Sheetname" "leakDet")
    (attr smd)
    (fp_text reference "U14" (at 0 2) (layer "B.SilkS"))
    (fp_text value "~" (at 0 -2) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd rect (at -1.33 0.65 180) (size 1.5 0.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 29 "GNDD") (pinfunction "S1") (pintype "input"))
    (pad "2" smd rect (at -1.33 0 180) (size 1.5 0.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 101 "/LeakCTRL") (pinfunction "G1") (pintype "passive"))
    (pad "3" smd rect (at -1.33 -0.65 180) (size 1.5 0.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 98 "Net-(U13-N1G)") (pinfunction "D2") (pintype "passive"))
    (pad "4" smd rect (at 1.33 -0.65 180) (size 1.5 0.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 97 "/LeakSig") (pinfunction "S2") (pintype "passive"))
    (pad "5" smd rect (at 1.33 0 180) (size 1.5 0.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 100 "Net-(U13-N2G)") (pinfunction "G2") (pintype "passive"))
    (pad "6" smd rect (at 1.33 0.65 180) (size 1.5 0.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 100 "Net-(U13-N2G)") (pinfunction "D1") (pintype "input"))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-363_SC-70-6.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder" (layer "B.Cu")
    (at 135.17 85.87 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "channelCard.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C2" (at 2.69 -0.21) (layer "B.SilkS"))
    (fp_text value "22pF" (at 0 -1.43) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.8625 0 180) (size 1.075 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 29 "GNDD") (pintype "passive"))
    (pad "2" smd roundrect (at 0.8625 0 180) (size 1.075 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 31 "Net-(U9-PA01)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "B.Cu")
    (at 144.48 96.55 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "channelCard.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R39" (at 0 1.43) (layer "B.SilkS"))
    (fp_text value "4.7k" (at 0 -1.43) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 180) (size 0.975 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 75 "/+3.3V") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 180) (size 0.975 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 110 "/Reset_L") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "B.Cu")
    (at 164 71.74 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "channelCard.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R23" (at 0 1.43) (layer "B.SilkS"))
    (fp_text value "4.7k" (at 0 -1.43) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 180) (size 0.975 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 86 "/20E'") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 180) (size 0.975 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 87 "Net-(U8-ANODE2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Diode_SMD:D_SOD-123F" (layer "B.Cu")
    (at 159.055 69.65 180)
    (descr "D_SOD-123F")
    (tags "D_SOD-123F")
    (property "Sheetfile" "channelCard.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Schottky diode")
    (property "ki_keywords" "diode Schottky")
    (attr smd)
    (fp_text reference "D1" (at -0.127 1.905) (layer "B.SilkS"))
    (fp_text value "PMEG6010CEH,115" (at 0 -2.1) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at -0.127 1.905) (layer "B.Fab"))
    (pad "1" smd roundrect (at -1.4 0 180) (size 1.1 1.1) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.2272727273)
      (net 77 "Net-(D1-K)") (pinfunction "K") (pintype "passive"))
    (pad "2" smd roundrect (at 1.4 0 180) (size 1.1 1.1) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.2272727273)
      (net 49 "Net-(D1-A)") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Diode_SMD.3dshapes/D_SOD-123F.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "B.Cu")
    (at 123.2 77.06 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "channelCard.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R4" (at 2.57 -0.08) (layer "B.SilkS"))
    (fp_text value "4.7k" (at 0 -1.43) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 180) (size 0.975 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 40 "/Iso3.3V") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 180) (size 0.975 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 38 "/IsoSCL") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder" (layer "B.Cu")
    (at 124.5375 92.94)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "rs485.kicad_sch")
    (property "Sheetname" "rs485")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (property "rating" "50V")
    (attr smd)
    (fp_text reference "C16" (at 0 1.43) (layer "B.SilkS"))
    (fp_text value "0.1uF" (at 0 -1.43) (layer "B.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab") hide)
    (pad "1" smd roundrect (at -0.8625 0) (size 1.075 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 54 "Net-(U6-VREG)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.8625 0) (size 1.075 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 29 "GNDD") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "B.Cu")
    (at 112.370296 60.222534 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "gndDet.kicad_sch")
    (property "Sheetname" "Gnd Det")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R12" (at 3.3 0.04 90) (layer "B.SilkS"))
    (fp_text value "4.7k" (at 0 -1.43 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 90) (size 0.975 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 37 "GND") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 90) (size 0.975 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 56 "Net-(U3-VBUS)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "acsl6400:SOIC_6400-00TE" (layer "B.Cu")
    (at 133.22 72.96 -90)
    (tags "ACSL-6400-00TE ")
    (property "Sheetfile" "channelCard.kicad_sch")
    (property "Sheetname" "")
    (property "ki_keywords" "ACSL-6400-00TE")
    (attr smd)
    (fp_text reference "U8" (at 0 0 90 unlocked) (layer "B.SilkS"))
    (fp_text value "ACSL-6400-00TE" (at 0 0 90 unlocked) (layer "B.Fab"))
    (fp_text user "*" (at -2.97815 6.1468 90) (layer "B.SilkS"))
    (fp_text user "*" (at -2.97815 6.1468 90 unlocked) (layer "B.SilkS"))
    (fp_text user "*" (at -1.6129 4.9276 90 unlocked) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90 unlocked) (layer "B.Fab"))
    (fp_text user "*" (at -1.6129 4.9276 90) (layer "B.Fab"))
    (pad "1" smd rect (at -2.72415 4.445 270) (size 1.4605 0.5588) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 85 "Net-(U8-ANODE1)") (pinfunction "ANODE1") (pintype "bidirectional"))
    (pad "2" smd rect (at -2.72415 3.175 270) (size 1.4605 0.5588) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 29 "GNDD") (pinfunction "CATHODE1") (pintype "bidirectional"))
    (pad "3" smd rect (at -2.72415 1.905 270) (size 1.4605 0.5588) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 87 "Net-(U8-ANODE2)") (pinfunction "ANODE2") (pintype "bidirectional"))
    (pad "4" smd rect (at -2.72415 0.635 270) (size 1.4605 0.5588) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 29 "GNDD") (pinfunction "CATHODE2") (pintype "bidirectional"))
    (pad "5" smd rect (at -2.72415 -0.635 270) (size 1.4605 0.5588) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 89 "Net-(U8-ANODE3)") (pinfunction "ANODE3") (pintype "bidirectional"))
    (pad "6" smd rect (at -2.72415 -1.905 270) (size 1.4605 0.5588) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 29 "GNDD") (pinfunction "CATHODE3") (pintype "bidirectional"))
    (pad "7" smd rect (at -2.72415 -3.175 270) (size 1.4605 0.5588) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 91 "Net-(U8-ANODE4)") (pinfunction "ANODE4") (pintype "bidirectional"))
    (pad "8" smd rect (at -2.72415 -4.445 270) (size 1.4605 0.5588) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 29 "GNDD") (pinfunction "CATHODE4") (pintype "bidirectional"))
    (pad "9" smd rect (at 2.72415 -4.445 270) (size 1.4605 0.5588) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 37 "GND") (pinfunction "GND") (pintype "power_out"))
    (pad "10" smd rect (at 2.72415 -3.175 270) (size 1.4605 0.5588) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 40 "/Iso3.3V") (pinfunction "VDD") (pintype "power_in"))
    (pad "11" smd rect (at 2.72415 -1.905 270) (size 1.4605 0.5588) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 70 "Net-(U1-2A1)") (pinfunction "V04") (pintype "bidirectional"))
    (pad "12" smd rect (at 2.72415 -0.635 270) (size 1.4605 0.5588) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 69 "Net-(U1-1A1)") (pinfunction "V03") (pintype "bidirectional"))
    (pad "13" smd rect (at 2.72415 0.635 270) (size 1.4605 0.5588) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 71 "Net-(U1-~{2OE})") (pinfunction "V02") (pintype "bidirectional"))
    (pad "14" smd rect (at 2.72415 1.905 270) (size 1.4605 0.5588) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 68 "Net-(U1-~{1OE})") (pinfunction "V01") (pintype "bidirectional"))
    (pad "15" smd rect (at 2.72415 3.175 270) (size 1.4605 0.5588) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 40 "/Iso3.3V") (pinfunction "VDD") (pintype "power_in"))
    (pad "16" smd rect (at 2.72415 4.445 270) (size 1.4605 0.5588) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 37 "GND") (pinfunction "GND") (pintype "power_out"))
    (model ":ATLAS:ACSL-6400-00TE/DS3231SN.STEP"
      (offset (xyz 2.5 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
    (model ":ATLAS:ACSL-6400-00TE/MAX3232ESE.STEP"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder" (layer "B.Cu")
    (at 127.41 90.65 90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "channelCard.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C3" (at 0.03 1.51 90) (layer "B.SilkS"))
    (fp_text value ".1uF" (at 0 -1.43 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.8625 0 90) (size 1.075 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 29 "GNDD") (pintype "passive"))
    (pad "2" smd roundrect (at 0.8625 0 90) (size 1.075 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 32 "Net-(U9-VDDCORE)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "74hc240:IC_SN74HC240PWR" (layer "B.Cu")
    (at 132.24 64.58 -90)
    (property "MANUFACTURER" "Texas Instruments")
    (property "MAXIMUM_PACKAGE_HEIGHT" "1.2mm")
    (property "PARTREV" "28-Sep-2022")
    (property "SNAPEDA_PN" "SN74HC240PWR")
    (property "STANDARD" "Manufacturer Recommendations")
    (property "Sheetfile" "channelCard.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "U1" (at -0.325 4.385 90) (layer "B.SilkS"))
    (fp_text value "SN74HC240PWR" (at 6.025 -4.385 90) (layer "B.Fab"))
    (pad "1" smd rect (at -2.9 2.925 270) (size 1.5 0.45) (layers "B.Cu" "B.Paste")
      (net 68 "Net-(U1-~{1OE})") (pinfunction "~{1OE}") (pintype "input"))
    (pad "2" smd rect (at -2.9 2.275 270) (size 1.5 0.45) (layers "B.Cu" "B.Paste")
      (net 69 "Net-(U1-1A1)") (pinfunction "1A1") (pintype "bidirectional"))
    (pad "3" smd rect (at -2.9 1.625 270) (size 1.5 0.45) (layers "B.Cu" "B.Paste")
      (net 6 "unconnected-(U1-2Y4-Pad3)") (pinfunction "2Y4") (pintype "bidirectional"))
    (pad "4" smd rect (at -2.9 0.975 270) (size 1.5 0.45) (layers "B.Cu" "B.Paste")
      (net 37 "GND") (pinfunction "1A2") (pintype "bidirectional"))
    (pad "5" smd rect (at -2.9 0.325 270) (size 1.5 0.45) (layers "B.Cu" "B.Paste")
      (net 7 "unconnected-(U1-2Y3-Pad5)") (pinfunction "2Y3") (pintype "bidirectional"))
    (pad "6" smd rect (at -2.9 -0.325 270) (size 1.5 0.45) (layers "B.Cu" "B.Paste")
      (net 37 "GND") (pinfunction "1A3") (pintype "bidirectional"))
    (pad "7" smd rect (at -2.9 -0.975 270) (size 1.5 0.45) (layers "B.Cu" "B.Paste")
      (net 8 "unconnected-(U1-2Y2-Pad7)") (pinfunction "2Y2") (pintype "bidirectional"))
    (pad "8" smd rect (at -2.9 -1.625 270) (size 1.5 0.45) (layers "B.Cu" "B.Paste")
      (net 37 "GND") (pinfunction "1A4") (pintype "bidirectional"))
    (pad "9" smd rect (at -2.9 -2.275 270) (size 1.5 0.45) (layers "B.Cu" "B.Paste")
      (net 64 "/Ctl B") (pinfunction "2Y1") (pintype "bidirectional"))
    (pad "10" smd rect (at -2.9 -2.925 270) (size 1.5 0.45) (layers "B.Cu" "B.Paste")
      (net 37 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "11" smd rect (at 2.9 -2.925 270) (size 1.5 0.45) (layers "B.Cu" "B.Paste")
      (net 70 "Net-(U1-2A1)") (pinfunction "2A1") (pintype "bidirectional"))
    (pad "12" smd rect (at 2.9 -2.275 270) (size 1.5 0.45) (layers "B.Cu" "B.Paste")
      (net 9 "unconnected-(U1-1Y4-Pad12)") (pinfunction "1Y4") (pintype "bidirectional"))
    (pad "13" smd rect (at 2.9 -1.625 270) (size 1.5 0.45) (layers "B.Cu" "B.Paste")
      (net 37 "GND") (pinfunction "2A2") (pintype "bidirectional"))
    (pad "14" smd rect (at 2.9 -0.975 270) (size 1.5 0.45) (layers "B.Cu" "B.Paste")
      (net 10 "unconnected-(U1-1Y3-Pad14)") (pinfunction "1Y3") (pintype "bidirectional"))
    (pad "15" smd rect (at 2.9 -0.325 270) (size 1.5 0.45) (layers "B.Cu" "B.Paste")
      (net 37 "GND") (pinfunction "2A3") (pintype "bidirectional"))
    (pad "16" smd rect (at 2.9 0.325 270) (size 1.5 0.45) (layers "B.Cu" "B.Paste")
      (net 11 "unconnected-(U1-1Y2-Pad16)") (pinfunction "1Y2") (pintype "bidirectional"))
    (pad "17" smd rect (at 2.9 0.975 270) (size 1.5 0.45) (layers "B.Cu" "B.Paste")
      (net 37 "GND") (pinfunction "2A4") (pintype "bidirectional"))
    (pad "18" smd rect (at 2.9 1.625 270) (size 1.5 0.45) (layers "B.Cu" "B.Paste")
      (net 65 "/Ctl A") (pinfunction "1Y1") (pintype "bidirectional"))
    (pad "19" smd rect (at 2.9 2.275 270) (size 1.5 0.45) (layers "B.Cu" "B.Paste")
      (net 71 "Net-(U1-~{2OE})") (pinfunction "~{2OE}") (pintype "input"))
    (pad "20" smd rect (at 2.9 2.925 270) (size 1.5 0.45) (layers "B.Cu" "B.Paste")
      (net 40 "/Iso3.3V") (pinfunction "VCC") (pintype "power_in"))
    (model ":ATLAS:74hc240/SN74HC240PWR.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "B.Cu")
    (at 161.759524 93.82 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "leakDet.kicad_sch")
    (property "Sheetname" "leakDet")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R35" (at 0 1.43) (layer "B.SilkS"))
    (fp_text value "4.7K" (at 0 -1.43) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 180) (size 0.975 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 101 "/LeakCTRL") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 180) (size 0.975 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 29 "GNDD") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "B.Cu")
    (at 161.759524 88.8 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "leakDet.kicad_sch")
    (property "Sheetname" "leakDet")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R32" (at 0 1.43) (layer "B.SilkS"))
    (fp_text value "4.7K" (at 0 -1.43) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 180) (size 0.975 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 98 "Net-(U13-N1G)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 180) (size 0.975 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 29 "GNDD") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "footprint_Library:DMHC4035LSD-13" (layer "B.Cu")
    (at 155.769524 88.15 180)
    (property "Sheetfile" "leakDet.kicad_sch")
    (property "Sheetname" "leakDet")
    (attr smd)
    (fp_text reference "U13" (at 0.08 3.41 unlocked) (layer "B.SilkS"))
    (fp_text value "~" (at 0 5.08 unlocked) (layer "B.Fab"))
    (fp_text user "*" (at -2.54 2.54 unlocked) (layer "B.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 7.62 unlocked) (layer "B.Fab"))
    (pad "1" smd roundrect (at -2.7 1.905 180) (size 1.55 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 98 "Net-(U13-N1G)") (pinfunction "N1G") (pintype "passive") (thermal_bridge_angle 45))
    (pad "2" smd roundrect (at -2.7 0.635 180) (size 1.55 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 104 "/Leak+") (pinfunction "P1D/N1D") (pintype "input") (thermal_bridge_angle 45))
    (pad "3" smd roundrect (at -2.7 -0.635 180) (size 1.55 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 29 "GNDD") (pinfunction "N1S/N2S") (pintype "input") (thermal_bridge_angle 45))
    (pad "4" smd roundrect (at -2.7 -1.905 180) (size 1.55 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 100 "Net-(U13-N2G)") (pinfunction "N2G") (pintype "input") (thermal_bridge_angle 45))
    (pad "5" smd roundrect (at 2.7 -1.905 180) (size 1.55 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 100 "Net-(U13-N2G)") (pinfunction "P2G") (pintype "input") (thermal_bridge_angle 45))
    (pad "6" smd roundrect (at 2.7 -0.635 180) (size 1.55 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 103 "/Leak-") (pinfunction "P2D/N2D") (pintype "input") (thermal_bridge_angle 45))
    (pad "7" smd roundrect (at 2.7 0.635 180) (size 1.55 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 97 "/LeakSig") (pinfunction "P1S/P2S") (pintype "input") (thermal_bridge_angle 45))
    (pad "8" smd roundrect (at 2.7 1.905 180) (size 1.55 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 98 "Net-(U13-N1G)") (pinfunction "P1G") (pintype "input") (thermal_bridge_angle 45))
    (model ":KICAD7_3DMODEL_DIR:Package_SO.3dshapes/SO-8_3.9x4.9mm_P1.27mm.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "B.Cu")
    (at 116.3511 61.06 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "gndDet.kicad_sch")
    (property "Sheetname" "Gnd Det")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R15" (at 0.190804 3.207466) (layer "B.SilkS"))
    (fp_text value "10 Ohm" (at 0 -1.43) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 180) (size 0.975 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 59 "Net-(U3-IN-)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 180) (size 0.975 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 57 "/Gnd Det/Seawater") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MAX13412EESA+T:SOIC127P600X168-9N" (layer "B.Cu")
    (at 118.9425 95.43 180)
    (property "AVAILABILITY" "Unavailable")
    (property "DESCRIPTION" "RS-485 Transceiver with Integrated Low-Dropout Regulator andAutoDirection Contro")
    (property "MF" "Maxim Integrated")
    (property "MP" "MAX13412EESA+T")
    (property "PACKAGE" "SOIC-8 Maxim")
    (property "PRICE" "None")
    (property "Sheetfile" "rs485.kicad_sch")
    (property "Sheetname" "rs485")
    (attr smd)
    (fp_text reference "U6" (at -0.48 3.332) (layer "B.SilkS"))
    (fp_text value "MAX13412EESA+T" (at 7.775 -3.332) (layer "B.Fab"))
    (pad "1" smd roundrect (at -2.63 1.905 180) (size 1.66 0.59) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.07)
      (net 67 "/UART RX") (pinfunction "RO") (pintype "output"))
    (pad "2" smd roundrect (at -2.63 0.635 180) (size 1.66 0.59) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.07)
      (net 54 "Net-(U6-VREG)") (pinfunction "~{RE}") (pintype "output"))
    (pad "3" smd roundrect (at -2.63 -0.635 180) (size 1.66 0.59) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.07)
      (net 54 "Net-(U6-VREG)") (pinfunction "VREG") (pintype "output"))
    (pad "4" smd roundrect (at -2.63 -1.905 180) (size 1.66 0.59) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.07)
      (net 66 "/UART TX") (pinfunction "DI") (pintype "input"))
    (pad "5" smd roundrect (at 2.63 -1.905 180) (size 1.66 0.59) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.07)
      (net 29 "GNDD") (pinfunction "GND") (pintype "power_in"))
    (pad "6" smd roundrect (at 2.63 -0.635 180) (size 1.66 0.59) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.07)
      (net 41 "/A") (pinfunction "A") (pintype "bidirectional"))
    (pad "7" smd roundrect (at 2.63 0.635 180) (size 1.66 0.59) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.07)
      (net 42 "/B") (pinfunction "B") (pintype "bidirectional"))
    (pad "8" smd roundrect (at 2.63 1.905 180) (size 1.66 0.59) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.07)
      (net 46 "/+24V") (pinfunction "VCC") (pintype "power_in"))
    (pad "9" smd rect (at 0 0 180) (size 2.15 2.835) (layers "B.Cu" "B.Mask")
      (net 29 "GNDD") (pinfunction "EP") (pintype "power_in"))
    (model ":ATLAS:MAX13412EESA+T/MAX13412EESA_T.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )
  (footprint "atsamd21g18a:TQFP48_7x7MC_MCH" (layer "B.Cu")
    (at 133.53 92.13 -90)
    (tags "ATSAMD21G18A-AU ")
    (property "Sheetfile" "channelCard.kicad_sch")
    (property "Sheetname" "")
    (property "ki_keywords" "ATSAMD21G18A-AU")
    (attr smd)
    (fp_text reference "U9" (at 0 0 90 unlocked) (layer "B.SilkS"))
    (fp_text value "ATSAMD21G18A-AU" (at 0 0 90 unlocked) (layer "B.Fab"))
    (fp_text user "*" (at -5.4864 3.381 90) (layer "B.SilkS"))
    (fp_text user "*" (at -5.4864 3.381 90 unlocked) (layer "B.SilkS"))
    (fp_text user "*" (at -3.1242 3 90 unlocked) (layer "B.Fab"))
    (fp_text user "*" (at -3.1242 3 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90 unlocked) (layer "B.Fab"))
    (pad "1" smd rect (at -4.1783 2.75 180) (size 0.2794 1.3462) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 30 "Net-(U9-PA00)") (pinfunction "PA00") (pintype "bidirectional"))
    (pad "2" smd rect (at -4.1783 2.250001 180) (size 0.2794 1.3462) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 31 "Net-(U9-PA01)") (pinfunction "PA01") (pintype "bidirectional"))
    (pad "3" smd rect (at -4.1783 1.749999 180) (size 0.2794 1.3462) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "unconnected-(U9-PA02-Pad3)") (pinfunction "PA02") (pintype "bidirectional"))
    (pad "4" smd rect (at -4.1783 1.25 180) (size 0.2794 1.3462) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 13 "unconnected-(U9-PA03-Pad4)") (pinfunction "PA03") (pintype "bidirectional"))
    (pad "5" smd rect (at -4.1783 0.750001 180) (size 0.2794 1.3462) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 29 "GNDD") (pinfunction "GNDANA") (pintype "power_out"))
    (pad "6" smd rect (at -4.1783 0.25 180) (size 0.2794 1.3462) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 75 "/+3.3V") (pinfunction "VDDANA") (pintype "power_in"))
    (pad "7" smd rect (at -4.1783 -0.25 180) (size 0.2794 1.3462) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 14 "unconnected-(U9-PB08-Pad7)") (pinfunction "PB08") (pintype "bidirectional"))
    (pad "8" smd rect (at -4.1783 -0.750001 180) (size 0.2794 1.3462) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 15 "unconnected-(U9-PB09-Pad8)") (pinfunction "PB09") (pintype "bidirectional"))
    (pad "9" smd rect (at -4.1783 -1.25 180) (size 0.2794 1.3462) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 16 "unconnected-(U9-PA04-Pad9)") (pinfunction "PA04") (pintype "bidirectional"))
    (pad "10" smd rect (at -4.1783 -1.749999 180) (size 0.2794 1.3462) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 17 "unconnected-(U9-PA05-Pad10)") (pinfunction "PA05") (pintype "bidirectional"))
    (pad "11" smd rect (at -4.1783 -2.250001 180) (size 0.2794 1.3462) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 53 "/BrdAdd4") (pinfunction "PA06") (pintype "bidirectional"))
    (pad "12" smd rect (at -4.1783 -2.75 180) (size 0.2794 1.3462) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 51 "/BrdAdd3") (pinfunction "PA07") (pintype "bidirectional"))
    (pad "13" smd rect (at -2.75 -4.1783 270) (size 0.2794 1.3462) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 52 "/BrdAdd2") (pinfunction "PA08") (pintype "bidirectional"))
    (pad "14" smd rect (at -2.250001 -4.1783 270) (size 0.2794 1.3462) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 50 "/BrdAdd1") (pinfunction "PA09") (pintype "bidirectional"))
    (pad "15" smd rect (at -1.749999 -4.1783 270) (size 0.2794 1.3462) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 67 "/UART RX") (pinfunction "PA10") (pintype "bidirectional"))
    (pad "16" smd rect (at -1.25 -4.1783 270) (size 0.2794 1.3462) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 66 "/UART TX") (pinfunction "PA11") (pintype "bidirectional"))
    (pad "17" smd rect (at -0.750001 -4.1783 270) (size 0.2794 1.3462) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 75 "/+3.3V") (pinfunction "VDDIO") (pintype "power_in"))
    (pad "18" smd rect (at -0.25 -4.1783 270) (size 0.2794 1.3462) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 29 "GNDD") (pinfunction "GND") (pintype "power_out"))
    (pad "19" smd rect (at 0.25 -4.1783 270) (size 0.2794 1.3462) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 18 "unconnected-(U9-PB10-Pad19)") (pinfunction "PB10") (pintype "bidirectional"))
    (pad "20" smd rect (at 0.750001 -4.1783 270) (size 0.2794 1.3462) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 19 "unconnected-(U9-PB11-Pad20)") (pinfunction "PB11") (pintype "bidirectional"))
    (pad "21" smd rect (at 1.25 -4.1783 270) (size 0.2794 1.3462) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 101 "/LeakCTRL") (pinfunction "PA12") (pintype "bidirectional"))
    (pad "22" smd rect (at 1.749999 -4.1783 270) (size 0.2794 1.3462) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 102 "/LeakSIG") (pinfunction "PA13") (pintype "bidirectional"))
    (pad "23" smd rect (at 2.250001 -4.1783 270) (size 0.2794 1.3462) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 99 "/RelayCtrl") (pinfunction "PA14") (pintype "bidirectional"))
    (pad "24" smd rect (at 2.75 -4.1783 270) (size 0.2794 1.3462) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 95 "/FuseDet") (pinfunction "PA15") (pintype "bidirectional"))
    (pad "25" smd rect (at 4.1783 -2.75 180) (size 0.2794 1.3462) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 90 "/2A1") (pinfunction "PA16") (pintype "bidirectional"))
    (pad "26" smd rect (at 4.1783 -2.250001 180) (size 0.2794 1.3462) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 88 "/1A1") (pinfunction "PA17") (pintype "bidirectional"))
    (pad "27" smd rect (at 4.1783 -1.749999 180) (size 0.2794 1.3462) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 86 "/20E'") (pinfunction "PA18") (pintype "bidirectional"))
    (pad "28" smd rect (at 4.1783 -1.25 180) (size 0.2794 1.3462) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 84 "/10E'") (pinfunction "PA19") (pintype "bidirectional"))
    (pad "29" smd rect (at 4.1783 -0.750001 180) (size 0.2794 1.3462) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 92 "/PwrCTRL") (pinfunction "PA20") (pintype "bidirectional"))
    (pad "30" smd rect (at 4.1783 -0.25 180) (size 0.2794 1.3462) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 81 "/GndDetEn") (pinfunction "PA21") (pintype "bidirectional"))
    (pad "31" smd rect (at 4.1783 0.25 180) (size 0.2794 1.3462) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "/SDA") (pinfunction "PA22") (pintype "bidirectional"))
    (pad "32" smd rect (at 4.1783 0.750001 180) (size 0.2794 1.3462) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 36 "/SCL") (pinfunction "PA23") (pintype "bidirectional"))
    (pad "33" smd rect (at 4.1783 1.25 180) (size 0.2794 1.3462) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 34 "/D-") (pinfunction "PA24") (pintype "bidirectional"))
    (pad "34" smd rect (at 4.1783 1.749999 180) (size 0.2794 1.3462) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 33 "/D+") (pinfunction "PA25") (pintype "bidirectional"))
    (pad "35" smd rect (at 4.1783 2.250001 180) (size 0.2794 1.3462) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 29 "GNDD") (pinfunction "GND") (pintype "power_out"))
    (pad "36" smd rect (at 4.1783 2.75 180) (size 0.2794 1.3462) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 75 "/+3.3V") (pinfunction "VDDIO") (pintype "power_in"))
    (pad "37" smd rect (at 2.75 4.1783 270) (size 0.2794 1.3462) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 20 "unconnected-(U9-PB22-Pad37)") (pinfunction "PB22") (pintype "bidirectional"))
    (pad "38" smd rect (at 2.250001 4.1783 270) (size 0.2794 1.3462) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 21 "unconnected-(U9-PB23-Pad38)") (pinfunction "PB23") (pintype "bidirectional"))
    (pad "39" smd rect (at 1.749999 4.1783 270) (size 0.2794 1.3462) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 22 "unconnected-(U9-PA27-Pad39)") (pinfunction "PA27") (pintype "bidirectional"))
    (pad "40" smd rect (at 1.25 4.1783 270) (size 0.2794 1.3462) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 110 "/Reset_L") (pinfunction "*RESET") (pintype "unspecified"))
    (pad "41" smd rect (at 0.750001 4.1783 270) (size 0.2794 1.3462) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 23 "unconnected-(U9-PA28-Pad41)") (pinfunction "PA28") (pintype "bidirectional"))
    (pad "42" smd rect (at 0.25 4.1783 270) (size 0.2794 1.3462) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 29 "GNDD") (pinfunction "GND") (pintype "power_out"))
    (pad "43" smd rect (at -0.25 4.1783 270) (size 0.2794 1.3462) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 32 "Net-(U9-VDDCORE)") (pinfunction "VDDCORE") (pintype "power_in"))
    (pad "44" smd rect (at -0.750001 4.1783 270) (size 0.2794 1.3462) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 75 "/+3.3V") (pinfunction "VDDIN") (pintype "power_in"))
    (pad "45" smd rect (at -1.25 4.1783 270) (size 0.2794 1.3462) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 106 "/SWCLK") (pinfunction "PA30") (pintype "bidirectional"))
    (pad "46" smd rect (at -1.749999 4.1783 270) (size 0.2794 1.3462) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 105 "/SWD") (pinfunction "PA31") (pintype "bidirectional"))
    (pad "47" smd rect (at -2.250001 4.1783 270) (size 0.2794 1.3462) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 24 "unconnected-(U9-PB02-Pad47)") (pinfunction "PB02") (pintype "bidirectional"))
    (pad "48" smd rect (at -2.75 4.1783 270) (size 0.2794 1.3462) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 25 "unconnected-(U9-PB03-Pad48)") (pinfunction "PB03") (pintype "bidirectional"))
    (pad "EPAD" smd rect (at 0 0 270) (size 3.5052 3.5052) (layers "B.Cu" "B.Mask")
      (net 29 "GNDD") (pinfunction "EPAD") (pintype "unspecified"))
    (model ":ATLAS:atsamd21g18a/footprints/ATSAMD21G18A-AU--3DModel-STEP-56544.STEP"
      (offset (xyz 0 0 0.66))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )
  (footprint "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm" (layer "B.Cu")
    (at 122.46 81.92 90)
    (descr "SOIC, 8 Pin (JEDEC MS-012AA, https://www.analog.com/media/en/package-pcb-resources/package/pkg_pdf/soic_narrow-r/r_8.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOIC SO")
    (property "Sheetfile" "channelCard.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Dual-channel I2C digital isolator, Bidirectional communication, 3V/5V level translation, SOIC-8")
    (property "ki_keywords" "Dual-channel digital isolator I2C")
    (attr smd)
    (fp_text reference "U4" (at 0.01 0 90) (layer "B.SilkS"))
    (fp_text value "ADuM1250" (at 0 -3.4 90) (layer "B.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab") hide)
    (pad "1" smd roundrect (at -2.475 1.905 90) (size 1.95 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 75 "/+3.3V") (pinfunction "VDD1") (pintype "power_in"))
    (pad "2" smd roundrect (at -2.475 0.635 90) (size 1.95 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 35 "/SDA") (pinfunction "SDA1") (pintype "bidirectional"))
    (pad "3" smd roundrect (at -2.475 -0.635 90) (size 1.95 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 36 "/SCL") (pinfunction "SCL1") (pintype "bidirectional"))
    (pad "4" smd roundrect (at -2.475 -1.905 90) (size 1.95 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 29 "GNDD") (pinfunction "GND1") (pintype "power_in"))
    (pad "5" smd roundrect (at 2.475 -1.905 90) (size 1.95 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 37 "GND") (pinfunction "GND2") (pintype "power_in"))
    (pad "6" smd roundrect (at 2.475 -0.635 90) (size 1.95 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 38 "/IsoSCL") (pinfunction "SCL2") (pintype "bidirectional"))
    (pad "7" smd roundrect (at 2.475 0.635 90) (size 1.95 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 39 "/IsoSDA") (pinfunction "SDA2") (pintype "bidirectional"))
    (pad "8" smd roundrect (at 2.475 1.905 90) (size 1.95 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 40 "/Iso3.3V") (pinfunction "VDD2") (pintype "power_in"))
    (model "${KICAD6_3DMODEL_DIR}/Package_SO.3dshapes/SOIC-8_3.9x4.9mm_P1.27mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_SMD:SOT-23" (layer "B.Cu")
    (at 111.5845 95.4 180)
    (descr "SOT, 3 Pin (https://www.jedec.org/system/files/docs/to-236h.pdf variant AB), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOT TO_SOT_SMD")
    (property "Sheetfile" "rs485.kicad_sch")
    (property "Sheetname" "rs485")
    (property "ki_description" "7V/12V, 600W Asymmetrical TVS Diode Array, SOT-23")
    (property "ki_keywords" "transient voltage suppressor thyrector transil")
    (attr smd)
    (fp_text reference "D4" (at 0 2.4) (layer "B.SilkS"))
    (fp_text value "SM712_SOT23" (at 0 -2.4) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.9375 0.95 180) (size 1.475 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 42 "/B") (pinfunction "A1") (pintype "passive"))
    (pad "2" smd roundrect (at -0.9375 -0.95 180) (size 1.475 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 41 "/A") (pinfunction "A2") (pintype "passive"))
    (pad "3" smd roundrect (at 0.9375 0 180) (size 1.475 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 29 "GNDD") (pinfunction "common") (pintype "input"))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "B.Cu")
    (at 164 69.23 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "channelCard.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R22" (at 0 1.43) (layer "B.SilkS"))
    (fp_text value "4.7k" (at 0 -1.43) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 180) (size 0.975 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 84 "/10E'") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 180) (size 0.975 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 85 "Net-(U8-ANODE1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "B.Cu")
    (at 110.690296 60.182534 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "gndDet.kicad_sch")
    (property "Sheetname" "Gnd Det")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R11" (at 3.2 0 90) (layer "B.SilkS"))
    (fp_text value "4.7k" (at 0 -1.43 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0.45 0.78 90) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 90) (size 0.975 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 76 "/3v3LDO1/VIN") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 90) (size 0.975 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 56 "Net-(U3-VBUS)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "usb:AMPHENOL_10118192-0001LF" (layer "B.Cu")
    (at 127.55 109.1 180)
    (property "MANUFACTURER" "Amphenol")
    (property "PARTREV" "B")
    (property "STANDARD" "Manufacturer Recommendation")
    (property "Sheetfile" "channelCard.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "J1" (at -2.45306 2.27805) (layer "B.SilkS"))
    (fp_text value "10118192-0001LF" (at 6.92043 -5.85033) (layer "B.Fab"))
    (fp_text user "PCB Edge" (at 5.20496 -3.90372) (layer "B.Fab"))
    (pad "1" smd rect (at -1.3 0 180) (size 0.4 1.35) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 49 "Net-(D1-A)") (pinfunction "VUSB") (pintype "passive"))
    (pad "2" smd rect (at -0.65 0 180) (size 0.4 1.35) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 34 "/D-") (pinfunction "D-") (pintype "passive"))
    (pad "3" smd rect (at 0 0 180) (size 0.4 1.35) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 33 "/D+") (pinfunction "D+") (pintype "passive"))
    (pad "4" smd rect (at 0.65 0 180) (size 0.4 1.35) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 26 "unconnected-(J1-ID-Pad4)") (pinfunction "ID") (pintype "passive"))
    (pad "5" smd rect (at 1.3 0 180) (size 0.4 1.35) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 29 "GNDD") (pinfunction "GND") (pintype "passive"))
    (pad "SH1" smd rect (at -3.1 -0.125 180) (size 2.1 1.6) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 29 "GNDD") (pinfunction "SHIELD") (pintype "passive"))
    (pad "SH2" smd rect (at 3.1 -0.125 180) (size 2.1 1.6) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 29 "GNDD") (pinfunction "SHIELD__1") (pintype "passive"))
    (pad "SH3" smd rect (at -3.8 -2.675) (size 1.8 1.9) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 29 "GNDD") (pinfunction "SHIELD__2") (pintype "passive"))
    (pad "SH4" smd rect (at -1.2 -2.675 180) (size 1.9 1.9) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 29 "GNDD") (pinfunction "SHIELD__3") (pintype "passive"))
    (pad "SH5" smd rect (at 1.2 -2.675 180) (size 1.9 1.9) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 29 "GNDD") (pinfunction "SHIELD__4") (pintype "passive"))
    (pad "SH6" smd rect (at 3.8 -2.675) (size 1.8 1.9) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 29 "GNDD") (pinfunction "SHIELD__5") (pintype "passive"))
    (model ":ATLAS:usb/10118192-0001LF.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder" (layer "B.Cu")
    (at 139.25 91.91 90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "channelCard.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C4" (at 0.07 -1.41 -270) (layer "B.SilkS"))
    (fp_text value ".1uF" (at 0 -1.43 -270) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 -270) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.8625 0 90) (size 1.075 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 29 "GNDD") (pintype "passive"))
    (pad "2" smd roundrect (at 0.8625 0 90) (size 1.075 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 75 "/+3.3V") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "B.Cu")
    (at 161.759524 91.31 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "leakDet.kicad_sch")
    (property "Sheetname" "leakDet")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R34" (at 0 1.43) (layer "B.SilkS"))
    (fp_text value "4.7K" (at 0 -1.43) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 180) (size 0.975 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 97 "/LeakSig") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 180) (size 0.975 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 100 "Net-(U13-N2G)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "B.Cu")
    (at 144.48 94.04 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "channelCard.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R38" (at 0 1.43) (layer "B.SilkS"))
    (fp_text value "1k" (at 0 -1.43) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 180) (size 0.975 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 75 "/+3.3V") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 180) (size 0.975 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 106 "/SWCLK") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "B.Cu")
    (at 116.3511 59.28 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "gndDet.kicad_sch")
    (property "Sheetname" "Gnd Det")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R14" (at 0.150804 3.017466) (layer "B.SilkS"))
    (fp_text value "10 Ohm" (at 0 -1.43) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 180) (size 0.975 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 58 "Net-(U3-IN+)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 180) (size 0.975 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 56 "Net-(U3-VBUS)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder" (layer "B.Cu")
    (at 118.07 91.83)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "rs485.kicad_sch")
    (property "Sheetname" "rs485")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (property "rating" "50V")
    (attr smd)
    (fp_text reference "C12" (at 0 1.43) (layer "B.SilkS"))
    (fp_text value "0.1uF" (at 0 -1.43) (layer "B.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab") hide)
    (pad "1" smd roundrect (at -0.8625 0) (size 1.075 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 46 "/+24V") (pintype "passive"))
    (pad "2" smd roundrect (at 0.8625 0) (size 1.075 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 29 "GNDD") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_rect locked (start 100 50) (end 140 113)
    (fill none) (layer "Edge.Cuts"))
)
