(kicad_sch (version 20230121) (generator eeschema)
  (paper "A4")
  (lib_symbols
    (symbol "2023-07-25_19-26-39:INA228AIDGSR" (pin_names (offset 0.254)) (in_bom yes) (on_board yes)
      (property "Reference" "U" (at 20.32 10.16 0))
      (property "Value" "INA228AIDGSR" (at 20.32 7.62 0))
      (property "Footprint" "VSSOP10_DGS_TEX" (at 0 0 0))
      (property "Datasheet" "INA228AIDGSR" (at 0 0 0))
      (property "ki_locked" "" (at 0 0 0))
      (property "ki_keywords" "INA228AIDGSR" (at 0 0 0))
      (property "ki_fp_filters" "VSSOP10_DGS_TEX VSSOP10_DGS_TEX-M VSSOP10_DGS_TEX-L" (at 0 0 0))
      (symbol "INA228AIDGSR_0_1"
        (polyline
          (pts
            (xy 7.62 -15.24)
            (xy 33.02 -15.24)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 7.62 5.08)
            (xy 7.62 -15.24)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 33.02 -15.24)
            (xy 33.02 5.08)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 33.02 5.08)
            (xy 7.62 5.08)
          )
          (fill (type none))
        )
        (pin input line (at 0 0 0) (length 7.62)
          (name "A1")
          (number "1")
        )
        (pin input line (at 40.64 0 180) (length 7.62)
          (name "IN+")
          (number "10")
        )
        (pin input line (at 0 -2.54 0) (length 7.62)
          (name "A0")
          (number "2")
        )
        (pin output line (at 0 -5.08 0) (length 7.62)
          (name "ALERT")
          (number "3")
        )
        (pin bidirectional line (at 0 -7.62 0) (length 7.62)
          (name "SDA")
          (number "4")
        )
        (pin input line (at 0 -10.16 0) (length 7.62)
          (name "SCL")
          (number "5")
        )
        (pin power_in line (at 40.64 -10.16 180) (length 7.62)
          (name "VS")
          (number "6")
        )
        (pin power_out line (at 40.64 -7.62 180) (length 7.62)
          (name "GND")
          (number "7")
        )
        (pin power_in line (at 40.64 -5.08 180) (length 7.62)
          (name "VBUS")
          (number "8")
        )
        (pin input line (at 40.64 -2.54 180) (length 7.62)
          (name "IN-")
          (number "9")
        )
      )
    )
    (symbol "Device:C" (pin_numbers hide) (pin_names (offset 0.254)) (in_bom yes) (on_board yes)
      (property "Reference" "C" (at 0.635 2.54 0))
      (property "Value" "C" (at 0.635 -2.54 0))
      (property "Footprint" "" (at 0.9652 -3.81 0))
      (property "Datasheet" "~" (at 0 0 0))
      (property "ki_keywords" "cap capacitor" (at 0 0 0))
      (property "ki_description" "Unpolarized capacitor" (at 0 0 0))
      (property "ki_fp_filters" "C_*" (at 0 0 0))
      (symbol "C_0_1"
        (polyline
          (pts
            (xy -2.032 -0.762)
            (xy 2.032 -0.762)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -2.032 0.762)
            (xy 2.032 0.762)
          )
          (fill (type none))
        )
      )
      (symbol "C_1_1"
        (pin passive line (at 0 3.81 270) (length 2.794)
          (name "~")
          (number "1")
        )
        (pin passive line (at 0 -3.81 90) (length 2.794)
          (name "~")
          (number "2")
        )
      )
    )
    (symbol "Device:R" (pin_numbers hide) (pin_names (offset 0)) (in_bom yes) (on_board yes)
      (property "Reference" "R" (at 2.032 0 90))
      (property "Value" "R" (at 0 0 90))
      (property "Footprint" "" (at -1.778 0 90))
      (property "Datasheet" "~" (at 0 0 0))
      (property "ki_keywords" "R res resistor" (at 0 0 0))
      (property "ki_description" "Resistor" (at 0 0 0))
      (property "ki_fp_filters" "R_*" (at 0 0 0))
      (symbol "R_0_1"
        (rectangle (start -1.016 -2.54) (end 1.016 2.54)
          (fill (type none))
        )
      )
      (symbol "R_1_1"
        (pin passive line (at 0 3.81 270) (length 1.27)
          (name "~")
          (number "1")
        )
        (pin passive line (at 0 -3.81 90) (length 1.27)
          (name "~")
          (number "2")
        )
      )
    )
  )
  (junction (at 167.64 68.58) (diameter 0) (color 0 0 0 0))
  (junction (at 115.57 76.2) (diameter 0) (color 0 0 0 0))
  (junction (at 105.537 55.88) (diameter 0) (color 0 0 0 0))
  (junction (at 121.92 78.74) (diameter 0) (color 0 0 0 0))
  (junction (at 105.537 71.12) (diameter 0) (color 0 0 0 0))
  (wire (pts (xy 124.46 71.12) (xy 105.537 71.12)))
  (wire (pts (xy 121.92 78.74) (xy 120.65 78.74)))
  (wire (pts (xy 124.46 73.66) (xy 120.65 73.66)))
  (wire (pts (xy 170.18 78.74) (xy 165.1 78.74)))
  (wire (pts (xy 167.64 68.58) (xy 172.72 68.58)))
  (wire (pts (xy 121.92 88.9) (xy 115.57 88.9)))
  (wire (pts (xy 105.537 55.88) (xy 105.537 60.833)))
  (wire (pts (xy 100.33 76.2) (xy 115.57 76.2)))
  (wire (pts (xy 124.46 78.74) (xy 121.92 78.74)))
  (wire (pts (xy 100.33 55.88) (xy 105.537 55.88)))
  (wire (pts (xy 121.92 55.88) (xy 105.537 55.88)))
  (wire (pts (xy 165.1 68.58) (xy 167.64 68.58)))
  (wire (pts (xy 105.537 68.453) (xy 105.537 71.12)))
  (wire (pts (xy 121.92 55.88) (xy 121.92 68.58)))
  (wire (pts (xy 170.18 76.2) (xy 165.1 76.2)))
  (wire (pts (xy 121.92 68.58) (xy 124.46 68.58)))
  (wire (pts (xy 121.92 88.9) (xy 121.92 86.36)))
  (wire (pts (xy 124.46 76.2) (xy 115.57 76.2)))
  (wire (pts (xy 167.64 71.12) (xy 167.64 68.58)))
  (wire (pts (xy 165.1 71.12) (xy 167.64 71.12)))
  (wire (pts (xy 115.57 76.2) (xy 115.57 88.9)))
  (wire (pts (xy 100.33 71.12) (xy 105.537 71.12)))
  (label "GND" (at 172.72 68.58 0) (fields_autoplaced))
  (hierarchical_label "IN+" (shape input) (at 100.33 55.88 180) (fields_autoplaced))
  (hierarchical_label "GND" (shape input) (at 100.33 76.2 180) (fields_autoplaced))
  (hierarchical_label "IN-" (shape input) (at 100.33 71.12 180) (fields_autoplaced))
  (hierarchical_label "SDA" (shape input) (at 170.18 76.2 0) (fields_autoplaced))
  (hierarchical_label "VS" (shape input) (at 120.65 78.74 180) (fields_autoplaced))
  (hierarchical_label "SCL" (shape input) (at 170.18 78.74 0) (fields_autoplaced))
  (hierarchical_label "VBUS" (shape input) (at 120.65 73.66 180) (fields_autoplaced))
  (symbol (lib_id "2023-07-25_19-26-39:INA228AIDGSR") (at 165.1 68.58 0) (mirror y) (unit 1)
    (in_bom yes) (on_board yes) (dnp no) (fields_autoplaced)
    (property "Reference" "U2" (at 144.78 58.42 0))
    (property "Value" "INA228AIDGSR" (at 144.78 60.96 0))
    (property "Footprint" "VSSOP10_DGS_TEX" (at 165.1 68.58 0))
    (property "Datasheet" "INA228AIDGSR" (at 165.1 68.58 0))
    (pin "1")
    (pin "10")
    (pin "2")
    (pin "3")
    (pin "4")
    (pin "5")
    (pin "6")
    (pin "7")
    (pin "8")
    (pin "9")
    (instances
      (project "channelCard"
        (path
          (reference "U2") (unit 1)
        )
        (path
          (reference "U2") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "Device:R") (at 105.537 64.643 180) (unit 1)
    (in_bom yes) (on_board yes) (dnp no)
    (property "Reference" "R17" (at 108.077 63.373 0))
    (property "Value" "0.1 Ohm" (at 108.077 65.913 0))
    (property "Footprint" "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (at 107.315 64.643 90))
    (property "Datasheet" "1/4 W" (at 111.76 68.453 0))
    (property "Field4" "" (at 105.537 64.643 0))
    (pin "1")
    (pin "2")
    (instances
      (project "channelCard"
        (path
          (reference "R17") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "Device:C") (at 121.92 82.55 0) (unit 1)
    (in_bom yes) (on_board yes) (dnp no) (fields_autoplaced)
    (property "Reference" "C19" (at 125.73 81.28 0))
    (property "Value" "0.1uF" (at 125.73 83.82 0))
    (property "Footprint" "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder" (at 122.8852 86.36 0))
    (property "Datasheet" "~" (at 121.92 82.55 0))
    (pin "1")
    (pin "2")
    (instances
      (project "channelCard"
        (path
          (reference "C19") (unit 1)
        )
      )
    )
  )
)
