(kicad_sch (version 20230121) (generator eeschema)
  (paper "A4")
  (lib_symbols
    (symbol "Device:C" (pin_numbers hide) (pin_names (offset 0.254)) (in_bom yes) (on_board yes)
      (property "Reference" "C" (at 0.635 2.54 0))
      (property "Value" "C" (at 0.635 -2.54 0))
      (property "Footprint" "" (at 0.9652 -3.81 0))
      (property "Datasheet" "~" (at 0 0 0))
      (property "ki_keywords" "cap capacitor" (at 0 0 0))
      (property "ki_description" "Unpolarized capacitor" (at 0 0 0))
      (property "ki_fp_filters" "C_*" (at 0 0 0))
      (symbol "C_0_1"
        (polyline
          (pts
            (xy -2.032 -0.762)
            (xy 2.032 -0.762)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -2.032 0.762)
            (xy 2.032 0.762)
          )
          (fill (type none))
        )
      )
      (symbol "C_1_1"
        (pin passive line (at 0 3.81 270) (length 2.794)
          (name "~")
          (number "1")
        )
        (pin passive line (at 0 -3.81 90) (length 2.794)
          (name "~")
          (number "2")
        )
      )
    )
    (symbol "Device:LED" (pin_numbers hide) (pin_names (offset 1.016) hide) (in_bom yes) (on_board yes)
      (property "Reference" "D" (at 0 2.54 0))
      (property "Value" "LED" (at 0 -2.54 0))
      (property "Footprint" "" (at 0 0 0))
      (property "Datasheet" "~" (at 0 0 0))
      (property "ki_keywords" "LED diode" (at 0 0 0))
      (property "ki_description" "Light emitting diode" (at 0 0 0))
      (property "ki_fp_filters" "LED* LED_SMD:* LED_THT:*" (at 0 0 0))
      (symbol "LED_0_1"
        (polyline
          (pts
            (xy -1.27 -1.27)
            (xy -1.27 1.27)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -1.27 0)
            (xy 1.27 0)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 1.27 -1.27)
            (xy 1.27 1.27)
            (xy -1.27 0)
            (xy 1.27 -1.27)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -3.048 -0.762)
            (xy -4.572 -2.286)
            (xy -3.81 -2.286)
            (xy -4.572 -2.286)
            (xy -4.572 -1.524)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -1.778 -0.762)
            (xy -3.302 -2.286)
            (xy -2.54 -2.286)
            (xy -3.302 -2.286)
            (xy -3.302 -1.524)
          )
          (fill (type none))
        )
      )
      (symbol "LED_1_1"
        (pin passive line (at -3.81 0 0) (length 2.54)
          (name "K")
          (number "1")
        )
        (pin passive line (at 3.81 0 180) (length 2.54)
          (name "A")
          (number "2")
        )
      )
    )
    (symbol "Device:R" (pin_numbers hide) (pin_names (offset 0)) (in_bom yes) (on_board yes)
      (property "Reference" "R" (at 2.032 0 90))
      (property "Value" "R" (at 0 0 90))
      (property "Footprint" "" (at -1.778 0 90))
      (property "Datasheet" "~" (at 0 0 0))
      (property "ki_keywords" "R res resistor" (at 0 0 0))
      (property "ki_description" "Resistor" (at 0 0 0))
      (property "ki_fp_filters" "R_*" (at 0 0 0))
      (symbol "R_0_1"
        (rectangle (start -1.016 -2.54) (end 1.016 2.54)
          (fill (type none))
        )
      )
      (symbol "R_1_1"
        (pin passive line (at 0 3.81 270) (length 1.27)
          (name "~")
          (number "1")
        )
        (pin passive line (at 0 -3.81 90) (length 1.27)
          (name "~")
          (number "2")
        )
      )
    )
    (symbol "Diode:SM712_SOT23" (pin_names (offset 1.016) hide) (in_bom yes) (on_board yes)
      (property "Reference" "D" (at 0 4.445 0))
      (property "Value" "SM712_SOT23" (at 0 2.54 0))
      (property "Footprint" "Package_TO_SOT_SMD:SOT-23" (at 0 -8.89 0))
      (property "Datasheet" "https://www.littelfuse.com/~/media/electronics/datasheets/tvs_diode_arrays/littelfuse_tvs_diode_array_sm712_datasheet.pdf.pdf" (at -3.81 0 0))
      (property "ki_keywords" "transient voltage suppressor thyrector transil" (at 0 0 0))
      (property "ki_description" "7V/12V, 600W Asymmetrical TVS Diode Array, SOT-23" (at 0 0 0))
      (property "ki_fp_filters" "SOT?23*" (at 0 0 0))
      (symbol "SM712_SOT23_0_0"
        (polyline
          (pts
            (xy 0 -1.27)
            (xy 0 0)
          )
          (fill (type none))
        )
      )
      (symbol "SM712_SOT23_0_1"
        (polyline
          (pts
            (xy -6.35 0)
            (xy 6.35 0)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -3.302 1.27)
            (xy -3.81 1.27)
            (xy -3.81 -1.27)
            (xy -4.318 -1.27)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 4.318 1.27)
            (xy 3.81 1.27)
            (xy 3.81 -1.27)
            (xy 3.302 -1.27)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -6.35 -1.27)
            (xy -1.27 1.27)
            (xy -1.27 -1.27)
            (xy -6.35 1.27)
            (xy -6.35 -1.27)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 1.27 -1.27)
            (xy 1.27 1.27)
            (xy 6.35 -1.27)
            (xy 6.35 1.27)
            (xy 1.27 -1.27)
          )
          (fill (type none))
        )
        (circle (center 0 0) (radius 0.254)
          (fill (type outline))
        )
      )
      (symbol "SM712_SOT23_1_1"
        (pin passive line (at -8.89 0 0) (length 2.54)
          (name "A1")
          (number "1")
        )
        (pin passive line (at 8.89 0 180) (length 2.54)
          (name "A2")
          (number "2")
        )
        (pin input line (at 0 -3.81 90) (length 2.54)
          (name "common")
          (number "3")
        )
      )
    )
    (symbol "MAX13412EESA_T:MAX13412EESA+T" (pin_names (offset 1.016)) (in_bom yes) (on_board yes)
      (property "Reference" "U6" (at -1.27 11.43 0))
      (property "Value" "MAX13412EESA+T" (at 0 -7.62 0))
      (property "Footprint" "SOIC127P600X168-9N" (at 0 0 0))
      (property "Datasheet" "" (at 0 0 0))
      (property "MF" "Maxim Integrated" (at 0 0 0))
      (property "DESCRIPTION" "RS-485 Transceiver with Integrated Low-Dropout Regulator andAutoDirection Contro" (at 0 0 0))
      (property "PACKAGE" "SOIC-8 Maxim" (at 0 0 0))
      (property "PRICE" "None" (at 0 0 0))
      (property "MP" "MAX13412EESA+T" (at 0 0 0))
      (property "AVAILABILITY" "Unavailable" (at 0 0 0))
      (property "ki_locked" "" (at 0 0 0))
      (symbol "MAX13412EESA+T_0_0"
        (rectangle (start -10.16 -15.24) (end 10.16 12.7)
          (fill (type background))
        )
        (pin output line (at 15.24 2.54 180) (length 5.08)
          (name "RO")
          (number "1")
        )
        (pin output line (at 15.24 5.08 180) (length 5.08)
          (name "~{RE}")
          (number "2")
        )
        (pin output line (at 15.24 0 180) (length 5.08)
          (name "VREG")
          (number "3")
        )
        (pin input line (at 15.24 7.62 180) (length 5.08)
          (name "DI")
          (number "4")
        )
        (pin power_in line (at 15.24 -12.7 180) (length 5.08)
          (name "GND")
          (number "5")
        )
        (pin bidirectional line (at -15.24 -2.54 0) (length 5.08)
          (name "A")
          (number "6")
        )
        (pin bidirectional line (at -15.24 -5.08 0) (length 5.08)
          (name "B")
          (number "7")
        )
        (pin power_in line (at 15.24 10.16 180) (length 5.08)
          (name "VCC")
          (number "8")
        )
        (pin power_in line (at 15.24 -10.16 180) (length 5.08)
          (name "EP")
          (number "9")
        )
      )
    )
  )
  (junction (at 226.06 92.71) (diameter 0) (color 0 0 0 0))
  (junction (at 91.44 78.74) (diameter 0) (color 0 0 0 0))
  (junction (at 73.66 90.17) (diameter 0) (color 0 0 0 0))
  (junction (at 142.24 74.93) (diameter 0) (color 0 0 0 0))
  (junction (at 194.31 74.93) (diameter 0) (color 0 0 0 0))
  (junction (at 154.94 74.93) (diameter 0) (color 0 0 0 0))
  (junction (at 142.24 92.71) (diameter 0) (color 0 0 0 0))
  (junction (at 93.98 78.74) (diameter 0) (color 0 0 0 0))
  (junction (at 138.43 92.71) (diameter 0) (color 0 0 0 0))
  (junction (at 93.98 90.17) (diameter 0) (color 0 0 0 0))
  (junction (at 226.06 69.85) (diameter 0) (color 0 0 0 0))
  (junction (at 154.94 92.71) (diameter 0) (color 0 0 0 0))
  (junction (at 139.7 74.93) (diameter 0) (color 0 0 0 0))
  (wire (pts (xy 226.06 92.71) (xy 231.14 92.71)))
  (wire (pts (xy 91.44 78.74) (xy 93.98 78.74)))
  (wire (pts (xy 154.94 92.71) (xy 226.06 92.71)))
  (wire (pts (xy 93.98 78.74) (xy 101.6 78.74)))
  (wire (pts (xy 186.69 74.93) (xy 194.31 74.93)))
  (wire (pts (xy 142.24 92.71) (xy 154.94 92.71)))
  (wire (pts (xy 226.06 85.09) (xy 226.06 92.71)))
  (wire (pts (xy 73.66 90.17) (xy 73.66 101.6)))
  (wire (pts (xy 73.66 90.17) (xy 93.98 90.17)))
  (wire (pts (xy 71.12 78.74) (xy 91.44 78.74)))
  (wire (pts (xy 177.8 74.93) (xy 179.07 74.93)))
  (wire (pts (xy 194.31 72.39) (xy 194.31 74.93)))
  (wire (pts (xy 138.43 90.17) (xy 138.43 92.71)))
  (wire (pts (xy 132.08 74.93) (xy 139.7 74.93)))
  (wire (pts (xy 138.43 105.41) (xy 138.43 92.71)))
  (wire (pts (xy 142.24 74.93) (xy 154.94 74.93)))
  (wire (pts (xy 154.94 74.93) (xy 170.18 74.93)))
  (wire (pts (xy 154.94 85.09) (xy 154.94 92.71)))
  (wire (pts (xy 93.98 90.17) (xy 101.6 90.17)))
  (wire (pts (xy 71.12 90.17) (xy 73.66 90.17)))
  (wire (pts (xy 132.08 77.47) (xy 134.62 77.47)))
  (wire (pts (xy 132.08 92.71) (xy 138.43 92.71)))
  (wire (pts (xy 139.7 74.93) (xy 142.24 74.93)))
  (wire (pts (xy 194.31 74.93) (xy 204.47 74.93)))
  (wire (pts (xy 138.43 92.71) (xy 142.24 92.71)))
  (wire (pts (xy 154.94 74.93) (xy 154.94 77.47)))
  (wire (pts (xy 142.24 74.93) (xy 142.24 77.47)))
  (wire (pts (xy 93.98 78.74) (xy 93.98 81.28)))
  (wire (pts (xy 101.6 78.74) (xy 101.6 82.55)))
  (wire (pts (xy 132.08 90.17) (xy 138.43 90.17)))
  (wire (pts (xy 142.24 85.09) (xy 142.24 92.71)))
  (wire (pts (xy 132.08 72.39) (xy 194.31 72.39)))
  (wire (pts (xy 132.08 69.85) (xy 226.06 69.85)))
  (wire (pts (xy 139.7 74.93) (xy 139.7 80.01)))
  (wire (pts (xy 91.44 101.6) (xy 91.44 78.74)))
  (wire (pts (xy 82.55 105.41) (xy 138.43 105.41)))
  (wire (pts (xy 93.98 88.9) (xy 93.98 90.17)))
  (wire (pts (xy 132.08 80.01) (xy 139.7 80.01)))
  (wire (pts (xy 101.6 90.17) (xy 101.6 85.09)))
  (wire (pts (xy 226.06 69.85) (xy 226.06 77.47)))
  (wire (pts (xy 226.06 69.85) (xy 229.87 69.85)))
  (text "TX\n" (at 198.12 73.66 0))
  (hierarchical_label "Gnd" (shape input) (at 231.14 92.71 0) (fields_autoplaced))
  (hierarchical_label "RE'" (shape input) (at 204.47 74.93 0) (fields_autoplaced))
  (hierarchical_label "A" (shape input) (at 71.12 78.74 180) (fields_autoplaced))
  (hierarchical_label "R0" (shape input) (at 134.62 77.47 0) (fields_autoplaced))
  (hierarchical_label "Vin" (shape input) (at 229.87 69.85 0) (fields_autoplaced))
  (hierarchical_label "B" (shape input) (at 71.12 90.17 180) (fields_autoplaced))
  (symbol (lib_id "Device:R") (at 93.98 85.09 0) (unit 1)
    (in_bom yes) (on_board yes) (dnp no) (fields_autoplaced)
    (property "Reference" "R6" (at 96.52 83.82 0))
    (property "Value" "120" (at 96.52 86.36 0))
    (property "Footprint" "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (at 92.202 85.09 90))
    (property "Datasheet" "~" (at 93.98 85.09 0))
    (pin "1")
    (pin "2")
    (instances
      (project "channelCard"
        (path
          (reference "R6") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "Device:LED") (at 182.88 74.93 180) (unit 1)
    (in_bom yes) (on_board yes) (dnp no)
    (property "Reference" "D3" (at 181.61 77.47 0))
    (property "Value" "LED" (at 181.61 80.01 0))
    (property "Footprint" "LED_SMD:LED_0603_1608Metric_Pad1.05x0.95mm_HandSolder" (at 182.88 74.93 0))
    (property "Datasheet" "~" (at 182.88 74.93 0))
    (pin "1")
    (pin "2")
    (instances
      (project "channelCard"
        (path
          (reference "D3") (unit 1)
        )
        (path
          (reference "D2") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "Device:C") (at 226.06 81.28 0) (unit 1)
    (in_bom yes) (on_board yes) (dnp no) (fields_autoplaced)
    (property "Reference" "C12" (at 229.87 80.01 0))
    (property "Value" "0.1uF" (at 229.87 82.55 0))
    (property "Footprint" "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder" (at 227.0252 85.09 0))
    (property "Datasheet" "~" (at 226.06 81.28 0))
    (property "rating" "50V" (at 226.06 81.28 0))
    (pin "1")
    (pin "2")
    (instances
      (project "channelCard"
        (path
          (reference "C12") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "MAX13412EESA_T:MAX13412EESA+T") (at 116.84 80.01 0) (unit 1)
    (in_bom yes) (on_board yes) (dnp no)
    (property "Reference" "U6" (at 115.57 68.58 0))
    (property "Value" "MAX13412EESA+T" (at 116.84 87.63 0))
    (property "Footprint" "SOIC127P600X168-9N" (at 116.84 80.01 0))
    (property "Datasheet" "" (at 116.84 80.01 0))
    (property "MF" "Maxim Integrated" (at 116.84 80.01 0))
    (property "DESCRIPTION" "RS-485 Transceiver with Integrated Low-Dropout Regulator andAutoDirection Contro" (at 116.84 80.01 0))
    (property "PACKAGE" "SOIC-8 Maxim" (at 116.84 80.01 0))
    (property "PRICE" "None" (at 116.84 80.01 0))
    (property "MP" "MAX13412EESA+T" (at 116.84 80.01 0))
    (property "AVAILABILITY" "Unavailable" (at 116.84 80.01 0))
    (pin "1")
    (pin "2")
    (pin "3")
    (pin "4")
    (pin "5")
    (pin "6")
    (pin "7")
    (pin "8")
    (pin "9")
    (instances
      (project "channelCard"
        (path
          (reference "U6") (unit 1)
        )
        (path
          (reference "U6") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "Device:C") (at 154.94 81.28 0) (unit 1)
    (in_bom yes) (on_board yes) (dnp no) (fields_autoplaced)
    (property "Reference" "C16" (at 158.75 80.01 0))
    (property "Value" "0.1uF" (at 158.75 82.55 0))
    (property "Footprint" "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder" (at 155.9052 85.09 0))
    (property "Datasheet" "~" (at 154.94 81.28 0))
    (property "rating" "50V" (at 154.94 81.28 0))
    (pin "1")
    (pin "2")
    (instances
      (project "channelCard"
        (path
          (reference "C16") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "Diode:SM712_SOT23") (at 82.55 101.6 0) (unit 1)
    (in_bom yes) (on_board yes) (dnp no) (fields_autoplaced)
    (property "Reference" "D4" (at 82.55 95.25 0))
    (property "Value" "SM712_SOT23" (at 82.55 97.79 0))
    (property "Footprint" "Package_TO_SOT_SMD:SOT-23" (at 82.55 110.49 0))
    (property "Datasheet" "https://www.littelfuse.com/~/media/electronics/datasheets/tvs_diode_arrays/littelfuse_tvs_diode_array_sm712_datasheet.pdf.pdf" (at 78.74 101.6 0))
    (pin "1")
    (pin "2")
    (pin "3")
    (instances
      (project "channelCard"
        (path
          (reference "D4") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "Device:C") (at 142.24 81.28 0) (unit 1)
    (in_bom yes) (on_board yes) (dnp no)
    (property "Reference" "C13" (at 146.05 80.01 0))
    (property "Value" "1.0uF" (at 146.05 82.55 0))
    (property "Footprint" "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder" (at 143.2052 85.09 0))
    (property "Datasheet" "~" (at 142.24 81.28 0))
    (property "Rating" "50v" (at 147.32 85.09 0))
    (pin "1")
    (pin "2")
    (instances
      (project "channelCard"
        (path
          (reference "C13") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "Device:R") (at 173.99 74.93 90) (unit 1)
    (in_bom yes) (on_board yes) (dnp no)
    (property "Reference" "R7" (at 173.99 77.47 90))
    (property "Value" "3.3k" (at 173.99 80.01 90))
    (property "Footprint" "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (at 173.99 76.708 90))
    (property "Datasheet" "~" (at 173.99 74.93 0))
    (pin "1")
    (pin "2")
    (instances
      (project "channelCard"
        (path
          (reference "R7") (unit 1)
        )
      )
    )
  )
)
