(kicad_pcb (version 4) (host pcbnew 4.0.6)
  (general
    (links 215)
    (no_connects 0)
    (area -1.82508 -1.737 57.50748 57.25348)
    (thickness 1.6)
    (drawings 4)
    (tracks 1112)
    (zones 0)
    (modules 74)
    (nets 78)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user hide)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.254)
    (user_trace_width 0.254)
    (user_trace_width 0.381)
    (user_trace_width 0.508)
    (user_trace_width 1.016)
    (user_trace_width 1.27)
    (user_trace_width 1.524)
    (user_trace_width 1.778)
    (user_trace_width 2.032)
    (trace_clearance 0.2)
    (zone_clearance 0.381)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.635)
    (via_drill 0.381)
    (via_min_size 0.635)
    (via_min_drill 0.381)
    (user_via 0.762 0.4572)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 2.794 2.794)
    (pad_drill 2.032)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements 7FFEF7FF)
    (pcbplotparams
      (layerselection 0x011fc_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue false)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk true)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory fab3/))
  )
  (net 0 "")
  (net 1 /3V3)
  (net 2 /GND)
  (net 3 "Net-(C3-Pad1)")
  (net 4 "Net-(C3-Pad2)")
  (net 5 "Net-(C4-Pad1)")
  (net 6 "Net-(C4-Pad2)")
  (net 7 /+5V)
  (net 8 /VBat)
  (net 9 "Net-(C8-Pad2)")
  (net 10 "Net-(C10-Pad1)")
  (net 11 "Net-(C11-Pad1)")
  (net 12 /GND_EXT)
  (net 13 /Vin_EXT)
  (net 14 "Net-(D2-Pad1)")
  (net 15 "Net-(D3-Pad2)")
  (net 16 "Net-(D4-Pad2)")
  (net 17 /Vin)
  (net 18 "Net-(JP1-Pad1)")
  (net 19 "Net-(JP1-Pad2)")
  (net 20 /ATX_ON)
  (net 21 "/Power Output/ATX_12V")
  (net 22 "/Power Output/ATX_5V")
  (net 23 "Net-(P2-Pad3)")
  (net 24 "Net-(P2-Pad2)")
  (net 25 /SDA)
  (net 26 /SCL)
  (net 27 "Net-(R5-Pad1)")
  (net 28 "/Power Output/ATX_5V_SB")
  (net 29 "Net-(U2-Pad2)")
  (net 30 /RTC32k)
  (net 31 /RTCINT)
  (net 32 "Net-(U4-Pad10)")
  (net 33 /RAZ_TX)
  (net 34 /RAZ_RX)
  (net 35 "Net-(P7-Pad4)")
  (net 36 "Net-(P7-Pad1)")
  (net 37 "Net-(P7-Pad2)")
  (net 38 "Net-(P7-Pad3)")
  (net 39 /ODROID_1.8V)
  (net 40 /ODROID_TX)
  (net 41 /ODROID_RX)
  (net 42 /ODROID_TX_3V3)
  (net 43 /ODROID_RX_3V3)
  (net 44 "Net-(U1-Pad6)")
  (net 45 "Net-(C12-Pad2)")
  (net 46 "Net-(C13-Pad2)")
  (net 47 "Net-(C17-Pad1)")
  (net 48 /InRushLimit/V_IR_IN)
  (net 49 "Net-(C19-Pad2)")
  (net 50 /InRushLimit/V_IR_OUT)
  (net 51 "Net-(C20-Pad2)")
  (net 52 "Net-(D5-Pad2)")
  (net 53 "Net-(P7-Pad5)")
  (net 54 "Net-(Q3-Pad1)")
  (net 55 "Net-(Q3-Pad4)")
  (net 56 "Net-(Q5-Pad4)")
  (net 57 "Net-(R13-Pad2)")
  (net 58 "Net-(R14-Pad2)")
  (net 59 /RTC_RST)
  (net 60 "Net-(U3-Pad7)")
  (net 61 "Net-(U3-Pad8)")
  (net 62 "Net-(U3-Pad9)")
  (net 63 "Net-(U3-Pad10)")
  (net 64 "Net-(U6-Pad6)")
  (net 65 "Net-(U8-Pad1)")
  (net 66 "Net-(U8-Pad2)")
  (net 67 "Net-(U8-Pad3)")
  (net 68 "Net-(U8-Pad4)")
  (net 69 "Net-(U8-Pad5)")
  (net 70 "Net-(U8-Pad7)")
  (net 71 "Net-(U8-Pad11)")
  (net 72 "Net-(U8-Pad12)")
  (net 73 "Net-(U8-Pad18)")
  (net 74 "Net-(U9-Pad1)")
  (net 75 "Net-(U9-Pad4)")
  (net 76 "Net-(U9-Pad5)")
  (net 77 "Net-(U8-Pad6)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.635)
    (via_drill 0.381)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /+5V)
    (add_net /3V3)
    (add_net /ATX_ON)
    (add_net /GND)
    (add_net /GND_EXT)
    (add_net /InRushLimit/V_IR_IN)
    (add_net /InRushLimit/V_IR_OUT)
    (add_net /ODROID_1.8V)
    (add_net /ODROID_RX)
    (add_net /ODROID_RX_3V3)
    (add_net /ODROID_TX)
    (add_net /ODROID_TX_3V3)
    (add_net "/Power Output/ATX_12V")
    (add_net "/Power Output/ATX_5V")
    (add_net "/Power Output/ATX_5V_SB")
    (add_net /RAZ_RX)
    (add_net /RAZ_TX)
    (add_net /RTC32k)
    (add_net /RTCINT)
    (add_net /RTC_RST)
    (add_net /SCL)
    (add_net /SDA)
    (add_net /VBat)
    (add_net /Vin)
    (add_net /Vin_EXT)
    (add_net "Net-(C10-Pad1)")
    (add_net "Net-(C11-Pad1)")
    (add_net "Net-(C12-Pad2)")
    (add_net "Net-(C13-Pad2)")
    (add_net "Net-(C17-Pad1)")
    (add_net "Net-(C19-Pad2)")
    (add_net "Net-(C20-Pad2)")
    (add_net "Net-(C3-Pad1)")
    (add_net "Net-(C3-Pad2)")
    (add_net "Net-(C4-Pad1)")
    (add_net "Net-(C4-Pad2)")
    (add_net "Net-(C8-Pad2)")
    (add_net "Net-(D2-Pad1)")
    (add_net "Net-(D3-Pad2)")
    (add_net "Net-(D4-Pad2)")
    (add_net "Net-(D5-Pad2)")
    (add_net "Net-(JP1-Pad1)")
    (add_net "Net-(JP1-Pad2)")
    (add_net "Net-(P2-Pad2)")
    (add_net "Net-(P2-Pad3)")
    (add_net "Net-(P7-Pad1)")
    (add_net "Net-(P7-Pad2)")
    (add_net "Net-(P7-Pad3)")
    (add_net "Net-(P7-Pad4)")
    (add_net "Net-(P7-Pad5)")
    (add_net "Net-(Q3-Pad1)")
    (add_net "Net-(Q3-Pad4)")
    (add_net "Net-(Q5-Pad4)")
    (add_net "Net-(R13-Pad2)")
    (add_net "Net-(R14-Pad2)")
    (add_net "Net-(R5-Pad1)")
    (add_net "Net-(U1-Pad6)")
    (add_net "Net-(U2-Pad2)")
    (add_net "Net-(U3-Pad10)")
    (add_net "Net-(U3-Pad7)")
    (add_net "Net-(U3-Pad8)")
    (add_net "Net-(U3-Pad9)")
    (add_net "Net-(U4-Pad10)")
    (add_net "Net-(U6-Pad6)")
    (add_net "Net-(U8-Pad1)")
    (add_net "Net-(U8-Pad11)")
    (add_net "Net-(U8-Pad12)")
    (add_net "Net-(U8-Pad18)")
    (add_net "Net-(U8-Pad2)")
    (add_net "Net-(U8-Pad3)")
    (add_net "Net-(U8-Pad4)")
    (add_net "Net-(U8-Pad5)")
    (add_net "Net-(U8-Pad6)")
    (add_net "Net-(U8-Pad7)")
    (add_net "Net-(U9-Pad1)")
    (add_net "Net-(U9-Pad4)")
    (add_net "Net-(U9-Pad5)")
  )
  (module SPCInterfaceBoard-SPCPWSSC:BME280 (layer F.Cu) (tedit 59488A62)
    (at 23.795 26.817)
    (fp_text reference U5 (at 2.621 -2.306) (layer F.SilkS))
    (fp_text value BME280 (at 0 -0.5) (layer F.Fab))
    (pad 1 smd rect (at 1.125 -0.975) (size 0.7 0.35) (layers F.Cu F.Paste F.Mask)
      (net 2 /GND))
    (pad 2 smd rect (at 1.125 -0.325) (size 0.7 0.35) (layers F.Cu F.Paste F.Mask)
      (net 1 /3V3))
    (pad 3 smd rect (at 1.125 0.325) (size 0.7 0.35) (layers F.Cu F.Paste F.Mask)
      (net 25 /SDA))
    (pad 4 smd rect (at 1.125 0.975) (size 0.7 0.35) (layers F.Cu F.Paste F.Mask)
      (net 26 /SCL))
    (pad 5 smd rect (at -1.125 0.975) (size 0.7 0.35) (layers F.Cu F.Paste F.Mask)
      (net 2 /GND))
    (pad 6 smd rect (at -1.125 0.325) (size 0.7 0.35) (layers F.Cu F.Paste F.Mask)
      (net 1 /3V3))
    (pad 7 smd rect (at -1.125 -0.325) (size 0.7 0.35) (layers F.Cu F.Paste F.Mask)
      (net 2 /GND))
    (pad 8 smd rect (at -1.125 -0.975) (size 0.7 0.35) (layers F.Cu F.Paste F.Mask)
      (net 1 /3V3))
  )
  (module Capacitors_Tantalum_SMD:TantalC_SizeX_EIA-7343 (layer F.Cu) (tedit 59363468)
    (at 45.72 17.272 90)
    (descr TantalC_SizeX_EIA-7343)
    (fp_text reference C10 (at -5.461 0 360) (layer F.SilkS))
    (fp_text value 100uF (at 0 2.7305 90) (layer F.Fab))
    (pad 1 smd rect (at 2.99974 0 90) (size 2.55016 2.70002) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(C10-Pad1)"))
    (pad 2 smd rect (at -2.99974 0 90) (size 2.55016 3.79984) (layers F.Cu F.Paste F.Mask)
      (net 2 /GND))
    (model Capacitors_Tantalum_SMD.3dshapes/TantalC_SizeX_EIA-7343.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_Tantalum_SMD:TantalC_SizeX_EIA-7343 (layer F.Cu) (tedit 59363412)
    (at 45.72 7.62 90)
    (descr TantalC_SizeX_EIA-7343)
    (fp_text reference C11 (at 5.461 0.127 360) (layer F.SilkS))
    (fp_text value 100uF (at 0 2.7305 90) (layer F.Fab))
    (pad 1 smd rect (at 2.99974 0 90) (size 2.55016 2.70002) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(C11-Pad1)"))
    (pad 2 smd rect (at -2.99974 0 90) (size 2.55016 3.79984) (layers F.Cu F.Paste F.Mask)
      (net 2 /GND))
    (model Capacitors_Tantalum_SMD.3dshapes/TantalC_SizeX_EIA-7343.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_0603 (layer F.Cu) (tedit 59498035)
    (at 13.3858 44.0944 180)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D3 (at 2.2606 0.4572 180) (layer F.SilkS))
    (fp_text value "2.1V 20mA" (at -6 0.2 180) (layer F.Fab))
    (pad 2 smd rect (at 0.7493 0) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(D3-Pad2)"))
    (pad 1 smd rect (at -0.7493 0) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 2 /GND))
    (model LEDs.3dshapes/LED_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_0603 (layer F.Cu) (tedit 59488E16)
    (at 45.085 37.338 180)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D4 (at -2.286 0.127 180) (layer F.SilkS))
    (fp_text value "1.95V 5mA" (at 0 1.5 180) (layer F.Fab))
    (pad 2 smd rect (at 0.7493 0) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(D4-Pad2)"))
    (pad 1 smd rect (at -0.7493 0) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 2 /GND))
    (model LEDs.3dshapes/LED_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module w_misc_comp:fuse_smf (layer F.Cu) (tedit 5949804F)
    (at 6.295 47.017 180)
    (descr "Fuse Holder SMF, Littelfuse")
    (tags Fuse)
    (autoplace_cost180 10)
    (fp_text reference F1 (at 0.0466 -3.8592 180) (layer F.SilkS))
    (fp_text value 10A (at 0 3.302 180) (layer F.SilkS))
    (pad 1 smd rect (at -3.1877 0 180) (size 4.23926 3.81) (layers F.Cu F.Paste F.Mask)
      (net 48 /InRushLimit/V_IR_IN))
    (pad 2 smd rect (at 3.1877 0 180) (size 4.23926 3.81) (layers F.Cu F.Paste F.Mask)
      (net 13 /Vin_EXT))
    (model walter/misc_comp/fuse_smf.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SparkFun-Connectors:1X03 (layer F.Cu) (tedit 59497FD8)
    (at 40.795 44.792 180)
    (fp_text reference JP1 (at -0.099 -2.3758 180) (layer Eco1.User))
    (fp_text value . (at 2.54 3.81 180) (layer Eco1.User))
    (pad 1 thru_hole oval (at 0 0 270) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 18 "Net-(JP1-Pad1)"))
    (pad 2 thru_hole oval (at 2.54 0 270) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 19 "Net-(JP1-Pad2)"))
    (pad 3 thru_hole oval (at 5.08 0 270) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 20 /ATX_ON))
  )
  (module PowerControlBoard:IHLP2525CZERR10M01 (layer B.Cu) (tedit 5949811F)
    (at 46.228 17.399 90)
    (fp_text reference L1 (at -5.1562 -0.1778 180) (layer B.SilkS))
    (fp_text value "100 nH" (at 0 4.8 90) (layer B.Fab))
    (pad 1 smd rect (at -2.8448 0 90) (size 2.3622 3.429) (layers B.Cu B.Paste B.Mask)
      (net 10 "Net-(C10-Pad1)"))
    (pad 2 smd rect (at 2.8448 0 90) (size 2.3622 3.429) (layers B.Cu B.Paste B.Mask)
      (net 21 "/Power Output/ATX_12V"))
  )
  (module PowerControlBoard:IHLP2525CZERR10M01 (layer B.Cu) (tedit 59498121)
    (at 46.228 7.366 90)
    (fp_text reference L2 (at 5.0546 0.1016 360) (layer B.SilkS))
    (fp_text value "100 nH" (at 0 4.8 90) (layer B.Fab))
    (pad 1 smd rect (at -2.8448 0 90) (size 2.3622 3.429) (layers B.Cu B.Paste B.Mask)
      (net 11 "Net-(C11-Pad1)"))
    (pad 2 smd rect (at 2.8448 0 90) (size 2.3622 3.429) (layers B.Cu B.Paste B.Mask)
      (net 22 "/Power Output/ATX_5V"))
  )
  (module PowerControlBoard:CoinCell12mm (layer F.Cu) (tedit 59498074)
    (at 14.595 8.217)
    (fp_text reference P1 (at -7.5846 -5.7532) (layer F.SilkS))
    (fp_text value BATT (at 0.1524 4.8514) (layer F.Fab))
    (pad 1 smd rect (at -7.62 0) (size 4.064 4.064) (layers F.Cu F.Paste F.Mask)
      (net 8 /VBat))
    (pad 1 smd rect (at 7.62 0) (size 4.064 4.064) (layers F.Cu F.Paste F.Mask)
      (net 8 /VBat))
    (pad 2 smd rect (at 0 0) (size 3.96 3.96) (layers F.Cu F.Paste F.Mask)
      (net 2 /GND))
  )
  (module w_conn_mpt:mpt_0,5%2f3-2,54 (layer F.Cu) (tedit 59497FE5)
    (at 51.308 32.385 90)
    (descr "3-way 2.54mm pitch terminal block, Phoenix MPT series")
    (fp_text reference P2 (at -2.6924 -4.8768 180) (layer F.SilkS))
    (fp_text value RS-232 (at 0 4.50088 90) (layer F.SilkS))
    (pad 3 thru_hole oval (at -2.54 0 90) (size 1.99898 1.99898) (drill 1.09728) (layers *.Cu *.Mask F.SilkS)
      (net 23 "Net-(P2-Pad3)"))
    (pad 1 thru_hole rect (at 2.54 0 90) (size 1.99898 1.99898) (drill 1.09728) (layers *.Cu *.Mask F.SilkS)
      (net 2 /GND))
    (pad 2 thru_hole oval (at 0 0 90) (size 1.99898 1.99898) (drill 1.09728) (layers *.Cu *.Mask F.SilkS)
      (net 24 "Net-(P2-Pad2)"))
    (model walter/conn_mpt/mpt_0,5-3-2,54.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module w_conn_mpt:mpt_0,5%2f4-2,54 (layer F.Cu) (tedit 59497FEC)
    (at 51.308 22.352 90)
    (descr "4-way 2.54mm pitch terminal block, Phoenix MPT series")
    (fp_text reference P3 (at -4.2926 -4.9022 180) (layer F.SilkS))
    (fp_text value CONN_01X04 (at 0 4.50088 90) (layer F.SilkS))
    (pad 4 thru_hole oval (at -3.81 0 90) (size 1.99898 1.99898) (drill 1.09728) (layers *.Cu *.Mask F.SilkS)
      (net 2 /GND))
    (pad 1 thru_hole rect (at 3.81 0 90) (size 1.99898 1.99898) (drill 1.09728) (layers *.Cu *.Mask F.SilkS)
      (net 10 "Net-(C10-Pad1)"))
    (pad 2 thru_hole oval (at 1.27 0 90) (size 1.99898 1.99898) (drill 1.09728) (layers *.Cu *.Mask F.SilkS)
      (net 10 "Net-(C10-Pad1)"))
    (pad 3 thru_hole oval (at -1.27 0 90) (size 1.99898 1.99898) (drill 1.09728) (layers *.Cu *.Mask F.SilkS)
      (net 2 /GND))
    (model walter/conn_mpt/mpt_0,5-4-2,54.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module w_conn_mpt:mpt_0,5%2f4-2,54 (layer F.Cu) (tedit 59497FF7)
    (at 51.435 9.906 90)
    (descr "4-way 2.54mm pitch terminal block, Phoenix MPT series")
    (fp_text reference P4 (at -6.2992 0 360) (layer F.SilkS))
    (fp_text value CONN_01X04 (at 0 4.50088 90) (layer F.SilkS))
    (pad 4 thru_hole oval (at -3.81 0 90) (size 1.99898 1.99898) (drill 1.09728) (layers *.Cu *.Mask F.SilkS)
      (net 2 /GND))
    (pad 1 thru_hole rect (at 3.81 0 90) (size 1.99898 1.99898) (drill 1.09728) (layers *.Cu *.Mask F.SilkS)
      (net 11 "Net-(C11-Pad1)"))
    (pad 2 thru_hole oval (at 1.27 0 90) (size 1.99898 1.99898) (drill 1.09728) (layers *.Cu *.Mask F.SilkS)
      (net 11 "Net-(C11-Pad1)"))
    (pad 3 thru_hole oval (at -1.27 0 90) (size 1.99898 1.99898) (drill 1.09728) (layers *.Cu *.Mask F.SilkS)
      (net 2 /GND))
    (model walter/conn_mpt/mpt_0,5-4-2,54.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module w_conn_mpt:mpt_0,5%2f4-2,54 (layer F.Cu) (tedit 59497FE0)
    (at 51.435 42.926 270)
    (descr "4-way 2.54mm pitch terminal block, Phoenix MPT series")
    (fp_text reference P5 (at 6.5786 0.3556 540) (layer F.SilkS))
    (fp_text value CONN_01X04 (at 0 4.50088 270) (layer F.SilkS))
    (pad 4 thru_hole oval (at -3.81 0 270) (size 1.99898 1.99898) (drill 1.09728) (layers *.Cu *.Mask F.SilkS)
      (net 2 /GND))
    (pad 1 thru_hole rect (at 3.81 0 270) (size 1.99898 1.99898) (drill 1.09728) (layers *.Cu *.Mask F.SilkS)
      (net 39 /ODROID_1.8V))
    (pad 2 thru_hole oval (at 1.27 0 270) (size 1.99898 1.99898) (drill 1.09728) (layers *.Cu *.Mask F.SilkS)
      (net 40 /ODROID_TX))
    (pad 3 thru_hole oval (at -1.27 0 270) (size 1.99898 1.99898) (drill 1.09728) (layers *.Cu *.Mask F.SilkS)
      (net 41 /ODROID_RX))
    (model walter/conn_mpt/mpt_0,5-4-2,54.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module PowerControlBoard:8-PowerTDFN (layer B.Cu) (tedit 59498104)
    (at 10.67 37.967 90)
    (fp_text reference Q1 (at 0.4766 -3.4818 270) (layer B.SilkS))
    (fp_text value FDMS86550 (at 0 5.08 90) (layer B.Fab))
    (pad 2 smd rect (at -2.667 0.635 180) (size 0.61 1.27) (layers B.Cu B.Paste B.Mask)
      (net 2 /GND))
    (pad 1 smd rect (at -2.667 1.905 180) (size 0.61 1.27) (layers B.Cu B.Paste B.Mask)
      (net 2 /GND))
    (pad 3 smd rect (at -2.667 -0.635 180) (size 0.61 1.27) (layers B.Cu B.Paste B.Mask)
      (net 2 /GND))
    (pad 4 smd rect (at -2.667 -1.905 180) (size 0.61 1.27) (layers B.Cu B.Paste B.Mask)
      (net 14 "Net-(D2-Pad1)"))
    (pad 8 smd rect (at 2.698 1.905 180) (size 0.61 1.27) (layers B.Cu B.Paste B.Mask)
      (net 12 /GND_EXT))
    (pad 7 smd rect (at 2.698 0.635 180) (size 0.61 1.27) (layers B.Cu B.Paste B.Mask)
      (net 12 /GND_EXT))
    (pad 6 smd rect (at 2.698 -0.635 180) (size 0.61 1.27) (layers B.Cu B.Paste B.Mask)
      (net 12 /GND_EXT))
    (pad 5 smd rect (at 2.698 -1.905 180) (size 0.61 1.27) (layers B.Cu B.Paste B.Mask)
      (net 12 /GND_EXT))
    (pad 8 smd rect (at 0.254 0 180) (size 4.42 3.65) (layers B.Cu B.Paste B.Mask)
      (net 12 /GND_EXT))
  )
  (module PowerControlBoard:RAZIMUM0 (layer F.Cu) (tedit 5949809B)
    (at 0.995 32.617)
    (fp_text reference U1 (at 24.4304 -30.966) (layer F.SilkS))
    (fp_text value RAZIMUM0 (at 5.715 -6.985) (layer F.Fab))
    (fp_text user "9DoF Razor IMU" (at 14.1942 -31.1438) (layer F.SilkS))
    (fp_text user GND (at 28.0118 -24.362) (layer F.SilkS))
    (fp_text user 3V3 (at 28.0372 -21.9744) (layer F.SilkS))
    (fp_text user RX (at 28.575 -19.685) (layer F.SilkS))
    (fp_text user TX (at 28.575 -17.145) (layer F.SilkS))
    (fp_text user 10 (at 28.575 -14.605) (layer F.SilkS))
    (fp_text user 11 (at 28.575 -12.065) (layer F.SilkS))
    (fp_text user 12 (at 28.575 -9.525) (layer F.SilkS))
    (fp_text user 13 (at 28.575 -6.985) (layer F.SilkS))
    (fp_text user A0 (at 22.86 -12.065) (layer F.SilkS))
    (fp_text user A1 (at 22.86 -14.605) (layer F.SilkS))
    (fp_text user A2 (at 22.86 -17.145) (layer F.SilkS))
    (fp_text user A3 (at 22.86 -19.685) (layer F.SilkS))
    (fp_text user A4 (at 23.7446 -21.3648) (layer F.SilkS))
    (fp_text user 08 (at 26.7164 -25.9876) (layer F.SilkS))
    (fp_text user 09 (at 26.7926 -28.68) (layer F.SilkS))
    (fp_text user VIN (at 16.51 -3.175) (layer F.SilkS))
    (fp_text user SCL (at 3.2976 -15.8276) (layer F.SilkS))
    (fp_text user SDA (at 3.3738 -18.4946) (layer F.SilkS))
    (fp_text user 3V3 (at 3.3484 -21.06) (layer F.SilkS))
    (fp_text user GND (at 1.5958 -26.5464) (layer F.SilkS))
    (pad 1 thru_hole rect (at 1.27 -24.765) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 2 /GND))
    (pad V thru_hole circle (at 16.51 -1.27) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 7 /+5V))
    (pad 22 thru_hole circle (at 2.54 -29.21) (size 2.794 2.794) (drill 2.032) (layers *.Cu *.Mask))
    (pad 23 thru_hole circle (at 29.21 -29.21) (size 2.794 2.794) (drill 2.032) (layers *.Cu *.Mask))
    (pad 24 thru_hole circle (at 29.21 -2.54) (size 2.794 2.794) (drill 2.032) (layers *.Cu *.Mask))
    (pad 25 thru_hole circle (at 2.54 -2.54) (size 2.794 2.794) (drill 2.032) (layers *.Cu *.Mask))
    (pad 2 thru_hole circle (at 1.27 -22.225) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 1 /3V3))
    (pad 3 thru_hole circle (at 1.27 -19.685) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 25 /SDA))
    (pad 4 thru_hole circle (at 1.27 -17.145) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 26 /SCL))
    (pad A0 thru_hole circle (at 25.4 -12.065) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 53 "Net-(P7-Pad5)"))
    (pad A1 thru_hole circle (at 25.4 -14.605) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 35 "Net-(P7-Pad4)"))
    (pad A2 thru_hole circle (at 25.4 -17.145) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 38 "Net-(P7-Pad3)"))
    (pad A3 thru_hole circle (at 25.4 -19.685) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 59 /RTC_RST))
    (pad A4 thru_hole circle (at 25.4 -22.225) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 20 /ATX_ON))
    (pad 08 thru_hole circle (at 25.4 -24.765) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 37 "Net-(P7-Pad2)"))
    (pad 09 thru_hole circle (at 25.4 -27.305) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 31 /RTCINT))
    (pad D13 thru_hole circle (at 30.48 -6.985) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 30 /RTC32k))
    (pad D12 thru_hole circle (at 30.48 -9.525) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 42 /ODROID_TX_3V3))
    (pad D11 thru_hole circle (at 30.48 -12.065) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 36 "Net-(P7-Pad1)"))
    (pad D10 thru_hole circle (at 30.48 -14.605) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 43 /ODROID_RX_3V3))
    (pad TXO thru_hole circle (at 30.48 -17.145) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 33 /RAZ_TX))
    (pad RXI thru_hole circle (at 30.48 -19.685) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 34 /RAZ_RX))
    (pad 6 thru_hole circle (at 30.48 -22.225) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 44 "Net-(U1-Pad6)"))
    (pad 5 thru_hole circle (at 30.48 -24.765) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 2 /GND))
  )
  (module PowerControlBoard:POLOLUBUCKREG (layer F.Cu) (tedit 594980A9)
    (at 14.945 49.492)
    (fp_text reference U2 (at 4.5876 -3.0354) (layer F.SilkS))
    (fp_text value PololuStepDown (at 6.35 -17.78) (layer F.Fab))
    (fp_text user VOUT (at 4.1558 -4.9404) (layer F.SilkS))
    (fp_text user GND (at 3.6224 -7.582) (layer F.SilkS))
    (fp_text user VIN (at 3.4192 -10.0458) (layer F.SilkS))
    (fp_text user SHDN (at 3.851 -13.678) (layer F.SilkS))
    (fp_text user PG (at 3.1906 -15.2782) (layer F.SilkS))
    (pad 1 thru_hole circle (at 1.27 -15.24) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 15 "Net-(D3-Pad2)"))
    (pad 2 thru_hole circle (at 1.27 -12.7) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 29 "Net-(U2-Pad2)"))
    (pad 3 thru_hole circle (at 1.27 -10.16) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 17 /Vin))
    (pad 4 thru_hole circle (at 1.27 -7.62) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 2 /GND))
    (pad 5 thru_hole circle (at 1.27 -5.08) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 7 /+5V))
  )
  (module w_conn_mpt:mpt_0,5%2f4-2,54 (layer F.Cu) (tedit 5949803E)
    (at 4.095 38.467 270)
    (descr "4-way 2.54mm pitch terminal block, Phoenix MPT series")
    (fp_text reference P6 (at -6.844 -2.2804 540) (layer F.SilkS))
    (fp_text value CONN_01X04 (at 0 4.50088 270) (layer F.SilkS))
    (pad 4 thru_hole oval (at -3.81 0 270) (size 1.99898 1.99898) (drill 1.09728) (layers *.Cu *.Mask F.SilkS)
      (net 12 /GND_EXT))
    (pad 1 thru_hole rect (at 3.81 0 270) (size 1.99898 1.99898) (drill 1.09728) (layers *.Cu *.Mask F.SilkS)
      (net 13 /Vin_EXT))
    (pad 2 thru_hole oval (at 1.27 0 270) (size 1.99898 1.99898) (drill 1.09728) (layers *.Cu *.Mask F.SilkS)
      (net 13 /Vin_EXT))
    (pad 3 thru_hole oval (at -1.27 0 270) (size 1.99898 1.99898) (drill 1.09728) (layers *.Cu *.Mask F.SilkS)
      (net 12 /GND_EXT))
    (model walter/conn_mpt/mpt_0,5-4-2,54.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module kicad-libraries-master:SOT363 (layer B.Cu) (tedit 59488BA4)
    (at 11.811 25.908)
    (attr smd)
    (fp_text reference Q2 (at 0 -2.159 180) (layer B.SilkS))
    (fp_text value BSS138DW (at 0.025 -0.125 90) (layer B.SilkS))
    (pad 1 smd rect (at -0.9 0.75) (size 0.6 0.6) (layers B.Cu B.Paste B.Mask)
      (net 41 /ODROID_RX))
    (pad 3 smd rect (at -0.9 -0.75) (size 0.6 0.6) (layers B.Cu B.Paste B.Mask)
      (net 42 /ODROID_TX_3V3))
    (pad 4 smd rect (at 0.9 -0.75) (size 0.6 0.6) (layers B.Cu B.Paste B.Mask)
      (net 40 /ODROID_TX))
    (pad 6 smd rect (at 0.9 0.75) (size 0.6 0.6) (layers B.Cu B.Paste B.Mask)
      (net 43 /ODROID_RX_3V3))
    (pad 2 smd rect (at -0.9 0) (size 0.6 0.4) (layers B.Cu B.Paste B.Mask)
      (net 39 /ODROID_1.8V))
    (pad 5 smd rect (at 0.9 0) (size 0.6 0.4) (layers B.Cu B.Paste B.Mask)
      (net 39 /ODROID_1.8V))
  )
  (module w_conn_mpt:mpt_0,5%2f6-2,54 (layer F.Cu) (tedit 593634DD)
    (at 39.751 51.181)
    (descr "6-way 2.54mm pitch terminal block, Phoenix MPT series")
    (fp_text reference P7 (at -6.858 -4.191) (layer F.SilkS))
    (fp_text value CONN_01X06 (at 0 4.50088) (layer F.SilkS))
    (pad 4 thru_hole oval (at -1.27 0) (size 1.99898 1.99898) (drill 1.09728) (layers *.Cu *.Mask F.SilkS)
      (net 35 "Net-(P7-Pad4)"))
    (pad 1 thru_hole rect (at 6.35 0) (size 1.99898 1.99898) (drill 1.09728) (layers *.Cu *.Mask F.SilkS)
      (net 36 "Net-(P7-Pad1)"))
    (pad 2 thru_hole oval (at 3.81 0) (size 1.99898 1.99898) (drill 1.09728) (layers *.Cu *.Mask F.SilkS)
      (net 37 "Net-(P7-Pad2)"))
    (pad 3 thru_hole oval (at 1.27 0) (size 1.99898 1.99898) (drill 1.09728) (layers *.Cu *.Mask F.SilkS)
      (net 38 "Net-(P7-Pad3)"))
    (pad 5 thru_hole oval (at -3.81 0) (size 1.99898 1.99898) (drill 1.09728) (layers *.Cu *.Mask F.SilkS)
      (net 53 "Net-(P7-Pad5)"))
    (pad 6 thru_hole oval (at -6.35 0) (size 1.99898 1.99898) (drill 1.09728) (layers *.Cu *.Mask F.SilkS)
      (net 2 /GND))
    (model walter/conn_mpt/mpt_0,5-6-2,54.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module PowerControlBoard:SmallHoleRAZIMU (layer F.Cu) (tedit 58DA9F88)
    (at 51.054 52.324)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference "" (at 0 -3.048) (layer F.SilkS))
    (fp_text value "" (at 0 2.794) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 2.794 2.794) (drill 2.032) (layers *.Cu *.Mask F.SilkS))
  )
  (module PowerControlBoard:SmallHoleRAZIMU (layer F.Cu) (tedit 58DA9F88)
    (at 51.054 2.286)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference "" (at 0 -3.048) (layer F.SilkS))
    (fp_text value "" (at 0 2.794) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 2.794 2.794) (drill 2.032) (layers *.Cu *.Mask F.SilkS))
  )
  (module PowerControlBoard:SmallHoleRAZIMU (layer F.Cu) (tedit 58DA9F88)
    (at 2.54 52.324)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference "" (at 0 -3.048) (layer F.SilkS))
    (fp_text value "" (at 0 2.794) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 2.794 2.794) (drill 2.032) (layers *.Cu *.Mask F.SilkS))
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 594876E6)
    (at 17.399 23.241 270)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C5 (at 2.413 0 270) (layer F.SilkS))
    (fp_text value "100 nF" (at 0 1.5 270) (layer F.Fab))
    (fp_text user %R (at 2.413 0 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 /3V3))
    (pad 2 smd rect (at 0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 /GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer B.Cu) (tedit 59498117)
    (at 20.435 43.307 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C8 (at -2.6536 0 180) (layer B.SilkS))
    (fp_text value "100 nF" (at 0 -1.5 180) (layer B.Fab))
    (fp_text user %R (at 0 1.5 180) (layer B.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers B.Cu B.Paste B.Mask)
      (net 2 /GND))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers B.Cu B.Paste B.Mask)
      (net 9 "Net-(C8-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59487716)
    (at 19.05 23.241 270)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C9 (at 2.413 0 270) (layer F.SilkS))
    (fp_text value "100 nF" (at 0 1.5 270) (layer F.Fab))
    (fp_text user %R (at 2.413 0 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 /3V3))
    (pad 2 smd rect (at 0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 /GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59363B10)
    (at 21.082 38.227 270)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C15 (at 3.048 -0.127 270) (layer F.SilkS))
    (fp_text value "100 nF" (at 0 1.5 270) (layer F.Fab))
    (fp_text user %R (at 3.048 -0.127 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 17 /Vin))
    (pad 2 smd rect (at 0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 /GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_Tantalum_SMD:CP_Tantalum_Case-V_EIA-7343-20_Reflow (layer B.Cu) (tedit 59498110)
    (at 21.2852 37.7698 270)
    (descr "Tantalum capacitor, Case V, EIA 7343-20, 7.3x4.3x2.0mm, Reflow soldering footprint")
    (tags "capacitor tantalum smd")
    (attr smd)
    (fp_text reference C16 (at -5.6134 -0.1524 360) (layer B.SilkS))
    (fp_text value 33uF (at 0 -3.9 270) (layer B.Fab))
    (pad 1 smd rect (at -3.175 0 270) (size 2.55 2.7) (layers B.Cu B.Paste B.Mask)
      (net 17 /Vin))
    (pad 2 smd rect (at 3.175 0 270) (size 2.55 2.7) (layers B.Cu B.Paste B.Mask)
      (net 2 /GND))
    (model Capacitors_Tantalum_SMD.3dshapes/CP_Tantalum_Case-V_EIA-7343-20.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_Tantalum_SMD:CP_Tantalum_Case-V_EIA-7343-20_Reflow (layer B.Cu) (tedit 59487754)
    (at 30.2768 37.9222 270)
    (descr "Tantalum capacitor, Case V, EIA 7343-20, 7.3x4.3x2.0mm, Reflow soldering footprint")
    (tags "capacitor tantalum smd")
    (attr smd)
    (fp_text reference C17 (at 5.842 -0.254 360) (layer B.SilkS))
    (fp_text value 33uF (at 0 -3.9 270) (layer B.Fab))
    (pad 1 smd rect (at -3.175 0 270) (size 2.55 2.7) (layers B.Cu B.Paste B.Mask)
      (net 47 "Net-(C17-Pad1)"))
    (pad 2 smd rect (at 3.175 0 270) (size 2.55 2.7) (layers B.Cu B.Paste B.Mask)
      (net 2 /GND))
    (model Capacitors_Tantalum_SMD.3dshapes/CP_Tantalum_Case-V_EIA-7343-20.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer B.Cu) (tedit 5936365F)
    (at 6.985 50.546 90)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C18 (at -0.127 -1.778 90) (layer B.SilkS))
    (fp_text value "1 uF" (at 0 -1.75 90) (layer B.Fab))
    (fp_text user %R (at -0.127 -1.778 90) (layer B.Fab))
    (pad 1 smd rect (at -1 0 90) (size 1 1.25) (layers B.Cu B.Paste B.Mask)
      (net 48 /InRushLimit/V_IR_IN))
    (pad 2 smd rect (at 1 0 90) (size 1 1.25) (layers B.Cu B.Paste B.Mask)
      (net 2 /GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer B.Cu) (tedit 59363743)
    (at 8.89 50.546 90)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C19 (at -2.413 0.254 360) (layer B.SilkS))
    (fp_text value "1 uF" (at 0 -1.75 90) (layer B.Fab))
    (fp_text user %R (at -2.413 0.254 360) (layer B.Fab))
    (pad 1 smd rect (at -1 0 90) (size 1 1.25) (layers B.Cu B.Paste B.Mask)
      (net 48 /InRushLimit/V_IR_IN))
    (pad 2 smd rect (at 1 0 90) (size 1 1.25) (layers B.Cu B.Paste B.Mask)
      (net 49 "Net-(C19-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer B.Cu) (tedit 58AA8463)
    (at 15.748 50.546 90)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C20 (at 0 1.5 90) (layer B.SilkS))
    (fp_text value "1 uF" (at 0 -1.75 90) (layer B.Fab))
    (fp_text user %R (at 0 1.5 90) (layer B.Fab))
    (pad 1 smd rect (at -1 0 90) (size 1 1.25) (layers B.Cu B.Paste B.Mask)
      (net 50 /InRushLimit/V_IR_OUT))
    (pad 2 smd rect (at 1 0 90) (size 1 1.25) (layers B.Cu B.Paste B.Mask)
      (net 51 "Net-(C20-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_0603 (layer F.Cu) (tedit 59363A88)
    (at 31.115 39.751)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D5 (at 0 1.524) (layer F.SilkS))
    (fp_text value "1.95V 5mA" (at 0 1.35) (layer F.Fab))
    (pad 2 smd rect (at 0.8 0 180) (size 0.8 0.8) (layers F.Cu F.Paste F.Mask)
      (net 52 "Net-(D5-Pad2)"))
    (pad 1 smd rect (at -0.8 0 180) (size 0.8 0.8) (layers F.Cu F.Paste F.Mask)
      (net 2 /GND))
    (model LEDs.3dshapes/LED_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module SPIC_modules:SiS443DN (layer F.Cu) (tedit 594980B1)
    (at 23.368 34.798 180)
    (fp_text reference Q3 (at 3.1242 0.9144 180) (layer F.SilkS))
    (fp_text value SiS443DN (at -0.03 2.61 180) (layer F.Fab))
    (pad 5 smd rect (at 1.52 0.9975 180) (size 0.76 0.405) (layers F.Cu F.Paste F.Mask)
      (net 17 /Vin))
    (pad 6 smd rect (at 1.52 0.3375 180) (size 0.76 0.405) (layers F.Cu F.Paste F.Mask)
      (net 17 /Vin))
    (pad 7 smd rect (at 1.52 -0.3225 180) (size 0.76 0.405) (layers F.Cu F.Paste F.Mask)
      (net 17 /Vin))
    (pad 8 smd rect (at 1.53 -0.9825 180) (size 0.76 0.405) (layers F.Cu F.Paste F.Mask)
      (net 17 /Vin))
    (pad 1 smd rect (at -1.457 -0.9825 180) (size 0.99 0.405) (layers F.Cu F.Paste F.Mask)
      (net 54 "Net-(Q3-Pad1)"))
    (pad 2 smd rect (at -1.457 -0.3225 180) (size 0.99 0.405) (layers F.Cu F.Paste F.Mask)
      (net 54 "Net-(Q3-Pad1)"))
    (pad 3 smd rect (at -1.457 0.3375 180) (size 0.99 0.405) (layers F.Cu F.Paste F.Mask)
      (net 54 "Net-(Q3-Pad1)"))
    (pad 4 smd rect (at -1.457 0.9975 180) (size 0.99 0.405) (layers F.Cu F.Paste F.Mask)
      (net 55 "Net-(Q3-Pad4)"))
    (pad 8 smd rect (at 0.54 -0.01 180) (size 1.725 2.235) (layers F.Cu F.Paste F.Mask)
      (net 17 /Vin))
  )
  (module SPIC_modules:SiS443DN (layer F.Cu) (tedit 59363B41)
    (at 28.321 35.433)
    (fp_text reference Q4 (at 3.302 -0.762) (layer F.SilkS))
    (fp_text value SiS443DN (at -0.03 2.61) (layer F.Fab))
    (pad 5 smd rect (at 1.52 0.9975) (size 0.76 0.405) (layers F.Cu F.Paste F.Mask)
      (net 47 "Net-(C17-Pad1)"))
    (pad 6 smd rect (at 1.52 0.3375) (size 0.76 0.405) (layers F.Cu F.Paste F.Mask)
      (net 47 "Net-(C17-Pad1)"))
    (pad 7 smd rect (at 1.52 -0.3225) (size 0.76 0.405) (layers F.Cu F.Paste F.Mask)
      (net 47 "Net-(C17-Pad1)"))
    (pad 8 smd rect (at 1.53 -0.9825) (size 0.76 0.405) (layers F.Cu F.Paste F.Mask)
      (net 47 "Net-(C17-Pad1)"))
    (pad 1 smd rect (at -1.457 -0.9825) (size 0.99 0.405) (layers F.Cu F.Paste F.Mask)
      (net 54 "Net-(Q3-Pad1)"))
    (pad 2 smd rect (at -1.457 -0.3225) (size 0.99 0.405) (layers F.Cu F.Paste F.Mask)
      (net 54 "Net-(Q3-Pad1)"))
    (pad 3 smd rect (at -1.457 0.3375) (size 0.99 0.405) (layers F.Cu F.Paste F.Mask)
      (net 54 "Net-(Q3-Pad1)"))
    (pad 4 smd rect (at -1.457 0.9975) (size 0.99 0.405) (layers F.Cu F.Paste F.Mask)
      (net 55 "Net-(Q3-Pad4)"))
    (pad 8 smd rect (at 0.54 -0.01) (size 1.725 2.235) (layers F.Cu F.Paste F.Mask)
      (net 47 "Net-(C17-Pad1)"))
  )
  (module SPIC_modules:SiS443DN (layer B.Cu) (tedit 58E0747D)
    (at 12.319 51.435)
    (fp_text reference Q5 (at 0 2.5) (layer B.SilkS))
    (fp_text value SiS443DN (at -0.03 -2.61) (layer B.Fab))
    (pad 5 smd rect (at 1.52 -0.9975) (size 0.76 0.405) (layers B.Cu B.Paste B.Mask)
      (net 50 /InRushLimit/V_IR_OUT))
    (pad 6 smd rect (at 1.52 -0.3375) (size 0.76 0.405) (layers B.Cu B.Paste B.Mask)
      (net 50 /InRushLimit/V_IR_OUT))
    (pad 7 smd rect (at 1.52 0.3225) (size 0.76 0.405) (layers B.Cu B.Paste B.Mask)
      (net 50 /InRushLimit/V_IR_OUT))
    (pad 8 smd rect (at 1.53 0.9825) (size 0.76 0.405) (layers B.Cu B.Paste B.Mask)
      (net 50 /InRushLimit/V_IR_OUT))
    (pad 1 smd rect (at -1.457 0.9825) (size 0.99 0.405) (layers B.Cu B.Paste B.Mask)
      (net 48 /InRushLimit/V_IR_IN))
    (pad 2 smd rect (at -1.457 0.3225) (size 0.99 0.405) (layers B.Cu B.Paste B.Mask)
      (net 48 /InRushLimit/V_IR_IN))
    (pad 3 smd rect (at -1.457 -0.3375) (size 0.99 0.405) (layers B.Cu B.Paste B.Mask)
      (net 48 /InRushLimit/V_IR_IN))
    (pad 4 smd rect (at -1.457 -0.9975) (size 0.99 0.405) (layers B.Cu B.Paste B.Mask)
      (net 56 "Net-(Q5-Pad4)"))
    (pad 8 smd rect (at 0.54 0.01) (size 1.725 2.235) (layers B.Cu B.Paste B.Mask)
      (net 50 /InRushLimit/V_IR_OUT))
  )
  (module Resistors_SMD:R_2010 (layer F.Cu) (tedit 58AADAEF)
    (at 14.351 50.419 270)
    (descr "Resistor SMD 2010, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 2010")
    (attr smd)
    (fp_text reference R12 (at 0 -2.25 270) (layer F.SilkS))
    (fp_text value 0.02 (at 0 2.4 270) (layer F.Fab))
    (fp_text user %R (at 0 -2.25 270) (layer F.Fab))
    (pad 1 smd rect (at -2.45 0 270) (size 1 2.5) (layers F.Cu F.Paste F.Mask)
      (net 17 /Vin))
    (pad 2 smd rect (at 2.45 0 270) (size 1 2.5) (layers F.Cu F.Paste F.Mask)
      (net 50 /InRushLimit/V_IR_OUT))
    (model Resistors_SMD.3dshapes/R_2010.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58AAD9CA)
    (at 25.654 42.545 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R16 (at 0 -1.45 180) (layer F.SilkS))
    (fp_text value 50K (at 0 1.5 180) (layer F.Fab))
    (fp_text user %R (at 0 -1.45 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 17 /Vin))
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 20 /ATX_ON))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5949800A)
    (at 30.861 38.227)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R17 (at 1.3462 -1.4732) (layer F.SilkS))
    (fp_text value 50K (at 0 1.5) (layer F.Fab))
    (fp_text user %R (at 0 -1.45) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 47 "Net-(C17-Pad1)"))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 52 "Net-(D5-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer B.Cu) (tedit 59363718)
    (at 9.271 47.371 180)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R18 (at -0.127 1.651 180) (layer B.SilkS))
    (fp_text value 100 (at 0 -1.75 180) (layer B.Fab))
    (fp_text user %R (at -0.127 1.651 180) (layer B.Fab))
    (pad 1 smd rect (at -0.95 0 180) (size 0.7 1.3) (layers B.Cu B.Paste B.Mask)
      (net 56 "Net-(Q5-Pad4)"))
    (pad 2 smd rect (at 0.95 0 180) (size 0.7 1.3) (layers B.Cu B.Paste B.Mask)
      (net 49 "Net-(C19-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer B.Cu) (tedit 59363737)
    (at 12.065 46.736 90)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R19 (at -2.286 0 360) (layer B.SilkS))
    (fp_text value 500k (at 0 -1.75 90) (layer B.Fab))
    (fp_text user %R (at -2.286 0 360) (layer B.Fab))
    (pad 1 smd rect (at -0.95 0 90) (size 0.7 1.3) (layers B.Cu B.Paste B.Mask)
      (net 56 "Net-(Q5-Pad4)"))
    (pad 2 smd rect (at 0.95 0 90) (size 0.7 1.3) (layers B.Cu B.Paste B.Mask)
      (net 2 /GND))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer B.Cu) (tedit 59363702)
    (at 14.859 47.371 180)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R20 (at 0.254 1.778 180) (layer B.SilkS))
    (fp_text value 100 (at 0 -1.75 180) (layer B.Fab))
    (fp_text user %R (at 0.254 1.651 180) (layer B.Fab))
    (pad 1 smd rect (at -0.95 0 180) (size 0.7 1.3) (layers B.Cu B.Paste B.Mask)
      (net 51 "Net-(C20-Pad2)"))
    (pad 2 smd rect (at 0.95 0 180) (size 0.7 1.3) (layers B.Cu B.Paste B.Mask)
      (net 56 "Net-(Q5-Pad4)"))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_SSOP:TSSOP-16_4.4x5mm_Pitch0.65mm (layer F.Cu) (tedit 59487589)
    (at 12.065 25.908)
    (descr "16-Lead Plastic Thin Shrink Small Outline (ST)-4.4 mm Body [TSSOP] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SSOP 0.65")
    (attr smd)
    (fp_text reference U3 (at -3.429 -3.81) (layer F.SilkS))
    (fp_text value MAX3232E (at 0 3.55) (layer F.Fab))
    (pad 1 smd rect (at -2.95 -2.275) (size 1.5 0.45) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C3-Pad1)"))
    (pad 2 smd rect (at -2.95 -1.625) (size 1.5 0.45) (layers F.Cu F.Paste F.Mask)
      (net 45 "Net-(C12-Pad2)"))
    (pad 3 smd rect (at -2.95 -0.975) (size 1.5 0.45) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(C3-Pad2)"))
    (pad 4 smd rect (at -2.95 -0.325) (size 1.5 0.45) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(C4-Pad1)"))
    (pad 5 smd rect (at -2.95 0.325) (size 1.5 0.45) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(C4-Pad2)"))
    (pad 6 smd rect (at -2.95 0.975) (size 1.5 0.45) (layers F.Cu F.Paste F.Mask)
      (net 46 "Net-(C13-Pad2)"))
    (pad 7 smd rect (at -2.95 1.625) (size 1.5 0.45) (layers F.Cu F.Paste F.Mask)
      (net 60 "Net-(U3-Pad7)"))
    (pad 8 smd rect (at -2.95 2.275) (size 1.5 0.45) (layers F.Cu F.Paste F.Mask)
      (net 61 "Net-(U3-Pad8)"))
    (pad 9 smd rect (at 2.95 2.275) (size 1.5 0.45) (layers F.Cu F.Paste F.Mask)
      (net 62 "Net-(U3-Pad9)"))
    (pad 10 smd rect (at 2.95 1.625) (size 1.5 0.45) (layers F.Cu F.Paste F.Mask)
      (net 63 "Net-(U3-Pad10)"))
    (pad 11 smd rect (at 2.95 0.975) (size 1.5 0.45) (layers F.Cu F.Paste F.Mask)
      (net 33 /RAZ_TX))
    (pad 12 smd rect (at 2.95 0.325) (size 1.5 0.45) (layers F.Cu F.Paste F.Mask)
      (net 34 /RAZ_RX))
    (pad 13 smd rect (at 2.95 -0.325) (size 1.5 0.45) (layers F.Cu F.Paste F.Mask)
      (net 24 "Net-(P2-Pad2)"))
    (pad 14 smd rect (at 2.95 -0.975) (size 1.5 0.45) (layers F.Cu F.Paste F.Mask)
      (net 23 "Net-(P2-Pad3)"))
    (pad 15 smd rect (at 2.95 -1.625) (size 1.5 0.45) (layers F.Cu F.Paste F.Mask)
      (net 2 /GND))
    (pad 16 smd rect (at 2.95 -2.275) (size 1.5 0.45) (layers F.Cu F.Paste F.Mask)
      (net 1 /3V3))
    (model Housings_SSOP.3dshapes/TSSOP-16_4.4x5mm_Pitch0.65mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_SSOP:MSOP-12_3x4mm_Pitch0.65mm (layer B.Cu) (tedit 59498134)
    (at 20.193 46.736 270)
    (descr "MS Package; 12-Lead Plastic MSOP; (see Linear Technology 05081668_A_MS12.pdf)")
    (tags "SSOP 0.65")
    (attr smd)
    (fp_text reference U4 (at -0.1016 -3.2512 270) (layer B.SilkS))
    (fp_text value LTC2945 (at 0 -3.05 270) (layer B.Fab))
    (pad 1 smd rect (at -2.105 1.625 270) (size 0.89 0.42) (layers B.Cu B.Paste B.Mask)
      (net 50 /InRushLimit/V_IR_OUT))
    (pad 2 smd rect (at -2.105 0.975 270) (size 0.89 0.42) (layers B.Cu B.Paste B.Mask)
      (net 9 "Net-(C8-Pad2)"))
    (pad 3 smd rect (at -2.105 0.325 270) (size 0.89 0.42) (layers B.Cu B.Paste B.Mask)
      (net 2 /GND))
    (pad 4 smd rect (at -2.105 -0.325 270) (size 0.89 0.42) (layers B.Cu B.Paste B.Mask)
      (net 9 "Net-(C8-Pad2)"))
    (pad 5 smd rect (at -2.105 -0.975 270) (size 0.89 0.42) (layers B.Cu B.Paste B.Mask)
      (net 2 /GND))
    (pad 6 smd rect (at -2.105 -1.625 270) (size 0.89 0.42) (layers B.Cu B.Paste B.Mask)
      (net 2 /GND))
    (pad 7 smd rect (at 2.105 -1.625 270) (size 0.89 0.42) (layers B.Cu B.Paste B.Mask)
      (net 26 /SCL))
    (pad 8 smd rect (at 2.105 -0.975 270) (size 0.89 0.42) (layers B.Cu B.Paste B.Mask)
      (net 25 /SDA))
    (pad 9 smd rect (at 2.105 -0.325 270) (size 0.89 0.42) (layers B.Cu B.Paste B.Mask)
      (net 25 /SDA))
    (pad 10 smd rect (at 2.105 0.325 270) (size 0.89 0.42) (layers B.Cu B.Paste B.Mask)
      (net 32 "Net-(U4-Pad10)"))
    (pad 11 smd rect (at 2.105 0.975 270) (size 0.89 0.42) (layers B.Cu B.Paste B.Mask)
      (net 17 /Vin))
    (pad 12 smd rect (at 2.105 1.625 270) (size 0.89 0.42) (layers B.Cu B.Paste B.Mask)
      (net 50 /InRushLimit/V_IR_OUT))
    (model Housings_SSOP.3dshapes/MSOP-12_3x4mm_Pitch0.65mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_SSOP:MSOP-10_3x3mm_Pitch0.5mm (layer F.Cu) (tedit 54130A77)
    (at 13.462 18.542)
    (descr "10-Lead Plastic Micro Small Outline Package (MS) [MSOP] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SSOP 0.5")
    (attr smd)
    (fp_text reference U6 (at 0 -2.6) (layer F.SilkS))
    (fp_text value LTC4316 (at 0 2.6) (layer F.Fab))
    (pad 1 smd rect (at -2.2 -1) (size 1.4 0.3) (layers F.Cu F.Paste F.Mask)
      (net 2 /GND))
    (pad 2 smd rect (at -2.2 -0.5) (size 1.4 0.3) (layers F.Cu F.Paste F.Mask)
      (net 2 /GND))
    (pad 3 smd rect (at -2.2 0) (size 1.4 0.3) (layers F.Cu F.Paste F.Mask)
      (net 1 /3V3))
    (pad 4 smd rect (at -2.2 0.5) (size 1.4 0.3) (layers F.Cu F.Paste F.Mask)
      (net 1 /3V3))
    (pad 5 smd rect (at -2.2 1) (size 1.4 0.3) (layers F.Cu F.Paste F.Mask)
      (net 1 /3V3))
    (pad 6 smd rect (at 2.2 1) (size 1.4 0.3) (layers F.Cu F.Paste F.Mask)
      (net 64 "Net-(U6-Pad6)"))
    (pad 7 smd rect (at 2.2 0.5) (size 1.4 0.3) (layers F.Cu F.Paste F.Mask)
      (net 25 /SDA))
    (pad 8 smd rect (at 2.2 0) (size 1.4 0.3) (layers F.Cu F.Paste F.Mask)
      (net 58 "Net-(R14-Pad2)"))
    (pad 9 smd rect (at 2.2 -0.5) (size 1.4 0.3) (layers F.Cu F.Paste F.Mask)
      (net 57 "Net-(R13-Pad2)"))
    (pad 10 smd rect (at 2.2 -1) (size 1.4 0.3) (layers F.Cu F.Paste F.Mask)
      (net 26 /SCL))
    (model Housings_SSOP.3dshapes/MSOP-10_3x3mm_Pitch0.5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_SOIC:SOIC-20W_7.5x12.8mm_Pitch1.27mm (layer B.Cu) (tedit 59498127)
    (at 15.113 8.001 180)
    (descr "20-Lead Plastic Small Outline (SO) - Wide, 7.50 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (attr smd)
    (fp_text reference U7 (at 0 -7.7216 180) (layer B.SilkS))
    (fp_text value DS3232 (at 0 -7.5 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 1 smd rect (at -4.7 5.715 180) (size 1.95 0.6) (layers B.Cu B.Paste B.Mask)
      (net 2 /GND))
    (pad 2 smd rect (at -4.7 4.445 180) (size 1.95 0.6) (layers B.Cu B.Paste B.Mask)
      (net 2 /GND))
    (pad 3 smd rect (at -4.7 3.175 180) (size 1.95 0.6) (layers B.Cu B.Paste B.Mask)
      (net 30 /RTC32k))
    (pad 4 smd rect (at -4.7 1.905 180) (size 1.95 0.6) (layers B.Cu B.Paste B.Mask)
      (net 1 /3V3))
    (pad 5 smd rect (at -4.7 0.635 180) (size 1.95 0.6) (layers B.Cu B.Paste B.Mask)
      (net 31 /RTCINT))
    (pad 6 smd rect (at -4.7 -0.635 180) (size 1.95 0.6) (layers B.Cu B.Paste B.Mask)
      (net 59 /RTC_RST))
    (pad 7 smd rect (at -4.7 -1.905 180) (size 1.95 0.6) (layers B.Cu B.Paste B.Mask)
      (net 2 /GND))
    (pad 8 smd rect (at -4.7 -3.175 180) (size 1.95 0.6) (layers B.Cu B.Paste B.Mask)
      (net 2 /GND))
    (pad 9 smd rect (at -4.7 -4.445 180) (size 1.95 0.6) (layers B.Cu B.Paste B.Mask)
      (net 2 /GND))
    (pad 10 smd rect (at -4.7 -5.715 180) (size 1.95 0.6) (layers B.Cu B.Paste B.Mask)
      (net 2 /GND))
    (pad 11 smd rect (at 4.7 -5.715 180) (size 1.95 0.6) (layers B.Cu B.Paste B.Mask)
      (net 2 /GND))
    (pad 12 smd rect (at 4.7 -4.445 180) (size 1.95 0.6) (layers B.Cu B.Paste B.Mask)
      (net 2 /GND))
    (pad 13 smd rect (at 4.7 -3.175 180) (size 1.95 0.6) (layers B.Cu B.Paste B.Mask)
      (net 2 /GND))
    (pad 14 smd rect (at 4.7 -1.905 180) (size 1.95 0.6) (layers B.Cu B.Paste B.Mask)
      (net 2 /GND))
    (pad 15 smd rect (at 4.7 -0.635 180) (size 1.95 0.6) (layers B.Cu B.Paste B.Mask)
      (net 2 /GND))
    (pad 16 smd rect (at 4.7 0.635 180) (size 1.95 0.6) (layers B.Cu B.Paste B.Mask)
      (net 8 /VBat))
    (pad 17 smd rect (at 4.7 1.905 180) (size 1.95 0.6) (layers B.Cu B.Paste B.Mask)
      (net 58 "Net-(R14-Pad2)"))
    (pad 18 smd rect (at 4.7 3.175 180) (size 1.95 0.6) (layers B.Cu B.Paste B.Mask)
      (net 57 "Net-(R13-Pad2)"))
    (pad 19 smd rect (at 4.7 4.445 180) (size 1.95 0.6) (layers B.Cu B.Paste B.Mask)
      (net 2 /GND))
    (pad 20 smd rect (at 4.7 5.715 180) (size 1.95 0.6) (layers B.Cu B.Paste B.Mask)
      (net 57 "Net-(R13-Pad2)"))
    (model Housings_SOIC.3dshapes/SOIC-20_7.5x12.8mm_Pitch1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SPIC_modules:M3-ATX-HV (layer F.Cu) (tedit 594889F5)
    (at 33.401 21.844)
    (fp_text reference U8 (at 4.826 -0.635) (layer F.SilkS))
    (fp_text value ATX-M3-HV (at -6 -13.5) (layer F.Fab))
    (fp_text user 3V3 (at 4.953 20.193) (layer F.SilkS))
    (fp_text user -12V (at 6.858 17.018) (layer F.SilkS))
    (fp_text user GND (at 7.747 12.827) (layer F.SilkS))
    (fp_text user PS_ON (at 7.239 8.636) (layer F.SilkS))
    (fp_text user GND (at 7.62 4.318) (layer F.SilkS))
    (fp_text user GND (at 7.747 0.254) (layer F.SilkS))
    (fp_text user GND (at 7.62 -3.937) (layer F.SilkS))
    (fp_text user -5V (at 7.747 -8.255) (layer F.SilkS))
    (fp_text user 5V (at 7.747 -12.319) (layer F.SilkS))
    (fp_text user 5V (at 7.747 -16.51) (layer F.SilkS))
    (fp_text user 12V (at 2.032 -16.51) (layer F.SilkS))
    (fp_text user 5V_SB (at 2.54 -12.446) (layer F.SilkS))
    (fp_text user PWR_OK (at 3.302 -8.255) (layer F.SilkS))
    (fp_text user GND (at 2.286 -4.064) (layer F.SilkS))
    (fp_text user 5V (at 2.032 0.127) (layer F.SilkS))
    (fp_text user GND (at 2.413 4.318) (layer F.SilkS))
    (fp_text user 5V (at 2.286 8.636) (layer F.SilkS))
    (fp_text user GND (at 2.286 12.827) (layer F.SilkS))
    (fp_text user 3V3 (at 4.318 15.113 90) (layer F.SilkS))
    (fp_text user 3V3 (at 2.159 17.018) (layer F.SilkS))
    (pad 1 thru_hole circle (at 2.2 19.1 270) (size 2.25 2.25) (drill 1.4) (layers *.Cu *.Mask)
      (net 65 "Net-(U8-Pad1)"))
    (pad 2 thru_hole circle (at 2.2 14.9 270) (size 2.25 2.25) (drill 1.4) (layers *.Cu *.Mask)
      (net 66 "Net-(U8-Pad2)"))
    (pad 3 thru_hole circle (at 2.2 10.7 270) (size 2.25 2.25) (drill 1.4) (layers *.Cu *.Mask)
      (net 67 "Net-(U8-Pad3)"))
    (pad 4 thru_hole circle (at 2.2 6.5 270) (size 2.25 2.25) (drill 1.4) (layers *.Cu *.Mask)
      (net 68 "Net-(U8-Pad4)"))
    (pad 5 thru_hole circle (at 2.2 2.3 270) (size 2.25 2.25) (drill 1.4) (layers *.Cu *.Mask)
      (net 69 "Net-(U8-Pad5)"))
    (pad 6 thru_hole circle (at 2.2 -1.9 270) (size 2.25 2.25) (drill 1.4) (layers *.Cu *.Mask)
      (net 77 "Net-(U8-Pad6)"))
    (pad 7 thru_hole circle (at 2.2 -6.1 270) (size 2.25 2.25) (drill 1.4) (layers *.Cu *.Mask)
      (net 70 "Net-(U8-Pad7)"))
    (pad 8 thru_hole circle (at 2.2 -10.3 270) (size 2.25 2.25) (drill 1.4) (layers *.Cu *.Mask)
      (net 27 "Net-(R5-Pad1)"))
    (pad 9 thru_hole circle (at 2.2 -14.5 270) (size 2.25 2.25) (drill 1.4) (layers *.Cu *.Mask)
      (net 28 "/Power Output/ATX_5V_SB"))
    (pad 10 thru_hole circle (at 2.2 -18.7 270) (size 2.25 2.25) (drill 1.4) (layers *.Cu *.Mask)
      (net 21 "/Power Output/ATX_12V"))
    (pad 11 thru_hole circle (at 7.7 19.1 270) (size 2.25 2.25) (drill 1.4) (layers *.Cu *.Mask)
      (net 71 "Net-(U8-Pad11)"))
    (pad 12 thru_hole circle (at 7.7 14.9 270) (size 2.25 2.25) (drill 1.4) (layers *.Cu *.Mask)
      (net 72 "Net-(U8-Pad12)"))
    (pad 13 thru_hole circle (at 7.7 10.7 270) (size 2.25 2.25) (drill 1.4) (layers *.Cu *.Mask)
      (net 2 /GND))
    (pad 14 thru_hole circle (at 7.7 6.5 270) (size 2.25 2.25) (drill 1.4) (layers *.Cu *.Mask)
      (net 19 "Net-(JP1-Pad2)"))
    (pad 15 thru_hole circle (at 7.7 2.3 270) (size 2.25 2.25) (drill 1.4) (layers *.Cu *.Mask)
      (net 2 /GND))
    (pad 16 thru_hole circle (at 7.7 -1.9 270) (size 2.25 2.25) (drill 1.4) (layers *.Cu *.Mask)
      (net 2 /GND))
    (pad 17 thru_hole circle (at 7.7 -6.1 270) (size 2.25 2.25) (drill 1.4) (layers *.Cu *.Mask)
      (net 2 /GND))
    (pad 18 thru_hole circle (at 7.7 -10.3 270) (size 2.25 2.25) (drill 1.4) (layers *.Cu *.Mask)
      (net 73 "Net-(U8-Pad18)"))
    (pad 19 thru_hole circle (at 7.7 -14.5 270) (size 2.25 2.25) (drill 1.4) (layers *.Cu *.Mask)
      (net 22 "/Power Output/ATX_5V"))
    (pad 20 thru_hole circle (at 7.7 -18.7 270) (size 2.25 2.25) (drill 1.4) (layers *.Cu *.Mask)
      (net 22 "/Power Output/ATX_5V"))
  )
  (module Housings_SSOP:MSOP-8_3x3mm_Pitch0.65mm (layer F.Cu) (tedit 59363A0C)
    (at 25.781 39.37)
    (descr "8-Lead Plastic Micro Small Outline Package (MS) [MSOP] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SSOP 0.65")
    (attr smd)
    (fp_text reference U9 (at 2.286 2.667) (layer F.SilkS))
    (fp_text value LTC4414 (at 0 2.6) (layer F.Fab))
    (pad 1 smd rect (at -2.2 -0.975) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 74 "Net-(U9-Pad1)"))
    (pad 2 smd rect (at -2.2 -0.325) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 20 /ATX_ON))
    (pad 3 smd rect (at -2.2 0.325) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 2 /GND))
    (pad 4 smd rect (at -2.2 0.975) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 75 "Net-(U9-Pad4)"))
    (pad 5 smd rect (at 2.2 0.975) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 76 "Net-(U9-Pad5)"))
    (pad 6 smd rect (at 2.2 0.325) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 2 /GND))
    (pad 7 smd rect (at 2.2 -0.325) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 17 /Vin))
    (pad 8 smd rect (at 2.2 -0.975) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 55 "Net-(Q3-Pad4)"))
    (model Housings_SSOP.3dshapes/MSOP-8_3x3mm_Pitch0.65mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59488AC5)
    (at 23.876 24.511)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C1 (at -0.127 -1.397) (layer F.SilkS))
    (fp_text value "100 nF" (at 0 1.5) (layer F.Fab))
    (fp_text user %R (at -0.127 -1.397) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 /3V3))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 /GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 594876EF)
    (at 20.995 26.817 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C2 (at -2.52 0.087 90) (layer F.SilkS))
    (fp_text value "100 nF" (at 0 1.5 90) (layer F.Fab))
    (fp_text user %R (at -2.52 0.087 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 /3V3))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 /GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer B.Cu) (tedit 594870E2)
    (at 23.368 3.556 270)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C6 (at 0 -1.524 270) (layer B.SilkS))
    (fp_text value "0.47 uF" (at 0 -1.5 270) (layer B.Fab))
    (fp_text user %R (at 0 -1.524 270) (layer B.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.8 0.75) (layers B.Cu B.Paste B.Mask)
      (net 2 /GND))
    (pad 2 smd rect (at 0.75 0 270) (size 0.8 0.75) (layers B.Cu B.Paste B.Mask)
      (net 1 /3V3))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer B.Cu) (tedit 5949812A)
    (at 6.858 3.556 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C7 (at -2.54 0.0508 90) (layer B.SilkS))
    (fp_text value "0.47 uF" (at 0 -1.5 90) (layer B.Fab))
    (fp_text user %R (at 0 -1.651 90) (layer B.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers B.Cu B.Paste B.Mask)
      (net 8 /VBat))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers B.Cu B.Paste B.Mask)
      (net 2 /GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 594876CD)
    (at 8.509 18.288 270)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C14 (at -0.127 1.397 270) (layer F.SilkS))
    (fp_text value "0.47 uF" (at 0 1.5 270) (layer F.Fab))
    (fp_text user %R (at -0.127 1.397 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 /GND))
    (pad 2 smd rect (at 0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 /3V3))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diodes_SMD:D_SMC_Standard (layer F.Cu) (tedit 59498059)
    (at 10.845 37.517 90)
    (descr "Diode SMC Standard = DO-214AB")
    (tags "Diode SMC Standard DO-214AB")
    (attr smd)
    (fp_text reference D1 (at 5.767 2.4138 180) (layer F.SilkS))
    (fp_text value SMCJ40CA (at 0 5.08 90) (layer F.Fab))
    (pad 1 smd rect (at -3.4 0 180) (size 3.3 2.5) (layers F.Cu F.Paste F.Mask)
      (net 13 /Vin_EXT))
    (pad 2 smd rect (at 3.4 0 180) (size 3.3 2.5) (layers F.Cu F.Paste F.Mask)
      (net 12 /GND_EXT))
    (model Diodes_SMD.3dshapes/D_SMC_Standard.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diodes_SMD:D_SOD-523 (layer B.Cu) (tedit 586419F0)
    (at 8.763 42.926 270)
    (descr "http://www.diodes.com/datasheets/ap02001.pdf p.144")
    (tags "Diode SOD523")
    (attr smd)
    (fp_text reference D2 (at 0 1.5 270) (layer B.SilkS))
    (fp_text value BZT52C20T-7 (at 0 -1.7 270) (layer B.Fab))
    (pad 2 smd rect (at 0.7 0 90) (size 0.6 0.7) (layers B.Cu B.Paste B.Mask)
      (net 2 /GND))
    (pad 1 smd rect (at -0.7 0 90) (size 0.6 0.7) (layers B.Cu B.Paste B.Mask)
      (net 14 "Net-(D2-Pad1)"))
  )
  (module w_conn_mpt:mpt_0,5%2f4-2,54 (layer F.Cu) (tedit 594980C0)
    (at 25.4 51.181)
    (descr "4-way 2.54mm pitch terminal block, Phoenix MPT series")
    (fp_text reference P8 (at -2.4638 -4.2164) (layer F.SilkS))
    (fp_text value PWR_THRU_1 (at 0 4.50088) (layer F.SilkS))
    (pad 4 thru_hole oval (at -3.81 0) (size 1.99898 1.99898) (drill 1.09728) (layers *.Cu *.Mask F.SilkS)
      (net 2 /GND))
    (pad 1 thru_hole rect (at 3.81 0) (size 1.99898 1.99898) (drill 1.09728) (layers *.Cu *.Mask F.SilkS)
      (net 47 "Net-(C17-Pad1)"))
    (pad 2 thru_hole oval (at 1.27 0) (size 1.99898 1.99898) (drill 1.09728) (layers *.Cu *.Mask F.SilkS)
      (net 47 "Net-(C17-Pad1)"))
    (pad 3 thru_hole oval (at -1.27 0) (size 1.99898 1.99898) (drill 1.09728) (layers *.Cu *.Mask F.SilkS)
      (net 2 /GND))
    (model walter/conn_mpt/mpt_0,5-4-2,54.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer B.Cu) (tedit 59498107)
    (at 11.049 42.926 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R1 (at -2.2098 0.1016 180) (layer B.SilkS))
    (fp_text value 10K (at 0 -1.5 180) (layer B.Fab))
    (fp_text user %R (at 0 1.45 180) (layer B.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 48 /InRushLimit/V_IR_IN))
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 14 "Net-(D2-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 59498033)
    (at 13.474 45.593 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R2 (at -2.274 -0.889 180) (layer F.SilkS))
    (fp_text value 10K (at 0 1.5 180) (layer F.Fab))
    (fp_text user %R (at 0 -1.45 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 7 /+5V))
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(D3-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 59488A7D)
    (at 26.543 26.797 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R3 (at 2.413 -0.127 270) (layer F.SilkS))
    (fp_text value 10K (at 0 1.5 270) (layer F.Fab))
    (fp_text user %R (at 2.413 -0.127 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 1 /3V3))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 25 /SDA))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 59488A93)
    (at 23.864 29.591)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R4 (at 0 1.524) (layer F.SilkS))
    (fp_text value 10K (at 0 1.5) (layer F.Fab))
    (fp_text user %R (at 0 1.524) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 1 /3V3))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 26 /SCL))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 59488DDA)
    (at 45.095 39.142 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R5 (at -2.149 0.026 180) (layer F.SilkS))
    (fp_text value 10K (at 0 1.5 180) (layer F.Fab))
    (fp_text user %R (at -2.149 0.026 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 27 "Net-(R5-Pad1)"))
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(D4-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 59488DD3)
    (at 45.085 42.799 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R6 (at -2.159 -0.127 180) (layer F.SilkS))
    (fp_text value 1k (at 0 1.5 180) (layer F.Fab))
    (fp_text user %R (at -2.159 -0.127 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(JP1-Pad1)"))
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 2 /GND))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 59488DE5)
    (at 45.145 41.017)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R7 (at 2.099 0.004) (layer F.SilkS))
    (fp_text value 1k (at 0 1.5) (layer F.Fab))
    (fp_text user %R (at 2.099 0.004) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 28 "/Power Output/ATX_5V_SB"))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 20 /ATX_ON))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer B.Cu) (tedit 59488931)
    (at 14.986 24.384 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R8 (at 0.127 1.778 90) (layer B.SilkS))
    (fp_text value 10K (at 0 -1.5 90) (layer B.Fab))
    (fp_text user %R (at 0.127 1.778 90) (layer B.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 39 /ODROID_1.8V))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 40 /ODROID_TX))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer B.Cu) (tedit 59488990)
    (at 9.017 24.003 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R9 (at 0.127 1.651 270) (layer B.SilkS))
    (fp_text value 10K (at 0 -1.5 270) (layer B.Fab))
    (fp_text user %R (at 0.127 1.651 270) (layer B.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 1 /3V3))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 42 /ODROID_TX_3V3))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer B.Cu) (tedit 58AAD9CA)
    (at 8.89 27.051 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R10 (at 0 1.45 270) (layer B.SilkS))
    (fp_text value 10K (at 0 -1.5 270) (layer B.Fab))
    (fp_text user %R (at 0 1.45 270) (layer B.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 39 /ODROID_1.8V))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 41 /ODROID_RX))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer B.Cu) (tedit 59488967)
    (at 14.986 27.178 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R11 (at 0.127 1.778 90) (layer B.SilkS))
    (fp_text value 10K (at 0 -1.5 90) (layer B.Fab))
    (fp_text user %R (at 0.127 1.778 90) (layer B.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 1 /3V3))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 43 /ODROID_RX_3V3))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5948765F)
    (at 18.415 17.018 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R13 (at 2.794 0.127 360) (layer F.SilkS))
    (fp_text value 10K (at 0 1.5 270) (layer F.Fab))
    (fp_text user %R (at 2.794 0.127 360) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 1 /3V3))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 57 "Net-(R13-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5948764E)
    (at 20.066 17.78 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R14 (at -2.032 -0.635 360) (layer F.SilkS))
    (fp_text value 10K (at 0 1.5 270) (layer F.Fab))
    (fp_text user %R (at -2.032 -0.635 360) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 1 /3V3))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 58 "Net-(R14-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer B.Cu) (tedit 58AAD9CA)
    (at 23.114 8.509 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R15 (at 0 1.45 180) (layer B.SilkS))
    (fp_text value 10K (at 0 -1.5 180) (layer B.Fab))
    (fp_text user %R (at 0 1.45 180) (layer B.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 1 /3V3))
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 59 /RTC_RST))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5948746C)
    (at 6.35 24.257 270)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C3 (at -0.127 1.397 270) (layer F.SilkS))
    (fp_text value "1 uF" (at 0 1.5 270) (layer F.Fab))
    (fp_text user %R (at -0.127 1.397 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C3-Pad1)"))
    (pad 2 smd rect (at 0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(C3-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5948747F)
    (at 6.35 27.305 270)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C4 (at -0.127 1.397 270) (layer F.SilkS))
    (fp_text value "1 uF" (at 0 1.5 270) (layer F.Fab))
    (fp_text user %R (at -0.127 1.397 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(C4-Pad1)"))
    (pad 2 smd rect (at 0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(C4-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5948749B)
    (at 11.938 21.971 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C12 (at -2.921 0 180) (layer F.SilkS))
    (fp_text value "1 uF" (at 0 1.5 180) (layer F.Fab))
    (fp_text user %R (at -2.921 0 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 /GND))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 45 "Net-(C12-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59487583)
    (at 12.065 29.718 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C13 (at 3.175 -0.127 180) (layer F.SilkS))
    (fp_text value "1 uF" (at 0 1.5 180) (layer F.Fab))
    (fp_text user %R (at 3.175 -0.127 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 /GND))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 46 "Net-(C13-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_line (start 0 54.61) (end 0 0) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 54.61 54.61) (end 0 54.61) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 54.61 0) (end 54.61 54.61) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 0 0) (end 54.61 0) (angle 90) (layer Edge.Cuts) (width 0.15))
  (zone (net 2) (net_name /GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.381))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.254) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 0.127 0.127) (xy 54.483 0.127) (xy 54.483 54.483) (xy 0.127 54.483)
      )
    )
  )
  (zone (net 2) (net_name /GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.254))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.254) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 0.127 0.127) (xy 54.483 0.127) (xy 54.483 54.483) (xy 0.127 54.483)
      )
    )
  )
)
