(kicad_pcb (version 4) (host pcbnew "(2015-07-16 BZR 5955, Git 27eafcb)-product")
  (general
    (links 190)
    (no_connects 190)
    (area 125.608739 51.971999 282.118524 207.151)
    (thickness 1.6)
    (drawings 4)
    (tracks 7)
    (zones 0)
    (modules 83)
    (nets 90)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (user_trace_width 0.254)
    (user_trace_width 0.508)
    (user_trace_width 1.016)
    (user_trace_width 1.524)
    (user_trace_width 2.032)
    (user_trace_width 2.54)
    (trace_clearance 0.2)
    (zone_clearance 0.127)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.1)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.5 1.5)
    (pad_drill 0.6)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 0 0)
    (visible_elements 7FFEF7FF)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 /GND)
  (net 2 "Net-(C1-Pad2)")
  (net 3 "Net-(C2-Pad2)")
  (net 4 /Vin)
  (net 5 "Net-(C5-Pad1)")
  (net 6 "Net-(C5-Pad2)")
  (net 7 "Net-(C6-Pad1)")
  (net 8 "Net-(C6-Pad2)")
  (net 9 /VCP)
  (net 10 /Vcc)
  (net 11 "Net-(C16-Pad1)")
  (net 12 "Net-(C17-Pad1)")
  (net 13 "Net-(C18-Pad1)")
  (net 14 "Net-(C19-Pad1)")
  (net 15 "Net-(C19-Pad2)")
  (net 16 "Net-(C20-Pad1)")
  (net 17 "Net-(C20-Pad2)")
  (net 18 "Net-(C21-Pad1)")
  (net 19 "Net-(C21-Pad2)")
  (net 20 "Net-(C22-Pad2)")
  (net 21 "Net-(C23-Pad2)")
  (net 22 "Net-(C24-Pad1)")
  (net 23 "Net-(C25-Pad2)")
  (net 24 /PC6)
  (net 25 "Net-(D1-Pad1)")
  (net 26 "Net-(D2-Pad1)")
  (net 27 "Net-(D3-Pad1)")
  (net 28 "Net-(D4-Pad1)")
  (net 29 "Net-(D5-Pad1)")
  (net 30 "Net-(D6-Pad1)")
  (net 31 "Net-(F1-Pad1)")
  (net 32 /DIR2)
  (net 33 /FAULT2)
  (net 34 /DIR1)
  (net 35 /STEP1)
  (net 36 /PD7)
  (net 37 /PB0)
  (net 38 /PB1)
  (net 39 /PB2)
  (net 40 /PB3)
  (net 41 /PB4)
  (net 42 /PB5)
  (net 43 /ADC6)
  (net 44 /ADC7)
  (net 45 /SLEEP1)
  (net 46 /SLEEP2)
  (net 47 /HOME1)
  (net 48 /HOME2)
  (net 49 /SDA)
  (net 50 /SCL)
  (net 51 /RX0)
  (net 52 /TX0)
  (net 53 /FAULT1)
  (net 54 /RX)
  (net 55 /TX)
  (net 56 "Net-(P3-Pad2)")
  (net 57 "Net-(P3-Pad1)")
  (net 58 "Net-(P4-Pad2)")
  (net 59 "Net-(P4-Pad1)")
  (net 60 "Net-(P5-Pad2)")
  (net 61 "Net-(P5-Pad1)")
  (net 62 "Net-(P6-Pad2)")
  (net 63 "Net-(P6-Pad1)")
  (net 64 "Net-(R1-Pad2)")
  (net 65 "Net-(R2-Pad2)")
  (net 66 "Net-(R7-Pad2)")
  (net 67 "Net-(R8-Pad2)")
  (net 68 "Net-(R9-Pad2)")
  (net 69 "Net-(R10-Pad2)")
  (net 70 "Net-(RV1-Pad2)")
  (net 71 "Net-(RV2-Pad2)")
  (net 72 "Net-(S1-Pad5)")
  (net 73 "Net-(S1-Pad6)")
  (net 74 "Net-(S1-Pad7)")
  (net 75 "Net-(S1-Pad8)")
  (net 76 "Net-(S2-Pad5)")
  (net 77 "Net-(S2-Pad6)")
  (net 78 "Net-(S2-Pad7)")
  (net 79 "Net-(S2-Pad8)")
  (net 80 "Net-(U1-Pad21)")
  (net 81 "Net-(U1-Pad23)")
  (net 82 "Net-(U2-Pad21)")
  (net 83 "Net-(U2-Pad23)")
  (net 84 "Net-(U4-Pad5)")
  (net 85 "Net-(U5-Pad7)")
  (net 86 "Net-(U5-Pad8)")
  (net 87 "Net-(U5-Pad9)")
  (net 88 "Net-(U5-Pad10)")
  (net 89 "Net-(X1-Pad2)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /ADC6)
    (add_net /ADC7)
    (add_net /DIR1)
    (add_net /DIR2)
    (add_net /FAULT1)
    (add_net /FAULT2)
    (add_net /GND)
    (add_net /HOME1)
    (add_net /HOME2)
    (add_net /PB0)
    (add_net /PB1)
    (add_net /PB2)
    (add_net /PB3)
    (add_net /PB4)
    (add_net /PB5)
    (add_net /PC6)
    (add_net /PD7)
    (add_net /RX)
    (add_net /RX0)
    (add_net /SCL)
    (add_net /SDA)
    (add_net /SLEEP1)
    (add_net /SLEEP2)
    (add_net /STEP1)
    (add_net /TX)
    (add_net /TX0)
    (add_net /VCP)
    (add_net /Vcc)
    (add_net /Vin)
    (add_net "Net-(C1-Pad2)")
    (add_net "Net-(C16-Pad1)")
    (add_net "Net-(C17-Pad1)")
    (add_net "Net-(C18-Pad1)")
    (add_net "Net-(C19-Pad1)")
    (add_net "Net-(C19-Pad2)")
    (add_net "Net-(C2-Pad2)")
    (add_net "Net-(C20-Pad1)")
    (add_net "Net-(C20-Pad2)")
    (add_net "Net-(C21-Pad1)")
    (add_net "Net-(C21-Pad2)")
    (add_net "Net-(C22-Pad2)")
    (add_net "Net-(C23-Pad2)")
    (add_net "Net-(C24-Pad1)")
    (add_net "Net-(C25-Pad2)")
    (add_net "Net-(C5-Pad1)")
    (add_net "Net-(C5-Pad2)")
    (add_net "Net-(C6-Pad1)")
    (add_net "Net-(C6-Pad2)")
    (add_net "Net-(D1-Pad1)")
    (add_net "Net-(D2-Pad1)")
    (add_net "Net-(D3-Pad1)")
    (add_net "Net-(D4-Pad1)")
    (add_net "Net-(D5-Pad1)")
    (add_net "Net-(D6-Pad1)")
    (add_net "Net-(F1-Pad1)")
    (add_net "Net-(P3-Pad1)")
    (add_net "Net-(P3-Pad2)")
    (add_net "Net-(P4-Pad1)")
    (add_net "Net-(P4-Pad2)")
    (add_net "Net-(P5-Pad1)")
    (add_net "Net-(P5-Pad2)")
    (add_net "Net-(P6-Pad1)")
    (add_net "Net-(P6-Pad2)")
    (add_net "Net-(R1-Pad2)")
    (add_net "Net-(R10-Pad2)")
    (add_net "Net-(R2-Pad2)")
    (add_net "Net-(R7-Pad2)")
    (add_net "Net-(R8-Pad2)")
    (add_net "Net-(R9-Pad2)")
    (add_net "Net-(RV1-Pad2)")
    (add_net "Net-(RV2-Pad2)")
    (add_net "Net-(S1-Pad5)")
    (add_net "Net-(S1-Pad6)")
    (add_net "Net-(S1-Pad7)")
    (add_net "Net-(S1-Pad8)")
    (add_net "Net-(S2-Pad5)")
    (add_net "Net-(S2-Pad6)")
    (add_net "Net-(S2-Pad7)")
    (add_net "Net-(S2-Pad8)")
    (add_net "Net-(U1-Pad21)")
    (add_net "Net-(U1-Pad23)")
    (add_net "Net-(U2-Pad21)")
    (add_net "Net-(U2-Pad23)")
    (add_net "Net-(U4-Pad5)")
    (add_net "Net-(U5-Pad10)")
    (add_net "Net-(U5-Pad7)")
    (add_net "Net-(U5-Pad8)")
    (add_net "Net-(U5-Pad9)")
    (add_net "Net-(X1-Pad2)")
  )
  (module StepperFootprints:4-40-Plated (layer F.Cu) (tedit 55DD067D)
    (at 196.644 181.896)
    (fp_text reference "" (at 0 0.5) (layer F.SilkS))
    (fp_text value "" (at 0 -0.5) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 3.81 3.81) (drill 3.048) (layers *.Cu *.Mask F.SilkS))
  )
  (module StepperFootprints:4-40-Plated (layer F.Cu) (tedit 55DD067D)
    (at 192.434 181.896)
    (fp_text reference "" (at 0 0.5) (layer F.SilkS))
    (fp_text value "" (at 0 -0.5) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 3.81 3.81) (drill 3.048) (layers *.Cu *.Mask F.SilkS))
  )
  (module StepperFootprints:4-40-Plated (layer F.Cu) (tedit 55DD067D)
    (at 244.984 201.406)
    (fp_text reference "" (at 0 0.5) (layer F.SilkS))
    (fp_text value "" (at 0 -0.5) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 3.81 3.81) (drill 3.048) (layers *.Cu *.Mask F.SilkS))
  )
  (module StepperFootprints:4-40-Plated (layer F.Cu) (tedit 55DD067D)
    (at 210.924 202.756)
    (fp_text reference "" (at 0 0.5) (layer F.SilkS))
    (fp_text value "" (at 0 -0.5) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 3.81 3.81) (drill 3.048) (layers *.Cu *.Mask F.SilkS))
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 5415D6EA)
    (at 279.161619 150.926)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C1 (at 0 -2.1) (layer F.SilkS))
    (fp_text value 0.47uF (at 0 2.1) (layer F.Fab))
    (pad 1 smd rect (at -1 0) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 /GND))
    (pad 2 smd rect (at 1 0) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(C1-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 5415D6EA)
    (at 246.451619 182.916)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C2 (at 0 -2.1) (layer F.SilkS))
    (fp_text value 0.47uF (at 0 2.1) (layer F.Fab))
    (pad 1 smd rect (at -1 0) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 /GND))
    (pad 2 smd rect (at 1 0) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C2-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 5415D6EA)
    (at 273.995428 150.926)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C3 (at 0 -2.1) (layer F.SilkS))
    (fp_text value 4.7uF (at 0 2.1) (layer F.Fab))
    (pad 1 smd rect (at -1 0) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 4 /Vin))
    (pad 2 smd rect (at 1 0) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 /GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 5415D6EA)
    (at 264.065428 160.026)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C4 (at 0 -2.1) (layer F.SilkS))
    (fp_text value 4.7uF (at 0 2.1) (layer F.Fab))
    (pad 1 smd rect (at -1 0) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 4 /Vin))
    (pad 2 smd rect (at 1 0) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 /GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 5415D6EA)
    (at 254.907333 164.726)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C5 (at 0 -2.1) (layer F.SilkS))
    (fp_text value 10nF (at 0 2.1) (layer F.Fab))
    (pad 1 smd rect (at -1 0) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(C5-Pad1)"))
    (pad 2 smd rect (at 1 0) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(C5-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 55DD3F5A)
    (at 136.6901 54.3814 270)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C6 (at -2.5908 -0.0381 360) (layer F.SilkS))
    (fp_text value 10nF (at 0 2.1 270) (layer F.Fab))
    (pad 1 smd rect (at -1 0 270) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(C6-Pad1)"))
    (pad 2 smd rect (at 1 0 270) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(C6-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 5415D6EA)
    (at 250.455428 175.776)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C7 (at 0 -2.1) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 2.1) (layer F.Fab))
    (pad 1 smd rect (at -1 0) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 4 /Vin))
    (pad 2 smd rect (at 1 0) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 /GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 5415D6EA)
    (at 255.145428 171.026)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C8 (at 0 -2.1) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 2.1) (layer F.Fab))
    (pad 1 smd rect (at -1 0) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 4 /Vin))
    (pad 2 smd rect (at 1 0) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 /GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 5415D6EA)
    (at 275.835428 169.826)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C9 (at 0 -2.1) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 2.1) (layer F.Fab))
    (pad 1 smd rect (at -1 0) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 4 /Vin))
    (pad 2 smd rect (at 1 0) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 /GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 5415D6EA)
    (at 259.355428 164.726)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C10 (at 0 -2.1) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 2.1) (layer F.Fab))
    (pad 1 smd rect (at -1 0) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 4 /Vin))
    (pad 2 smd rect (at 1 0) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 /GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 5415D6EA)
    (at 253.285428 196.226)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C11 (at 0 -2.1) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 2.1) (layer F.Fab))
    (pad 1 smd rect (at -1 0) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 4 /Vin))
    (pad 2 smd rect (at 1 0) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 9 /VCP))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 5415D6EA)
    (at 278.045428 157.226)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C12 (at 0 -2.1) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 2.1) (layer F.Fab))
    (pad 1 smd rect (at -1 0) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 4 /Vin))
    (pad 2 smd rect (at 1 0) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 9 /VCP))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:c_elec_10x10 (layer F.Cu) (tedit 55DD0A94)
    (at 155.1305 58.547 90)
    (descr "SMT capacitor, aluminium electrolytic, 10x10")
    (attr smd)
    (fp_text reference C13 (at -5.1435 -6.477 90) (layer F.SilkS))
    (fp_text value MAL214699103E3 (at 0 6.35 90) (layer F.Fab))
    (pad 1 smd rect (at 4.0005 0 90) (size 4.0005 2.4003) (layers F.Cu F.Paste F.Mask)
      (net 4 /Vin))
    (pad 2 smd rect (at -4.0005 0 90) (size 4.0005 2.4003) (layers F.Cu F.Paste F.Mask)
      (net 1 /GND))
    (model Capacitors_SMD.3dshapes/c_elec_10x10.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:c_elec_10x10 (layer F.Cu) (tedit 55DD0ACA)
    (at 180.1495 58.547 90)
    (descr "SMT capacitor, aluminium electrolytic, 10x10")
    (attr smd)
    (fp_text reference C14 (at -3.937 -6.4135 90) (layer F.SilkS))
    (fp_text value MAL214699103E3 (at 0 6.35 90) (layer F.Fab))
    (pad 1 smd rect (at 4.0005 0 90) (size 4.0005 2.4003) (layers F.Cu F.Paste F.Mask)
      (net 4 /Vin))
    (pad 2 smd rect (at -4.0005 0 90) (size 4.0005 2.4003) (layers F.Cu F.Paste F.Mask)
      (net 1 /GND))
    (model Capacitors_SMD.3dshapes/c_elec_10x10.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 5415D6EA)
    (at 262.565428 185.226)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C15 (at 0 -2.1) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 2.1) (layer F.Fab))
    (pad 1 smd rect (at -1 0) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 10 /Vcc))
    (pad 2 smd rect (at 1 0) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 /GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 5415D6EA)
    (at 267.755428 178.926)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C16 (at 0 -2.1) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 2.1) (layer F.Fab))
    (pad 1 smd rect (at -1 0) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(C16-Pad1)"))
    (pad 2 smd rect (at 1 0) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 /GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 5415D6EA)
    (at 256.087333 189.926)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C17 (at 0 -2.1) (layer F.SilkS))
    (fp_text value 10nF (at 0 2.1) (layer F.Fab))
    (pad 1 smd rect (at -1 0) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(C17-Pad1)"))
    (pad 2 smd rect (at 1 0) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 /GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:c_elec_10x10 (layer F.Cu) (tedit 55DD3050)
    (at 219.74175 109.89945 90)
    (descr "SMT capacitor, aluminium electrolytic, 10x10")
    (attr smd)
    (fp_text reference C18 (at 1.37795 -6.24205 90) (layer F.SilkS))
    (fp_text value MAL214699103E3 (at 0 6.35 90) (layer F.Fab))
    (pad 1 smd rect (at 4.0005 0 90) (size 4.0005 2.4003) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(C18-Pad1)"))
    (pad 2 smd rect (at -4.0005 0 90) (size 4.0005 2.4003) (layers F.Cu F.Paste F.Mask)
      (net 1 /GND))
    (model Capacitors_SMD.3dshapes/c_elec_10x10.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 5415D6EA)
    (at 232.874001 195.276)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C19 (at 0 -2.1) (layer F.SilkS))
    (fp_text value 1uF (at 0 2.1) (layer F.Fab))
    (pad 1 smd rect (at -1 0) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(C19-Pad1)"))
    (pad 2 smd rect (at 1 0) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(C19-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 5415D6EA)
    (at 259.034001 177.326)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C20 (at 0 -2.1) (layer F.SilkS))
    (fp_text value 1uF (at 0 2.1) (layer F.Fab))
    (pad 1 smd rect (at -1 0) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(C20-Pad1)"))
    (pad 2 smd rect (at 1 0) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(C20-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 55DD0D2D)
    (at 206.85125 113.64595 270)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C21 (at 2.8575 0.0635 360) (layer F.SilkS))
    (fp_text value 10nF (at 0 2.1 270) (layer F.Fab))
    (pad 1 smd rect (at -1 0 270) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(C21-Pad1)"))
    (pad 2 smd rect (at 1 0 270) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 19 "Net-(C21-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 5415D6EA)
    (at 232.777333 201.576)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C22 (at 0 -2.1) (layer F.SilkS))
    (fp_text value 10pF (at 0 2.1) (layer F.Fab))
    (pad 1 smd rect (at -1 0) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 /GND))
    (pad 2 smd rect (at 1 0) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 20 "Net-(C22-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 5415D6EA)
    (at 254.907333 177.326)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C23 (at 0 -2.1) (layer F.SilkS))
    (fp_text value 10pF (at 0 2.1) (layer F.Fab))
    (pad 1 smd rect (at -1 0) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 /GND))
    (pad 2 smd rect (at 1 0) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 21 "Net-(C23-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 5415D6EA)
    (at 259.514001 171.026)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C24 (at 0 -2.1) (layer F.SilkS))
    (fp_text value 1uF (at 0 2.1) (layer F.Fab))
    (pad 1 smd rect (at -1 0) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 22 "Net-(C24-Pad1)"))
    (pad 2 smd rect (at 1 0) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 /GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 5415D6EA)
    (at 273.674001 157.226)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C25 (at 0 -2.1) (layer F.SilkS))
    (fp_text value 1uF (at 0 2.1) (layer F.Fab))
    (pad 1 smd rect (at -1 0) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 /GND))
    (pad 2 smd rect (at 1 0) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 23 "Net-(C25-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 5415D6EA)
    (at 225.665428 203.266)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C26 (at 0 -2.1) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 2.1) (layer F.Fab))
    (pad 1 smd rect (at -1 0) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 24 /PC6))
    (pad 2 smd rect (at 1 0) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 /GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_Tantalum_SMD:TantalC_SizeD_EIA-7343_HandSoldering (layer F.Cu) (tedit 55DD0D13)
    (at 215.6968 120.5865)
    (descr "Tantal Cap. , Size D, EIA-7343, Hand Soldering,")
    (tags "Tantal Cap. , Size D, EIA-7343, Hand Soldering,")
    (attr smd)
    (fp_text reference C27 (at 3.683 -3.2385) (layer F.SilkS))
    (fp_text value 10TPE68M (at -0.09906 3.59918) (layer F.Fab))
    (fp_text user + (at -6.85546 -2.70002) (layer F.SilkS))
    (pad 2 smd rect (at 3.88874 0) (size 4.0005 2.70002) (layers F.Cu F.Paste F.Mask)
      (net 1 /GND))
    (pad 1 smd rect (at -3.88874 0) (size 4.0005 2.70002) (layers F.Cu F.Paste F.Mask)
      (net 10 /Vcc))
    (model Capacitors_Tantalum_SMD.3dshapes/TantalC_SizeD_EIA-7343_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 5415D6EA)
    (at 268.434001 160.026)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C28 (at 0 -2.1) (layer F.SilkS))
    (fp_text value 1uF (at 0 2.1) (layer F.Fab))
    (pad 1 smd rect (at -1 0) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 10 /Vcc))
    (pad 2 smd rect (at 1 0) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 /GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diodes_SMD:D-Pak_TO252AA (layer F.Cu) (tedit 552FE2A5)
    (at 217.1065 81.153)
    (descr "D-Pak, TO252AA, Diode")
    (tags "D-Pak TO252AA Diode")
    (attr smd)
    (fp_text reference D1 (at 0 -7.5) (layer F.SilkS))
    (fp_text value SCHDPAK (at 0 8.1) (layer F.Fab))
    (pad 3 smd rect (at 2.18 4.3) (size 1.55 2.78) (layers F.Cu F.Paste F.Mask)
      (net 25 "Net-(D1-Pad1)"))
    (pad 4 smd rect (at 0 -2.335) (size 6.74 6.73) (layers F.Cu F.Paste F.Mask))
    (pad 1 smd rect (at -2.18 4.3) (size 1.55 2.78) (layers F.Cu F.Paste F.Mask)
      (net 25 "Net-(D1-Pad1)"))
    (model Diodes_SMD.3dshapes/D-Pak_TO252AA.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module StepperFootprints:LED-0805-POS (layer F.Cu) (tedit 55DCD526)
    (at 234.719238 189.326)
    (descr "LED 0805 smd package")
    (tags "LED 0805 SMD")
    (attr smd)
    (fp_text reference D2 (at 0 -1.75) (layer F.SilkS))
    (fp_text value "2mA Blue" (at 0 1.75) (layer F.Fab))
    (pad 2 smd rect (at 1.04902 0 180) (size 1.19888 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 1 /GND))
    (pad 1 smd rect (at -1.04902 0 180) (size 1.19888 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 26 "Net-(D2-Pad1)"))
    (model LEDs.3dshapes/LED-0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module StepperFootprints:LED-0805-POS (layer F.Cu) (tedit 55DCD526)
    (at 204.243524 204.426)
    (descr "LED 0805 smd package")
    (tags "LED 0805 SMD")
    (attr smd)
    (fp_text reference D3 (at 0 -1.75) (layer F.SilkS))
    (fp_text value "2mA Yellow" (at 0 1.75) (layer F.Fab))
    (pad 2 smd rect (at 1.04902 0 180) (size 1.19888 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 1 /GND))
    (pad 1 smd rect (at -1.04902 0 180) (size 1.19888 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 27 "Net-(D3-Pad1)"))
    (model LEDs.3dshapes/LED-0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module StepperFootprints:LED-0805-POS (layer F.Cu) (tedit 55DCD526)
    (at 194.815429 204.426)
    (descr "LED 0805 smd package")
    (tags "LED 0805 SMD")
    (attr smd)
    (fp_text reference D4 (at 0 -1.75) (layer F.SilkS))
    (fp_text value "2mA Orange" (at 0 1.75) (layer F.Fab))
    (pad 2 smd rect (at 1.04902 0 180) (size 1.19888 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 1 /GND))
    (pad 1 smd rect (at -1.04902 0 180) (size 1.19888 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 28 "Net-(D4-Pad1)"))
    (model LEDs.3dshapes/LED-0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module StepperFootprints:LED-0805-POS (layer F.Cu) (tedit 55DCD526)
    (at 226.998762 197.316)
    (descr "LED 0805 smd package")
    (tags "LED 0805 SMD")
    (attr smd)
    (fp_text reference D5 (at 0 -1.75) (layer F.SilkS))
    (fp_text value "2mA RED" (at 0 1.75) (layer F.Fab))
    (pad 2 smd rect (at 1.04902 0 180) (size 1.19888 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 1 /GND))
    (pad 1 smd rect (at -1.04902 0 180) (size 1.19888 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 29 "Net-(D5-Pad1)"))
    (model LEDs.3dshapes/LED-0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module StepperFootprints:LED-0805-POS (layer F.Cu) (tedit 55DCD526)
    (at 243.765429 176.966)
    (descr "LED 0805 smd package")
    (tags "LED 0805 SMD")
    (attr smd)
    (fp_text reference D6 (at 0 -1.75) (layer F.SilkS))
    (fp_text value "2mA Green" (at 0 1.75) (layer F.Fab))
    (pad 2 smd rect (at 1.04902 0 180) (size 1.19888 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 1 /GND))
    (pad 1 smd rect (at -1.04902 0 180) (size 1.19888 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 30 "Net-(D6-Pad1)"))
    (model LEDs.3dshapes/LED-0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module StepperFootprints:DO-221BC (layer F.Cu) (tedit 55DD0D32)
    (at 210.7819 106.1466 180)
    (descr DO-221BC)
    (fp_text reference D7 (at 0.127 2.032 180) (layer F.SilkS))
    (fp_text value V4PAN50-M3/I (at 0 1.9685 180) (layer F.SilkS) hide)
    (pad 2 smd rect (at 1.55 0 180) (size 3.1 2.2) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(C21-Pad1)"))
    (pad 1 smd rect (at -1.7 0 180) (size 1.5 1.5) (layers F.Cu F.Paste F.Mask)
      (net 1 /GND))
    (model walter/smd_diode/do214ac.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMD_Packages:Fuse_SMD (layer F.Cu) (tedit 0)
    (at 200.66 85.4075 90)
    (attr smd)
    (fp_text reference F1 (at 0 -0.508 90) (layer F.SilkS))
    (fp_text value 5A (at 0 0.762 90) (layer F.Fab))
    (pad 1 smd rect (at 0 -3.175 90) (size 3.556 4.191) (layers F.Cu F.Paste F.Mask)
      (net 31 "Net-(F1-Pad1)"))
    (pad 2 smd rect (at 0 3.175 90) (size 3.556 4.191) (layers F.Cu F.Paste F.Mask)
      (net 25 "Net-(D1-Pad1)"))
    (model SMD_Packages.3dshapes/Fuse_SMD.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 90))
    )
  )
  (module Housings_QFP:LQFP-32_7x7mm_Pitch0.8mm (layer F.Cu) (tedit 54130A77)
    (at 255.712095 154.676)
    (descr "LQFP32: plastic low profile quad flat package; 32 leads; body 7 x 7 x 1.4 mm (see NXP sot358-1_po.pdf and sot358-1_fr.pdf)")
    (tags "QFP 0.8")
    (attr smd)
    (fp_text reference IC1 (at 0 -5.85) (layer F.SilkS))
    (fp_text value ATMEGA328P-A (at 0 5.85) (layer F.Fab))
    (pad 1 smd rect (at -4.25 -2.8) (size 1.2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 32 /DIR2))
    (pad 2 smd rect (at -4.25 -2) (size 1.2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 33 /FAULT2))
    (pad 3 smd rect (at -4.25 -1.2) (size 1.2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 /GND))
    (pad 4 smd rect (at -4.25 -0.4) (size 1.2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 10 /Vcc))
    (pad 5 smd rect (at -4.25 0.4) (size 1.2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 /GND))
    (pad 6 smd rect (at -4.25 1.2) (size 1.2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 10 /Vcc))
    (pad 7 smd rect (at -4.25 2) (size 1.2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 20 "Net-(C22-Pad2)"))
    (pad 8 smd rect (at -4.25 2.8) (size 1.2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 21 "Net-(C23-Pad2)"))
    (pad 9 smd rect (at -2.8 4.25 90) (size 1.2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 34 /DIR1))
    (pad 10 smd rect (at -2 4.25 90) (size 1.2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 35 /STEP1))
    (pad 11 smd rect (at -1.2 4.25 90) (size 1.2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 36 /PD7))
    (pad 12 smd rect (at -0.4 4.25 90) (size 1.2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 37 /PB0))
    (pad 13 smd rect (at 0.4 4.25 90) (size 1.2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 38 /PB1))
    (pad 14 smd rect (at 1.2 4.25 90) (size 1.2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 39 /PB2))
    (pad 15 smd rect (at 2 4.25 90) (size 1.2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 40 /PB3))
    (pad 16 smd rect (at 2.8 4.25 90) (size 1.2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 41 /PB4))
    (pad 17 smd rect (at 4.25 2.8) (size 1.2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 42 /PB5))
    (pad 18 smd rect (at 4.25 2) (size 1.2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(C16-Pad1)"))
    (pad 19 smd rect (at 4.25 1.2) (size 1.2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 43 /ADC6))
    (pad 20 smd rect (at 4.25 0.4) (size 1.2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(C17-Pad1)"))
    (pad 21 smd rect (at 4.25 -0.4) (size 1.2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 /GND))
    (pad 22 smd rect (at 4.25 -1.2) (size 1.2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 44 /ADC7))
    (pad 23 smd rect (at 4.25 -2) (size 1.2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 45 /SLEEP1))
    (pad 24 smd rect (at 4.25 -2.8) (size 1.2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 46 /SLEEP2))
    (pad 25 smd rect (at 2.8 -4.25 90) (size 1.2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 47 /HOME1))
    (pad 26 smd rect (at 2 -4.25 90) (size 1.2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 48 /HOME2))
    (pad 27 smd rect (at 1.2 -4.25 90) (size 1.2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 49 /SDA))
    (pad 28 smd rect (at 0.4 -4.25 90) (size 1.2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 50 /SCL))
    (pad 29 smd rect (at -0.4 -4.25 90) (size 1.2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 24 /PC6))
    (pad 30 smd rect (at -1.2 -4.25 90) (size 1.2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 51 /RX0))
    (pad 31 smd rect (at -2 -4.25 90) (size 1.2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 52 /TX0))
    (pad 32 smd rect (at -2.8 -4.25 90) (size 1.2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 53 /FAULT1))
    (model Housings_QFP.3dshapes/LQFP-32_7x7mm_Pitch0.8mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 5415CDEB)
    (at 263.902571 166.326)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference L1 (at 0 -2.1) (layer F.SilkS))
    (fp_text value 10uH (at 0 2.1) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(C16-Pad1)"))
    (pad 2 smd rect (at 0.95 0) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 10 /Vcc))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_2x03 (layer F.Cu) (tedit 54EA0A4B)
    (at 218.217333 197.596)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P1 (at 0 -5.1) (layer F.SilkS))
    (fp_text value CONN_02X03 (at 0 -3.1) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 41 /PB4))
    (pad 2 thru_hole oval (at 2.54 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 10 /Vcc))
    (pad 3 thru_hole oval (at 0 2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 42 /PB5))
    (pad 4 thru_hole oval (at 2.54 2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 40 /PB3))
    (pad 5 thru_hole oval (at 0 5.08) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 24 /PC6))
    (pad 6 thru_hole oval (at 2.54 5.08) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 /GND))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_2x03.wrl
      (at (xyz 0.05 -0.1 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module w_conn_mpt:mpt_0,5%2f4-2,54 (layer F.Cu) (tedit 55DD0B0C)
    (at 162.6235 132.9055)
    (descr "4-way 2.54mm pitch terminal block, Phoenix MPT series")
    (fp_text reference P2 (at 7.0485 2.159) (layer F.SilkS))
    (fp_text value CONN_01X04 (at 0 4.50088) (layer F.SilkS))
    (pad 4 thru_hole oval (at -3.81 0) (size 1.99898 1.99898) (drill 1.09728) (layers *.Cu *.Mask F.SilkS)
      (net 54 /RX))
    (pad 1 thru_hole rect (at 3.81 0) (size 1.99898 1.99898) (drill 1.09728) (layers *.Cu *.Mask F.SilkS)
      (net 1 /GND))
    (pad 2 thru_hole oval (at 1.27 0) (size 1.99898 1.99898) (drill 1.09728) (layers *.Cu *.Mask F.SilkS)
      (net 31 "Net-(F1-Pad1)"))
    (pad 3 thru_hole oval (at -1.27 0) (size 1.99898 1.99898) (drill 1.09728) (layers *.Cu *.Mask F.SilkS)
      (net 55 /TX))
    (model walter/conn_mpt/mpt_0,5-4-2,54.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module w_conn_mpt:mpt_0,5%2f2-2,54 (layer F.Cu) (tedit 512665B4)
    (at 167.8305 78.613 180)
    (descr "2-way 2.54mm pitch terminal block, Phoenix MPT series")
    (fp_text reference P3 (at 0 -4.50088 180) (layer F.SilkS))
    (fp_text value CONN_01X02 (at 0 4.50088 180) (layer F.SilkS))
    (pad 2 thru_hole oval (at -1.27 0 180) (size 1.99898 1.99898) (drill 1.09728) (layers *.Cu *.Mask F.SilkS)
      (net 56 "Net-(P3-Pad2)"))
    (pad 1 thru_hole rect (at 1.27 0 180) (size 1.99898 1.99898) (drill 1.09728) (layers *.Cu *.Mask F.SilkS)
      (net 57 "Net-(P3-Pad1)"))
    (model walter/conn_mpt/mpt_0,5-2-2,54.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module w_conn_mpt:mpt_0,5%2f2-2,54 (layer F.Cu) (tedit 512665B4)
    (at 144.9705 78.8035 180)
    (descr "2-way 2.54mm pitch terminal block, Phoenix MPT series")
    (fp_text reference P4 (at 0 -4.50088 180) (layer F.SilkS))
    (fp_text value CONN_01X02 (at 0 4.50088 180) (layer F.SilkS))
    (pad 2 thru_hole oval (at -1.27 0 180) (size 1.99898 1.99898) (drill 1.09728) (layers *.Cu *.Mask F.SilkS)
      (net 58 "Net-(P4-Pad2)"))
    (pad 1 thru_hole rect (at 1.27 0 180) (size 1.99898 1.99898) (drill 1.09728) (layers *.Cu *.Mask F.SilkS)
      (net 59 "Net-(P4-Pad1)"))
    (model walter/conn_mpt/mpt_0,5-2-2,54.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module w_conn_mpt:mpt_0,5%2f2-2,54 (layer F.Cu) (tedit 512665B4)
    (at 161.7345 78.74 180)
    (descr "2-way 2.54mm pitch terminal block, Phoenix MPT series")
    (fp_text reference P5 (at 0 -4.50088 180) (layer F.SilkS))
    (fp_text value CONN_01X02 (at 0 4.50088 180) (layer F.SilkS))
    (pad 2 thru_hole oval (at -1.27 0 180) (size 1.99898 1.99898) (drill 1.09728) (layers *.Cu *.Mask F.SilkS)
      (net 60 "Net-(P5-Pad2)"))
    (pad 1 thru_hole rect (at 1.27 0 180) (size 1.99898 1.99898) (drill 1.09728) (layers *.Cu *.Mask F.SilkS)
      (net 61 "Net-(P5-Pad1)"))
    (model walter/conn_mpt/mpt_0,5-2-2,54.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module w_conn_mpt:mpt_0,5%2f2-2,54 (layer F.Cu) (tedit 512665B4)
    (at 138.938 78.8035 180)
    (descr "2-way 2.54mm pitch terminal block, Phoenix MPT series")
    (fp_text reference P6 (at 0 -4.50088 180) (layer F.SilkS))
    (fp_text value CONN_01X02 (at 0 4.50088 180) (layer F.SilkS))
    (pad 2 thru_hole oval (at -1.27 0 180) (size 1.99898 1.99898) (drill 1.09728) (layers *.Cu *.Mask F.SilkS)
      (net 62 "Net-(P6-Pad2)"))
    (pad 1 thru_hole rect (at 1.27 0 180) (size 1.99898 1.99898) (drill 1.09728) (layers *.Cu *.Mask F.SilkS)
      (net 63 "Net-(P6-Pad1)"))
    (model walter/conn_mpt/mpt_0,5-2-2,54.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module w_conn_mpt:mpt_0,5%2f8-2,54 (layer F.Cu) (tedit 512673E7)
    (at 136.3345 136.271)
    (descr "8-way 2.54mm pitch terminal block, Phoenix MPT series")
    (fp_text reference P7 (at 0 -4.50088) (layer F.SilkS))
    (fp_text value CONN_01X08 (at 0 4.50088) (layer F.SilkS))
    (pad 4 thru_hole oval (at 1.27 0) (size 1.99898 1.99898) (drill 1.09728) (layers *.Cu *.Mask F.SilkS)
      (net 36 /PD7))
    (pad 1 thru_hole rect (at 8.89 0) (size 1.99898 1.99898) (drill 1.09728) (layers *.Cu *.Mask F.SilkS)
      (net 37 /PB0))
    (pad 2 thru_hole oval (at 6.35 0) (size 1.99898 1.99898) (drill 1.09728) (layers *.Cu *.Mask F.SilkS)
      (net 38 /PB1))
    (pad 3 thru_hole oval (at 3.81 0) (size 1.99898 1.99898) (drill 1.09728) (layers *.Cu *.Mask F.SilkS)
      (net 39 /PB2))
    (pad 5 thru_hole oval (at -1.27 0) (size 1.99898 1.99898) (drill 1.09728) (layers *.Cu *.Mask F.SilkS)
      (net 44 /ADC7))
    (pad 6 thru_hole oval (at -3.81 0) (size 1.99898 1.99898) (drill 1.09728) (layers *.Cu *.Mask F.SilkS)
      (net 43 /ADC6))
    (pad 7 thru_hole oval (at -6.35 0) (size 1.99898 1.99898) (drill 1.09728) (layers *.Cu *.Mask F.SilkS)
      (net 1 /GND))
    (pad 8 thru_hole oval (at -8.89 0) (size 1.99898 1.99898) (drill 1.09728) (layers *.Cu *.Mask F.SilkS)
      (net 1 /GND))
    (model walter/conn_mpt/mpt_0,5-8-2,54.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Wire_Pads:SolderWirePad_single_1mmDrill (layer F.Cu) (tedit 0)
    (at 226.027095 182.206)
    (fp_text reference P8 (at 0 -3.81) (layer F.SilkS))
    (fp_text value TST (at -1.905 3.175) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 2.49936 2.49936) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 12 "Net-(C17-Pad1)"))
  )
  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 5415CDEB)
    (at 244.764001 195.516)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R1 (at 0 -2.1) (layer F.SilkS))
    (fp_text value 10k (at 0 2.1) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 10 /Vcc))
    (pad 2 smd rect (at 0.95 0) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 64 "Net-(R1-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 5415CDEB)
    (at 275.934001 163.526)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R2 (at 0 -2.1) (layer F.SilkS))
    (fp_text value 10k (at 0 2.1) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 10 /Vcc))
    (pad 2 smd rect (at 0.95 0) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 65 "Net-(R2-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 5415CDEB)
    (at 254.744001 183.626)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R3 (at 0 -2.1) (layer F.SilkS))
    (fp_text value 10k (at 0 2.1) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 10 /Vcc))
    (pad 2 smd rect (at 0.95 0) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 48 /HOME2))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 5415CDEB)
    (at 251.094001 183.626)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R4 (at 0 -2.1) (layer F.SilkS))
    (fp_text value 10k (at 0 2.1) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 33 /FAULT2))
    (pad 2 smd rect (at 0.95 0) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 10 /Vcc))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 5415CDEB)
    (at 240.934001 195.976)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R5 (at 0 -2.1) (layer F.SilkS))
    (fp_text value 10k (at 0 2.1) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 10 /Vcc))
    (pad 2 smd rect (at 0.95 0) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 47 /HOME1))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 5415CDEB)
    (at 272.284001 163.526)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R6 (at 0 -2.1) (layer F.SilkS))
    (fp_text value 10k (at 0 2.1) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 53 /FAULT1))
    (pad 2 smd rect (at 0.95 0) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 10 /Vcc))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 5415CDEB)
    (at 244.764001 189.216)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R7 (at 0 -2.1) (layer F.SilkS))
    (fp_text value 0.1 (at 0 2.1) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 1 /GND))
    (pad 2 smd rect (at 0.95 0) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 66 "Net-(R7-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 5415CDEB)
    (at 263.364001 172.626)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R8 (at 0 -2.1) (layer F.SilkS))
    (fp_text value 0.1 (at 0 2.1) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 1 /GND))
    (pad 2 smd rect (at 0.95 0) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 67 "Net-(R8-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 5415CDEB)
    (at 267.924001 166.326)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R9 (at 0 -2.1) (layer F.SilkS))
    (fp_text value 0.1 (at 0 2.1) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 1 /GND))
    (pad 2 smd rect (at 0.95 0) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 68 "Net-(R9-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 5415CDEB)
    (at 258.394001 183.626)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R10 (at 0 -2.1) (layer F.SilkS))
    (fp_text value 0.1 (at 0 2.1) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 1 /GND))
    (pad 2 smd rect (at 0.95 0) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 69 "Net-(R10-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 5415CDEB)
    (at 248.768762 196.226)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R11 (at 0 -2.1) (layer F.SilkS))
    (fp_text value 1150 (at 0 2.1) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 26 "Net-(D2-Pad1)"))
    (pad 2 smd rect (at 0.95 0) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 10 /Vcc))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 5415CDEB)
    (at 240.768762 189.676)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R12 (at 0 -2.1) (layer F.SilkS))
    (fp_text value 1600 (at 0 2.1) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 27 "Net-(D3-Pad1)"))
    (pad 2 smd rect (at 0.95 0) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 35 /STEP1))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 5415CDEB)
    (at 279.938762 163.526)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R13 (at 0 -2.1) (layer F.SilkS))
    (fp_text value 1600 (at 0 2.1) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 28 "Net-(D4-Pad1)"))
    (pad 2 smd rect (at 0.95 0) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 40 /PB3))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 5415CDEB)
    (at 240.708762 202.276)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R14 (at 0 -2.1) (layer F.SilkS))
    (fp_text value 1600 (at 0 2.1) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 29 "Net-(D5-Pad1)"))
    (pad 2 smd rect (at 0.95 0) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 52 /TX0))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 5415CDEB)
    (at 263.238762 178.926)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R15 (at 0 -2.1) (layer F.SilkS))
    (fp_text value 1150 (at 0 2.1) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 30 "Net-(D6-Pad1)"))
    (pad 2 smd rect (at 0.95 0) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 51 /RX0))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 5415CDEB)
    (at 271.619238 169.826)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R16 (at 0 -2.1) (layer F.SilkS))
    (fp_text value 4.7k (at 0 2.1) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 10 /Vcc))
    (pad 2 smd rect (at 0.95 0) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 49 /SDA))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 5415CDEB)
    (at 252.109238 189.926)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R17 (at 0 -2.1) (layer F.SilkS))
    (fp_text value 4.7k (at 0 2.1) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 10 /Vcc))
    (pad 2 smd rect (at 0.95 0) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 50 /SCL))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 5415CDEB)
    (at 248.414001 189.926)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R18 (at 0 -2.1) (layer F.SilkS))
    (fp_text value 10k (at 0 2.1) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 10 /Vcc))
    (pad 2 smd rect (at 0.95 0) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 24 /PC6))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 5415CDEB)
    (at 267.014001 172.626)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference RV1 (at 0 -2.1) (layer F.SilkS))
    (fp_text value 10K (at 0 2.1) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(C1-Pad2)"))
    (pad 2 smd rect (at 0.95 0) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 70 "Net-(RV1-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 5415CDEB)
    (at 236.704001 202.276)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference RV2 (at 0 -2.1) (layer F.SilkS))
    (fp_text value 10K (at 0 2.1) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C2-Pad2)"))
    (pad 2 smd rect (at 0.95 0) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 71 "Net-(RV2-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMD_Packages:DIP-8_SMD (layer F.Cu) (tedit 0)
    (at 233.980666 181.427)
    (descr "DIP-8_300 smd shape")
    (tags "smd cms 8dip")
    (attr smd)
    (fp_text reference S1 (at 0.381 -1.143) (layer F.SilkS))
    (fp_text value DIP_4_SWITCH (at 0 0.762) (layer F.Fab))
    (pad 1 smd rect (at -3.81 3.81) (size 1.524 2.032) (layers F.Cu F.Paste F.Mask)
      (net 64 "Net-(R1-Pad2)"))
    (pad 2 smd rect (at -1.27 3.81) (size 1.524 2.032) (layers F.Cu F.Paste F.Mask)
      (net 64 "Net-(R1-Pad2)"))
    (pad 3 smd rect (at 1.27 3.81) (size 1.524 2.032) (layers F.Cu F.Paste F.Mask)
      (net 64 "Net-(R1-Pad2)"))
    (pad 4 smd rect (at 3.81 3.81) (size 1.524 2.032) (layers F.Cu F.Paste F.Mask)
      (net 64 "Net-(R1-Pad2)"))
    (pad 5 smd rect (at 3.81 -3.81) (size 1.524 2.032) (layers F.Cu F.Paste F.Mask)
      (net 72 "Net-(S1-Pad5)"))
    (pad 6 smd rect (at 1.27 -3.81) (size 1.524 2.032) (layers F.Cu F.Paste F.Mask)
      (net 73 "Net-(S1-Pad6)"))
    (pad 7 smd rect (at -1.27 -3.81) (size 1.524 2.032) (layers F.Cu F.Paste F.Mask)
      (net 74 "Net-(S1-Pad7)"))
    (pad 8 smd rect (at -3.81 -3.81) (size 1.524 2.032) (layers F.Cu F.Paste F.Mask)
      (net 75 "Net-(S1-Pad8)"))
    (model SMD_Packages.3dshapes/DIP-8_SMD.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 0.5 0.8))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMD_Packages:DIP-8_SMD (layer F.Cu) (tedit 0)
    (at 247.360666 167.527)
    (descr "DIP-8_300 smd shape")
    (tags "smd cms 8dip")
    (attr smd)
    (fp_text reference S2 (at 0.381 -1.143) (layer F.SilkS))
    (fp_text value DIP_4_SWITCH (at 0 0.762) (layer F.Fab))
    (pad 1 smd rect (at -3.81 3.81) (size 1.524 2.032) (layers F.Cu F.Paste F.Mask)
      (net 65 "Net-(R2-Pad2)"))
    (pad 2 smd rect (at -1.27 3.81) (size 1.524 2.032) (layers F.Cu F.Paste F.Mask)
      (net 65 "Net-(R2-Pad2)"))
    (pad 3 smd rect (at 1.27 3.81) (size 1.524 2.032) (layers F.Cu F.Paste F.Mask)
      (net 65 "Net-(R2-Pad2)"))
    (pad 4 smd rect (at 3.81 3.81) (size 1.524 2.032) (layers F.Cu F.Paste F.Mask)
      (net 65 "Net-(R2-Pad2)"))
    (pad 5 smd rect (at 3.81 -3.81) (size 1.524 2.032) (layers F.Cu F.Paste F.Mask)
      (net 76 "Net-(S2-Pad5)"))
    (pad 6 smd rect (at 1.27 -3.81) (size 1.524 2.032) (layers F.Cu F.Paste F.Mask)
      (net 77 "Net-(S2-Pad6)"))
    (pad 7 smd rect (at -1.27 -3.81) (size 1.524 2.032) (layers F.Cu F.Paste F.Mask)
      (net 78 "Net-(S2-Pad7)"))
    (pad 8 smd rect (at -3.81 -3.81) (size 1.524 2.032) (layers F.Cu F.Paste F.Mask)
      (net 79 "Net-(S2-Pad8)"))
    (model SMD_Packages.3dshapes/DIP-8_SMD.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 0.5 0.8))
      (rotate (xyz 0 0 0))
    )
  )
  (module StepperFootprints:TSSOP-28_4.4x9.7mm_Pitch0.65mmLargeHeatsink (layer F.Cu) (tedit 55DD0ACE)
    (at 167.513 58.2295 270)
    (descr "TSSOP28: plastic thin shrink small outline package; 28 leads; body width 4.4 mm; (see NXP SSOP-TSSOP-VSO-REFLOW.pdf and sot361-1_po.pdf)")
    (tags "SSOP 0.65")
    (attr smd)
    (fp_text reference U1 (at -4.3815 -4.2545 360) (layer F.SilkS))
    (fp_text value DRV8825 (at 0 5.9 270) (layer F.Fab))
    (pad 1 smd rect (at -2.85 -4.225 270) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(C5-Pad1)"))
    (pad 2 smd rect (at -2.85 -3.575 270) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(C5-Pad2)"))
    (pad 3 smd rect (at -2.85 -2.925 270) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 9 /VCP))
    (pad 4 smd rect (at -2.85 -2.275 270) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 4 /Vin))
    (pad 5 smd rect (at -2.85 -1.625 270) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 57 "Net-(P3-Pad1)"))
    (pad 6 smd rect (at -2.85 -0.975 270) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 66 "Net-(R7-Pad2)"))
    (pad 7 smd rect (at -2.85 -0.325 270) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 56 "Net-(P3-Pad2)"))
    (pad 8 smd rect (at -2.85 0.325 270) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 60 "Net-(P5-Pad2)"))
    (pad 9 smd rect (at -2.85 0.975 270) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 67 "Net-(R8-Pad2)"))
    (pad 10 smd rect (at -2.85 1.625 270) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 61 "Net-(P5-Pad1)"))
    (pad 11 smd rect (at -2.85 2.275 270) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 4 /Vin))
    (pad 12 smd rect (at -2.85 2.925 270) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 70 "Net-(RV1-Pad2)"))
    (pad 13 smd rect (at -2.85 3.575 270) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 70 "Net-(RV1-Pad2)"))
    (pad 14 smd rect (at -2.85 4.225 270) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 1 /GND))
    (pad 15 smd rect (at 2.85 4.225 270) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(C1-Pad2)"))
    (pad 16 smd rect (at 2.85 3.575 270) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 10 /Vcc))
    (pad 17 smd rect (at 2.85 2.925 270) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 46 /SLEEP2))
    (pad 18 smd rect (at 2.85 2.275 270) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 33 /FAULT2))
    (pad 19 smd rect (at 2.85 1.625 270) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 72 "Net-(S1-Pad5)"))
    (pad 20 smd rect (at 2.85 0.975 270) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 32 /DIR2))
    (pad 21 smd rect (at 2.85 0.325 270) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 80 "Net-(U1-Pad21)"))
    (pad 22 smd rect (at 2.85 -0.325 270) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 40 /PB3))
    (pad 23 smd rect (at 2.85 -0.975 270) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 81 "Net-(U1-Pad23)"))
    (pad 24 smd rect (at 2.85 -1.625 270) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 75 "Net-(S1-Pad8)"))
    (pad 25 smd rect (at 2.85 -2.275 270) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 74 "Net-(S1-Pad7)"))
    (pad 26 smd rect (at 2.85 -2.925 270) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 73 "Net-(S1-Pad6)"))
    (pad 27 smd rect (at 2.85 -3.575 270) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 48 /HOME2))
    (pad 28 smd rect (at 2.85 -4.225 270) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 1 /GND))
    (pad 1 smd rect (at 0 0 270) (size 3.1 12) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(C5-Pad1)"))
    (model Housings_SSOP.3dshapes/TSSOP-28_4.4x9.7mm_Pitch0.65mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module StepperFootprints:TSSOP-28_4.4x9.7mm_Pitch0.65mmLargeHeatsink (layer F.Cu) (tedit 55DD3F60)
    (at 143.3195 58.42)
    (descr "TSSOP28: plastic thin shrink small outline package; 28 leads; body width 4.4 mm; (see NXP SSOP-TSSOP-VSO-REFLOW.pdf and sot361-1_po.pdf)")
    (tags "SSOP 0.65")
    (attr smd)
    (fp_text reference U2 (at -3.1115 -6.096 180) (layer F.SilkS))
    (fp_text value DRV8825 (at 0 5.9) (layer F.Fab))
    (pad 1 smd rect (at -2.85 -4.225) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(C6-Pad1)"))
    (pad 2 smd rect (at -2.85 -3.575) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(C6-Pad2)"))
    (pad 3 smd rect (at -2.85 -2.925) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 9 /VCP))
    (pad 4 smd rect (at -2.85 -2.275) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 4 /Vin))
    (pad 5 smd rect (at -2.85 -1.625) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 59 "Net-(P4-Pad1)"))
    (pad 6 smd rect (at -2.85 -0.975) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 68 "Net-(R9-Pad2)"))
    (pad 7 smd rect (at -2.85 -0.325) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 58 "Net-(P4-Pad2)"))
    (pad 8 smd rect (at -2.85 0.325) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 62 "Net-(P6-Pad2)"))
    (pad 9 smd rect (at -2.85 0.975) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 69 "Net-(R10-Pad2)"))
    (pad 10 smd rect (at -2.85 1.625) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 63 "Net-(P6-Pad1)"))
    (pad 11 smd rect (at -2.85 2.275) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 4 /Vin))
    (pad 12 smd rect (at -2.85 2.925) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 71 "Net-(RV2-Pad2)"))
    (pad 13 smd rect (at -2.85 3.575) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 71 "Net-(RV2-Pad2)"))
    (pad 14 smd rect (at -2.85 4.225) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 1 /GND))
    (pad 15 smd rect (at 2.85 4.225) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C2-Pad2)"))
    (pad 16 smd rect (at 2.85 3.575) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 10 /Vcc))
    (pad 17 smd rect (at 2.85 2.925) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 45 /SLEEP1))
    (pad 18 smd rect (at 2.85 2.275) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 53 /FAULT1))
    (pad 19 smd rect (at 2.85 1.625) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 76 "Net-(S2-Pad5)"))
    (pad 20 smd rect (at 2.85 0.975) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 34 /DIR1))
    (pad 21 smd rect (at 2.85 0.325) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 82 "Net-(U2-Pad21)"))
    (pad 22 smd rect (at 2.85 -0.325) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 35 /STEP1))
    (pad 23 smd rect (at 2.85 -0.975) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 83 "Net-(U2-Pad23)"))
    (pad 24 smd rect (at 2.85 -1.625) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 79 "Net-(S2-Pad8)"))
    (pad 25 smd rect (at 2.85 -2.275) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 78 "Net-(S2-Pad7)"))
    (pad 26 smd rect (at 2.85 -2.925) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 77 "Net-(S2-Pad6)"))
    (pad 27 smd rect (at 2.85 -3.575) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 47 /HOME1))
    (pad 28 smd rect (at 2.85 -4.225) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 1 /GND))
    (pad 1 smd rect (at 0 0) (size 3.1 12) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(C6-Pad1)"))
    (model Housings_SSOP.3dshapes/TSSOP-28_4.4x9.7mm_Pitch0.65mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SparkFun-Sensors:SHT1X (layer F.Cu) (tedit 55316B9A)
    (at 227.08516 190.450841)
    (descr <b>SHT1x</b>)
    (fp_text reference U3 (at 0 0) (layer Cmts.User) hide)
    (fp_text value SHT1XSMD_SHT1X (at 0 0) (layer Eco1.User) hide)
    (pad 1 smd rect (at -2.667 -1.905 180) (size 1.79832 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 1 /GND))
    (pad 2 smd rect (at -2.667 -0.635 180) (size 1.79832 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 49 /SDA))
    (pad 3 smd rect (at -2.667 0.635 180) (size 1.79832 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 50 /SCL))
    (pad 4 smd rect (at -2.667 1.905 180) (size 1.79832 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 10 /Vcc))
    (pad 5 smd rect (at 2.667 1.905 180) (size 1.79832 0.79756) (layers F.Cu F.Paste F.Mask))
    (pad 6 smd rect (at 2.667 0.635 180) (size 1.79832 0.79756) (layers F.Cu F.Paste F.Mask))
    (pad 7 smd rect (at 2.667 -0.635 180) (size 1.79832 0.79756) (layers F.Cu F.Paste F.Mask))
    (pad 8 smd rect (at 2.667 -1.905 180) (size 1.79832 0.79756) (layers F.Cu F.Paste F.Mask))
  )
  (module Housings_SOIC:SOIC-8_3.9x4.9mm_Pitch1.27mm (layer F.Cu) (tedit 55DD2DA5)
    (at 211.10575 113.77295 90)
    (descr "8-Lead Plastic Small Outline (SN) - Narrow, 3.90 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (attr smd)
    (fp_text reference U4 (at 3.35915 -4.18465 90) (layer F.SilkS))
    (fp_text value LM2675-5.0 (at 0 3.5 90) (layer F.Fab))
    (pad 1 smd rect (at -2.7 -1.905 90) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 19 "Net-(C21-Pad2)"))
    (pad 2 smd rect (at -2.7 -0.635 90) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask))
    (pad 3 smd rect (at -2.7 0.635 90) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask))
    (pad 4 smd rect (at -2.7 1.905 90) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 10 /Vcc))
    (pad 5 smd rect (at 2.7 1.905 90) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 84 "Net-(U4-Pad5)"))
    (pad 6 smd rect (at 2.7 0.635 90) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 /GND))
    (pad 7 smd rect (at 2.7 -0.635 90) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(C18-Pad1)"))
    (pad 8 smd rect (at 2.7 -1.905 90) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(C21-Pad1)"))
    (model Housings_SOIC.3dshapes/SOIC-8_3.9x4.9mm_Pitch1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_SOIC:SOIC-16_3.9x9.9mm_Pitch1.27mm (layer F.Cu) (tedit 54130A77)
    (at 218.684001 184.396)
    (descr "16-Lead Plastic Small Outline (SL) - Narrow, 3.90 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (attr smd)
    (fp_text reference U5 (at 0 -6) (layer F.SilkS))
    (fp_text value MAX232 (at 0 6) (layer F.Fab))
    (pad 1 smd rect (at -2.7 -4.445) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(C19-Pad1)"))
    (pad 2 smd rect (at -2.7 -3.175) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 22 "Net-(C24-Pad1)"))
    (pad 3 smd rect (at -2.7 -1.905) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(C19-Pad2)"))
    (pad 4 smd rect (at -2.7 -0.635) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(C20-Pad1)"))
    (pad 5 smd rect (at -2.7 0.635) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(C20-Pad2)"))
    (pad 6 smd rect (at -2.7 1.905) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 23 "Net-(C25-Pad2)"))
    (pad 7 smd rect (at -2.7 3.175) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 85 "Net-(U5-Pad7)"))
    (pad 8 smd rect (at -2.7 4.445) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 86 "Net-(U5-Pad8)"))
    (pad 9 smd rect (at 2.7 4.445) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 87 "Net-(U5-Pad9)"))
    (pad 10 smd rect (at 2.7 3.175) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 88 "Net-(U5-Pad10)"))
    (pad 11 smd rect (at 2.7 1.905) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 52 /TX0))
    (pad 12 smd rect (at 2.7 0.635) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 51 /RX0))
    (pad 13 smd rect (at 2.7 -0.635) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 54 /RX))
    (pad 14 smd rect (at 2.7 -1.905) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 55 /TX))
    (pad 15 smd rect (at 2.7 -3.175) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 /GND))
    (pad 16 smd rect (at 2.7 -4.445) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 10 /Vcc))
    (model Housings_SOIC.3dshapes/SOIC-16_3.9x9.9mm_Pitch1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module StepperFootprints:AbraconABM3B (layer F.Cu) (tedit 55DCE97D)
    (at 188.582737 151.5565)
    (descr "crystal Abracon ABM3B")
    (fp_text reference X1 (at 0 -2.7305) (layer F.SilkS))
    (fp_text value ABM3B-20.000MHZ-10-1-U-T (at -0.0635 2.9845) (layer F.Fab))
    (pad 1 smd rect (at -2.2 1.3) (size 2 1.4) (layers F.Cu F.Paste F.Mask)
      (net 20 "Net-(C22-Pad2)"))
    (pad 2 smd rect (at 2.2 1.3) (size 2 1.4) (layers F.Cu F.Paste F.Mask)
      (net 89 "Net-(X1-Pad2)"))
    (pad 4 smd rect (at -2.2 -1.3) (size 2 1.4) (layers F.Cu F.Paste F.Mask)
      (net 1 /GND))
    (pad 3 smd rect (at 2.2 -1.3) (size 2 1.4) (layers F.Cu F.Paste F.Mask)
      (net 21 "Net-(C23-Pad2)"))
    (model Crystals_Oscillators_SMD.3dshapes/crystal_FA238-TSX3225.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.24 0.24 0.24))
      (rotate (xyz 0 0 0))
    )
  )
  (module StepperFootprints:DO5022P (layer F.Cu) (tedit 55DD0867)
    (at 198.53275 113.83645 90)
    (fp_text reference L2 (at 0 0.5 90) (layer F.SilkS))
    (fp_text value DO5022P-683MLD (at 0 -0.5 90) (layer F.Fab))
    (pad 1 smd rect (at -8 0 90) (size 3 3) (layers F.Cu F.Paste F.Mask)
      (net 10 /Vcc))
    (pad 2 smd rect (at 8 0 90) (size 3 3) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(C21-Pad1)"))
  )
  (module StepperFootprints:4-40-Plated (layer F.Cu) (tedit 55DD067D)
    (at 132.0165 78.486)
    (fp_text reference "" (at 0 0.5) (layer F.SilkS))
    (fp_text value "" (at 0 -0.5) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 3.81 3.81) (drill 3.048) (layers *.Cu *.Mask F.SilkS))
  )
  (module StepperFootprints:4-40-Plated (layer F.Cu) (tedit 55DD067D)
    (at 132.0165 122.936)
    (fp_text reference "" (at 0 0.5) (layer F.SilkS))
    (fp_text value "" (at 0 -0.5) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 3.81 3.81) (drill 3.048) (layers *.Cu *.Mask F.SilkS))
  )
  (module StepperFootprints:4-40-Plated (layer F.Cu) (tedit 55DD067D)
    (at 176.4665 122.936)
    (fp_text reference "" (at 0 0.5) (layer F.SilkS))
    (fp_text value "" (at 0 -0.5) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 3.81 3.81) (drill 3.048) (layers *.Cu *.Mask F.SilkS))
  )
  (module StepperFootprints:4-40-Plated (layer F.Cu) (tedit 55DD067D)
    (at 176.4665 78.486)
    (fp_text reference "" (at 0 0.5) (layer F.SilkS))
    (fp_text value "" (at 0 -0.5) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 3.81 3.81) (drill 3.048) (layers *.Cu *.Mask F.SilkS))
  )
  (gr_line (start 128.778 75.3745) (end 128.778 126.1745) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 128.778 126.1745) (end 179.578 126.1745) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 179.578 75.3745) (end 179.578 126.1745) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 128.778 75.3745) (end 179.578 75.3745) (angle 90) (layer Edge.Cuts) (width 0.1))
  (zone (net 10) (net_name /Vcc) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.127))
    (min_thickness 0.127)
    (fill (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 213.5505 116.5098) (xy 213.5505 122.6566) (xy 224.6376 122.682) (xy 224.6376 124.4346) (xy 196.0245 124.46)
        (xy 196.0245 109.474) (xy 203.1238 109.4105) (xy 203.073 118.9736) (xy 212.6234 118.9736) (xy 212.6742 116.4971)
        (xy 213.5251 116.5098)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.127))
    (min_thickness 0.127)
    (fill (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 212.2551 118.491) (xy 210.0199 118.4148) (xy 210.0199 116.1161) (xy 212.2551 116.1161)
      )
    )
  )
  (zone (net 19) (net_name "Net-(C21-Pad2)") (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.127))
    (min_thickness 0.127)
    (fill (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 209.5119 116.1161) (xy 209.5119 118.4275) (xy 208.0387 118.4275) (xy 204.978 118.4148) (xy 205.0288 113.9825)
        (xy 207.9625 113.9317) (xy 207.9625 117.5766) (xy 208.8896 117.5893) (xy 208.915 116.0526) (xy 209.4865 116.1161)
      )
    )
  )
  (zone (net 18) (net_name "Net-(C21-Pad1)") (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.127))
    (min_thickness 0.127)
    (fill (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 207.7847 113.3221) (xy 205.0288 113.3221) (xy 205.0542 108.3183) (xy 196.0499 108.2675) (xy 196.0372 103.9368)
        (xy 209.5754 103.9368) (xy 209.55 111.8997) (xy 207.8482 111.9505)
      )
    )
  )
  (zone (net 1) (net_name /GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.127))
    (min_thickness 0.127)
    (fill (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 211.5312 105.2068) (xy 211.5312 104.1654) (xy 214.5538 104.1654) (xy 217.3732 109.5502) (xy 225.1456 109.5248)
        (xy 225.1456 121.9962) (xy 214.7316 121.9581) (xy 214.7697 115.1382) (xy 209.804 115.1128) (xy 209.7786 112.5093)
        (xy 211.3153 112.5093) (xy 211.2899 107.5563) (xy 211.5312 107.4928)
      )
    )
  )
  (zone (net 13) (net_name "Net-(C18-Pad1)") (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.127))
    (min_thickness 0.127)
    (fill (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 225.0313 108.1786) (xy 225.0313 101.5365) (xy 195.8086 101.3714) (xy 195.8594 102.9843) (xy 209.6643 103.0478)
        (xy 210.185 104.013) (xy 210.7565 104.0003) (xy 211.201 103.0859) (xy 215.3666 103.1494) (xy 217.9828 108.2675)
        (xy 224.9805 108.2802)
      )
    )
  )
)
