Functional Requirements 2500 m. LRAUV
1/6/23

1. 2500 m. Safe working depth
2. 1.25 safety factor in Yield / 2.0 Safety factor in Buckling
3. Clear Hull I.D. greater than 12 inch.
4. Hull buoyancy  - 250 lbf. Positive
a. V.B system will be bigger, 2kg. ? , all the wet hardware and sensors will be heavier. We need a weight budget.
5. Neutral Bulk modulus with sea water.
a. [bookmark: _GoBack]Is this necessary?
