September 2026 AUV solar dock deployment notes
Engineer: François Cazenave
Date: 08/28/2026

Moorings length:
Water line to bottom of bridle: 1.2 m
EM Chain: 2 m
Flange adapter: 0.2 m
EM cable: 65 m
Float adapter: 0.8 m
Stretch hose: 15.8 m
Anchor: 0.5 m 
Total length: 85.5 m

Seafloor cable (eye to eye): 28.5 m
Distance between two anchors: 29 m

Deployment line lengths:
Anchor slip line (3/8” red spectra) 200 m
Dock anchor recovery line (3/8” white spectra); approx. 30 m
Popup float line (5/16” red spectra): 135 m 

