PB Docking Update: 6 October, 2011

1. Still planning on conducting Test 2 during the week of October 17th
2. AUV 
a. Daphne still not in the test tank. Depth sensor and GF issues
b.   Docking payload is calibrated, integrated and operational.
3. Dock
a. Next test uses the acoustic modem hanging on a hand deployed mooring
i. Compass is installed in the modem and new firmware (including fast update) is installed and ready for testing.  
b. Mock Dock
i. Mooring
1. Scrambling to find an armored cable solution for the buoy to subsea float.
a. Probably uses Non-CAT5 cable: 2-wire Ethernet
i. Enable-IT Ethernet extender (~8W!)
ii. Patton, or other DSL type
ii. PVC Target – ready to glue
iii. Need a swivel
iv. Anchor, risers, shackles…etc.
c. Electronic design 
i. Camera + encoder in house and transmitting HD video over the radio link at 2 Mbs, but didn’t work at 5 Mbps.  Need to reconfigure the radios
ii. Electrical test/power measurement of camera stuff and relay today or tomorrow.  Followed by a final power budget and locked-down design
d. Mechanical design is at the same point – close but not done
i. Need to finalize and order final electrical components
4. Software
a. Code conversion is done
b. Still chasing bugs  
c. 
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