Team:
Roman and Francois: back deck.
Quinn: boat driving during recovery 
Jim: hydraulics
Brett: winch if needed and deck assistant

Before recovery:

- Set winch gear to low.
- Clear winch of long line if needed.
- Secure large plastic bin to deck.
- Install small block. 
- Prepare short winch line through block
- prepare heavy line over A-frame for buoy recovery
- verify acoustic release deck box and bring codes

Recovery plan

1- Drive boat 100 m from the buoy

2- trigger acoustic pop float

3- acquire pop up float. Detach float from line and attach to winch line

4- lift main anchor from seafloor and keep going up about 30 meters more so that docking anchor is also off the seafloor. 

5- Let boat align with wind/current so that the buoy is trailing behind the boat.

6- keep lifting main anchor and set it on the deck. Secure anchor with line.

7- Detach winch line from anchor and tie it to the second recovery line that is zip-tied to the seafloor cable.

8 - Recover dock anchor using winch (cut zip-ties as they come up and set it on the port side of the deck). Put cable in bin.

9- Recover AUV dock by hand and set it on the port side of the deck


10 - Recover stretch hose by hand (might need capstan assistance for float)
11- Recover EM cable (50 m long) by hand and put in bin


[bookmark: _GoBack]12 - Using large line going over A-frame and capstan, recover the buoy and set it on the deck, solar panel facing aft.
