List of DORN fittings on docking buoy:
04/24/2023, Francois Cazenave
Junction box
8 x solar panel cables, cable diameter: 0.237”
NYST-1-001 + NYST-16-005
1 x 14-conductor cable to main box, diameter:  0.480”
NYST-1-002 + NYST-17-005

Main Box
1 x 14-conductor cable to junction box, diameter:  0.480”
NYST-1-002 + NYST-17-005
2 x Cell modem antenna, diameter: cable diameter 0.196”
NYST-1-001 + NYST-16-004
1 x WIFI antenna
NYST-1-001 + NYST-16-006
1 x Tether to dock. Cable diameter 0.33”
NYST-1-002 + NYST-17-001 or 002
1 x Ground wire
NYST-1-001 + NYST-16-001
[bookmark: _GoBack]1 x charge cable
NYST-1-001





