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H.Lundin, 6-14-99

ASSEMBLY PROCESS, MOTOR CONTROLLER HEAT SINK ASSEMBLY SEQUENCE.

Drawing 100514.DWG.

Note: Loctite No: 243 to be used on all threaded fasteners, per above assembly dwg. 

1.
Install Heli-coils, 4 each in Heatsink wedge. 


Dwg. 100487DWG.

2.
Attach Driveblock using Thermagon compound. See process sheet. No:100595.doc

3. Fasten Bulkhead assembly, item 9 to Item 1, with shoulder screws,

4 ea.
Torque to 5 in/lbs.




Dwg. 100514DWG

4.
Install Standoff legs. Item 2 & 6.




“   “

5.
Add Disc Springs & Standoff Bushing. Items 5, 7 & 13,

“   “

6.
Install clamp bridges Item , 2 ea. Onto standoffs.


“   “

7.
Install Heatsink clamp assy. Item 3.




“   “

8.
Install plastic Capacitor Clamp, Item 11.



“   “

9. Re-check all fasteners for tightness.
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