InertialSense SSH Commands:


To view RTK status:
· tail -f /data/is_status.log
· Control +C to exit.
· screen -r inertial_sense
· Use control+a, control+d to exit screen
· df -h
· See SD card status
· sudo systemctl start is_logging.service
· Starts logging
