VN-300 Blueboat Installation
· EAHRS_TYPE = 1 (VectorNav)
· EAHRS_SENSORS = 15 (all)
· EAHRS_RATE = 50 (set this up in control center software)
· GPS_TYPE = 21 (ExternalAHRS)
· GPS_TYPE2 = 21 (ExternalAHRS)
· SerialX_Protocol = 36 (AHRS) – Whichever serial port the VN-300 is plugged into, change this parameter
· SerialX_Baud = 115 (Confirm Baud of VN-300)
· AHRS_EKF_TYPE = 11 (External AHRS)
· SERIAL3_Options -> Used as null modem (if needed)

INS_USE

Others:
· WP_SPEED – this is the speed of the vessel in auto mode.



More info here
