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 Operation Checklist


Start Up
	
· Verify pre-cruise has been submitted
· Identify Shore Contact, fill out Float Plan & deliver to manifest box
· Fill out visitor waivers and deposit in manifest box if required
· Fill out Cruise Log
· Determine if fuel is sufficient for trip (dip if any uncertainty of level)
· Engine Power PERKO- Switch ON
· House Power PERKO- Switch ON
· Check high water alarm
· Check fuel level in gas hydraulics motor and refill if low
· Run blowers for 3 minutes prior to starting engines
· Remove engine covers and lower engines
· Center and secure boom
· Tie down and secure loads
· Secure anchor, chain and winch 
· Set one VHF Radio to channel 16
· Turn on Garmin displays
· Brief new passengers on vessel safety 
· Hazard of falling overboard
· Man overboard procedure – ring, sling, throw bag, and cargo net
· Whereabouts of PFDs and survival suits
· Requirements for work vests, hardhats, and steel-toed shoes
· Watch head on boom capstan and T-bit
· Radar – make sure it is off before going forward
· Emergency communication on VHF 16, Garmin DSC, SPOT, cell phones and EPIRB
· Fire extinguishers – location and procedure 
· First Aid and AED locations
· Location of Flares 
· Abandon ship – Mayday call, Don immersion suit, take EPIRB and ditch bag, stay with vessel as long as possible, stay together
· Confirm that everyone on deck is wearing work vests
· Cast off once crew is ready 


	
Underway

· Confirm lines and buoys are inboard and secured
· Confirm passengers on back deck are wearing proper safety gear
· Turn on navigation lights in restricted visibility
· Turn on radar in restricted visibility
· Monitor blind spot for hazards
· Monitor engine diagnostics
· Always ask whether the crew and passengers are ready before accelerating

Shut Down

· Fuel boat if under 100 gallons on board
· Notify shore contact of your safe return
· Complete logs- Cruise, Maintenance, and Fuel logs 
· Rinse Engines through cowling when vertical for 30 seconds each
· Raise Engines 
· Rinse exterior of engines, bracket and tie-bar thoroughly
· Gravity flush engines 5 minutes apiece – DO NOT START ENGINE
· Replace rinse-hose fittings on engine 
· Rinse boat thoroughly including windows, deck, and anchor winch
· Rinse water off windows with RO and Rain-X sprayer.
· Empty trash
· Stow work vests and hardhats NEATLY in V-berth
· Close and lock windows 
· Tidy up the V-berth and cabin
· Clean Garmin monitors if smudges – ONLY use the cleaning kit stored behind the helm seat
· Replace covers on GPS and engine display
· Turn Engine Power PERKO Switch OFF
· Turn House Power PERKO Switch OFF
· Turn inverter OFF
· Confirm all tools are clean and returned
· Rinse lines and hang on the rail aft of the helm
· Rinse and bundle ratchet straps.  Stow in green bin in cabin.
· Center and secure the boom.  Add half hitch on a bight to both side-lines.
· Lock cabin and aft hatch with combo locks oriented right-side-up
· Stow and depressurize the dock hose - run the hose down and back on the Flyer dock
· Confirm the boat is secured to dock properly (Fenders in place and lines secure to cleats)
· Finish lines with a Flemish Flake (yes please.  It is quite nice)
· Plug in sealion electric fence on Flyer dock.
· Replace the caution sign at top of ramp on exit.


Fueling

· Dip fuel tanks and note volume of each tank in cruise log
· [bookmark: _GoBack]Insert fuel nozzle and make contact with the fill port to discharge static 
· Fuel with 89 Octane gas to a volume of 100 gallons in the saddle tanks
· Do NOT leave the nozzle while filling
· Add Ring Free Plus to fuel (1 oz/10 gallons)
· Fill out Cruise Log
· Fill out Fuel Log
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