Configuration for bench test on 6/17/23
Power: Hooked to port C1 on Daphne
App Settings: 1080/60/Continuous
Controller Settings: EF: 20, EF: 20, ES: 00
Warp Speed.  Samples from 20 to 00 every hour.  Should generate 2 files.  One about 24 minutes and the other about 16 minutes.

First record should start at 11:20 AM on 6/17 (18:20 GMT)

Setup:

Invalid command. Type "help" for more.
> help 
The following commands are available:
  help
  event
  power
  button
  wifi
  record
  clock
  battery
  deploy

You can for instance type "help clock" for more info on the clock command.
> power on 
Turning on the camera power.
> wifi 
Pressing the wifi button.
> wifi 
Pressing the wifi button.
> wifi 
Pressing the wifi button.
> wifiPressing the wifi button.
> wifi 
Pressing the wifi button.
> wifi 
Pressing the wifi button.
> wifi 
Pressing the wifi button.
> wifi 
Pressing the wifi button.
> wifi 
Pressing the wifi button.
> wifi 
Pressing the wifi button.
> clock set 
Enter current time (HHMM, 24-hour format): 0040
Clock set to 40
> clock set 
Enter current time (HHMM, 24-hour format): 0041
Clock set to 41
> clock set 
Enter current time (HHMM, 24-hour format): 1741
Clock set to 1741
> event first
Invalid command. Type "help event" to see how to use the event command.
> event firs 
Invalid command. Type "help event" to see how to use the event command.
> event first 

Enter camera start time for first day (HHMM, 24-hour format): 0020
First time set to 0020
> event start 
Enter camera start time (HHMM, 24-hour format): 0020
Start time set to 0020
> event stop 
Enter camera stop time (HHMM, 24-hour format): 0000
Stop time set to 0000
> event list 
First time is 0020
Start time is 0020
Stop time is  0000
> battery main 
Main battery is at 8.92 V
> battery cont 
Controller battery is at 4.26 V
> deploy 
Are you sure you want to deploy the camera? [y/n] y
Deployment started.
Disconnect USB cable now.
Camera will record for 1 minute before sleep.
Turning on the camera power.
Pressing the record button.