(kicad_sch (version 20211123) (generator eeschema)
  (paper "A4")
  (lib_symbols
    (symbol "Device:C" (pin_numbers hide) (pin_names (offset 0.254)) (in_bom yes) (on_board yes)
      (property "Reference" "C" (id 0) (at 0.635 2.54 0))
      (property "Value" "C" (id 1) (at 0.635 -2.54 0))
      (property "Footprint" "" (id 2) (at 0.9652 -3.81 0))
      (property "Datasheet" "~" (id 3) (at 0 0 0))
      (property "ki_keywords" "cap capacitor" (id 4) (at 0 0 0))
      (property "ki_description" "Unpolarized capacitor" (id 5) (at 0 0 0))
      (property "ki_fp_filters" "C_*" (id 6) (at 0 0 0))
      (symbol "C_0_1"
        (polyline
          (pts
            (xy -2.032 -0.762)
            (xy 2.032 -0.762)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -2.032 0.762)
            (xy 2.032 0.762)
          )
          (fill (type none))
        )
      )
      (symbol "C_1_1"
        (pin passive line (at 0 3.81 270) (length 2.794)
          (name "~")
          (number "1")
        )
        (pin passive line (at 0 -3.81 90) (length 2.794)
          (name "~")
          (number "2")
        )
      )
    )
  )
  (junction (at 162.56 78.74) (diameter 0) (color 0 0 0 0))
  (junction (at 182.88 68.58) (diameter 0) (color 0 0 0 0))
  (junction (at 132.08 78.74) (diameter 0) (color 0 0 0 0))
  (junction (at 172.72 78.74) (diameter 0) (color 0 0 0 0))
  (junction (at 121.92 68.58) (diameter 0) (color 0 0 0 0))
  (junction (at 142.24 68.58) (diameter 0) (color 0 0 0 0))
  (junction (at 162.56 68.58) (diameter 0) (color 0 0 0 0))
  (junction (at 111.76 68.58) (diameter 0) (color 0 0 0 0))
  (junction (at 152.4 78.74) (diameter 0) (color 0 0 0 0))
  (junction (at 101.6 78.74) (diameter 0) (color 0 0 0 0))
  (junction (at 172.72 68.58) (diameter 0) (color 0 0 0 0))
  (junction (at 182.88 78.74) (diameter 0) (color 0 0 0 0))
  (junction (at 121.92 78.74) (diameter 0) (color 0 0 0 0))
  (junction (at 152.4 68.58) (diameter 0) (color 0 0 0 0))
  (junction (at 142.24 78.74) (diameter 0) (color 0 0 0 0))
  (junction (at 132.08 68.58) (diameter 0) (color 0 0 0 0))
  (junction (at 111.76 78.74) (diameter 0) (color 0 0 0 0))
  (junction (at 101.6 68.58) (diameter 0) (color 0 0 0 0))
  (wire (pts (xy 152.4 68.58) (xy 152.4 69.85)))
  (wire (pts (xy 132.08 68.58) (xy 121.92 68.58)))
  (wire (pts (xy 111.76 77.47) (xy 111.76 78.74)))
  (wire (pts (xy 152.4 78.74) (xy 142.24 78.74)))
  (wire (pts (xy 111.76 68.58) (xy 101.6 68.58)))
  (wire (pts (xy 152.4 68.58) (xy 142.24 68.58)))
  (wire (pts (xy 132.08 68.58) (xy 132.08 69.85)))
  (wire (pts (xy 172.72 68.58) (xy 162.56 68.58)))
  (wire (pts (xy 132.08 77.47) (xy 132.08 78.74)))
  (wire (pts (xy 182.88 69.85) (xy 182.88 68.58)))
  (wire (pts (xy 182.88 68.58) (xy 193.04 68.58)))
  (wire (pts (xy 172.72 68.58) (xy 172.72 69.85)))
  (wire (pts (xy 172.72 77.47) (xy 172.72 78.74)))
  (wire (pts (xy 121.92 77.47) (xy 121.92 78.74)))
  (wire (pts (xy 111.76 78.74) (xy 101.6 78.74)))
  (wire (pts (xy 152.4 77.47) (xy 152.4 78.74)))
  (wire (pts (xy 142.24 68.58) (xy 132.08 68.58)))
  (wire (pts (xy 132.08 78.74) (xy 121.92 78.74)))
  (wire (pts (xy 101.6 68.58) (xy 101.6 69.85)))
  (wire (pts (xy 193.04 77.47) (xy 193.04 78.74)))
  (wire (pts (xy 121.92 68.58) (xy 121.92 69.85)))
  (wire (pts (xy 193.04 68.58) (xy 193.04 69.85)))
  (wire (pts (xy 121.92 78.74) (xy 111.76 78.74)))
  (wire (pts (xy 193.04 78.74) (xy 182.88 78.74)))
  (wire (pts (xy 182.88 68.58) (xy 172.72 68.58)))
  (wire (pts (xy 142.24 78.74) (xy 132.08 78.74)))
  (wire (pts (xy 101.6 78.74) (xy 91.44 78.74)))
  (wire (pts (xy 162.56 68.58) (xy 162.56 69.85)))
  (wire (pts (xy 101.6 77.47) (xy 101.6 78.74)))
  (wire (pts (xy 172.72 78.74) (xy 162.56 78.74)))
  (wire (pts (xy 162.56 77.47) (xy 162.56 78.74)))
  (wire (pts (xy 121.92 68.58) (xy 111.76 68.58)))
  (wire (pts (xy 182.88 78.74) (xy 172.72 78.74)))
  (wire (pts (xy 142.24 68.58) (xy 142.24 69.85)))
  (wire (pts (xy 111.76 68.58) (xy 111.76 69.85)))
  (wire (pts (xy 101.6 68.58) (xy 91.44 68.58)))
  (wire (pts (xy 162.56 78.74) (xy 152.4 78.74)))
  (wire (pts (xy 162.56 68.58) (xy 152.4 68.58)))
  (wire (pts (xy 142.24 77.47) (xy 142.24 78.74)))
  (wire (pts (xy 182.88 77.47) (xy 182.88 78.74)))
  (label "V_XD16_A" (at 154.305 68.58 0))
  (label "GND" (at 156.845 78.74 0))
  (hierarchical_label "Kathode" (shape bidirectional) (at 91.44 78.74 180))
  (hierarchical_label "Anode" (shape bidirectional) (at 91.44 68.58 180))
  (symbol (lib_id "Device:C") (at 152.4 73.66 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "C51" (id 0) (at 154.94 71.12 0))
    (property "Value" "22uF" (id 1) (at 154.94 76.2 0))
    (property "Footprint" "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder" (id 2) (at 153.3652 77.47 0))
    (property "Datasheet" "https://product.tdk.com/en/search/capacitor/ceramic/mlcc/info?part_no=C2012X6S1C226M125AC&utm_source=mlcc_commercial_general_en.pdf&utm_medium=catalog" (id 3) (at 152.4 73.66 0))
    (property "PartNum" "C2012X6S1C226M125AC" (id 4) (at 152.4 73.66 0))
    (property "Digikey" "445-11435-1-ND" (id 5) (at 152.4 73.66 0))
    (property "Mouser" "" (id 6) (at 152.4 73.66 0))
    (property "Other" "" (id 7) (at 152.4 73.66 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Device:C") (at 142.24 73.66 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "C50" (id 0) (at 144.78 71.12 0))
    (property "Value" "22uF" (id 1) (at 144.78 76.2 0))
    (property "Footprint" "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder" (id 2) (at 143.2052 77.47 0))
    (property "Datasheet" "https://product.tdk.com/en/search/capacitor/ceramic/mlcc/info?part_no=C2012X6S1C226M125AC&utm_source=mlcc_commercial_general_en.pdf&utm_medium=catalog" (id 3) (at 142.24 73.66 0))
    (property "PartNum" "C2012X6S1C226M125AC" (id 4) (at 142.24 73.66 0))
    (property "Digikey" "445-11435-1-ND" (id 5) (at 142.24 73.66 0))
    (property "Mouser" "" (id 6) (at 142.24 73.66 0))
    (property "Other" "" (id 7) (at 142.24 73.66 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Device:C") (at 162.56 73.66 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "C52" (id 0) (at 165.1 71.12 0))
    (property "Value" "22uF" (id 1) (at 165.1 76.2 0))
    (property "Footprint" "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder" (id 2) (at 163.5252 77.47 0))
    (property "Datasheet" "https://product.tdk.com/en/search/capacitor/ceramic/mlcc/info?part_no=C2012X6S1C226M125AC&utm_source=mlcc_commercial_general_en.pdf&utm_medium=catalog" (id 3) (at 162.56 73.66 0))
    (property "PartNum" "C2012X6S1C226M125AC" (id 4) (at 162.56 73.66 0))
    (property "Digikey" "445-11435-1-ND" (id 5) (at 162.56 73.66 0))
    (property "Mouser" "" (id 6) (at 162.56 73.66 0))
    (property "Other" "" (id 7) (at 162.56 73.66 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Device:C") (at 182.88 73.66 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "C54" (id 0) (at 185.42 71.12 0))
    (property "Value" "22uF" (id 1) (at 185.42 76.2 0))
    (property "Footprint" "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder" (id 2) (at 183.8452 77.47 0))
    (property "Datasheet" "https://product.tdk.com/en/search/capacitor/ceramic/mlcc/info?part_no=C2012X6S1C226M125AC&utm_source=mlcc_commercial_general_en.pdf&utm_medium=catalog" (id 3) (at 182.88 73.66 0))
    (property "PartNum" "C2012X6S1C226M125AC" (id 4) (at 182.88 73.66 0))
    (property "Digikey" "445-11435-1-ND" (id 5) (at 182.88 73.66 0))
    (property "Mouser" "" (id 6) (at 182.88 73.66 0))
    (property "Other" "" (id 7) (at 182.88 73.66 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Device:C") (at 132.08 73.66 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "C49" (id 0) (at 134.62 71.12 0))
    (property "Value" "22uF" (id 1) (at 134.62 76.2 0))
    (property "Footprint" "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder" (id 2) (at 133.0452 77.47 0))
    (property "Datasheet" "https://product.tdk.com/en/search/capacitor/ceramic/mlcc/info?part_no=C2012X6S1C226M125AC&utm_source=mlcc_commercial_general_en.pdf&utm_medium=catalog" (id 3) (at 132.08 73.66 0))
    (property "PartNum" "C2012X6S1C226M125AC" (id 4) (at 132.08 73.66 0))
    (property "Digikey" "445-11435-1-ND" (id 5) (at 132.08 73.66 0))
    (property "Mouser" "" (id 6) (at 132.08 73.66 0))
    (property "Other" "" (id 7) (at 132.08 73.66 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Device:C") (at 121.92 73.66 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "C48" (id 0) (at 124.46 71.12 0))
    (property "Value" "22uF" (id 1) (at 124.46 76.2 0))
    (property "Footprint" "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder" (id 2) (at 122.8852 77.47 0))
    (property "Datasheet" "https://product.tdk.com/en/search/capacitor/ceramic/mlcc/info?part_no=C2012X6S1C226M125AC&utm_source=mlcc_commercial_general_en.pdf&utm_medium=catalog" (id 3) (at 121.92 73.66 0))
    (property "PartNum" "C2012X6S1C226M125AC" (id 4) (at 121.92 73.66 0))
    (property "Digikey" "445-11435-1-ND" (id 5) (at 121.92 73.66 0))
    (property "Mouser" "" (id 6) (at 121.92 73.66 0))
    (property "Other" "" (id 7) (at 121.92 73.66 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Device:C") (at 111.76 73.66 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "C47" (id 0) (at 114.3 71.12 0))
    (property "Value" "22uF" (id 1) (at 114.3 76.2 0))
    (property "Footprint" "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder" (id 2) (at 112.7252 77.47 0))
    (property "Datasheet" "https://product.tdk.com/en/search/capacitor/ceramic/mlcc/info?part_no=C2012X6S1C226M125AC&utm_source=mlcc_commercial_general_en.pdf&utm_medium=catalog" (id 3) (at 111.76 73.66 0))
    (property "PartNum" "C2012X6S1C226M125AC" (id 4) (at 111.76 73.66 0))
    (property "Digikey" "445-11435-1-ND" (id 5) (at 111.76 73.66 0))
    (property "Mouser" "" (id 6) (at 111.76 73.66 0))
    (property "Other" "" (id 7) (at 111.76 73.66 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Device:C") (at 172.72 73.66 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "C53" (id 0) (at 175.26 71.12 0))
    (property "Value" "22uF" (id 1) (at 175.26 76.2 0))
    (property "Footprint" "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder" (id 2) (at 173.6852 77.47 0))
    (property "Datasheet" "https://product.tdk.com/en/search/capacitor/ceramic/mlcc/info?part_no=C2012X6S1C226M125AC&utm_source=mlcc_commercial_general_en.pdf&utm_medium=catalog" (id 3) (at 172.72 73.66 0))
    (property "PartNum" "C2012X6S1C226M125AC" (id 4) (at 172.72 73.66 0))
    (property "Digikey" "445-11435-1-ND" (id 5) (at 172.72 73.66 0))
    (property "Mouser" "" (id 6) (at 172.72 73.66 0))
    (property "Other" "" (id 7) (at 172.72 73.66 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Device:C") (at 193.04 73.66 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "C55" (id 0) (at 195.58 71.12 0))
    (property "Value" "22uF" (id 1) (at 195.58 76.2 0))
    (property "Footprint" "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder" (id 2) (at 194.0052 77.47 0))
    (property "Datasheet" "https://product.tdk.com/en/search/capacitor/ceramic/mlcc/info?part_no=C2012X6S1C226M125AC&utm_source=mlcc_commercial_general_en.pdf&utm_medium=catalog" (id 3) (at 193.04 73.66 0))
    (property "PartNum" "C2012X6S1C226M125AC" (id 4) (at 193.04 73.66 0))
    (property "Digikey" "445-11435-1-ND" (id 5) (at 193.04 73.66 0))
    (property "Mouser" "" (id 6) (at 193.04 73.66 0))
    (property "Other" "" (id 7) (at 193.04 73.66 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Device:C") (at 101.6 73.66 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "C46" (id 0) (at 104.14 71.12 0))
    (property "Value" "22uF" (id 1) (at 104.14 76.2 0))
    (property "Footprint" "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder" (id 2) (at 102.5652 77.47 0))
    (property "Datasheet" "https://product.tdk.com/en/search/capacitor/ceramic/mlcc/info?part_no=C2012X6S1C226M125AC&utm_source=mlcc_commercial_general_en.pdf&utm_medium=catalog" (id 3) (at 101.6 73.66 0))
    (property "PartNum" "C2012X6S1C226M125AC" (id 4) (at 101.6 73.66 0))
    (property "Digikey" "445-11435-1-ND" (id 5) (at 101.6 73.66 0))
    (property "Mouser" "" (id 6) (at 101.6 73.66 0))
    (property "Other" "" (id 7) (at 101.6 73.66 0))
    (pin "1")
    (pin "2")
  )
)
