(kicad_pcb (version 20211014) (generator pcbnew)
  (general
    (thickness 4.69)
  )
  (paper "A4")
  (layers
    (0 "F.Cu" signal)
    (1 "In1.Cu" signal)
    (2 "In2.Cu" signal)
    (31 "B.Cu" signal)
    (32 "B.Adhes" user "B.Adhesive")
    (33 "F.Adhes" user "F.Adhesive")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (43 "Eco2.User" user "User.Eco2")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
    (50 "User.1" user)
    (51 "User.2" user)
    (52 "User.3" user)
    (53 "User.4" user)
    (54 "User.5" user)
    (55 "User.6" user)
    (56 "User.7" user)
    (57 "User.8" user)
    (58 "User.9" user)
  )
  (setup
    (stackup
      (layer "F.SilkS" (type "Top Silk Screen"))
      (layer "F.Paste" (type "Top Solder Paste"))
      (layer "F.Mask" (type "Top Solder Mask") (thickness 0.01))
      (layer "F.Cu" (type "copper") (thickness 0.035))
      (layer "dielectric 1" (type "core") (thickness 1.51) (material "FR4") (epsilon_r 4.5) (loss_tangent 0.02))
      (layer "In1.Cu" (type "copper") (thickness 0.035))
      (layer "dielectric 2" (type "prepreg") (thickness 1.51) (material "FR4") (epsilon_r 4.5) (loss_tangent 0.02))
      (layer "In2.Cu" (type "copper") (thickness 0.035))
      (layer "dielectric 3" (type "core") (thickness 1.51) (material "FR4") (epsilon_r 4.5) (loss_tangent 0.02))
      (layer "B.Cu" (type "copper") (thickness 0.035))
      (layer "B.Mask" (type "Bottom Solder Mask") (thickness 0.01))
      (layer "B.Paste" (type "Bottom Solder Paste"))
      (layer "B.SilkS" (type "Bottom Silk Screen"))
      (copper_finish "None")
      (dielectric_constraints no)
    )
    (pad_to_mask_clearance 0)
    (grid_origin 74.1172 127.5334)
    (pcbplotparams
      (layerselection 0x00010fc_ffffffff)
      (disableapertmacros false)
      (usegerberextensions true)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile false)
      (svguseinch false)
      (svgprecision 6)
      (excludeedgelayer true)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue false)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "fab/")
    )
  )
  (net 0 "")
  (net 1 "VCC")
  (net 2 "GND")
  (net 3 "/~{BRD_WAKE}")
  (net 4 "Net-(R1-Pad1)")
  (net 5 "/VD2_I2C_SDA")
  (net 6 "/VD2_I2C_SCL")
  (net 7 "/~{SLEEP}")
  (net 8 "/~{SPI_CS}")
  (net 9 "/RX1_232")
  (net 10 "/BRD_WAKE_P")
  (net 11 "/CLK_OUT")
  (net 12 "/~{RTC_ALARM}")
  (net 13 "/~{VREG_EN}")
  (net 14 "/VREG_EN")
  (net 15 "/EVENT_CNT")
  (net 16 "/VIN")
  (net 17 "/PWR GOOD")
  (net 18 "/I2C_SDA")
  (net 19 "/I2C_SCL")
  (net 20 "Net-(D3-Pad1)")
  (net 21 "/~{PROC_SLEEP}")
  (net 22 "Net-(C8-Pad1)")
  (net 23 "Net-(C8-Pad2)")
  (net 24 "Net-(C9-Pad2)")
  (net 25 "Net-(Q1-Pad5)")
  (net 26 "Net-(Q2-Pad6)")
  (net 27 "Net-(Q4-Pad5)")
  (net 28 "/+3Vx_ON")
  (net 29 "Net-(R8-Pad2)")
  (net 30 "Net-(R19-Pad2)")
  (net 31 "Net-(D5-Pad1)")
  (net 32 "/+3Vx")
  (net 33 "unconnected-(C3-Pad1)")
  (net 34 "Net-(R9-Pad2)")
  (net 35 "unconnected-(U5-Pad4)")
  (net 36 "Net-(C3-Pad2)")
  (net 37 "Net-(C16-Pad2)")
  (net 38 "Net-(C10-Pad2)")
  (net 39 "unconnected-(D6-Pad1)")
  (net 40 "unconnected-(D6-Pad2)")
  (net 41 "Net-(R23-Pad2)")
  (footprint "ProjectFootprints:MSOP-10_MSE" (layer "F.Cu")
    (tedit 62DAC03F)
    (at 87.5284 121.5136)
    (property "Sheetfile" "wakestr_min_v1_2.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "U4" (at -2.8448 -1.7272) (layer "F.SilkS"))
    (fp_text value "LT3991EMS-ADJ" (at -0.7874 1.8034 270) (layer "F.Fab"))
    (pad "1" smd rect locked (at -2.1844 -1.00076) (size 1.397 0.2794) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 32 "/+3Vx") (pinfunction "BD") (pintype "input"))
    (pad "2" smd rect locked (at -2.1844 -0.500381) (size 1.397 0.2794) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 22 "Net-(C8-Pad1)") (pinfunction "BOOST") (pintype "output"))
    (pad "3" smd rect locked (at -2.1844 0) (size 1.397 0.2794) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 23 "Net-(C8-Pad2)") (pinfunction "SW") (pintype "output"))
    (pad "4" smd rect locked (at -2.1844 0.500381) (size 1.397 0.2794) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 16 "/VIN") (pinfunction "VIN") (pintype "input"))
    (pad "5" smd rect locked (at -2.1844 1.00076) (size 1.397 0.2794) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 14 "/VREG_EN") (pinfunction "EN") (pintype "input"))
    (pad "6" smd rect locked (at 2.1844 1.00076) (size 1.397 0.2794) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 38 "Net-(C10-Pad2)") (pinfunction "FB") (pintype "input"))
    (pad "7" smd rect locked (at 2.1844 0.500381) (size 1.397 0.2794) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 41 "Net-(R23-Pad2)") (pinfunction "SS") (pintype "input"))
    (pad "8" smd rect locked (at 2.1844 0) (size 1.397 0.2794) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 30 "Net-(R19-Pad2)") (pinfunction "RT") (pintype "input"))
    (pad "9" smd rect locked (at 2.1844 -0.500381) (size 1.397 0.2794) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 17 "/PWR GOOD") (pinfunction "PG") (pintype "output"))
    (pad "10" smd rect locked (at 2.1844 -1.00076) (size 1.397 0.2794) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pinfunction "SYNC") (pintype "input"))
    (pad "11" smd rect locked (at 0 0) (size 1.9304 2.159) (layers "F.Cu" "F.Mask")
      (net 2 "GND") (pinfunction "GND") (pintype "input"))
    (model "C:/Dropbox/KiCAD/3DModels/msop-10.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Diode_SMD:D_0603_1608Metric_Pad1.05x0.95mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEF0)
    (at 96.6724 111.6584 -90)
    (descr "Diode SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "diode handsolder")
    (property "Sheetfile" "wakestr_min_v1_2.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "D1" (at -2.6924 -0.1016 180) (layer "F.SilkS"))
    (fp_text value "‎B0240R‎" (at 0 -0.0254 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.875 0 270) (size 1.05 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "VCC") (pinfunction "K") (pintype "passive"))
    (pad "2" smd roundrect (at 0.875 0 270) (size 1.05 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 36 "Net-(C3-Pad2)") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Diode_SMD.3dshapes/D_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Diode_SMD:D_0603_1608Metric_Pad1.05x0.95mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEF0)
    (at 91.948 105.4608)
    (descr "Diode SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "diode handsolder")
    (property "Sheetfile" "wakestr_min_v1_2.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "D3" (at -0.0254 -1.2446) (layer "F.SilkS"))
    (fp_text value "‎B0240R‎" (at -0.254 -0.0254) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.875 0) (size 1.05 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 20 "Net-(D3-Pad1)") (pinfunction "K") (pintype "passive"))
    (pad "2" smd roundrect (at 0.875 0) (size 1.05 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Diode_SMD.3dshapes/D_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEF)
    (at 86.066053 116.5598 90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "wakestr_min_v1_2.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C14" (at 2.5392 -0.010853 270) (layer "F.SilkS"))
    (fp_text value "10uF" (at 0.0836 0.03 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.5392 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.8625 0 90) (size 1.075 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 32 "/+3Vx") (pintype "passive"))
    (pad "2" smd roundrect (at 0.8625 0 90) (size 1.075 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEF)
    (at 83.44 120.15 -90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "wakestr_min_v1_2.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C8" (at 2.1256 0.0264 180) (layer "F.SilkS"))
    (fp_text value "0.47uF" (at 0.7112 0.1016 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.8625 0 270) (size 1.075 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 22 "Net-(C8-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.8625 0 270) (size 1.075 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 23 "Net-(C8-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEF)
    (at 107.1372 121.9454 -90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "wakestr_min_v1_2.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C4" (at 2.032 0.127 180) (layer "F.SilkS"))
    (fp_text value "100nF" (at -0.1524 0.0762 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.0574 0.1524 180) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.8625 0 270) (size 1.075 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 32 "/+3Vx") (pintype "passive"))
    (pad "2" smd roundrect (at 0.8625 0 270) (size 1.075 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 90.9574 126.5428)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "wakestr_min_v1_2.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R18" (at -2.54 0.0254) (layer "F.SilkS"))
    (fp_text value "562K" (at 0.0442 0.0508) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at -2.5908 0.0508) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 38 "Net-(C10-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEF)
    (at 104.902 117.983 90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "wakestr_min_v1_2.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C2" (at 2.0574 0 180) (layer "F.SilkS"))
    (fp_text value "100nF" (at 0.508 -0.0254 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.0828 0.0508 180) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.8625 0 90) (size 1.075 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "VCC") (pintype "passive"))
    (pad "2" smd roundrect (at 0.8625 0 90) (size 1.075 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEF)
    (at 83.8012 109.1692)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "wakestr_min_v1_2.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C9" (at -2.699 -0.3556) (layer "F.SilkS"))
    (fp_text value "10uF" (at 0.4826 0.127) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at -2.699 -0.381) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.8625 0) (size 1.075 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 8 "/~{SPI_CS}") (pintype "passive"))
    (pad "2" smd roundrect (at 0.8625 0) (size 1.075 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 24 "Net-(C9-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEF)
    (at 108.6612 121.9454 -90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "wakestr_min_v1_2.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C5" (at 2.032 -0.0762 180) (layer "F.SilkS"))
    (fp_text value "100nF" (at 0.4572 -0.0254 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.032 -0.0762 180) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.8625 0 270) (size 1.075 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "VCC") (pintype "passive"))
    (pad "2" smd roundrect (at 0.8625 0 270) (size 1.075 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Diode_SMD:D_0603_1608Metric_Pad1.05x0.95mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEF0)
    (at 83.7946 110.7694 180)
    (descr "Diode SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "diode handsolder")
    (property "Sheetfile" "wakestr_min_v1_2.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "D4" (at 2.5908 0) (layer "F.SilkS"))
    (fp_text value "‎B0240R‎" (at -0.141 0.0438) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.875 0 180) (size 1.05 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "VCC") (pinfunction "K") (pintype "passive"))
    (pad "2" smd roundrect (at 0.875 0 180) (size 1.05 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 24 "Net-(C9-Pad2)") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Diode_SMD.3dshapes/D_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_SMD:SOT-363_SC-70-6" (layer "F.Cu")
    (tedit 5A02FF57)
    (at 98.9838 106.9848)
    (descr "SOT-363, SC-70-6")
    (tags "SOT-363 SC-70-6")
    (property "Sheetfile" "wakestr_min_v1_2.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "Q1" (at -0.7366 -1.7272) (layer "F.SilkS"))
    (fp_text value "BC846BS" (at 0.4064 0.0508 270) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at -0.762 -1.778 180) (layer "F.Fab"))
    (pad "1" smd rect (at -0.95 -0.65) (size 0.65 0.4) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "2" smd rect (at -0.95 0) (size 0.65 0.4) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "3" smd rect (at -0.95 0.65) (size 0.65 0.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 7 "/~{SLEEP}") (pinfunction "C2") (pintype "passive"))
    (pad "4" smd rect (at 0.95 0.65) (size 0.65 0.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pinfunction "E2") (pintype "passive"))
    (pad "5" smd rect (at 0.95 0) (size 0.65 0.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 25 "Net-(Q1-Pad5)") (pinfunction "B2") (pintype "input"))
    (pad "6" smd rect (at 0.95 -0.65) (size 0.65 0.4) (layers "F.Cu" "F.Paste" "F.Mask"))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-363_SC-70-6.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEF)
    (at 84.440453 116.5598 90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "wakestr_min_v1_2.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C13" (at 2.5392 -0.036253 270) (layer "F.SilkS"))
    (fp_text value "10uF" (at 0.0828 -0.0508 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.5392 -0.036253 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.8625 0 90) (size 1.075 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 32 "/+3Vx") (pintype "passive"))
    (pad "2" smd roundrect (at 0.8625 0 90) (size 1.075 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_1206_3216Metric_Pad1.33x1.80mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEF)
    (at 81.5134 121.2471 90)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "wakestr_min_v1_2.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C7" (at -2.9843 0.1984 180) (layer "F.SilkS"))
    (fp_text value "10uF 100v" (at -0.9144 -0.1016 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.5625 0 90) (size 1.325 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1886792453)
      (net 16 "/VIN") (pintype "passive"))
    (pad "2" smd roundrect (at 1.5625 0 90) (size 1.325 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1886792453)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_SO:VSSOP-8_2.3x2mm_P0.5mm" (layer "F.Cu")
    (tedit 5A02F25C)
    (at 99.8982 115.0874)
    (descr "VSSOP-8 2.3x2mm Pitch 0.5mm")
    (tags "VSSOP-8 2.3x2mm Pitch 0.5mm")
    (property "Part #" "74AUP1G74DC,125")
    (property "Sheetfile" "wakestr_min_v1_2.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "U2" (at -2.8956 -0.254 180) (layer "F.SilkS"))
    (fp_text value "74AUP1G74" (at -0.01 0.889 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at -2.8194 -0.254) (layer "F.Fab"))
    (pad "1" smd rect (at -1.55 -0.75 270) (size 0.3 0.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 10 "/BRD_WAKE_P") (pinfunction "C") (pintype "input"))
    (pad "2" smd rect (at -1.55 -0.25 270) (size 0.3 0.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "Net-(R1-Pad1)") (pinfunction "D") (pintype "input"))
    (pad "3" smd rect (at -1.55 0.25 270) (size 0.3 0.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 34 "Net-(R9-Pad2)") (pinfunction "~{Q}") (pintype "output"))
    (pad "4" smd rect (at -1.55 0.75 270) (size 0.3 0.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "5" smd rect (at 1.55 0.75 270) (size 0.3 0.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 29 "Net-(R8-Pad2)") (pinfunction "Q") (pintype "output"))
    (pad "6" smd rect (at 1.55 0.25 270) (size 0.3 0.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 7 "/~{SLEEP}") (pinfunction "~{CLR}") (pintype "input"))
    (pad "7" smd rect (at 1.55 -0.25 270) (size 0.3 0.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 3 "/~{BRD_WAKE}") (pinfunction "~{PRE}") (pintype "input"))
    (pad "8" smd rect (at 1.55 -0.75 270) (size 0.3 0.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "VCC") (pinfunction "VCC") (pintype "power_in"))
    (model "${KICAD6_3DMODEL_DIR}/Package_SO.3dshapes/VSSOP-8_2.3x2mm_P0.5mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 87.56 119.04)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "wakestr_min_v1_2.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R20" (at 2.22 0.04 90) (layer "F.SilkS"))
    (fp_text value "100K" (at 0.1344 0.0092) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.229 0.0352 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 32 "/+3Vx") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 17 "/PWR GOOD") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_SMD:SOT-23-5_HandSoldering" (layer "F.Cu")
    (tedit 5A0AB76C)
    (at 99.5172 121.4374)
    (descr "5-pin SOT23 package")
    (tags "SOT-23-5 hand-soldering")
    (property "Sheetfile" "wakestr_min_v1_2.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "U5" (at -1.8542 -2.0574) (layer "F.SilkS"))
    (fp_text value "R3117N" (at 1.27 0) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at -1.8542 -2.1082 180) (layer "F.Fab"))
    (pad "1" smd rect (at -1.35 -0.95) (size 1.56 0.65) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 28 "/+3Vx_ON") (pinfunction "OUT") (pintype "output"))
    (pad "2" smd rect (at -1.35 0) (size 1.56 0.65) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "VCC") (pinfunction "VDD") (pintype "power_in"))
    (pad "3" smd rect (at -1.35 0.95) (size 1.56 0.65) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "4" smd rect (at 1.35 0.95) (size 1.56 0.65) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "unconnected-(U5-Pad4)") (pinfunction "NC") (pintype "no_connect"))
    (pad "5" smd rect (at 1.35 -0.95) (size 1.56 0.65) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 32 "/+3Vx") (pinfunction "SENSE") (pintype "input"))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23-5.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 90.9574 123.571 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "wakestr_min_v1_2.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R21" (at -2.4384 -0.508) (layer "F.SilkS"))
    (fp_text value "1M" (at -0.0544 -0.0466) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at -2.4638 -0.508) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 180) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 32 "/+3Vx") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 180) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 38 "Net-(C10-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinSocket_1.27mm:PinSocket_1x01_P1.27mm_Vertical" (layer "F.Cu")
    (tedit 5A19A430)
    (at 97.3582 125.2474 90)
    (descr "Through hole straight socket strip, 1x01, 1.27mm pitch, single row (from Kicad 4.0.7), script generated")
    (tags "Through hole socket strip THT 1x01 1.27mm single row")
    (property "Sheetfile" "wakestr_min_v1_2.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J2" (at 1.778 0 180) (layer "F.SilkS"))
    (fp_text value "CLK" (at 0.508 1.1176 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 90) (size 1 1) (drill 0.7) (layers *.Cu *.Mask)
      (net 11 "/CLK_OUT") (pinfunction "Pin_1") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinSocket_1.27mm.3dshapes/PinSocket_1x01_P1.27mm_Vertical.wrl" hide
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 107.569 105.3338)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "wakestr_min_v1_2.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R12" (at 0.127 -1.1176) (layer "F.SilkS"))
    (fp_text value "100K" (at -0.0156 0.0162) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0.1016 -1.1684) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 26 "Net-(Q2-Pad6)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinSocket_1.27mm:PinSocket_1x01_P1.27mm_Vertical" (layer "F.Cu")
    (tedit 5A19A430)
    (at 88.2396 105.3846)
    (descr "Through hole straight socket strip, 1x01, 1.27mm pitch, single row (from Kicad 4.0.7), script generated")
    (tags "Through hole socket strip THT 1x01 1.27mm single row")
    (property "Sheetfile" "wakestr_min_v1_2.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J3" (at 0.0508 -1.2446) (layer "F.SilkS"))
    (fp_text value "~{WAKE}" (at -2.1844 0.0508 180) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 1 1) (drill 0.7) (layers *.Cu *.Mask)
      (net 3 "/~{BRD_WAKE}") (pinfunction "Pin_1") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinSocket_1.27mm.3dshapes/PinSocket_1x01_P1.27mm_Vertical.wrl" hide
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 91.948 107.1118)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "wakestr_min_v1_2.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R14" (at -2.5654 -0.0508) (layer "F.SilkS"))
    (fp_text value "100K" (at 0.0254 0.127) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at -2.5908 -0.0508) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 9 "/RX1_232") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 20 "Net-(D3-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 102.9716 117.983 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "wakestr_min_v1_2.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R6" (at 1.9812 -0.0254 180) (layer "F.SilkS"))
    (fp_text value "100K" (at 0.127 0.0254 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 1.9812 -0.0254 180) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 90) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 6 "/VD2_I2C_SCL") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 90) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "VCC") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Diode_SMD:D_PowerDI-123" (layer "F.Cu")
    (tedit 588FC24C)
    (at 106.9848 94.361)
    (descr "http://www.diodes.com/_files/datasheets/ds30497.pdf")
    (tags "PowerDI diode vishay")
    (property "Sheetfile" "wakestr_min_v1_2.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "D6" (at 0 -2) (layer "F.SilkS"))
    (fp_text value "DFLS2100" (at 0 2.5) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -2) (layer "F.Fab"))
    (pad "1" smd rect (at -0.85 0 180) (size 2.4 1.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 39 "unconnected-(D6-Pad1)") (pinfunction "K") (pintype "passive"))
    (pad "2" smd rect (at 1.525 0 180) (size 1.05 1.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 40 "unconnected-(D6-Pad2)") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Diode_SMD.3dshapes/D_PowerDI-123.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 94.4372 116.3066 -90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "wakestr_min_v1_2.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R23" (at -0.3048 -1.1938 90) (layer "F.SilkS"))
    (fp_text value "100K NS" (at 1.143 0 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at -0.3048 -1.1938 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 270) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 37 "Net-(C16-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 270) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 41 "Net-(R23-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEF)
    (at 90.9574 125.0442 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "wakestr_min_v1_2.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C10" (at 2.5146 0) (layer "F.SilkS"))
    (fp_text value "10pF" (at -0.0254 0.1778) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.5146 0.0254) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.8625 0 180) (size 1.075 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 32 "/+3Vx") (pintype "passive"))
    (pad "2" smd roundrect (at 0.8625 0 180) (size 1.075 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 38 "Net-(C10-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinSocket_1.27mm:PinSocket_1x01_P1.27mm_Vertical" (layer "F.Cu")
    (tedit 5A19A430)
    (at 95.0722 125.2474 90)
    (descr "Through hole straight socket strip, 1x01, 1.27mm pitch, single row (from Kicad 4.0.7), script generated")
    (tags "Through hole socket strip THT 1x01 1.27mm single row")
    (property "Sheetfile" "wakestr_min_v1_2.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J1" (at 1.778 0 180) (layer "F.SilkS"))
    (fp_text value "EVNT" (at 0.0254 -1.2192 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 90) (size 1 1) (drill 0.7) (layers *.Cu *.Mask)
      (net 15 "/EVENT_CNT") (pinfunction "Pin_1") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinSocket_1.27mm.3dshapes/PinSocket_1x01_P1.27mm_Vertical.wrl" hide
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 98.3742 111.6584 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "wakestr_min_v1_2.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R3" (at 2.0066 0.2286 180) (layer "F.SilkS"))
    (fp_text value "100K" (at 0.2032 0.0254 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.032 0.2286 180) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 90) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 90) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 10 "/BRD_WAKE_P") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 83.7946 107.4928 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "wakestr_min_v1_2.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R7" (at 2.717796 -0.0254) (layer "F.SilkS"))
    (fp_text value "100K NS" (at -1.0414 0.0254) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.6924 -0.0254) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 180) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 12 "/~{RTC_ALARM}") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 180) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "VCC") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 93.3958 111.6584 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "wakestr_min_v1_2.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R4" (at 1.9558 -0.0508 180) (layer "F.SilkS"))
    (fp_text value "100K" (at 0.0762 0.1016 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 1.9558 -0.0508 180) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 90) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 5 "/VD2_I2C_SDA") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 90) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "VCC") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 95.123 111.6584 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "wakestr_min_v1_2.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R1" (at 1.9558 0 180) (layer "F.SilkS"))
    (fp_text value "100K" (at 0 -0.0762 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 1.9558 -0.0254 180) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 90) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "Net-(R1-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 90) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "VCC") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 83.7946 112.4204 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "wakestr_min_v1_2.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R15" (at 2.6162 0.0508) (layer "F.SilkS"))
    (fp_text value "100K" (at 0.0762 0.0762) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.6162 0.0762) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 180) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "VCC") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 180) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 24 "Net-(C9-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "ProjectFootprints:RTC_RV-3032-C7" (layer "F.Cu")
    (tedit 62C862F0)
    (at 104.5972 123.2154)
    (property "Sheetfile" "wakestr_min_v1_2.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "U3" (at 0.622 -2.5764) (layer "F.SilkS"))
    (fp_text value "RTC-RV-3032" (at 3.8632 2.5514) (layer "F.Fab"))
    (pad "1" smd rect locked (at -0.6 -1.35) (size 0.8 0.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "VCC") (pinfunction "Vbackup") (pintype "bidirectional"))
    (pad "2" smd rect locked (at -0.6 -0.45) (size 0.8 0.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 5 "/VD2_I2C_SDA") (pinfunction "SDA") (pintype "bidirectional"))
    (pad "3" smd rect locked (at -0.6 0.45) (size 0.8 0.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "/~{RTC_ALARM}") (pinfunction "~{INT}") (pintype "output"))
    (pad "4" smd rect locked (at -0.6 1.35) (size 0.8 0.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "/EVENT_CNT") (pinfunction "EVI") (pintype "input"))
    (pad "5" smd rect locked (at 0.6 1.35) (size 0.8 0.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "6" smd rect locked (at 0.6 0.45) (size 0.8 0.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 32 "/+3Vx") (pinfunction "VDD") (pintype "power_in"))
    (pad "7" smd rect locked (at 0.6 -0.45) (size 0.8 0.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 11 "/CLK_OUT") (pinfunction "CLKOUT") (pintype "output"))
    (pad "8" smd rect locked (at 0.6 -1.35) (size 0.8 0.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 6 "/VD2_I2C_SCL") (pinfunction "SCL") (pintype "bidirectional"))
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEF)
    (at 82.814853 116.5598 90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "wakestr_min_v1_2.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C12" (at 2.5138 0.039947 270) (layer "F.SilkS"))
    (fp_text value "10uF" (at 0.02 0.072 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.5138 0.014547 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.8625 0 90) (size 1.075 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 32 "/+3Vx") (pintype "passive"))
    (pad "2" smd roundrect (at 0.8625 0 90) (size 1.075 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 101.3714 106.7816 -90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "wakestr_min_v1_2.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R13" (at -2.0828 -0.0508 180) (layer "F.SilkS"))
    (fp_text value "100K" (at 0 0.0508 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at -2.0828 -0.0762 180) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 270) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "VCC") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 270) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 36 "Net-(C3-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_SMD:SOT-363_SC-70-6" (layer "F.Cu")
    (tedit 5A02FF57)
    (at 87.3064 111.4552)
    (descr "SOT-363, SC-70-6")
    (tags "SOT-363 SC-70-6")
    (property "Sheetfile" "wakestr_min_v1_2.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "Q4" (at -0.8702 -1.9812) (layer "F.SilkS"))
    (fp_text value "BC856BS" (at 0.050804 0.3048 270) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at -0.8702 -1.9812 180) (layer "F.Fab"))
    (pad "1" smd rect (at -0.95 -0.65) (size 0.65 0.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "VCC") (pinfunction "E1") (pintype "passive"))
    (pad "2" smd rect (at -0.95 0) (size 0.65 0.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 24 "Net-(C9-Pad2)") (pinfunction "B1") (pintype "input"))
    (pad "3" smd rect (at -0.95 0.65) (size 0.65 0.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 10 "/BRD_WAKE_P") (pinfunction "C2") (pintype "passive"))
    (pad "4" smd rect (at 0.95 0.65) (size 0.65 0.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "VCC") (pinfunction "E2") (pintype "passive"))
    (pad "5" smd rect (at 0.95 0) (size 0.65 0.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 27 "Net-(Q4-Pad5)") (pinfunction "B2") (pintype "input"))
    (pad "6" smd rect (at 0.95 -0.65) (size 0.65 0.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 10 "/BRD_WAKE_P") (pinfunction "C1") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-363_SC-70-6.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 107.569 106.9086 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "wakestr_min_v1_2.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R11" (at -0.2286 -1.1176) (layer "F.SilkS"))
    (fp_text value "10K" (at 0 0) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at -0.2032 -1.1176) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 180) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 25 "Net-(Q1-Pad5)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 180) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 26 "Net-(Q2-Pad6)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEF)
    (at 87.691653 116.5598 90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "wakestr_min_v1_2.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C15" (at 2.4884 -0.010853 270) (layer "F.SilkS"))
    (fp_text value "10uF" (at 0.0516 0.0032 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.4884 -0.010853 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.8625 0 90) (size 1.075 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 32 "/+3Vx") (pintype "passive"))
    (pad "2" smd roundrect (at 0.8625 0 90) (size 1.075 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 100.2792 124.2314 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "wakestr_min_v1_2.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R25" (at 0 -1.143) (layer "F.SilkS"))
    (fp_text value "1M NS" (at -0.127 0) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0.0254 -1.143) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 180) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 180) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 28 "/+3Vx_ON") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 90.7354 112.268 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "wakestr_min_v1_2.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R16" (at -0.0188 -1.3462) (layer "F.SilkS"))
    (fp_text value "100K" (at 0.1016 0.0508) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at -0.0442 -1.3208) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 180) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "VCC") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 180) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 27 "Net-(Q4-Pad5)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 100.7872 111.6584 -90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "wakestr_min_v1_2.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R9" (at -2.0066 0.0254) (layer "F.SilkS"))
    (fp_text value "10K" (at 0.0254 0.0508 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at -1.9812 0.0508 180) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 270) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 13 "/~{VREG_EN}") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 270) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 34 "Net-(R9-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 103.251 113.03 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "wakestr_min_v1_2.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R8" (at -2.286 -0.1524) (layer "F.SilkS"))
    (fp_text value "10K" (at 0.0762 0) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at -2.2606 -0.127) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 180) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 14 "/VREG_EN") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 180) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 29 "Net-(R8-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 103.251 111.4552 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "wakestr_min_v1_2.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R10" (at -2.6416 -0.508 180) (layer "F.SilkS"))
    (fp_text value "100K" (at 0.0254 -0.0508) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at -2.032 0.0254 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 180) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 7 "/~{SLEEP}") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 180) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "VCC") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_SMD:SOT-363_SC-70-6" (layer "F.Cu")
    (tedit 5A02FF57)
    (at 95.5548 106.9594)
    (descr "SOT-363, SC-70-6")
    (tags "SOT-363 SC-70-6")
    (property "Sheetfile" "wakestr_min_v1_2.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "Q3" (at -0.5588 -1.7526) (layer "F.SilkS"))
    (fp_text value "BC846BS" (at 0.381 -0.0508 270) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at -0.5842 -1.7526 180) (layer "F.Fab"))
    (pad "1" smd rect (at -0.95 -0.65) (size 0.65 0.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pinfunction "E1") (pintype "passive"))
    (pad "2" smd rect (at -0.95 0) (size 0.65 0.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 20 "Net-(D3-Pad1)") (pinfunction "B1") (pintype "input"))
    (pad "3" smd rect (at -0.95 0.65) (size 0.65 0.4) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "4" smd rect (at 0.95 0.65) (size 0.65 0.4) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "5" smd rect (at 0.95 0) (size 0.65 0.4) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "6" smd rect (at 0.95 -0.65) (size 0.65 0.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 3 "/~{BRD_WAKE}") (pinfunction "C1") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-363_SC-70-6.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEF)
    (at 110.0836 106.5519 -90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "wakestr_min_v1_2.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C3" (at -2.0563 -0.0254 -180) (layer "F.SilkS"))
    (fp_text value "10uF" (at 0.508 0.0254 -270) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at -2.0817 -0.0508 -180) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.8625 0 270) (size 1.075 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 33 "unconnected-(C3-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.8625 0 270) (size 1.075 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 36 "Net-(C3-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEF)
    (at 103.251 109.9566 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "wakestr_min_v1_2.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C1" (at -2.2352 0.0254) (layer "F.SilkS"))
    (fp_text value "100nF" (at -0.2032 -0.0254) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at -2.2606 0.0508) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.8625 0 180) (size 1.075 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "VCC") (pintype "passive"))
    (pad "2" smd roundrect (at 0.8625 0 180) (size 1.075 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 95.4532 119.38)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "wakestr_min_v1_2.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R2" (at 0.1016 -1.143) (layer "F.SilkS"))
    (fp_text value "1M" (at 0.0762 0.0254) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0.127 -1.143) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 28 "/+3Vx_ON") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 92.2528 108.7882 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "wakestr_min_v1_2.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R5" (at 3.1242 0.508) (layer "F.SilkS"))
    (fp_text value "100K" (at 0.2286 0.0762) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 3.1242 0.5334) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 180) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 3 "/~{BRD_WAKE}") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 180) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "VCC") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEF)
    (at 91.9988 115.3922)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "wakestr_min_v1_2.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C16" (at 0.0254 1.2446) (layer "F.SilkS"))
    (fp_text value "0.001 uF" (at 0.254 0) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0.0254 1.2446) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.8625 0) (size 1.075 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive"))
    (pad "2" smd roundrect (at 0.8625 0) (size 1.075 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 37 "Net-(C16-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 90.7608 110.7186 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "wakestr_min_v1_2.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R17" (at -0.222 0.9652 180) (layer "F.SilkS"))
    (fp_text value "10K" (at -0.0762 0.0254) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at -0.1966 0.9652) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 180) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 12 "/~{RTC_ALARM}") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 180) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 27 "Net-(Q4-Pad5)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "ProjectFootprints:wakestr_slim_v1" (layer "F.Cu")
    (tedit 0)
    (at 92.9894 115.7859)
    (property "Sheetfile" "wakestr_min_v1_2.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "W1" (at 19.3548 -10.2235 unlocked) (layer "F.SilkS"))
    (fp_text value "Wakestr_Slim_v1" (at 11.9888 10.9855 unlocked) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 11.2014 3.9878 unlocked) (layer "F.Fab"))
    (pad "1" thru_hole rect (at -16.764 10.033) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "GND") (pintype "input"))
    (pad "2" thru_hole circle (at -16.764 7.493) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 16 "/VIN") (pinfunction "VIN") (pintype "input"))
    (pad "3" thru_hole circle (at -16.764 4.953) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 32 "/+3Vx") (pinfunction "+3VX") (pintype "output"))
    (pad "4" thru_hole circle (at -16.764 2.413) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 "VCC") (pinfunction "+3V_COIN") (pintype "output"))
    (pad "5" thru_hole circle (at -16.764 -0.127) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 14 "/VREG_EN") (pinfunction "VREG_EN") (pintype "output"))
    (pad "6" thru_hole circle (at -16.764 -2.667) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 "/~{BRD_WAKE}") (pinfunction "~{WAKE}") (pintype "input"))
    (pad "7" thru_hole circle (at -16.764 -5.207) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 21 "/~{PROC_SLEEP}") (pinfunction "~{PROC_SLEEP}") (pintype "input"))
    (pad "8" thru_hole circle (at -16.764 -7.747) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 18 "/I2C_SDA") (pinfunction "I2C_SDA") (pintype "bidirectional"))
    (pad "9" thru_hole circle (at -16.764 -10.287) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 19 "/I2C_SCL") (pinfunction "I2C_SCL") (pintype "bidirectional"))
    (pad "10" thru_hole circle (at 18.796 -5.207) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 "/RX1_232") (pinfunction "SER_RX") (pintype "input"))
    (pad "11" thru_hole circle (at 18.796 -2.667) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 "/~{SPI_CS}") (pinfunction "~{SPI_CS}") (pintype "input"))
    (pad "12" thru_hole circle (at 18.796 -0.127) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 "/BRD_WAKE_P") (pinfunction "WAKE_P") (pintype "input"))
    (pad "13" thru_hole circle (at 18.796 2.413) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 13 "/~{VREG_EN}") (pinfunction "~{VREG_EN}") (pintype "output"))
    (pad "14" thru_hole circle (at 18.796 4.953) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 12 "/~{RTC_ALARM}") (pinfunction "~{ALARM}") (pintype "output"))
    (pad "15" thru_hole circle (at 18.796 7.493) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 28 "/+3Vx_ON") (pinfunction "+3VX_ON") (pintype "output"))
    (pad "16" thru_hole rect (at 18.796 10.033) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "GND") (pintype "input"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x09_P2.54mm_Vertical.wrl"
      (offset (xyz -16.51 10.16 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x07_P2.54mm_Vertical.wrl"
      (offset (xyz 18.415 5.08 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 91.9859 118.6055 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "wakestr_min_v1_2.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R19" (at 0.1903 -1.1809) (layer "F.SilkS"))
    (fp_text value "118K" (at 0.1532 -0.0268) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0.1903 -1.2063) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 180) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 180) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 30 "Net-(R19-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_SO:VSSOP-8_2.3x2mm_P0.5mm" (layer "F.Cu")
    (tedit 5A02F25C)
    (at 99.8982 117.856)
    (descr "VSSOP-8 2.3x2mm Pitch 0.5mm")
    (tags "VSSOP-8 2.3x2mm Pitch 0.5mm")
    (property "Sheetfile" "wakestr_min_v1_2.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "U1" (at -2.8702 -1.4478) (layer "F.SilkS"))
    (fp_text value "NL7WB66USG" (at 1.1938 0.3048 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at -2.8702 -1.4478) (layer "F.Fab"))
    (pad "1" smd rect (at -1.55 -0.75 270) (size 0.3 0.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 18 "/I2C_SDA") (pintype "input"))
    (pad "2" smd rect (at -1.55 -0.25 270) (size 0.3 0.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 5 "/VD2_I2C_SDA") (pintype "tri_state"))
    (pad "3" smd rect (at -1.55 0.25 270) (size 0.3 0.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 28 "/+3Vx_ON") (pintype "input"))
    (pad "4" smd rect (at -1.55 0.75 270) (size 0.3 0.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "5" smd rect (at 1.55 0.75 270) (size 0.3 0.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 19 "/I2C_SCL") (pintype "input"))
    (pad "6" smd rect (at 1.55 0.25 270) (size 0.3 0.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 6 "/VD2_I2C_SCL") (pintype "tri_state"))
    (pad "7" smd rect (at 1.55 -0.25 270) (size 0.3 0.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 28 "/+3Vx_ON") (pintype "input"))
    (pad "8" smd rect (at 1.55 -0.75 270) (size 0.3 0.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "VCC") (pinfunction "VCC") (pintype "power_in"))
    (model "${KICAD6_3DMODEL_DIR}/Package_SO.3dshapes/VSSOP-8_2.3x2mm_P0.5mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEF)
    (at 81.240053 116.5598 90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "wakestr_min_v1_2.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C11" (at 2.4376 -0.010853 270) (layer "F.SilkS"))
    (fp_text value "10uF" (at 0.0704 -0.0204 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.463 -0.036253 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.8625 0 90) (size 1.075 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 32 "/+3Vx") (pintype "passive"))
    (pad "2" smd roundrect (at 0.8625 0 90) (size 1.075 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_SMD:SOT-363_SC-70-6" (layer "F.Cu")
    (tedit 5A02FF57)
    (at 104.2162 106.7308)
    (descr "SOT-363, SC-70-6")
    (tags "SOT-363 SC-70-6")
    (property "Sheetfile" "wakestr_min_v1_2.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "Q2" (at -0.6604 -2.0574) (layer "F.SilkS"))
    (fp_text value "BC856BS" (at 0.165608 0.009601 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at -0.7366 -2.032 180) (layer "F.Fab"))
    (pad "1" smd rect (at -0.95 -0.65) (size 0.65 0.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "VCC") (pinfunction "E1") (pintype "passive"))
    (pad "2" smd rect (at -0.95 0) (size 0.65 0.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 36 "Net-(C3-Pad2)") (pinfunction "B1") (pintype "input"))
    (pad "3" smd rect (at -0.95 0.65) (size 0.65 0.4) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "4" smd rect (at 0.95 0.65) (size 0.65 0.4) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "5" smd rect (at 0.95 0) (size 0.65 0.4) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "6" smd rect (at 0.95 -0.65) (size 0.65 0.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 26 "Net-(Q2-Pad6)") (pinfunction "C1") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-363_SC-70-6.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "ProjectFootprints:ML2020_F1AN" (layer "B.Cu")
    (tedit 62DC3AF7)
    (at 96.266 113.3602 180)
    (property "Sheetfile" "wakestr_min_v1_2.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "BT1" (at 0 0) (layer "B.SilkS"))
    (fp_text value "ML2020_F1AN" (at 0 0) (layer "B.Fab"))
    (pad "1" smd rect (at -10.8 -7.55 145) (size 2 3) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "VCC") (pinfunction "+") (pintype "passive"))
    (pad "2" smd rect (at 13 0 180) (size 2 3) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2 "GND") (pinfunction "-") (pintype "passive"))
    (model "C:/Dropbox/KiCAD/3DModels/Panasonic-ML2020.STEP"
      (offset (xyz 0 -0.635 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 180))
    )
  )
  (footprint "Button_Switch_SMD:SW_Push_1P1T_NO_CK_KMR2" (layer "B.Cu")
    (tedit 5A02FC95)
    (at 108.204 106.9594 -90)
    (descr "CK components KMR2 tactile switch http://www.ckswitches.com/media/1479/kmr2.pdf")
    (tags "tactile switch kmr2")
    (property "Sheetfile" "wakestr_min_v1_2.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "SW1" (at 3.2766 0.0508) (layer "B.SilkS"))
    (fp_text value "WAKE" (at -0.2032 -2.3876 90) (layer "B.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 2.45 90) (layer "B.Fab"))
    (pad "1" smd rect (at -2.05 0.8 270) (size 0.9 1) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 3 "/~{BRD_WAKE}") (pintype "passive"))
    (pad "1" smd rect (at 2.05 0.8 270) (size 0.9 1) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 3 "/~{BRD_WAKE}") (pintype "passive"))
    (pad "2" smd rect (at -2.05 -0.8 270) (size 0.9 1) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2 "GND") (pintype "passive"))
    (pad "2" smd rect (at 2.05 -0.8 270) (size 0.9 1) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2 "GND") (pintype "passive"))
    (model "C:/Dropbox/KiCAD/3DModels/KMR221GLFS--3DModel-STEP-56544.STEP"
      (offset (xyz 0 0 0.635))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_1210_3225Metric_Pad1.33x2.70mm_HandSolder" (layer "B.Cu")
    (tedit 5F68FEEF)
    (at 103.2764 124.3584 -90)
    (descr "Capacitor SMD 1210 (3225 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "wakestr_min_v1_2.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C6" (at -0.6096 -2.54 90) (layer "B.SilkS"))
    (fp_text value "11mF CPH3225A" (at -3.3528 -0.254 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd roundrect (at -1.5625 0 270) (size 1.325 2.7) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.1886792453)
      (net 1 "VCC") (pintype "passive"))
    (pad "2" smd roundrect (at 1.5625 0 270) (size 1.325 2.7) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.1886792453)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1210_3225Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "LED_SMD:LED_0603_1608Metric_Pad1.05x0.95mm_HandSolder" (layer "B.Cu")
    (tedit 5F68FEF1)
    (at 83.3882 106.5784 -90)
    (descr "LED SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "LED handsolder")
    (property "Sheetfile" "wakestr_min_v1_2.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "D5" (at 2.3368 -0.3302 90) (layer "B.SilkS"))
    (fp_text value "GREEN" (at 0.2286 0.1094 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.875 0 270) (size 1.05 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 31 "Net-(D5-Pad1)") (pinfunction "K") (pintype "passive"))
    (pad "2" smd roundrect (at 0.875 0 270) (size 1.05 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 32 "/+3Vx") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/LED_SMD.3dshapes/LED_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "ProjectFootprints:IND_MSS7341-563MLD" (layer "B.Cu")
    (tedit 62DACBB3)
    (at 82.9818 122.3518 180)
    (property "PartNum" "MSS7341-123MLD")
    (property "Sheetfile" "wakestr_min_v1_2.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "L1" (at -4.5849 0.6987) (layer "B.SilkS"))
    (fp_text value "MSS7341-123MLD" (at 0 -0.1524) (layer "B.Fab"))
    (pad "1" smd custom locked (at 0 3.2 180) (size 1.27 0.635) (layers "B.Cu")
      (net 32 "/+3Vx") (pinfunction "1") (pintype "input") (zone_connect 0)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_poly (pts
            (xy -3.55 0.35)
            (xy 3.55 0.35)
            (xy 3.55 -2.15)
            (xy 2.62 -2.15)
            (xy 2.57 -2.031)
            (xy 2.522 -1.931)
            (xy 2.47 -1.832)
            (xy 2.415 -1.736)
            (xy 2.356 -1.642)
            (xy 2.293 -1.55)
            (xy 2.226 -1.461)
            (xy 2.156 -1.374)
            (xy 2.083 -1.291)
            (xy 2.006 -1.21)
            (xy 1.926 -1.133)
            (xy 1.844 -1.058)
            (xy 1.758 -0.987)
            (xy 1.67 -0.92)
            (xy 1.579 -0.856)
            (xy 1.485 -0.795)
            (xy 1.39 -0.739)
            (xy 1.292 -0.686)
            (xy 1.192 -0.637)
            (xy 1.09 -0.592)
            (xy 0.987 -0.551)
            (xy 0.882 -0.515)
            (xy 0.775 -0.482)
            (xy 0.668 -0.454)
            (xy 0.559 -0.43)
            (xy 0.45 -0.41)
            (xy 0.339 -0.395)
            (xy 0.229 -0.384)
            (xy 0.118 -0.377)
            (xy 0 -0.375)
            (xy -0.118 -0.377)
            (xy -0.229 -0.384)
            (xy -0.339 -0.395)
            (xy -0.45 -0.41)
            (xy -0.559 -0.43)
            (xy -0.668 -0.454)
            (xy -0.775 -0.482)
            (xy -0.882 -0.515)
            (xy -0.987 -0.551)
            (xy -1.09 -0.592)
            (xy -1.192 -0.637)
            (xy -1.292 -0.686)
            (xy -1.39 -0.739)
            (xy -1.485 -0.795)
            (xy -1.579 -0.856)
            (xy -1.67 -0.92)
            (xy -1.758 -0.987)
            (xy -1.844 -1.058)
            (xy -1.926 -1.133)
            (xy -2.006 -1.21)
            (xy -2.083 -1.291)
            (xy -2.156 -1.374)
            (xy -2.226 -1.461)
            (xy -2.293 -1.55)
            (xy -2.356 -1.642)
            (xy -2.415 -1.736)
            (xy -2.47 -1.832)
            (xy -2.522 -1.931)
            (xy -2.57 -2.031)
            (xy -2.62 -2.15)
            (xy -3.55 -2.15)
            (xy -3.55 0.35)
          ) (width 0.01) (fill yes))
      ))
    (pad "2" smd custom locked (at 0 -3.2 180) (size 1.27 0.635) (layers "B.Cu")
      (net 23 "Net-(C8-Pad2)") (pinfunction "2") (pintype "input") (zone_connect 0)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_poly (pts
            (xy 3.55 -0.35)
            (xy -3.55 -0.35)
            (xy -3.55 2.15)
            (xy -2.62 2.15)
            (xy -2.57 2.031)
            (xy -2.522 1.931)
            (xy -2.47 1.832)
            (xy -2.415 1.736)
            (xy -2.356 1.642)
            (xy -2.293 1.55)
            (xy -2.226 1.461)
            (xy -2.156 1.374)
            (xy -2.083 1.291)
            (xy -2.006 1.21)
            (xy -1.926 1.133)
            (xy -1.844 1.058)
            (xy -1.758 0.987)
            (xy -1.67 0.92)
            (xy -1.579 0.856)
            (xy -1.485 0.795)
            (xy -1.39 0.739)
            (xy -1.292 0.686)
            (xy -1.192 0.637)
            (xy -1.09 0.592)
            (xy -0.987 0.551)
            (xy -0.882 0.515)
            (xy -0.775 0.482)
            (xy -0.668 0.454)
            (xy -0.559 0.43)
            (xy -0.45 0.41)
            (xy -0.339 0.395)
            (xy -0.229 0.384)
            (xy -0.118 0.377)
            (xy 0 0.375)
            (xy 0.118 0.377)
            (xy 0.229 0.384)
            (xy 0.339 0.395)
            (xy 0.45 0.41)
            (xy 0.559 0.43)
            (xy 0.668 0.454)
            (xy 0.775 0.482)
            (xy 0.882 0.515)
            (xy 0.987 0.551)
            (xy 1.09 0.592)
            (xy 1.192 0.637)
            (xy 1.292 0.686)
            (xy 1.39 0.739)
            (xy 1.485 0.795)
            (xy 1.579 0.856)
            (xy 1.67 0.92)
            (xy 1.758 0.987)
            (xy 1.844 1.058)
            (xy 1.926 1.133)
            (xy 2.006 1.21)
            (xy 2.083 1.291)
            (xy 2.156 1.374)
            (xy 2.226 1.461)
            (xy 2.293 1.55)
            (xy 2.356 1.642)
            (xy 2.415 1.736)
            (xy 2.47 1.832)
            (xy 2.522 1.931)
            (xy 2.57 2.031)
            (xy 2.62 2.15)
            (xy 3.55 2.15)
            (xy 3.55 -0.35)
          ) (width 0.01) (fill yes))
      ))
    (model "C:/Dropbox/KiCAD/3DModels/Coilcraft-MSS7341.STEP"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )
  (footprint "Diode_SMD:D_SMA" (layer "B.Cu")
    (tedit 586432E5)
    (at 90.6018 125.3998)
    (descr "Diode SMA (DO-214AC)")
    (tags "Diode SMA (DO-214AC)")
    (property "Sheetfile" "wakestr_min_v1_2.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "D2" (at -0.1016 -2.3114 180) (layer "B.SilkS"))
    (fp_text value "B120-E3" (at 0.086 0.1264) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 4.3688 -0.127) (layer "B.Fab"))
    (pad "1" smd rect (at -2 0) (size 2.5 1.8) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 23 "Net-(C8-Pad2)") (pinfunction "K") (pintype "passive"))
    (pad "2" smd rect (at 2 0) (size 2.5 1.8) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2 "GND") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Diode_SMD.3dshapes/D_SMA.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "B.Cu")
    (tedit 5F68FEEE)
    (at 81.8388 106.553 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "wakestr_min_v1_2.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R22" (at -2.667 0.5588 90) (layer "B.SilkS"))
    (fp_text value "10K" (at 0.0508 0.0254 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 90) (size 0.975 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 90) (size 0.975 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 31 "Net-(D5-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_rect (start 74.1172 127.5334) (end 113.919 103.1748) (layer "Edge.Cuts") (width 0.1) (fill none))
  (gr_text "Gnd" (at 113.284 125.7554 90) (layer "B.SilkS"))
  (gr_text "Ven" (at 74.7522 115.6462 270) (layer "B.SilkS"))
  (gr_text "wakestr_slim_v1_1.kicad_pcb" (at 99.5172 104.0384 180) (layer "B.SilkS"))
  (gr_text "WakeStr v1.1" (at 78.0288 112.1918 270) (layer "B.SilkS"))
  (gr_text "SCL" (at 74.7776 105.5116 270) (layer "B.SilkS"))
  (gr_text "Thom Maughan" (at 80.772 111.633 270) (layer "B.SilkS"))
  (gr_text "Gnd" (at 74.7014 125.8062 270) (layer "B.SilkS"))
  (gr_text "~{CS}" (at 113.3856 113.0046 90) (layer "B.SilkS"))
  (gr_text "Rx" (at 113.3094 110.5408 90) (layer "B.SilkS"))
  (gr_text "Sleep" (at 74.7014 110.7694 270) (layer "B.SilkS"))
  (gr_text "~{WAKE}" (at 86.0552 105.4354 180) (layer "B.SilkS"))
  (gr_text "~{Wake}" (at 74.6252 113.157 270) (layer "B.SilkS"))
  (gr_text "CLK\n" (at 97.9678 126.873) (layer "B.SilkS"))
  (gr_text "3on" (at 113.2586 123.1392 90) (layer "B.SilkS"))
  (gr_text "~{Ven}" (at 113.3602 118.11 90) (layer "B.SilkS"))
  (gr_text "25 Jul 2022" (at 84.963 104.14 180) (layer "B.SilkS"))
  (gr_text "Vbat" (at 74.7268 118.2878 270) (layer "B.SilkS"))
  (gr_text "EV\n" (at 95.9104 126.8984) (layer "B.SilkS"))
  (gr_text "~{Alrm}" (at 113.3094 120.6754 90) (layer "B.SilkS"))
  (gr_text "+3.3" (at 74.6252 120.904 270) (layer "B.SilkS"))
  (gr_text "Wakp" (at 113.1062 115.6208 90) (layer "B.SilkS"))
  (gr_text "SDA" (at 74.7268 108.1532 270) (layer "B.SilkS"))
  (gr_text "Vin" (at 74.7268 123.1646 270) (layer "B.SilkS"))
  (gr_text "~{Wake}" (at 74.6252 113.157 270) (layer "F.SilkS"))
  (gr_text "~{Ven}" (at 113.3602 118.1354 90) (layer "F.SilkS"))
  (gr_text "~{CS}" (at 113.3856 113.0046 90) (layer "F.SilkS"))
  (gr_text "SCL" (at 74.7522 105.5624 270) (layer "F.SilkS"))
  (gr_text "+3.3" (at 74.7014 120.777 -90) (layer "F.SilkS"))
  (gr_text "Ven" (at 74.6252 115.697 -90) (layer "F.SilkS"))
  (gr_text "Vbat" (at 74.7522 118.237 270) (layer "F.SilkS"))
  (gr_text "Gnd" (at 113.3094 125.8824 90) (layer "F.SilkS"))
  (gr_text "CLK" (at 96.9772 126.8984) (layer "F.SilkS"))
  (gr_text "Wakp" (at 113.157 115.5192 90) (layer "F.SilkS"))
  (gr_text "Rx\n" (at 113.284 110.4646 90) (layer "F.SilkS"))
  (gr_text "Gnd" (at 74.676 125.7554 -90) (layer "F.SilkS"))
  (gr_text "3on\n" (at 113.2332 123.19 90) (layer "F.SilkS"))
  (gr_text "SDA" (at 74.7014 108.0516 270) (layer "F.SilkS"))
  (gr_text "Vin" (at 74.6506 123.1392 -90) (layer "F.SilkS"))
  (gr_text "EV" (at 93.5482 125.3744) (layer "F.SilkS"))
  (gr_text "Sleep" (at 74.8538 110.6678 270) (layer "F.SilkS"))
  (gr_text "~{Alrm}" (at 113.3602 120.6754 90) (layer "F.SilkS"))
  (zone (net 2) (net_name "GND") (layer "F.Cu") (hatch edge 0.508)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 114.816905 113.682979)
        (xy 114.8334 127.7112)
        (xy 114.427 128.1684)
        (xy 72.8472 128.397)
        (xy 72.805305 113.606779)
      )
    )
  )
  (zone (net 2) (net_name "GND") (layer "In1.Cu") (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 114.0206 102.997)
        (xy 114.1222 103.0732)
        (xy 114.046 127.889)
        (xy 73.8886 127.8636)
        (xy 73.8378 102.8446)
      )
    )
  )
  (zone (net 2) (net_name "GND") (layer "In2.Cu") (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 114.3 127.7112)
        (xy 73.5076 127.7366)
        (xy 73.5584 102.8954)
        (xy 73.6092 102.9716)
        (xy 114.2492 102.7684)
      )
    )
  )
  (zone (net 32) (net_name "/+3Vx") (layer "B.Cu") (hatch edge 0.508)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 95.5548 127.4572)
        (xy 73.152 121.666)
        (xy 72.398694 121.189947)
        (xy 72.703494 116.744947)
        (xy 90.1954 116.7384)
        (xy 93.4974 114.554)
        (xy 95.504 114.554)
      )
    )
  )
)
