(kicad_sch (version 20211123) (generator eeschema)
  (paper "B")
  (title_block
    (title "Wakestr")
    (date "2022-07-16")
    (rev "V1.1")
    (company "Derived from TimePwr and Serial Monster from iSee Solutions")
  )
  (lib_symbols
    (symbol "74xGxx:74AUP1G74" (pin_names (offset 1.016)) (in_bom yes) (on_board yes)
      (property "Reference" "U" (id 0) (at -2.54 5.08 0))
      (property "Value" "74AUP1G74" (id 1) (at 5.08 -5.08 0))
      (property "Footprint" "" (id 2) (at 0 0 0))
      (property "Datasheet" "http://www.ti.com/lit/sg/scyt129e/scyt129e.pdf" (id 3) (at 0 0 0))
      (property "ki_keywords" "Single D Flip-Flop D CMOS" (id 4) (at 0 0 0))
      (property "ki_description" "Single D Flip-Flop, Low-Voltage CMOS" (id 5) (at 0 0 0))
      (property "ki_fp_filters" "SSOP* VSSOP*" (id 6) (at 0 0 0))
      (symbol "74AUP1G74_0_1"
        (rectangle (start -3.81 3.81) (end 3.81 -3.81)
          (fill (type none))
        )
      )
      (symbol "74AUP1G74_1_1"
        (pin input clock (at -6.35 -2.54 0) (length 2.54)
          (name "C")
          (number "1")
        )
        (pin input line (at -6.35 2.54 0) (length 2.54)
          (name "D")
          (number "2")
        )
        (pin output line (at 6.35 -2.54 180) (length 2.54)
          (name "~{Q}")
          (number "3")
        )
        (pin power_in line (at -3.81 -3.81 270) (length 0) hide
          (name "GND")
          (number "4")
        )
        (pin output line (at 6.35 2.54 180) (length 2.54)
          (name "Q")
          (number "5")
        )
        (pin input line (at 0 -6.35 90) (length 2.54)
          (name "~{CLR}")
          (number "6")
        )
        (pin input line (at 0 6.35 270) (length 2.54)
          (name "~{PRE}")
          (number "7")
        )
        (pin power_in line (at -3.81 3.81 90) (length 0) hide
          (name "VCC")
          (number "8")
        )
      )
    )
    (symbol "74xGxx:74LVC2G66" (pin_names (offset 1.016)) (in_bom yes) (on_board yes)
      (property "Reference" "U" (id 0) (at -2.54 5.08 0))
      (property "Value" "74LVC2G66" (id 1) (at 0 -5.08 0))
      (property "Footprint" "" (id 2) (at 0 0 0))
      (property "Datasheet" "http://www.ti.com/lit/sg/scyt129e/scyt129e.pdf" (id 3) (at 0 0 0))
      (property "ki_keywords" "Dual Analog Switch" (id 4) (at 0 0 0))
      (property "ki_description" "Dual Analog Switch" (id 5) (at 0 0 0))
      (property "ki_fp_filters" "SSOP* VSSOP*" (id 6) (at 0 0 0))
      (symbol "74LVC2G66_0_1"
        (circle (center -3.556 -3.81) (radius 0.127)
          (fill (type none))
        )
        (polyline
          (pts
            (xy -3.81 0)
            (xy -2.54 0)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -2.54 2.54)
            (xy -2.54 -2.54)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 2.54 0)
            (xy 3.81 0)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 2.54 2.54)
            (xy 2.54 -2.54)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -3.81 -3.81)
            (xy 0 -3.81)
            (xy 0 -1.27)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -2.54 -2.54)
            (xy 2.54 0)
            (xy -2.54 2.54)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 2.54 2.54)
            (xy -2.54 0)
            (xy 2.54 -2.54)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 0 2.159)
            (xy 0 3.302)
            (xy -3.556 3.302)
            (xy -3.556 -3.81)
          )
          (fill (type none))
        )
        (circle (center 0 1.778) (radius 0.381)
          (fill (type none))
        )
        (pin power_in line (at 1.27 -3.81 270) (length 0) hide
          (name "GND")
          (number "4")
        )
        (pin power_in line (at 1.27 3.81 90) (length 0) hide
          (name "VCC")
          (number "8")
        )
      )
      (symbol "74LVC2G66_1_1"
        (pin input line (at -6.35 0 0) (length 2.54)
          (name "~")
          (number "1")
        )
        (pin tri_state line (at 6.35 0 180) (length 2.54)
          (name "~")
          (number "2")
        )
        (pin input line (at -6.35 -3.81 0) (length 2.54)
          (name "~")
          (number "7")
        )
      )
      (symbol "74LVC2G66_2_1"
        (pin input line (at -6.35 -3.81 0) (length 2.54)
          (name "~")
          (number "3")
        )
        (pin input line (at -6.35 0 0) (length 2.54)
          (name "~")
          (number "5")
        )
        (pin tri_state line (at 6.35 0 180) (length 2.54)
          (name "~")
          (number "6")
        )
      )
    )
    (symbol "Connector_Generic:Conn_01x01" (pin_names (offset 1.016) hide) (in_bom yes) (on_board yes)
      (property "Reference" "J" (id 0) (at 0 2.54 0))
      (property "Value" "Conn_01x01" (id 1) (at 0 -2.54 0))
      (property "Footprint" "" (id 2) (at 0 0 0))
      (property "Datasheet" "~" (id 3) (at 0 0 0))
      (property "ki_keywords" "connector" (id 4) (at 0 0 0))
      (property "ki_description" "Generic connector, single row, 01x01, script generated (kicad-library-utils/schlib/autogen/connector/)" (id 5) (at 0 0 0))
      (property "ki_fp_filters" "Connector*:*_1x??_*" (id 6) (at 0 0 0))
      (symbol "Conn_01x01_1_1"
        (rectangle (start -1.27 0.127) (end 0 -0.127)
          (fill (type none))
        )
        (rectangle (start -1.27 1.27) (end 1.27 -1.27)
          (fill (type background))
        )
        (pin passive line (at -5.08 0 0) (length 3.81)
          (name "Pin_1")
          (number "1")
        )
      )
    )
    (symbol "Device:Battery_Cell" (pin_numbers hide) (pin_names (offset 0) hide) (in_bom yes) (on_board yes)
      (property "Reference" "BT" (id 0) (at 2.54 2.54 0))
      (property "Value" "Battery_Cell" (id 1) (at 2.54 0 0))
      (property "Footprint" "" (id 2) (at 0 1.524 90))
      (property "Datasheet" "~" (id 3) (at 0 1.524 90))
      (property "ki_keywords" "battery cell" (id 4) (at 0 0 0))
      (property "ki_description" "Single-cell battery" (id 5) (at 0 0 0))
      (symbol "Battery_Cell_0_1"
        (rectangle (start -2.286 1.778) (end 2.286 1.524)
          (fill (type outline))
        )
        (rectangle (start -1.5748 1.1938) (end 1.4732 0.6858)
          (fill (type outline))
        )
        (polyline
          (pts
            (xy 0 0.762)
            (xy 0 0)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 0 1.778)
            (xy 0 2.54)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 0.508 3.429)
            (xy 1.524 3.429)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 1.016 3.937)
            (xy 1.016 2.921)
          )
          (fill (type none))
        )
      )
      (symbol "Battery_Cell_1_1"
        (pin passive line (at 0 5.08 270) (length 2.54)
          (name "+")
          (number "1")
        )
        (pin passive line (at 0 -2.54 90) (length 2.54)
          (name "-")
          (number "2")
        )
      )
    )
    (symbol "Device:C" (pin_numbers hide) (pin_names (offset 0.254)) (in_bom yes) (on_board yes)
      (property "Reference" "C" (id 0) (at 0.635 2.54 0))
      (property "Value" "C" (id 1) (at 0.635 -2.54 0))
      (property "Footprint" "" (id 2) (at 0.9652 -3.81 0))
      (property "Datasheet" "~" (id 3) (at 0 0 0))
      (property "ki_keywords" "cap capacitor" (id 4) (at 0 0 0))
      (property "ki_description" "Unpolarized capacitor" (id 5) (at 0 0 0))
      (property "ki_fp_filters" "C_*" (id 6) (at 0 0 0))
      (symbol "C_0_1"
        (polyline
          (pts
            (xy -2.032 -0.762)
            (xy 2.032 -0.762)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -2.032 0.762)
            (xy 2.032 0.762)
          )
          (fill (type none))
        )
      )
      (symbol "C_1_1"
        (pin passive line (at 0 3.81 270) (length 2.794)
          (name "~")
          (number "1")
        )
        (pin passive line (at 0 -3.81 90) (length 2.794)
          (name "~")
          (number "2")
        )
      )
    )
    (symbol "Device:C_Small" (pin_numbers hide) (pin_names (offset 0.254) hide) (in_bom yes) (on_board yes)
      (property "Reference" "C" (id 0) (at 0.254 1.778 0))
      (property "Value" "C_Small" (id 1) (at 0.254 -2.032 0))
      (property "Footprint" "" (id 2) (at 0 0 0))
      (property "Datasheet" "~" (id 3) (at 0 0 0))
      (property "ki_keywords" "capacitor cap" (id 4) (at 0 0 0))
      (property "ki_description" "Unpolarized capacitor, small symbol" (id 5) (at 0 0 0))
      (property "ki_fp_filters" "C_*" (id 6) (at 0 0 0))
      (symbol "C_Small_0_1"
        (polyline
          (pts
            (xy -1.524 -0.508)
            (xy 1.524 -0.508)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -1.524 0.508)
            (xy 1.524 0.508)
          )
          (fill (type none))
        )
      )
      (symbol "C_Small_1_1"
        (pin passive line (at 0 2.54 270) (length 2.032)
          (name "~")
          (number "1")
        )
        (pin passive line (at 0 -2.54 90) (length 2.032)
          (name "~")
          (number "2")
        )
      )
    )
    (symbol "Device:LED_Small" (pin_numbers hide) (pin_names (offset 0.254) hide) (in_bom yes) (on_board yes)
      (property "Reference" "D" (id 0) (at -1.27 3.175 0))
      (property "Value" "LED_Small" (id 1) (at -4.445 -2.54 0))
      (property "Footprint" "" (id 2) (at 0 0 90))
      (property "Datasheet" "~" (id 3) (at 0 0 90))
      (property "ki_keywords" "LED diode light-emitting-diode" (id 4) (at 0 0 0))
      (property "ki_description" "Light emitting diode, small symbol" (id 5) (at 0 0 0))
      (property "ki_fp_filters" "LED* LED_SMD:* LED_THT:*" (id 6) (at 0 0 0))
      (symbol "LED_Small_0_1"
        (polyline
          (pts
            (xy -0.762 -1.016)
            (xy -0.762 1.016)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 1.016 0)
            (xy -0.762 0)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 0.762 -1.016)
            (xy -0.762 0)
            (xy 0.762 1.016)
            (xy 0.762 -1.016)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 0 0.762)
            (xy -0.508 1.27)
            (xy -0.254 1.27)
            (xy -0.508 1.27)
            (xy -0.508 1.016)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 0.508 1.27)
            (xy 0 1.778)
            (xy 0.254 1.778)
            (xy 0 1.778)
            (xy 0 1.524)
          )
          (fill (type none))
        )
      )
      (symbol "LED_Small_1_1"
        (pin passive line (at -2.54 0 0) (length 1.778)
          (name "K")
          (number "1")
        )
        (pin passive line (at 2.54 0 180) (length 1.778)
          (name "A")
          (number "2")
        )
      )
    )
    (symbol "Device:R_Small_US" (pin_numbers hide) (pin_names (offset 0.254) hide) (in_bom yes) (on_board yes)
      (property "Reference" "R" (id 0) (at 0.762 0.508 0))
      (property "Value" "R_Small_US" (id 1) (at 0.762 -1.016 0))
      (property "Footprint" "" (id 2) (at 0 0 0))
      (property "Datasheet" "~" (id 3) (at 0 0 0))
      (property "ki_keywords" "r resistor" (id 4) (at 0 0 0))
      (property "ki_description" "Resistor, small US symbol" (id 5) (at 0 0 0))
      (property "ki_fp_filters" "R_*" (id 6) (at 0 0 0))
      (symbol "R_Small_US_1_1"
        (polyline
          (pts
            (xy 0 0)
            (xy 1.016 -0.381)
            (xy 0 -0.762)
            (xy -1.016 -1.143)
            (xy 0 -1.524)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 0 1.524)
            (xy 1.016 1.143)
            (xy 0 0.762)
            (xy -1.016 0.381)
            (xy 0 0)
          )
          (fill (type none))
        )
        (pin passive line (at 0 2.54 270) (length 1.016)
          (name "~")
          (number "1")
        )
        (pin passive line (at 0 -2.54 90) (length 1.016)
          (name "~")
          (number "2")
        )
      )
    )
    (symbol "Diode:B120-E3" (pin_numbers hide) (pin_names hide) (in_bom yes) (on_board yes)
      (property "Reference" "D" (id 0) (at 0 2.54 0))
      (property "Value" "B120-E3" (id 1) (at 0 -2.54 0))
      (property "Footprint" "Diode_SMD:D_SMA" (id 2) (at 0 -4.445 0))
      (property "Datasheet" "http://www.vishay.com/docs/88946/b120.pdf" (id 3) (at 0 0 0))
      (property "ki_keywords" "diode Schottky" (id 4) (at 0 0 0))
      (property "ki_description" "20V 1A Schottky Barrier Rectifier Diode, SMA(DO-214AC)" (id 5) (at 0 0 0))
      (property "ki_fp_filters" "D*SMA*" (id 6) (at 0 0 0))
      (symbol "B120-E3_0_1"
        (polyline
          (pts
            (xy 1.27 0)
            (xy -1.27 0)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 1.27 1.27)
            (xy 1.27 -1.27)
            (xy -1.27 0)
            (xy 1.27 1.27)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -1.905 0.635)
            (xy -1.905 1.27)
            (xy -1.27 1.27)
            (xy -1.27 -1.27)
            (xy -0.635 -1.27)
            (xy -0.635 -0.635)
          )
          (fill (type none))
        )
      )
      (symbol "B120-E3_1_1"
        (pin passive line (at -3.81 0 0) (length 2.54)
          (name "K")
          (number "1")
        )
        (pin passive line (at 3.81 0 180) (length 2.54)
          (name "A")
          (number "2")
        )
      )
    )
    (symbol "Diode:BAT43W-V" (pin_numbers hide) (pin_names (offset 1.016) hide) (in_bom yes) (on_board yes)
      (property "Reference" "D" (id 0) (at 0 2.54 0))
      (property "Value" "BAT43W-V" (id 1) (at 0 -2.54 0))
      (property "Footprint" "Diode_SMD:D_SOD-123" (id 2) (at 0 -4.445 0))
      (property "Datasheet" "http://www.vishay.com/docs/85660/bat42.pdf" (id 3) (at 0 0 0))
      (property "ki_keywords" "diode Schottky" (id 4) (at 0 0 0))
      (property "ki_description" "30V 0.2A Small Signal Schottky diode, SOD-123" (id 5) (at 0 0 0))
      (property "ki_fp_filters" "D*SOD?123*" (id 6) (at 0 0 0))
      (symbol "BAT43W-V_0_1"
        (polyline
          (pts
            (xy 1.27 0)
            (xy -1.27 0)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 1.27 1.27)
            (xy 1.27 -1.27)
            (xy -1.27 0)
            (xy 1.27 1.27)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -1.905 0.635)
            (xy -1.905 1.27)
            (xy -1.27 1.27)
            (xy -1.27 -1.27)
            (xy -0.635 -1.27)
            (xy -0.635 -0.635)
          )
          (fill (type none))
        )
      )
      (symbol "BAT43W-V_1_1"
        (pin passive line (at -3.81 0 0) (length 2.54)
          (name "K")
          (number "1")
        )
        (pin passive line (at 3.81 0 180) (length 2.54)
          (name "A")
          (number "2")
        )
      )
    )
    (symbol "ProjectLib:LT3991EMS-ADJ" (in_bom yes) (on_board yes)
      (property "Reference" "U" (id 0) (at 0 11.43 0))
      (property "Value" "LT3991EMS-ADJ" (id 1) (at 0 8.89 0))
      (property "Footprint" "" (id 2) (at 0 0 0))
      (property "Datasheet" "" (id 3) (at 0 0 0))
      (symbol "LT3991EMS-ADJ_0_1"
        (rectangle (start -6.35 7.62) (end 6.35 -7.62)
          (fill (type none))
        )
      )
      (symbol "LT3991EMS-ADJ_1_1"
        (pin input line (at -8.89 5.08 0) (length 2.54)
          (name "BD")
          (number "1")
        )
        (pin input line (at 8.89 5.08 180) (length 2.54)
          (name "SYNC")
          (number "10")
        )
        (pin input line (at 0 -10.16 90) (length 2.54)
          (name "GND")
          (number "11")
        )
        (pin output line (at -8.89 2.54 0) (length 2.54)
          (name "BOOST")
          (number "2")
        )
        (pin output line (at -8.89 0 0) (length 2.54)
          (name "SW")
          (number "3")
        )
        (pin input line (at -8.89 -2.54 0) (length 2.54)
          (name "VIN")
          (number "4")
        )
        (pin input line (at -8.89 -5.08 0) (length 2.54)
          (name "EN")
          (number "5")
        )
        (pin input line (at 8.89 -5.08 180) (length 2.54)
          (name "FB")
          (number "6")
        )
        (pin input line (at 8.89 -2.54 180) (length 2.54)
          (name "SS")
          (number "7")
        )
        (pin input line (at 8.89 0 180) (length 2.54)
          (name "RT")
          (number "8")
        )
        (pin output line (at 8.89 2.54 180) (length 2.54)
          (name "PG")
          (number "9")
        )
      )
    )
    (symbol "ProjectLib:R3117N" (in_bom yes) (on_board yes)
      (property "Reference" "U" (id 0) (at 1.27 8.89 0))
      (property "Value" "R3117N" (id 1) (at 2.54 6.35 0))
      (property "Footprint" "" (id 2) (at 0 -10.16 0))
      (property "Datasheet" "" (id 3) (at 0 -10.16 0))
      (symbol "R3117N_0_1"
        (rectangle (start -6.35 5.08) (end 6.35 -5.08)
          (fill (type none))
        )
      )
      (symbol "R3117N_1_1"
        (pin output line (at -8.89 2.54 0) (length 2.54)
          (name "OUT")
          (number "1")
        )
        (pin power_in line (at -8.89 0 0) (length 2.54)
          (name "VDD")
          (number "2")
        )
        (pin power_in line (at -8.89 -2.54 0) (length 2.54)
          (name "GND")
          (number "3")
        )
        (pin no_connect line (at 8.89 -2.54 180) (length 2.54)
          (name "NC")
          (number "4")
        )
        (pin input line (at 8.89 2.54 180) (length 2.54)
          (name "SENSE")
          (number "5")
        )
      )
    )
    (symbol "ProjectLib:RTC-RV-3032" (in_bom yes) (on_board yes)
      (property "Reference" "U" (id 0) (at 3.81 7.62 0))
      (property "Value" "RTC-RV-3032" (id 1) (at 0 -7.62 0))
      (property "Footprint" "" (id 2) (at 0 0 0))
      (property "Datasheet" "" (id 3) (at 0 0 0))
      (symbol "RTC-RV-3032_0_0"
        (pin bidirectional line (at -12.7 3.81 0) (length 5.08)
          (name "Vbackup")
          (number "1")
        )
        (pin bidirectional line (at -12.7 1.27 0) (length 5.08)
          (name "SDA")
          (number "2")
        )
        (pin output line (at -12.7 -1.27 0) (length 5.08)
          (name "~{INT}")
          (number "3")
        )
        (pin input line (at -12.7 -3.81 0) (length 5.08)
          (name "EVI")
          (number "4")
        )
        (pin power_in line (at 12.7 -3.81 180) (length 5.08)
          (name "GND")
          (number "5")
        )
        (pin power_in line (at 12.7 -1.27 180) (length 5.08)
          (name "VDD")
          (number "6")
        )
        (pin output line (at 12.7 1.27 180) (length 5.08)
          (name "CLKOUT")
          (number "7")
        )
        (pin bidirectional line (at 12.7 3.81 180) (length 5.08)
          (name "SCL")
          (number "8")
        )
      )
      (symbol "RTC-RV-3032_0_1"
        (rectangle (start -7.62 6.35) (end 7.62 -6.35)
          (fill (type none))
        )
      )
    )
    (symbol "ProjectLib:Wakestr_Slim_v1" (in_bom yes) (on_board yes)
      (property "Reference" "U" (id 0) (at 1.27 13.97 0))
      (property "Value" "Wakestr_Slim_v1" (id 1) (at 16.51 13.97 0))
      (property "Footprint" "" (id 2) (at 0 0 0))
      (property "Datasheet" "" (id 3) (at 0 0 0))
      (symbol "Wakestr_Slim_v1_0_1"
        (rectangle (start -6.35 12.7) (end 25.4 -12.7)
          (fill (type none))
        )
      )
      (symbol "Wakestr_Slim_v1_1_1"
        (pin input line (at -8.89 -10.16 0) (length 2.54)
          (name "GND")
          (number "1")
        )
        (pin input line (at 27.94 5.08 180) (length 2.54)
          (name "SER_RX")
          (number "10")
        )
        (pin input line (at 27.94 2.54 180) (length 2.54)
          (name "~{SPI_CS}")
          (number "11")
        )
        (pin input line (at 27.94 0 180) (length 2.54)
          (name "WAKE_P")
          (number "12")
        )
        (pin output line (at 27.94 -2.54 180) (length 2.54)
          (name "~{VREG_EN}")
          (number "13")
        )
        (pin output line (at 27.94 -5.08 180) (length 2.54)
          (name "~{ALARM}")
          (number "14")
        )
        (pin output line (at 27.94 -7.62 180) (length 2.54)
          (name "+3VX_ON")
          (number "15")
        )
        (pin input line (at 27.94 -10.16 180) (length 2.54)
          (name "GND")
          (number "16")
        )
        (pin input line (at -8.89 -7.62 0) (length 2.54)
          (name "VIN")
          (number "2")
        )
        (pin output line (at -8.89 -5.08 0) (length 2.54)
          (name "+3VX")
          (number "3")
        )
        (pin output line (at -8.89 -2.54 0) (length 2.54)
          (name "+3V_COIN")
          (number "4")
        )
        (pin output line (at -8.89 0 0) (length 2.54)
          (name "VREG_EN")
          (number "5")
        )
        (pin input line (at -8.89 2.54 0) (length 2.54)
          (name "~{WAKE}")
          (number "6")
        )
        (pin input line (at -8.89 5.08 0) (length 2.54)
          (name "~{PROC_SLEEP}")
          (number "7")
        )
        (pin bidirectional line (at -8.89 7.62 0) (length 2.54)
          (name "I2C_SDA")
          (number "8")
        )
        (pin bidirectional line (at -8.89 10.16 0) (length 2.54)
          (name "I2C_SCL")
          (number "9")
        )
      )
    )
    (symbol "Switch:SW_DIP_x01" (pin_names (offset 0) hide) (in_bom yes) (on_board yes)
      (property "Reference" "SW" (id 0) (at 0 3.81 0))
      (property "Value" "SW_DIP_x01" (id 1) (at 0 -3.81 0))
      (property "Footprint" "" (id 2) (at 0 0 0))
      (property "Datasheet" "~" (id 3) (at 0 0 0))
      (property "ki_keywords" "dip switch" (id 4) (at 0 0 0))
      (property "ki_description" "1x DIP Switch, Single Pole Single Throw (SPST) switch, small symbol" (id 5) (at 0 0 0))
      (property "ki_fp_filters" "SW?DIP?x1*" (id 6) (at 0 0 0))
      (symbol "SW_DIP_x01_0_0"
        (circle (center -2.032 0) (radius 0.508)
          (fill (type none))
        )
        (polyline
          (pts
            (xy -1.524 0.127)
            (xy 2.3622 1.1684)
          )
          (fill (type none))
        )
        (circle (center 2.032 0) (radius 0.508)
          (fill (type none))
        )
      )
      (symbol "SW_DIP_x01_0_1"
        (rectangle (start -3.81 2.54) (end 3.81 -2.54)
          (fill (type background))
        )
      )
      (symbol "SW_DIP_x01_1_1"
        (pin passive line (at -7.62 0 0) (length 5.08)
          (name "~")
          (number "1")
        )
        (pin passive line (at 7.62 0 180) (length 5.08)
          (name "~")
          (number "2")
        )
      )
    )
    (symbol "Transistor_BJT:BC846BS" (pin_names (offset 0) hide) (in_bom yes) (on_board yes)
      (property "Reference" "Q" (id 0) (at 5.08 1.27 0))
      (property "Value" "BC846BS" (id 1) (at 5.08 -1.27 0))
      (property "Footprint" "Package_TO_SOT_SMD:SOT-363_SC-70-6" (id 2) (at 5.08 2.54 0))
      (property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/BC846BS.pdf" (id 3) (at 0 0 0))
      (property "ki_locked" "" (id 4) (at 0 0 0))
      (property "ki_keywords" "NPN/NPN Transistor" (id 5) (at 0 0 0))
      (property "ki_description" "100mA IC, 65V Vce, Dual NPN/NPN Transistors, SOT-363" (id 6) (at 0 0 0))
      (property "ki_fp_filters" "SOT?363*" (id 7) (at 0 0 0))
      (symbol "BC846BS_0_1"
        (polyline
          (pts
            (xy 0.635 0)
            (xy -2.54 0)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 0.635 0.635)
            (xy 2.54 2.54)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 0.635 -0.635)
            (xy 2.54 -2.54)
            (xy 2.54 -2.54)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 0.635 1.905)
            (xy 0.635 -1.905)
            (xy 0.635 -1.905)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 1.27 -1.778)
            (xy 1.778 -1.27)
            (xy 2.286 -2.286)
            (xy 1.27 -1.778)
            (xy 1.27 -1.778)
          )
          (fill (type outline))
        )
        (circle (center 1.27 0) (radius 2.8194)
          (fill (type none))
        )
      )
      (symbol "BC846BS_1_1"
        (pin passive line (at 2.54 -5.08 90) (length 2.54)
          (name "E1")
          (number "1")
        )
        (pin input line (at -5.08 0 0) (length 2.54)
          (name "B1")
          (number "2")
        )
        (pin passive line (at 2.54 5.08 270) (length 2.54)
          (name "C1")
          (number "6")
        )
      )
      (symbol "BC846BS_2_1"
        (pin passive line (at 2.54 5.08 270) (length 2.54)
          (name "C2")
          (number "3")
        )
        (pin passive line (at 2.54 -5.08 90) (length 2.54)
          (name "E2")
          (number "4")
        )
        (pin input line (at -5.08 0 0) (length 2.54)
          (name "B2")
          (number "5")
        )
      )
    )
    (symbol "Transistor_BJT:BC856BS" (pin_names (offset 0) hide) (in_bom yes) (on_board yes)
      (property "Reference" "Q" (id 0) (at 5.08 1.27 0))
      (property "Value" "BC856BS" (id 1) (at 5.08 -1.27 0))
      (property "Footprint" "Package_TO_SOT_SMD:SOT-363_SC-70-6" (id 2) (at 5.08 2.54 0))
      (property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/BC856BS.pdf" (id 3) (at 0 0 0))
      (property "ki_locked" "" (id 4) (at 0 0 0))
      (property "ki_keywords" "PNP/PNP Transistor" (id 5) (at 0 0 0))
      (property "ki_description" "100mA IC, 65V Vce, Dual PNP/PNP Transistors, SOT-363" (id 6) (at 0 0 0))
      (property "ki_fp_filters" "SOT?363*" (id 7) (at 0 0 0))
      (symbol "BC856BS_0_1"
        (polyline
          (pts
            (xy 0.635 0)
            (xy -2.54 0)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 0.635 0.635)
            (xy 2.54 2.54)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 0.635 -0.635)
            (xy 2.54 -2.54)
            (xy 2.54 -2.54)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 0.635 1.905)
            (xy 0.635 -1.905)
            (xy 0.635 -1.905)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 2.286 -1.778)
            (xy 1.778 -2.286)
            (xy 1.27 -1.27)
            (xy 2.286 -1.778)
            (xy 2.286 -1.778)
          )
          (fill (type outline))
        )
        (circle (center 1.27 0) (radius 2.8194)
          (fill (type none))
        )
      )
      (symbol "BC856BS_1_1"
        (pin passive line (at 2.54 -5.08 90) (length 2.54)
          (name "E1")
          (number "1")
        )
        (pin input line (at -5.08 0 0) (length 2.54)
          (name "B1")
          (number "2")
        )
        (pin passive line (at 2.54 5.08 270) (length 2.54)
          (name "C1")
          (number "6")
        )
      )
      (symbol "BC856BS_2_1"
        (pin passive line (at 2.54 5.08 270) (length 2.54)
          (name "C2")
          (number "3")
        )
        (pin passive line (at 2.54 -5.08 90) (length 2.54)
          (name "E2")
          (number "4")
        )
        (pin input line (at -5.08 0 0) (length 2.54)
          (name "B2")
          (number "5")
        )
      )
    )
    (symbol "power:GND" (power) (pin_names (offset 0)) (in_bom yes) (on_board yes)
      (property "Reference" "#PWR" (id 0) (at 0 -6.35 0))
      (property "Value" "GND" (id 1) (at 0 -3.81 0))
      (property "Footprint" "" (id 2) (at 0 0 0))
      (property "Datasheet" "" (id 3) (at 0 0 0))
      (property "ki_keywords" "power-flag" (id 4) (at 0 0 0))
      (property "ki_description" "Power symbol creates a global label with name \"GND\" , ground" (id 5) (at 0 0 0))
      (symbol "GND_0_1"
        (polyline
          (pts
            (xy 0 0)
            (xy 0 -1.27)
            (xy 1.27 -1.27)
            (xy 0 -2.54)
            (xy -1.27 -1.27)
            (xy 0 -1.27)
          )
          (fill (type none))
        )
      )
      (symbol "GND_1_1"
        (pin power_in line (at 0 0 270) (length 0) hide
          (name "GND")
          (number "1")
        )
      )
    )
    (symbol "pspice:INDUCTOR" (pin_numbers hide) (pin_names (offset 0)) (in_bom yes) (on_board yes)
      (property "Reference" "L" (id 0) (at 0 2.54 0))
      (property "Value" "INDUCTOR" (id 1) (at 0 -1.27 0))
      (property "Footprint" "" (id 2) (at 0 0 0))
      (property "Datasheet" "~" (id 3) (at 0 0 0))
      (property "ki_keywords" "simulation" (id 4) (at 0 0 0))
      (property "ki_description" "Inductor symbol for simulation only" (id 5) (at 0 0 0))
      (symbol "INDUCTOR_0_1"
        (arc (start -2.54 0) (mid -3.81 1.27) (end -5.08 0)
          (fill (type none))
        )
        (arc (start 0 0) (mid -1.27 1.27) (end -2.54 0)
          (fill (type none))
        )
        (arc (start 2.54 0) (mid 1.27 1.27) (end 0 0)
          (fill (type none))
        )
        (arc (start 5.08 0) (mid 3.81 1.27) (end 2.54 0)
          (fill (type none))
        )
      )
      (symbol "INDUCTOR_1_1"
        (pin input line (at -6.35 0 0) (length 1.27)
          (name "1")
          (number "1")
        )
        (pin input line (at 6.35 0 180) (length 1.27)
          (name "2")
          (number "2")
        )
      )
    )
  )
  (junction (at 288.29 201.93) (diameter 0) (color 0 0 0 0))
  (junction (at 50.8 88.9) (diameter 0) (color 0 0 0 0))
  (junction (at 161.29 144.78) (diameter 0) (color 0 0 0 0))
  (junction (at 325.12 196.85) (diameter 0) (color 0 0 0 0))
  (junction (at 317.5 196.85) (diameter 0) (color 0 0 0 0))
  (junction (at 46.99 74.93) (diameter 0) (color 0 0 0 0))
  (junction (at 78.74 157.48) (diameter 0) (color 0 0 0 0))
  (junction (at 134.62 97.79) (diameter 0) (color 0 0 0 0))
  (junction (at 275.59 118.11) (diameter 0) (color 0 0 0 0))
  (junction (at 283.21 214.63) (diameter 0) (color 0 0 0 0))
  (junction (at 67.31 72.39) (diameter 0) (color 0 0 0 0))
  (junction (at 317.5 187.96) (diameter 0) (color 0 0 0 0))
  (junction (at 73.66 134.62) (diameter 0) (color 0 0 0 0))
  (junction (at 64.77 134.62) (diameter 0) (color 0 0 0 0))
  (junction (at 48.26 138.43) (diameter 0) (color 0 0 0 0))
  (junction (at 288.29 187.96) (diameter 0) (color 0 0 0 0))
  (junction (at 294.64 187.96) (diameter 0) (color 0 0 0 0))
  (junction (at 267.97 106.68) (diameter 0) (color 0 0 0 0))
  (junction (at 55.88 74.93) (diameter 0) (color 0 0 0 0))
  (junction (at 143.51 91.44) (diameter 0) (color 0 0 0 0))
  (junction (at 144.78 91.44) (diameter 0) (color 0 0 0 0))
  (junction (at 267.97 139.7) (diameter 0) (color 0 0 0 0))
  (junction (at 254 195.58) (diameter 0) (color 0 0 0 0))
  (junction (at 172.72 144.78) (diameter 0) (color 0 0 0 0))
  (junction (at 240.03 204.47) (diameter 0) (color 0 0 0 0))
  (junction (at 255.27 64.77) (diameter 0) (color 0 0 0 0))
  (junction (at 85.09 144.78) (diameter 0) (color 0 0 0 0))
  (junction (at 149.225 91.44) (diameter 0) (color 0 0 0 0))
  (junction (at 302.26 196.85) (diameter 0) (color 0 0 0 0))
  (junction (at 111.76 91.44) (diameter 0) (color 0 0 0 0))
  (junction (at 278.13 209.55) (diameter 0) (color 0 0 0 0))
  (junction (at 134.62 81.28) (diameter 0) (color 0 0 0 0))
  (junction (at 294.64 214.63) (diameter 0) (color 0 0 0 0))
  (junction (at 267.97 132.08) (diameter 0) (color 0 0 0 0))
  (junction (at 325.12 187.96) (diameter 0) (color 0 0 0 0))
  (junction (at 267.97 118.11) (diameter 0) (color 0 0 0 0))
  (junction (at 64.77 123.19) (diameter 0) (color 0 0 0 0))
  (junction (at 73.66 123.19) (diameter 0) (color 0 0 0 0))
  (junction (at 81.28 123.19) (diameter 0) (color 0 0 0 0))
  (junction (at 246.38 207.01) (diameter 0) (color 0 0 0 0))
  (junction (at 309.88 196.85) (diameter 0) (color 0 0 0 0))
  (junction (at 143.51 81.28) (diameter 0) (color 0 0 0 0))
  (junction (at 309.88 187.96) (diameter 0) (color 0 0 0 0))
  (junction (at 248.92 204.47) (diameter 0) (color 0 0 0 0))
  (junction (at 302.26 187.96) (diameter 0) (color 0 0 0 0))
  (wire (pts (xy 127 212.09) (xy 139.7 212.09)))
  (wire (pts (xy 74.93 243.84) (xy 87.63 243.84)))
  (wire (pts (xy 74.93 264.16) (xy 87.63 264.16)))
  (wire (pts (xy 275.59 118.11) (xy 276.86 118.11)))
  (wire (pts (xy 302.26 194.31) (xy 302.26 196.85)))
  (wire (pts (xy 55.88 63.5) (xy 67.31 63.5)))
  (wire (pts (xy 127 201.93) (xy 139.7 201.93)))
  (wire (pts (xy 294.64 187.96) (xy 302.26 187.96)))
  (wire (pts (xy 90.17 209.55) (xy 77.47 209.55)))
  (wire (pts (xy 134.62 104.14) (xy 134.62 105.41)))
  (polyline (pts (xy 218.44 177.8) (xy 218.44 228.6)))
  (wire (pts (xy 275.59 106.68) (xy 275.59 109.22)))
  (wire (pts (xy 57.15 123.19) (xy 57.15 130.81)))
  (wire (pts (xy 27.94 240.03) (xy 40.64 240.03)))
  (wire (pts (xy 248.92 204.47) (xy 256.54 204.47)))
  (polyline (pts (xy 184.785 99.06) (xy 172.085 99.06)))
  (wire (pts (xy 64.77 134.62) (xy 64.77 151.13)))
  (wire (pts (xy 255.27 73.66) (xy 255.27 74.93)))
  (wire (pts (xy 73.66 123.19) (xy 81.28 123.19)))
  (wire (pts (xy 254 199.39) (xy 256.54 199.39)))
  (polyline (pts (xy 331.47 114.3) (xy 331.47 109.22)))
  (wire (pts (xy 143.51 88.9) (xy 143.51 91.44)))
  (wire (pts (xy 90.17 214.63) (xy 77.47 214.63)))
  (wire (pts (xy 90.17 204.47) (xy 77.47 204.47)))
  (polyline (pts (xy 218.44 177.8) (xy 346.71 177.8)))
  (wire (pts (xy 172.72 144.78) (xy 172.72 147.32)))
  (wire (pts (xy 35.56 170.18) (xy 25.4 170.18)))
  (wire (pts (xy 317.5 187.96) (xy 325.12 187.96)))
  (wire (pts (xy 67.31 69.85) (xy 67.31 72.39)))
  (wire (pts (xy 74.93 246.38) (xy 87.63 246.38)))
  (polyline (pts (xy 20.32 35.56) (xy 20.32 228.6)))
  (wire (pts (xy 288.29 187.96) (xy 283.21 187.96)))
  (wire (pts (xy 149.225 91.44) (xy 153.035 91.44)))
  (wire (pts (xy 125.73 152.4) (xy 138.43 152.4)))
  (wire (pts (xy 144.78 91.44) (xy 149.225 91.44)))
  (polyline (pts (xy 197.485 87.63) (xy 197.485 82.55)))
  (wire (pts (xy 46.99 82.55) (xy 46.99 83.82)))
  (polyline (pts (xy 187.325 90.17) (xy 193.675 90.17)))
  (wire (pts (xy 74.93 238.76) (xy 87.63 238.76)))
  (polyline (pts (xy 36.83 100.33) (xy 40.64 100.33)))
  (wire (pts (xy 127 209.55) (xy 139.7 209.55)))
  (wire (pts (xy 317.5 187.96) (xy 317.5 189.23)))
  (wire (pts (xy 88.9 154.94) (xy 100.33 154.94)))
  (wire (pts (xy 223.52 195.58) (xy 223.52 204.47)))
  (wire (pts (xy 278.13 139.7) (xy 298.45 139.7)))
  (wire (pts (xy 81.28 123.19) (xy 106.68 123.19)))
  (wire (pts (xy 294.64 214.63) (xy 294.64 220.98)))
  (wire (pts (xy 243.84 55.88) (xy 256.54 55.88)))
  (wire (pts (xy 134.62 81.28) (xy 111.76 81.28)))
  (wire (pts (xy 127 217.17) (xy 139.7 217.17)))
  (wire (pts (xy 302.26 187.96) (xy 302.26 189.23)))
  (wire (pts (xy 248.92 201.93) (xy 248.92 204.47)))
  (wire (pts (xy 78.74 146.05) (xy 78.74 144.78)))
  (wire (pts (xy 325.12 196.85) (xy 325.12 198.12)))
  (wire (pts (xy 50.8 88.9) (xy 50.8 90.17)))
  (wire (pts (xy 66.04 157.48) (xy 78.74 157.48)))
  (polyline (pts (xy 218.44 35.56) (xy 218.44 170.18)))
  (wire (pts (xy 255.27 64.77) (xy 255.27 66.04)))
  (wire (pts (xy 90.17 212.09) (xy 77.47 212.09)))
  (wire (pts (xy 187.96 144.78) (xy 187.96 147.32)))
  (wire (pts (xy 161.29 152.4) (xy 161.29 153.67)))
  (wire (pts (xy 339.09 200.66) (xy 339.09 201.93)))
  (wire (pts (xy 267.97 139.7) (xy 273.05 139.7)))
  (wire (pts (xy 271.78 160.02) (xy 276.86 160.02)))
  (wire (pts (xy 267.97 106.68) (xy 275.59 106.68)))
  (polyline (pts (xy 187.325 87.63) (xy 189.865 87.63)))
  (wire (pts (xy 106.68 97.79) (xy 106.68 91.44)))
  (wire (pts (xy 125.73 154.94) (xy 143.51 154.94)))
  (wire (pts (xy 34.29 175.26) (xy 34.29 177.8)))
  (wire (pts (xy 161.29 144.78) (xy 161.29 147.32)))
  (wire (pts (xy 64.77 123.19) (xy 73.66 123.19)))
  (wire (pts (xy 246.38 213.36) (xy 246.38 217.17)))
  (wire (pts (xy 35.56 175.26) (xy 34.29 175.26)))
  (wire (pts (xy 119.38 91.44) (xy 119.38 92.71)))
  (wire (pts (xy 255.27 201.93) (xy 256.54 201.93)))
  (wire (pts (xy 151.13 157.48) (xy 151.13 158.75)))
  (wire (pts (xy 278.13 209.55) (xy 278.13 210.82)))
  (wire (pts (xy 62.23 134.62) (xy 64.77 134.62)))
  (polyline (pts (xy 193.675 95.25) (xy 194.945 95.25)))
  (wire (pts (xy 274.32 207.01) (xy 275.59 207.01)))
  (polyline (pts (xy 330.2 228.6) (xy 346.71 228.6)))
  (polyline (pts (xy 193.675 90.17) (xy 193.675 95.25)))
  (wire (pts (xy 73.66 88.9) (xy 81.28 88.9)))
  (polyline (pts (xy 218.44 228.6) (xy 330.2 228.6)))
  (polyline (pts (xy 189.865 82.55) (xy 193.675 82.55)))
  (wire (pts (xy 309.88 196.85) (xy 317.5 196.85)))
  (wire (pts (xy 57.15 138.43) (xy 57.15 139.7)))
  (polyline (pts (xy 172.085 91.44) (xy 172.085 82.55)))
  (wire (pts (xy 267.97 118.11) (xy 275.59 118.11)))
  (wire (pts (xy 149.225 90.17) (xy 149.225 91.44)))
  (wire (pts (xy 50.8 88.9) (xy 60.96 88.9)))
  (polyline (pts (xy 184.785 82.55) (xy 184.785 99.06)))
  (wire (pts (xy 111.76 91.44) (xy 119.38 91.44)))
  (wire (pts (xy 267.97 132.08) (xy 267.97 133.35)))
  (wire (pts (xy 73.66 83.82) (xy 81.28 83.82)))
  (wire (pts (xy 63.5 74.93) (xy 63.5 82.55)))
  (wire (pts (xy 127 204.47) (xy 139.7 204.47)))
  (wire (pts (xy 143.51 154.94) (xy 143.51 140.97)))
  (wire (pts (xy 266.7 118.11) (xy 267.97 118.11)))
  (wire (pts (xy 259.08 127) (xy 241.3 127)))
  (wire (pts (xy 289.56 204.47) (xy 292.1 204.47)))
  (wire (pts (xy 67.31 64.77) (xy 67.31 63.5)))
  (wire (pts (xy 187.96 154.94) (xy 187.96 156.21)))
  (polyline (pts (xy 193.675 87.63) (xy 197.485 87.63)))
  (wire (pts (xy 127 207.01) (xy 139.7 207.01)))
  (wire (pts (xy 74.93 261.62) (xy 87.63 261.62)))
  (wire (pts (xy 143.51 81.28) (xy 143.51 83.82)))
  (wire (pts (xy 149.225 82.55) (xy 149.225 81.28)))
  (wire (pts (xy 27.94 250.19) (xy 40.64 250.19)))
  (wire (pts (xy 106.68 91.44) (xy 111.76 91.44)))
  (wire (pts (xy 325.12 196.85) (xy 325.12 194.31)))
  (polyline (pts (xy 194.945 90.17) (xy 210.185 90.17)))
  (wire (pts (xy 86.36 83.82) (xy 97.79 83.82)))
  (wire (pts (xy 243.84 207.01) (xy 246.38 207.01)))
  (wire (pts (xy 302.26 187.96) (xy 309.88 187.96)))
  (polyline (pts (xy 318.77 109.22) (xy 322.58 109.22)))
  (wire (pts (xy 50.8 95.25) (xy 50.8 96.52)))
  (wire (pts (xy 27.94 245.11) (xy 40.64 245.11)))
  (wire (pts (xy 74.93 259.08) (xy 87.63 259.08)))
  (wire (pts (xy 275.59 116.84) (xy 275.59 118.11)))
  (wire (pts (xy 280.67 207.01) (xy 285.75 207.01)))
  (polyline (pts (xy 20.32 228.6) (xy 209.55 228.6)))
  (wire (pts (xy 46.99 83.82) (xy 60.96 83.82)))
  (wire (pts (xy 142.24 91.44) (xy 143.51 91.44)))
  (wire (pts (xy 73.66 129.54) (xy 73.66 134.62)))
  (wire (pts (xy 294.64 194.31) (xy 294.64 196.85)))
  (wire (pts (xy 80.01 160.02) (xy 80.01 165.1)))
  (wire (pts (xy 223.52 195.58) (xy 254 195.58)))
  (wire (pts (xy 81.28 138.43) (xy 81.28 139.7)))
  (wire (pts (xy 67.31 92.71) (xy 67.31 97.79)))
  (wire (pts (xy 325.12 187.96) (xy 339.09 187.96)))
  (wire (pts (xy 250.19 201.93) (xy 248.92 201.93)))
  (wire (pts (xy 125.73 157.48) (xy 151.13 157.48)))
  (wire (pts (xy 240.03 204.47) (xy 248.92 204.47)))
  (polyline (pts (xy 322.58 114.3) (xy 323.85 114.3)))
  (wire (pts (xy 74.93 251.46) (xy 87.63 251.46)))
  (wire (pts (xy 259.08 106.68) (xy 259.08 113.03)))
  (wire (pts (xy 125.73 160.02) (xy 138.43 160.02)))
  (wire (pts (xy 254 195.58) (xy 254 199.39)))
  (wire (pts (xy 27.94 255.27) (xy 40.64 255.27)))
  (wire (pts (xy 67.31 97.79) (xy 106.68 97.79)))
  (wire (pts (xy 161.29 144.78) (xy 172.72 144.78)))
  (wire (pts (xy 267.97 132.08) (xy 270.51 132.08)))
  (wire (pts (xy 288.29 201.93) (xy 308.61 201.93)))
  (wire (pts (xy 276.86 160.02) (xy 276.86 162.56)))
  (polyline (pts (xy 218.44 35.56) (xy 346.71 35.56)))
  (wire (pts (xy 34.29 138.43) (xy 48.26 138.43)))
  (wire (pts (xy 223.52 204.47) (xy 226.06 204.47)))
  (wire (pts (xy 46.99 77.47) (xy 46.99 74.93)))
  (wire (pts (xy 255.27 64.77) (xy 257.81 64.77)))
  (wire (pts (xy 88.9 138.43) (xy 100.33 138.43)))
  (wire (pts (xy 309.88 194.31) (xy 309.88 196.85)))
  (wire (pts (xy 317.5 196.85) (xy 325.12 196.85)))
  (polyline (pts (xy 331.47 109.22) (xy 334.01 109.22)))
  (polyline (pts (xy 318.77 114.3) (xy 318.77 109.22)))
  (wire (pts (xy 309.88 187.96) (xy 317.5 187.96)))
  (wire (pts (xy 285.75 220.98) (xy 283.21 220.98)))
  (wire (pts (xy 36.83 74.93) (xy 36.83 76.2)))
  (wire (pts (xy 241.3 160.02) (xy 256.54 160.02)))
  (polyline (pts (xy 323.85 118.11) (xy 322.58 118.11)))
  (wire (pts (xy 90.17 201.93) (xy 77.47 201.93)))
  (wire (pts (xy 309.88 187.96) (xy 309.88 189.23)))
  (wire (pts (xy 134.62 96.52) (xy 134.62 97.79)))
  (polyline (pts (xy 346.71 228.6) (xy 346.71 177.8)))
  (polyline (pts (xy 322.58 109.22) (xy 322.58 114.3)))
  (wire (pts (xy 283.21 214.63) (xy 285.75 214.63)))
  (wire (pts (xy 138.43 160.02) (xy 138.43 161.29)))
  (wire (pts (xy 73.66 123.19) (xy 73.66 124.46)))
  (wire (pts (xy 111.76 81.28) (xy 111.76 82.55)))
  (wire (pts (xy 243.84 55.88) (xy 243.84 59.69)))
  (wire (pts (xy 339.09 194.31) (xy 339.09 195.58)))
  (polyline (pts (xy 34.29 104.14) (xy 36.83 104.14)))
  (wire (pts (xy 27.94 242.57) (xy 40.64 242.57)))
  (wire (pts (xy 74.93 248.92) (xy 87.63 248.92)))
  (wire (pts (xy 73.66 134.62) (xy 73.66 151.13)))
  (polyline (pts (xy 311.15 121.92) (xy 322.58 121.92)))
  (wire (pts (xy 106.68 123.19) (xy 106.68 125.73)))
  (polyline (pts (xy 323.85 121.92) (xy 334.01 121.92)))
  (wire (pts (xy 27.94 252.73) (xy 40.64 252.73)))
  (wire (pts (xy 90.17 199.39) (xy 77.47 199.39)))
  (polyline (pts (xy 312.42 114.3) (xy 318.77 114.3)))
  (wire (pts (xy 48.26 138.43) (xy 48.26 139.7)))
  (polyline (pts (xy 161.925 91.44) (xy 169.545 91.44)))
  (wire (pts (xy 240.03 213.36) (xy 240.03 217.17)))
  (wire (pts (xy 73.66 134.62) (xy 76.2 134.62)))
  (wire (pts (xy 53.34 170.18) (xy 59.69 170.18)))
  (polyline (pts (xy 36.83 104.14) (xy 36.83 100.33)))
  (wire (pts (xy 243.84 69.85) (xy 243.84 71.12)))
  (wire (pts (xy 325.12 187.96) (xy 325.12 189.23)))
  (wire (pts (xy 254 195.58) (xy 283.21 195.58)))
  (wire (pts (xy 238.76 204.47) (xy 240.03 204.47)))
  (wire (pts (xy 302.26 196.85) (xy 309.88 196.85)))
  (wire (pts (xy 134.62 81.28) (xy 143.51 81.28)))
  (wire (pts (xy 149.225 81.28) (xy 143.51 81.28)))
  (polyline (pts (xy 322.58 118.11) (xy 322.58 121.92)))
  (wire (pts (xy 143.51 91.44) (xy 144.78 91.44)))
  (wire (pts (xy 172.72 144.78) (xy 187.96 144.78)))
  (wire (pts (xy 259.08 148.59) (xy 241.3 148.59)))
  (wire (pts (xy 55.88 74.93) (xy 63.5 74.93)))
  (wire (pts (xy 67.31 72.39) (xy 67.31 80.01)))
  (wire (pts (xy 88.9 134.62) (xy 100.33 134.62)))
  (wire (pts (xy 266.7 139.7) (xy 267.97 139.7)))
  (wire (pts (xy 274.32 209.55) (xy 278.13 209.55)))
  (polyline (pts (xy 189.865 87.63) (xy 189.865 82.55)))
  (wire (pts (xy 85.09 144.78) (xy 161.29 144.78)))
  (wire (pts (xy 144.78 91.44) (xy 144.78 95.25)))
  (wire (pts (xy 259.08 144.78) (xy 259.08 148.59)))
  (wire (pts (xy 90.17 217.17) (xy 77.47 217.17)))
  (wire (pts (xy 290.83 220.98) (xy 294.64 220.98)))
  (wire (pts (xy 283.21 195.58) (xy 283.21 187.96)))
  (wire (pts (xy 133.35 97.79) (xy 134.62 97.79)))
  (wire (pts (xy 262.89 64.77) (xy 269.24 64.77)))
  (polyline (pts (xy 194.945 95.25) (xy 194.945 90.17)))
  (wire (pts (xy 81.28 123.19) (xy 81.28 130.81)))
  (wire (pts (xy 290.83 210.82) (xy 297.18 210.82)))
  (wire (pts (xy 64.77 124.46) (xy 64.77 123.19)))
  (wire (pts (xy 265.43 214.63) (xy 265.43 215.9)))
  (wire (pts (xy 78.74 151.13) (xy 78.74 157.48)))
  (wire (pts (xy 78.74 157.48) (xy 100.33 157.48)))
  (wire (pts (xy 288.29 190.5) (xy 288.29 187.96)))
  (wire (pts (xy 294.64 187.96) (xy 294.64 189.23)))
  (wire (pts (xy 172.72 154.94) (xy 172.72 156.21)))
  (wire (pts (xy 278.13 209.55) (xy 283.21 209.55)))
  (wire (pts (xy 27.94 172.72) (xy 35.56 172.72)))
  (wire (pts (xy 55.88 63.5) (xy 55.88 74.93)))
  (wire (pts (xy 74.93 254) (xy 87.63 254)))
  (wire (pts (xy 85.09 152.4) (xy 100.33 152.4)))
  (wire (pts (xy 67.31 72.39) (xy 97.79 72.39)))
  (wire (pts (xy 78.74 144.78) (xy 85.09 144.78)))
  (wire (pts (xy 27.94 247.65) (xy 40.64 247.65)))
  (polyline (pts (xy 209.55 228.6) (xy 209.55 35.56)))
  (wire (pts (xy 43.18 88.9) (xy 50.8 88.9)))
  (polyline (pts (xy 218.44 170.18) (xy 346.71 170.18)))
  (wire (pts (xy 63.5 90.17) (xy 60.96 90.17)))
  (wire (pts (xy 267.97 138.43) (xy 267.97 139.7)))
  (wire (pts (xy 60.96 90.17) (xy 60.96 92.71)))
  (wire (pts (xy 274.32 204.47) (xy 284.48 204.47)))
  (wire (pts (xy 246.38 207.01) (xy 256.54 207.01)))
  (wire (pts (xy 100.33 160.02) (xy 80.01 160.02)))
  (wire (pts (xy 246.38 207.01) (xy 246.38 208.28)))
  (wire (pts (xy 74.93 256.54) (xy 87.63 256.54)))
  (polyline (pts (xy 323.85 121.92) (xy 323.85 118.11)))
  (wire (pts (xy 25.4 170.18) (xy 25.4 173.99)))
  (wire (pts (xy 259.08 123.19) (xy 259.08 127)))
  (wire (pts (xy 283.21 214.63) (xy 283.21 220.98)))
  (wire (pts (xy 127 214.63) (xy 139.7 214.63)))
  (wire (pts (xy 119.38 102.87) (xy 119.38 104.14)))
  (wire (pts (xy 134.62 97.79) (xy 134.62 99.06)))
  (polyline (pts (xy 323.85 114.3) (xy 331.47 114.3)))
  (polyline (pts (xy 169.545 91.44) (xy 172.085 91.44)))
  (wire (pts (xy 240.03 204.47) (xy 240.03 205.74)))
  (wire (pts (xy 64.77 129.54) (xy 64.77 134.62)))
  (wire (pts (xy 90.17 207.01) (xy 77.47 207.01)))
  (wire (pts (xy 36.83 81.28) (xy 36.83 83.82)))
  (wire (pts (xy 259.08 106.68) (xy 267.97 106.68)))
  (wire (pts (xy 285.75 210.82) (xy 285.75 207.01)))
  (wire (pts (xy 259.08 132.08) (xy 259.08 134.62)))
  (wire (pts (xy 259.08 132.08) (xy 267.97 132.08)))
  (wire (pts (xy 158.115 91.44) (xy 161.925 91.44)))
  (wire (pts (xy 294.64 196.85) (xy 302.26 196.85)))
  (wire (pts (xy 25.4 179.07) (xy 25.4 180.34)))
  (wire (pts (xy 288.29 201.93) (xy 288.29 195.58)))
  (polyline (pts (xy 346.71 170.18) (xy 346.71 35.56)))
  (polyline (pts (xy 172.085 82.55) (xy 184.785 82.55)))
  (wire (pts (xy 46.99 74.93) (xy 55.88 74.93)))
  (wire (pts (xy 90.17 196.85) (xy 77.47 196.85)))
  (wire (pts (xy 64.77 123.19) (xy 57.15 123.19)))
  (wire (pts (xy 274.32 199.39) (xy 279.4 199.39)))
  (wire (pts (xy 288.29 187.96) (xy 294.64 187.96)))
  (wire (pts (xy 134.62 86.36) (xy 134.62 81.28)))
  (wire (pts (xy 74.93 241.3) (xy 87.63 241.3)))
  (wire (pts (xy 267.97 106.68) (xy 267.97 111.76)))
  (wire (pts (xy 36.83 74.93) (xy 46.99 74.93)))
  (wire (pts (xy 111.76 87.63) (xy 111.76 91.44)))
  (wire (pts (xy 278.13 215.9) (xy 278.13 217.17)))
  (polyline (pts (xy 172.085 99.06) (xy 172.085 91.44)))
  (wire (pts (xy 39.37 134.62) (xy 49.53 134.62)))
  (wire (pts (xy 48.26 144.78) (xy 48.26 146.05)))
  (wire (pts (xy 317.5 194.31) (xy 317.5 196.85)))
  (wire (pts (xy 251.46 64.77) (xy 255.27 64.77)))
  (wire (pts (xy 128.27 97.79) (xy 127 97.79)))
  (wire (pts (xy 283.21 214.63) (xy 283.21 209.55)))
  (wire (pts (xy 247.65 209.55) (xy 256.54 209.55)))
  (polyline (pts (xy 20.32 35.56) (xy 209.55 35.56)))
  (polyline (pts (xy 197.485 82.55) (xy 210.185 82.55)))
  (wire (pts (xy 274.32 201.93) (xy 288.29 201.93)))
  (wire (pts (xy 267.97 116.84) (xy 267.97 118.11)))
  (wire (pts (xy 86.36 88.9) (xy 97.79 88.9)))
  (wire (pts (xy 85.09 152.4) (xy 85.09 144.78)))
  (wire (pts (xy 281.94 118.11) (xy 293.37 118.11)))
  (wire (pts (xy 48.26 138.43) (xy 49.53 138.43)))
  (wire (pts (xy 294.64 214.63) (xy 297.18 214.63)))
  (polyline (pts (xy 193.675 82.55) (xy 193.675 87.63)))
  (wire (pts (xy 339.09 187.96) (xy 339.09 189.23)))
  (wire (pts (xy 290.83 214.63) (xy 294.64 214.63)))
  (wire (pts (xy 144.78 102.87) (xy 144.78 104.14)))
  (image (at 309.88 69.85) (scale 0.655763))
  (image (at 191.77 63.5) (scale 0.563001))
  (image (at 313.69 207.01))
  (text "Rising edge (Clk) \nturns on board power\n" (at 24.13 99.06 0))
  (text "RTC with board power control for Sleep / Wake" (at 29.21 41.91 0))
  (text "Iq = 0.90uA" (at 67.31 93.98 0))
  (text "Iq = 0.16uA" (at 107.95 165.1 0))
  (text "40 usec, 3.0v (2.8 to 3.2), Iq=0.3uA" (at 41.91 181.61 0))
  (text "GPIO" (at 172.085 92.71 0))
  (text "1Hz to 52MHz" (at 137.16 154.94 0))
  (text "Minimum Viable Interface" (at 16.51 236.22 0))
  (text "Switching Regulator +3v3 @ 1.2amp, \nIq=2.8uA, Ishdn=0.7uA, available"
    (at 222.25 187.96 0)
  )
  (text "Low leak SuperCap" (at 163.83 165.1 0))
  (text "Can't use TLV840 as there are no push-pull \noutput available in <100usec delay\nUse R3111N282C-TR-FE or\nR3117K313C-TR (0.3uA)"
    (at 165.1 210.82 0)
  )
  (text "With 1M:\n562K => 3.3v\n525K => 3.45v\n499K => 3.57v\n412K => 4.0v\n320K => 5.0v"
    (at 302.26 223.52 0)
  )
  (text "118K => 0.4Mhz\n35.7K => 1.0MHz\n11K => 2 MHz" (at 318.77 220.98 0))
  (text "~{PROC_SLEEP}" (at 198.755 87.63 0))
  (text "~{SLEEP}" (at 201.295 93.98 0))
  (text "~{PROC_SLEEP} is gpio output from processor, falling edge turns off Vreg"
    (at 88.9 63.5 0)
  )
  (text "Board Sleep Wake Notes:\n- Open Collector/Drain Wake circuits have almost no leakage (<100nA)\n- esd protect pins?  \n- Would be great to switch Vin on/off by RTC_Alarm, etc.\n"
    (at 220.98 245.11 0)
  )
  (text "‎CD0603-B0240R‎" (at 264.16 80.01 0))
  (text "VREG_EN = 0, turn Vreg off (~{SHUTDOWN})\n         = 1, Vreg on"
    (at 64.77 106.68 0)
  )
  (text "RS232 RX Console wakeup -12v to +12v, typical -5v to +5v"
    (at 236.22 83.82 0)
  )
  (text "12uH\n" (at 229.87 207.01 0))
  (text "PCB Layout is inverted vertical for ease of routing\n  - schematic flipped to match."
    (at 83.82 226.06 0)
  )
  (text "Rechargeable Lithium\n" (at 185.42 165.1 0))
  (text "SPI from an external Controller (Master)." (at 287.02 107.95 0))
  (text "Processor" (at 173.355 88.9 0))
  (text "Analog Mux to isolate i2c signals" (at 21.59 124.46 0))
  (text "v1.1 had an error on D1" (at 138.43 99.695 0))
  (text "Wake on ~{RTC Alarm}, ~{SPI_CS}, 1x rs232 Rx Serial \n"
    (at 233.68 43.18 0)
  )
  (text "Wake on SPI_CS or TTL Serial RX from another +3V3 power domain"
    (at 261.62 102.87 0)
  )
  (text "Optional signals" (at 74.93 234.315 0))
  (text "VREG_EN optional control of external voltage regulator.\n"
    (at 88.9 67.31 0)
  )
  (text "Wake on Alarm from this +3V_COIN power domain" (at 265.43 147.32 0))
  (text "Falling Edge, active hi output" (at 304.8 125.73 0))
  (text "B150\n" (at 227.33 215.9 0))
  (text "~{PROC_SLEEP} falling edge from processor, turns Vreg to processor off"
    (at 109.22 76.2 0)
  )
  (text "~{BRD_WAKE} (Preset#) = 0, turns on board power\n" (at 88.9 59.69 0))
  (text "Ven thresh = 1.01v" (at 251.46 223.52 0))
  (text "Push-Pull output, Active Lo\n\n" (at 41.91 185.42 0))
  (text "+3Vx_ON is used to enable muxs for i2c, etc." (at 22.86 162.56 0))
  (text "Board level Sleep:\n - Processor/+3v3 Vreg is turned off by processor active low gpio (PROC_SLEEP)\n - Wake on RTC interrupt.  Processor programs wakeup time before sleep\n - Wake on r232 serial console rx\n - Wake on SPI chip select or TTL serial rx(active low)\n - Wake on button push\n - Low shutdown current 3.3v 1.2 amp voltage regulator 4.5v to 50v input, Ishdn=0.7uA\n - Ishdn = 3.06uA = 0.9uA (74aup1g74) + 0.16uA (RV-3032) + 0.3uA (R3117) +\n     + 1uA (nl7WB66) + 0.7uA (LT3991 Vreg)"
    (at 120.65 256.54 0)
  )
  (label "~{BRD_WAKE}" (at 241.3 160.02 0))
  (label "GND" (at 27.94 240.03 0))
  (label "VIN" (at 90.17 214.63 180))
  (label "PWR GOOD" (at 308.61 201.93 180))
  (label "RX1_232" (at 74.93 243.84 0))
  (label "~{RTC_ALARM}" (at 74.93 261.62 0))
  (label "BRD_WAKE_P" (at 241.3 148.59 0))
  (label "GND" (at 127 217.17 0))
  (label "GND" (at 125.73 160.02 0))
  (label "BRD_WAKE_P" (at 127 207.01 0))
  (label "CLK_OUT" (at 74.93 256.54 0))
  (label "~{PROC_SLEEP}" (at 159.385 90.805 0))
  (label "~{VREG_EN}" (at 127 209.55 0))
  (label "I2C_SDA" (at 90.17 199.39 180))
  (label "+3Vx" (at 125.73 157.48 0))
  (label "RX1_232" (at 127 201.93 0))
  (label "+3V_COIN" (at 45.72 74.93 0))
  (label "VD2_I2C_SDA" (at 64.77 151.13 90))
  (label "+3V_COIN" (at 270.51 106.68 180))
  (label "BRD_WAKE_P" (at 74.93 241.3 0))
  (label "+3Vx" (at 293.37 214.63 0))
  (label "+3Vx_ON" (at 35.56 170.18 180))
  (label "VREG_EN" (at 97.79 83.82 180))
  (label "~{PROC_SLEEP}" (at 27.94 252.73 0))
  (label "GND" (at 90.17 217.17 180))
  (label "+3V_COIN" (at 100.33 152.4 180))
  (label "I2C_SDA" (at 39.37 134.62 0))
  (label "~{PROC_SLEEP}" (at 90.17 201.93 180))
  (label "+3Vx" (at 229.87 195.58 0))
  (label "~{RTC_ALARM}" (at 66.04 157.48 0))
  (label "~{RTC_ALARM}" (at 127 212.09 0))
  (label "~{SPI_CS}" (at 127 204.47 0))
  (label "EVENT_CNT" (at 100.33 160.02 180))
  (label "RX1_232" (at 269.24 64.77 0))
  (label "VREG_EN" (at 90.17 207.01 180))
  (label "~{BRD_WAKE}" (at 27.94 255.27 0))
  (label "PWR GOOD" (at 74.93 259.08 0))
  (label "+3Vx_ON" (at 100.33 138.43 180))
  (label "CLK_OUT" (at 125.73 154.94 0))
  (label "~{VREG_EN}" (at 97.79 88.9 180))
  (label "VIN" (at 243.84 207.01 0))
  (label "+3V_COIN" (at 176.53 144.78 0))
  (label "+3V_COIN" (at 270.51 132.08 180))
  (label "~{BRD_WAKE}" (at 256.54 55.88 180))
  (label "+3V_COIN" (at 123.19 81.28 0))
  (label "+3Vx" (at 148.59 157.48 0))
  (label "BRD_WAKE_P" (at 241.3 127 0))
  (label "+3Vx_ON" (at 39.37 138.43 0))
  (label "EVENT_CNT" (at 74.93 254 0))
  (label "+3Vx_ON" (at 74.93 264.16 0))
  (label "~{BRD_WAKE}" (at 90.17 204.47 180))
  (label "~{RTC_ALARM}" (at 295.91 139.7 180))
  (label "+3V_COIN" (at 90.17 209.55 180))
  (label "VREG_EN" (at 247.65 209.55 0))
  (label "~{VREG_EN}" (at 74.93 238.76 0))
  (label "~{SLEEP}" (at 119.38 91.44 180))
  (label "VD2_I2C_SDA" (at 100.33 154.94 180))
  (label "+3Vx" (at 299.72 187.96 180))
  (label "+3V_COIN" (at 27.94 242.57 0))
  (label "RX4_232" (at 74.93 251.46 0))
  (label "~{BRD_WAKE}" (at 97.79 72.39 180))
  (label "VREG_EN" (at 27.94 250.19 0))
  (label "GND" (at 35.56 175.26 180))
  (label "+3V_COIN" (at 73.66 123.19 180))
  (label "+3V_COIN" (at 35.56 172.72 180))
  (label "VD2_I2C_SCL" (at 73.66 151.13 90))
  (label "+3Vx" (at 90.17 212.09 180))
  (label "+3V_COIN" (at 55.88 63.5 0))
  (label "+3Vx_ON" (at 127 214.63 0))
  (label "RX2_232" (at 74.93 246.38 0))
  (label "VD2_I2C_SCL" (at 125.73 152.4 0))
  (label "RX3_232" (at 74.93 248.92 0))
  (label "I2C_SCL" (at 90.17 196.85 180))
  (label "~{RTC_ALARM}" (at 100.33 157.48 180))
  (label "VIN" (at 27.94 247.65 0))
  (label "+3Vx" (at 330.2 187.96 180))
  (label "~{SPI_CS}" (at 290.83 118.11 180))
  (label "BRD_WAKE_P" (at 43.18 88.9 0))
  (label "~{SLEEP}" (at 72.39 97.79 0))
  (label "+3V_COIN" (at 90.17 144.78 180))
  (label "+3Vx" (at 53.34 170.18 0))
  (label "I2C_SCL" (at 100.33 134.62 180))
  (label "+3Vx" (at 27.94 245.11 0))
  (hierarchical_label "GND" (shape input) (at 77.47 217.17 180))
  (hierarchical_label "~{VREG_EN}" (shape output) (at 87.63 238.76 0))
  (hierarchical_label "~{VREG_EN}" (shape output) (at 139.7 209.55 0))
  (hierarchical_label "EVENT_CNT" (shape input) (at 87.63 254 0))
  (hierarchical_label "~{BRD_WAKE}" (shape input) (at 77.47 204.47 180))
  (hierarchical_label "BRD_WAKE_P" (shape input) (at 87.63 241.3 0))
  (hierarchical_label "RX1_232" (shape input) (at 139.7 201.93 0))
  (hierarchical_label "RX1_232" (shape input) (at 87.63 243.84 0))
  (hierarchical_label "VREG_EN" (shape output) (at 40.64 250.19 0))
  (hierarchical_label "+3Vx_ON" (shape input) (at 139.7 214.63 0))
  (hierarchical_label "CLK_OUT" (shape input) (at 87.63 256.54 0))
  (hierarchical_label "RX2_232" (shape input) (at 87.63 246.38 0))
  (hierarchical_label "PWR GOOD" (shape output) (at 87.63 259.08 0))
  (hierarchical_label "~{PROC_SLEEP}" (shape input) (at 77.47 201.93 180))
  (hierarchical_label "+3V_COIN" (shape input) (at 40.64 242.57 0))
  (hierarchical_label "GND" (shape input) (at 139.7 217.17 0))
  (hierarchical_label "VIN" (shape input) (at 77.47 214.63 180))
  (hierarchical_label "~{RTC_ALARM}" (shape output) (at 139.7 212.09 0))
  (hierarchical_label "~{PROC_SLEEP}" (shape input) (at 40.64 252.73 0))
  (hierarchical_label "+3Vx" (shape input) (at 77.47 212.09 180))
  (hierarchical_label "BRD_WAKE_P" (shape input) (at 139.7 207.01 0))
  (hierarchical_label "~{RTC_ALARM}" (shape input) (at 87.63 261.62 0))
  (hierarchical_label "GND" (shape input) (at 40.64 240.03 0))
  (hierarchical_label "+3V_COIN" (shape input) (at 77.47 209.55 180))
  (hierarchical_label "VIN" (shape input) (at 40.64 247.65 0))
  (hierarchical_label "~{BRD_WAKE}" (shape input) (at 40.64 255.27 0))
  (hierarchical_label "RX4_232" (shape input) (at 87.63 251.46 0))
  (hierarchical_label "VREG_EN" (shape output) (at 77.47 207.01 180))
  (hierarchical_label "+3Vx_ON" (shape input) (at 87.63 264.16 0))
  (hierarchical_label "~{SPI_CS}" (shape input) (at 139.7 204.47 0))
  (hierarchical_label "I2C_SCL" (shape bidirectional) (at 77.47 196.85 180))
  (hierarchical_label "I2C_SDA" (shape bidirectional) (at 77.47 199.39 180))
  (hierarchical_label "+3Vx" (shape input) (at 40.64 245.11 0))
  (hierarchical_label "RX3_232" (shape input) (at 87.63 248.92 0))
  (symbol (lib_id "Device:R_Small_US") (at 111.76 85.09 180) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "R10" (id 0) (at 114.3 83.82 0))
    (property "Value" "100K" (id 1) (at 113.03 86.36 0))
    (property "Footprint" "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (id 2) (at 111.76 85.09 0))
    (property "Datasheet" "~" (id 3) (at 111.76 85.09 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Device:R_Small_US") (at 73.66 127 180) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "R6" (id 0) (at 69.85 125.73 0))
    (property "Value" "100K" (id 1) (at 68.58 129.54 0))
    (property "Footprint" "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (id 2) (at 73.66 127 0))
    (property "Datasheet" "~" (id 3) (at 73.66 127 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Connector_Generic:Conn_01x01") (at 148.59 140.97 0) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "J2" (id 0) (at 151.13 139.6999 0))
    (property "Value" "CLK" (id 1) (at 151.13 142.2399 0))
    (property "Footprint" "Connector_PinSocket_1.27mm:PinSocket_1x01_P1.27mm_Vertical" (id 2) (at 148.59 140.97 0))
    (property "Datasheet" "~" (id 3) (at 148.59 140.97 0))
    (pin "1")
  )
  (symbol (lib_id "ProjectLib:RTC-RV-3032") (at 113.03 156.21 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "U3" (id 0) (at 113.03 146.05 0))
    (property "Value" "" (id 1) (at 113.03 148.59 0))
    (property "Footprint" "" (id 2) (at 113.03 156.21 0))
    (property "Datasheet" "" (id 3) (at 113.03 156.21 0))
    (pin "1")
    (pin "2")
    (pin "3")
    (pin "4")
    (pin "5")
    (pin "6")
    (pin "7")
    (pin "8")
  )
  (symbol (lib_id "power:GND") (at 36.83 83.82 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "#PWR01" (id 0) (at 36.83 90.17 0))
    (property "Value" "GND" (id 1) (at 35.56 87.63 0))
    (property "Footprint" "" (id 2) (at 36.83 83.82 0))
    (property "Datasheet" "" (id 3) (at 36.83 83.82 0))
    (pin "1")
  )
  (symbol (lib_id "Transistor_BJT:BC846BS") (at 246.38 64.77 0) (mirror y) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "Q3" (id 0) (at 241.3 63.4999 0))
    (property "Value" "BC846BS" (id 1) (at 241.3 66.0399 0))
    (property "Footprint" "Package_TO_SOT_SMD:SOT-363_SC-70-6" (id 2) (at 241.3 62.23 0))
    (property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/BC846BS.pdf" (id 3) (at 246.38 64.77 0))
    (pin "1")
    (pin "2")
    (pin "6")
    (pin "3")
    (pin "4")
    (pin "5")
  )
  (symbol (lib_id "Device:C") (at 172.72 151.13 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "C6" (id 0) (at 173.99 148.59 0))
    (property "Value" "11mF CPH3225A" (id 1) (at 167.64 153.67 0))
    (property "Footprint" "Capacitor_SMD:C_1210_3225Metric_Pad1.33x2.70mm_HandSolder" (id 2) (at 173.6852 154.94 0))
    (property "Datasheet" "~" (id 3) (at 172.72 151.13 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "power:GND") (at 292.1 204.47 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "#PWR023" (id 0) (at 292.1 210.82 0))
    (property "Value" "GND" (id 1) (at 294.64 204.47 0))
    (property "Footprint" "" (id 2) (at 292.1 204.47 0))
    (property "Datasheet" "" (id 3) (at 292.1 204.47 0))
    (pin "1")
  )
  (symbol (lib_id "power:GND") (at 325.12 198.12 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "#PWR024" (id 0) (at 325.12 204.47 0))
    (property "Value" "GND" (id 1) (at 323.85 201.93 0))
    (property "Footprint" "" (id 2) (at 325.12 198.12 0))
    (property "Datasheet" "" (id 3) (at 325.12 198.12 0))
    (pin "1")
  )
  (symbol (lib_id "Device:C_Small") (at 246.38 210.82 0) (mirror y) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "C7" (id 0) (at 251.46 215.9 0))
    (property "Value" "10uF 100v" (id 1) (at 257.81 213.36 0))
    (property "Footprint" "Capacitor_SMD:C_1206_3216Metric_Pad1.33x1.80mm_HandSolder" (id 2) (at 246.38 210.82 0))
    (property "Datasheet" "445-C3216X6S2A106K160ACCT-ND" (id 3) (at 246.38 210.82 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Device:C_Small") (at 317.5 191.77 0) (mirror y) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "C14" (id 0) (at 322.58 190.5 0))
    (property "Value" "10uF" (id 1) (at 323.85 194.31 0))
    (property "Footprint" "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder" (id 2) (at 317.5 191.77 0))
    (property "Datasheet" "~" (id 3) (at 317.5 191.77 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "power:GND") (at 57.15 139.7 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "#PWR04" (id 0) (at 57.15 146.05 0))
    (property "Value" "GND" (id 1) (at 55.88 143.51 0))
    (property "Footprint" "" (id 2) (at 57.15 139.7 0))
    (property "Datasheet" "" (id 3) (at 57.15 139.7 0))
    (pin "1")
  )
  (symbol (lib_id "Transistor_BJT:BC856BS") (at 261.62 139.7 180) (unit 2)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "Q4" (id 0) (at 256.54 138.4299 0))
    (property "Value" "BC856BS" (id 1) (at 256.54 140.9699 0))
    (property "Footprint" "Package_TO_SOT_SMD:SOT-363_SC-70-6" (id 2) (at 256.54 142.24 0))
    (property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/BC856BS.pdf" (id 3) (at 261.62 139.7 0))
    (pin "1")
    (pin "2")
    (pin "6")
    (pin "3")
    (pin "4")
    (pin "5")
  )
  (symbol (lib_id "Device:C_Small") (at 106.68 128.27 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "C2" (id 0) (at 109.0168 127.1016 0))
    (property "Value" "100nF" (id 1) (at 109.0168 129.413 0))
    (property "Footprint" "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder" (id 2) (at 106.68 128.27 0))
    (property "Datasheet" "~" (id 3) (at 106.68 128.27 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Device:R_Small_US") (at 130.81 97.79 90) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "R11" (id 0) (at 128.27 95.25 90))
    (property "Value" "10K" (id 1) (at 129.54 100.33 90))
    (property "Footprint" "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (id 2) (at 130.81 97.79 0))
    (property "Datasheet" "~" (id 3) (at 130.81 97.79 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Device:C_Small") (at 309.88 191.77 0) (mirror y) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "C13" (id 0) (at 314.96 190.5 0))
    (property "Value" "10uF" (id 1) (at 316.23 194.31 0))
    (property "Footprint" "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder" (id 2) (at 309.88 191.77 0))
    (property "Datasheet" "~" (id 3) (at 309.88 191.77 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Transistor_BJT:BC856BS") (at 261.62 118.11 180) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "Q4" (id 0) (at 256.54 116.8399 0))
    (property "Value" "BC856BS" (id 1) (at 256.54 119.3799 0))
    (property "Footprint" "Package_TO_SOT_SMD:SOT-363_SC-70-6" (id 2) (at 256.54 120.65 0))
    (property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/BC856BS.pdf" (id 3) (at 261.62 118.11 0))
    (pin "1")
    (pin "2")
    (pin "6")
    (pin "3")
    (pin "4")
    (pin "5")
  )
  (symbol (lib_id "Device:LED_Small") (at 339.09 191.77 90) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "D5" (id 0) (at 340.868 190.6016 90))
    (property "Value" "GREEN" (id 1) (at 339.09 194.31 90))
    (property "Footprint" "LED_SMD:LED_0603_1608Metric_Pad1.05x0.95mm_HandSolder" (id 2) (at 339.09 191.77 90))
    (property "Datasheet" "~" (id 3) (at 339.09 191.77 90))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Device:C_Small") (at 302.26 191.77 0) (mirror y) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "C12" (id 0) (at 307.34 190.5 0))
    (property "Value" "10uF" (id 1) (at 308.61 194.31 0))
    (property "Footprint" "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder" (id 2) (at 302.26 191.77 0))
    (property "Datasheet" "~" (id 3) (at 302.26 191.77 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "power:GND") (at 48.26 146.05 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "#PWR02" (id 0) (at 48.26 152.4 0))
    (property "Value" "GND" (id 1) (at 46.99 149.86 0))
    (property "Footprint" "" (id 2) (at 48.26 146.05 0))
    (property "Datasheet" "" (id 3) (at 48.26 146.05 0))
    (pin "1")
  )
  (symbol (lib_id "power:GND") (at 144.78 104.14 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "#PWR011" (id 0) (at 144.78 110.49 0))
    (property "Value" "GND" (id 1) (at 144.78 107.95 0))
    (property "Footprint" "" (id 2) (at 144.78 104.14 0))
    (property "Datasheet" "" (id 3) (at 144.78 104.14 0))
    (pin "1")
  )
  (symbol (lib_id "Connector_Generic:Conn_01x01") (at 236.22 160.02 180) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "J3" (id 0) (at 236.22 153.67 0))
    (property "Value" "~{WAKE}" (id 1) (at 236.22 156.21 0))
    (property "Footprint" "Connector_PinSocket_1.27mm:PinSocket_1x01_P1.27mm_Vertical" (id 2) (at 236.22 160.02 0))
    (property "Datasheet" "~" (id 3) (at 236.22 160.02 0))
    (pin "1")
  )
  (symbol (lib_id "power:GND") (at 50.8 96.52 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "#PWR03" (id 0) (at 50.8 102.87 0))
    (property "Value" "GND" (id 1) (at 49.53 100.33 0))
    (property "Footprint" "" (id 2) (at 50.8 96.52 0))
    (property "Datasheet" "" (id 3) (at 50.8 96.52 0))
    (pin "1")
  )
  (symbol (lib_id "Device:C_Small") (at 279.4 118.11 270) (mirror x) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "C9" (id 0) (at 275.59 119.38 90))
    (property "Value" "10uF" (id 1) (at 275.59 121.92 90))
    (property "Footprint" "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder" (id 2) (at 279.4 118.11 0))
    (property "Datasheet" "~" (id 3) (at 279.4 118.11 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "power:GND") (at 278.13 217.17 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "#PWR022" (id 0) (at 278.13 223.52 0))
    (property "Value" "GND" (id 1) (at 276.86 220.98 0))
    (property "Footprint" "" (id 2) (at 278.13 217.17 0))
    (property "Datasheet" "" (id 3) (at 278.13 217.17 0))
    (pin "1")
  )
  (symbol (lib_id "Device:R_Small_US") (at 267.97 114.3 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "R15" (id 0) (at 273.05 110.49 0))
    (property "Value" "100K" (id 1) (at 274.32 114.3 0))
    (property "Footprint" "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (id 2) (at 267.97 114.3 0))
    (property "Datasheet" "~" (id 3) (at 267.97 114.3 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Device:R_Small_US") (at 50.8 92.71 180) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "R3" (id 0) (at 46.99 91.44 0))
    (property "Value" "100K" (id 1) (at 44.45 93.98 0))
    (property "Footprint" "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (id 2) (at 50.8 92.71 0))
    (property "Datasheet" "~" (id 3) (at 50.8 92.71 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Transistor_BJT:BC856BS") (at 137.16 91.44 180) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "Q2" (id 0) (at 133.35 83.82 0))
    (property "Value" "BC856BS" (id 1) (at 133.35 86.36 0))
    (property "Footprint" "Package_TO_SOT_SMD:SOT-363_SC-70-6" (id 2) (at 132.08 93.98 0))
    (property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/BC856BS.pdf" (id 3) (at 137.16 91.44 0))
    (pin "1")
    (pin "2")
    (pin "6")
    (pin "3")
    (pin "4")
    (pin "5")
  )
  (symbol (lib_id "Device:Battery_Cell") (at 187.96 152.4 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "BT1" (id 0) (at 189.23 153.67 0))
    (property "Value" "ML2020_F1AN" (id 1) (at 189.23 147.32 0))
    (property "Footprint" "ProjectFootprints:ML2020_F1AN" (id 2) (at 187.96 150.876 90))
    (property "Datasheet" "~" (id 3) (at 187.96 150.876 90))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Diode:BAT43W-V") (at 275.59 113.03 270) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "D4" (id 0) (at 278.13 109.22 90))
    (property "Value" "‎B0240R‎" (id 1) (at 278.13 113.03 90))
    (property "Footprint" "Diode_SMD:D_0603_1608Metric_Pad1.05x0.95mm_HandSolder" (id 2) (at 271.145 113.03 0))
    (property "Datasheet" "http://www.vishay.com/docs/85660/bat42.pdf" (id 3) (at 275.59 113.03 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Device:R_Small_US") (at 288.29 193.04 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "R20" (id 0) (at 287.02 195.58 90))
    (property "Value" "100K" (id 1) (at 285.75 190.5 90))
    (property "Footprint" "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (id 2) (at 288.29 193.04 0))
    (property "Datasheet" "~" (id 3) (at 288.29 193.04 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "74xGxx:74AUP1G74") (at 67.31 86.36 0) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "U2" (id 0) (at 68.9801 77.47 0))
    (property "Value" "74AUP1G74" (id 1) (at 68.9801 80.01 0))
    (property "Footprint" "Package_SO:VSSOP-8_2.3x2mm_P0.5mm" (id 2) (at 67.31 86.36 0))
    (property "Datasheet" "http://www.ti.com/lit/sg/scyt129e/scyt129e.pdf" (id 3) (at 67.31 86.36 0))
    (property "Part #" "74AUP1G74DC,125" (id 4) (at 67.31 86.36 0))
    (pin "1")
    (pin "2")
    (pin "3")
    (pin "4")
    (pin "5")
    (pin "6")
    (pin "7")
    (pin "8")
  )
  (symbol (lib_id "Device:R_Small_US") (at 267.97 135.89 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "R16" (id 0) (at 271.78 133.35 0))
    (property "Value" "100K" (id 1) (at 274.32 135.89 0))
    (property "Footprint" "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (id 2) (at 267.97 135.89 0))
    (property "Datasheet" "~" (id 3) (at 267.97 135.89 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Device:R_Small_US") (at 339.09 198.12 180) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "R22" (id 0) (at 340.8172 196.9516 0))
    (property "Value" "10K" (id 1) (at 340.8172 199.263 0))
    (property "Footprint" "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (id 2) (at 339.09 198.12 0))
    (property "Datasheet" "~" (id 3) (at 339.09 198.12 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "power:GND") (at 246.38 217.17 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "#PWR019" (id 0) (at 246.38 223.52 0))
    (property "Value" "GND" (id 1) (at 245.11 220.98 0))
    (property "Footprint" "" (id 2) (at 246.38 217.17 0))
    (property "Datasheet" "" (id 3) (at 246.38 217.17 0))
    (pin "1")
  )
  (symbol (lib_id "Device:R_Small_US") (at 83.82 88.9 270) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "R9" (id 0) (at 81.28 87.63 90))
    (property "Value" "10K" (id 1) (at 86.36 86.36 90))
    (property "Footprint" "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (id 2) (at 83.82 88.9 0))
    (property "Datasheet" "~" (id 3) (at 83.82 88.9 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "power:GND") (at 265.43 215.9 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "#PWR020" (id 0) (at 265.43 222.25 0))
    (property "Value" "GND" (id 1) (at 264.16 219.71 0))
    (property "Footprint" "" (id 2) (at 265.43 215.9 0))
    (property "Datasheet" "" (id 3) (at 265.43 215.9 0))
    (pin "1")
  )
  (symbol (lib_id "power:GND") (at 279.4 199.39 90) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "#PWR0101" (id 0) (at 285.75 199.39 0))
    (property "Value" "GND" (id 1) (at 283.21 199.39 0))
    (property "Footprint" "" (id 2) (at 279.4 199.39 0))
    (property "Datasheet" "" (id 3) (at 279.4 199.39 0))
    (pin "1")
  )
  (symbol (lib_id "Device:R_Small_US") (at 275.59 139.7 270) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "R17" (id 0) (at 280.67 142.24 90))
    (property "Value" "10K" (id 1) (at 281.94 138.43 90))
    (property "Footprint" "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (id 2) (at 275.59 139.7 0))
    (property "Datasheet" "~" (id 3) (at 275.59 139.7 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Device:R_Small_US") (at 278.13 207.01 270) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "R23" (id 0) (at 283.21 208.28 90))
    (property "Value" "100K NS" (id 1) (at 285.75 205.74 90))
    (property "Footprint" "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (id 2) (at 278.13 207.01 0))
    (property "Datasheet" "~" (id 3) (at 278.13 207.01 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Device:R_Small_US") (at 287.02 204.47 270) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "R19" (id 0) (at 284.48 203.2 90))
    (property "Value" "118K" (id 1) (at 293.37 203.2 90))
    (property "Footprint" "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (id 2) (at 287.02 204.47 0))
    (property "Datasheet" "~" (id 3) (at 287.02 204.47 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Switch:SW_DIP_x01") (at 264.16 160.02 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "SW1" (id 0) (at 264.16 163.83 0))
    (property "Value" "WAKE" (id 1) (at 264.16 155.5496 0))
    (property "Footprint" "Button_Switch_SMD:SW_Push_1P1T_NO_CK_KMR2" (id 2) (at 264.16 160.02 0))
    (property "Datasheet" "~" (id 3) (at 264.16 160.02 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "power:GND") (at 276.86 162.56 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "#PWR021" (id 0) (at 276.86 168.91 0))
    (property "Value" "GND" (id 1) (at 276.987 166.9542 0))
    (property "Footprint" "" (id 2) (at 276.86 162.56 0))
    (property "Datasheet" "" (id 3) (at 276.86 162.56 0))
    (pin "1")
  )
  (symbol (lib_id "power:GND") (at 187.96 156.21 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "#PWR015" (id 0) (at 187.96 162.56 0))
    (property "Value" "GND" (id 1) (at 188.087 160.6042 0))
    (property "Footprint" "" (id 2) (at 187.96 156.21 0))
    (property "Datasheet" "" (id 3) (at 187.96 156.21 0))
    (pin "1")
  )
  (symbol (lib_id "Device:R_Small_US") (at 78.74 148.59 180) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "R7" (id 0) (at 74.93 147.32 0))
    (property "Value" "100K NS" (id 1) (at 80.01 148.59 0))
    (property "Footprint" "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (id 2) (at 78.74 148.59 0))
    (property "Datasheet" "~" (id 3) (at 78.74 148.59 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "power:GND") (at 138.43 161.29 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "#PWR010" (id 0) (at 138.43 167.64 0))
    (property "Value" "GND" (id 1) (at 137.16 165.1 0))
    (property "Footprint" "" (id 2) (at 138.43 161.29 0))
    (property "Datasheet" "" (id 3) (at 138.43 161.29 0))
    (pin "1")
  )
  (symbol (lib_id "Device:R_Small_US") (at 25.4 176.53 180) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "R25" (id 0) (at 26.67 175.26 0))
    (property "Value" "1M NS" (id 1) (at 26.67 179.07 0))
    (property "Footprint" "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (id 2) (at 25.4 176.53 0))
    (property "Datasheet" "~" (id 3) (at 25.4 176.53 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Device:C_Small") (at 288.29 220.98 270) (mirror x) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "C10" (id 0) (at 283.21 219.71 90))
    (property "Value" "10pF" (id 1) (at 285.75 223.52 90))
    (property "Footprint" "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder" (id 2) (at 288.29 220.98 0))
    (property "Datasheet" "~" (id 3) (at 288.29 220.98 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "power:GND") (at 161.29 153.67 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "#PWR013" (id 0) (at 161.29 160.02 0))
    (property "Value" "GND" (id 1) (at 160.02 157.48 0))
    (property "Footprint" "" (id 2) (at 161.29 153.67 0))
    (property "Datasheet" "" (id 3) (at 161.29 153.67 0))
    (pin "1")
  )
  (symbol (lib_id "pspice:INDUCTOR") (at 232.41 204.47 0) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "L1" (id 0) (at 232.41 198.12 0))
    (property "Value" "MSS7341-123MLD" (id 1) (at 232.41 200.66 0))
    (property "Footprint" "ProjectFootprints:IND_MSS7341-563MLD" (id 2) (at 232.41 204.47 0))
    (property "Datasheet" "https://www.coilcraft.com/getmedia/7b464459-a4d6-47b0-83ca-9d96d4410863/MSS7341.pdf" (id 3) (at 232.41 204.47 0))
    (property "PartNum" "MSS7341-123MLD" (id 4) (at 232.41 204.47 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "power:GND") (at 60.96 92.71 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "#PWR05" (id 0) (at 60.96 99.06 0))
    (property "Value" "GND" (id 1) (at 59.69 96.52 0))
    (property "Footprint" "" (id 2) (at 60.96 92.71 0))
    (property "Datasheet" "" (id 3) (at 60.96 92.71 0))
    (pin "1")
  )
  (symbol (lib_id "Device:R_Small_US") (at 288.29 214.63 270) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "R21" (id 0) (at 293.37 213.36 90))
    (property "Value" "1M" (id 1) (at 293.37 215.9 90))
    (property "Footprint" "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (id 2) (at 288.29 214.63 0))
    (property "Datasheet" "~" (id 3) (at 288.29 214.63 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Diode:B120-E3") (at 224.79 212.09 270) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "D6" (id 0) (at 219.71 210.82 90))
    (property "Value" "DFLS2100" (id 1) (at 213.36 213.36 90))
    (property "Footprint" "Diode_SMD:D_PowerDI-123" (id 2) (at 220.345 212.09 0))
    (property "Datasheet" "http://www.vishay.com/docs/88946/b120.pdf" (id 3) (at 224.79 212.09 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "74xGxx:74LVC2G66") (at 82.55 134.62 0) (mirror y) (unit 2)
    (in_bom yes) (on_board yes)
    (property "Reference" "U1" (id 0) (at 87.63 127 0))
    (property "Value" "NL7WB66USG" (id 1) (at 88.9 129.54 0))
    (property "Footprint" "Package_SO:VSSOP-8_2.3x2mm_P0.5mm" (id 2) (at 82.55 134.62 0))
    (property "Datasheet" "http://www.ti.com/lit/sg/scyt129e/scyt129e.pdf" (id 3) (at 82.55 134.62 0))
    (pin "4")
    (pin "8")
    (pin "1")
    (pin "2")
    (pin "7")
    (pin "3")
    (pin "5")
    (pin "6")
  )
  (symbol (lib_id "ProjectLib:LT3991EMS-ADJ") (at 265.43 204.47 0) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "U4" (id 0) (at 265.43 191.77 0))
    (property "Value" "LT3991EMS-ADJ" (id 1) (at 265.43 194.31 0))
    (property "Footprint" "ProjectFootprints:MSOP-10_MSE" (id 2) (at 265.43 204.47 0))
    (property "Datasheet" "" (id 3) (at 265.43 204.47 0))
    (pin "1")
    (pin "10")
    (pin "11")
    (pin "2")
    (pin "3")
    (pin "4")
    (pin "5")
    (pin "6")
    (pin "7")
    (pin "8")
    (pin "9")
  )
  (symbol (lib_id "Device:C_Small") (at 151.13 161.29 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "C4" (id 0) (at 147.32 160.02 0))
    (property "Value" "100nF" (id 1) (at 144.78 163.83 0))
    (property "Footprint" "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder" (id 2) (at 151.13 161.29 0))
    (property "Datasheet" "~" (id 3) (at 151.13 161.29 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Device:C_Small") (at 252.73 201.93 270) (mirror x) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "C8" (id 0) (at 247.65 198.12 90))
    (property "Value" "0.47uF" (id 1) (at 245.11 200.66 90))
    (property "Footprint" "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder" (id 2) (at 252.73 201.93 0))
    (property "Datasheet" "~" (id 3) (at 252.73 201.93 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Device:C_Small") (at 325.12 191.77 0) (mirror y) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "C15" (id 0) (at 330.2 190.5 0))
    (property "Value" "10uF" (id 1) (at 331.47 194.31 0))
    (property "Footprint" "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder" (id 2) (at 325.12 191.77 0))
    (property "Datasheet" "~" (id 3) (at 325.12 191.77 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "power:GND") (at 255.27 74.93 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "#PWR018" (id 0) (at 255.27 81.28 0))
    (property "Value" "GND" (id 1) (at 255.397 79.3242 0))
    (property "Footprint" "" (id 2) (at 255.27 74.93 0))
    (property "Datasheet" "" (id 3) (at 255.27 74.93 0))
    (pin "1")
  )
  (symbol (lib_id "Device:C_Small") (at 155.575 91.44 270) (mirror x) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "C3" (id 0) (at 156.845 93.98 90))
    (property "Value" "10uF" (id 1) (at 160.655 95.25 90))
    (property "Footprint" "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder" (id 2) (at 155.575 91.44 0))
    (property "Datasheet" "~" (id 3) (at 155.575 91.44 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Device:R_Small_US") (at 48.26 142.24 180) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "R2" (id 0) (at 44.45 140.97 0))
    (property "Value" "1M" (id 1) (at 43.18 144.78 0))
    (property "Footprint" "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (id 2) (at 48.26 142.24 0))
    (property "Datasheet" "~" (id 3) (at 48.26 142.24 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "power:GND") (at 339.09 201.93 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "#PWR025" (id 0) (at 339.09 208.28 0))
    (property "Value" "GND" (id 1) (at 339.09 205.74 0))
    (property "Footprint" "" (id 2) (at 339.09 201.93 0))
    (property "Datasheet" "" (id 3) (at 339.09 201.93 0))
    (pin "1")
  )
  (symbol (lib_id "Connector_Generic:Conn_01x01") (at 85.09 165.1 0) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "J1" (id 0) (at 87.63 163.8299 0))
    (property "Value" "EVNT" (id 1) (at 87.63 166.3699 0))
    (property "Footprint" "Connector_PinSocket_1.27mm:PinSocket_1x01_P1.27mm_Vertical" (id 2) (at 85.09 165.1 0))
    (property "Datasheet" "~" (id 3) (at 85.09 165.1 0))
    (pin "1")
  )
  (symbol (lib_id "Device:C_Small") (at 288.29 210.82 270) (mirror x) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "C16" (id 0) (at 287.02 208.28 90))
    (property "Value" "0.001 uF" (id 1) (at 289.56 209.55 90))
    (property "Footprint" "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder" (id 2) (at 288.29 210.82 0))
    (property "Datasheet" "~" (id 3) (at 288.29 210.82 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "power:GND") (at 172.72 156.21 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "#PWR014" (id 0) (at 172.72 162.56 0))
    (property "Value" "GND" (id 1) (at 172.847 160.6042 0))
    (property "Footprint" "" (id 2) (at 172.72 156.21 0))
    (property "Datasheet" "" (id 3) (at 172.72 156.21 0))
    (pin "1")
  )
  (symbol (lib_id "ProjectLib:Wakestr_Slim_v1") (at 99.06 207.01 0) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "W1" (id 0) (at 108.585 189.23 0))
    (property "Value" "Wakestr_Slim_v1" (id 1) (at 108.585 191.77 0))
    (property "Footprint" "ProjectFootprints:wakestr_slim_v1" (id 2) (at 99.06 207.01 0))
    (property "Datasheet" "" (id 3) (at 99.06 207.01 0))
    (pin "1")
    (pin "10")
    (pin "11")
    (pin "12")
    (pin "13")
    (pin "14")
    (pin "15")
    (pin "16")
    (pin "2")
    (pin "3")
    (pin "4")
    (pin "5")
    (pin "6")
    (pin "7")
    (pin "8")
    (pin "9")
  )
  (symbol (lib_id "power:GND") (at 134.62 105.41 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "#PWR09" (id 0) (at 134.62 111.76 0))
    (property "Value" "GND" (id 1) (at 134.747 109.8042 0))
    (property "Footprint" "" (id 2) (at 134.62 105.41 0))
    (property "Datasheet" "" (id 3) (at 134.62 105.41 0))
    (pin "1")
  )
  (symbol (lib_id "Device:C_Small") (at 161.29 149.86 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "C5" (id 0) (at 163.6268 148.6916 0))
    (property "Value" "100nF" (id 1) (at 163.6268 151.003 0))
    (property "Footprint" "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder" (id 2) (at 161.29 149.86 0))
    (property "Datasheet" "~" (id 3) (at 161.29 149.86 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Device:R_Small_US") (at 64.77 127 180) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "R4" (id 0) (at 60.96 125.73 0))
    (property "Value" "100K" (id 1) (at 59.69 129.54 0))
    (property "Footprint" "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (id 2) (at 64.77 127 0))
    (property "Datasheet" "~" (id 3) (at 64.77 127 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Device:R_Small_US") (at 278.13 213.36 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "R18" (id 0) (at 283.21 215.9 0))
    (property "Value" "562K" (id 1) (at 275.59 210.82 90))
    (property "Footprint" "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (id 2) (at 278.13 213.36 0))
    (property "Datasheet" "~" (id 3) (at 278.13 213.36 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "power:GND") (at 119.38 104.14 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "#PWR08" (id 0) (at 119.38 110.49 0))
    (property "Value" "GND" (id 1) (at 119.507 108.5342 0))
    (property "Footprint" "" (id 2) (at 119.38 104.14 0))
    (property "Datasheet" "" (id 3) (at 119.38 104.14 0))
    (pin "1")
  )
  (symbol (lib_id "Diode:BAT43W-V") (at 149.225 86.36 270) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "D1" (id 0) (at 151.765 84.7724 90))
    (property "Value" "‎B0240R‎" (id 1) (at 151.765 87.3124 90))
    (property "Footprint" "Diode_SMD:D_0603_1608Metric_Pad1.05x0.95mm_HandSolder" (id 2) (at 144.78 86.36 0))
    (property "Datasheet" "http://www.vishay.com/docs/85660/bat42.pdf" (id 3) (at 149.225 86.36 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "power:GND") (at 34.29 177.8 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "#PWR0103" (id 0) (at 34.29 184.15 0))
    (property "Value" "GND" (id 1) (at 33.02 181.61 0))
    (property "Footprint" "" (id 2) (at 34.29 177.8 0))
    (property "Datasheet" "" (id 3) (at 34.29 177.8 0))
    (pin "1")
  )
  (symbol (lib_id "Device:R_Small_US") (at 134.62 101.6 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "R12" (id 0) (at 139.7 100.33 90))
    (property "Value" "100K" (id 1) (at 137.16 99.06 90))
    (property "Footprint" "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (id 2) (at 134.62 101.6 0))
    (property "Datasheet" "~" (id 3) (at 134.62 101.6 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Diode:B120-E3") (at 240.03 209.55 270) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "D2" (id 0) (at 234.95 208.28 90))
    (property "Value" "B120-E3" (id 1) (at 228.6 210.82 90))
    (property "Footprint" "Diode_SMD:D_SMA" (id 2) (at 235.585 209.55 0))
    (property "Datasheet" "http://www.vishay.com/docs/88946/b120.pdf" (id 3) (at 240.03 209.55 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Device:C_Small") (at 36.83 78.74 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "C1" (id 0) (at 39.37 77.47 0))
    (property "Value" "100nF" (id 1) (at 38.1 81.28 0))
    (property "Footprint" "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder" (id 2) (at 36.83 78.74 0))
    (property "Datasheet" "~" (id 3) (at 36.83 78.74 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Device:R_Small_US") (at 46.99 80.01 180) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "R1" (id 0) (at 49.53 78.74 0))
    (property "Value" "100K" (id 1) (at 49.53 81.28 0))
    (property "Footprint" "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (id 2) (at 46.99 80.01 0))
    (property "Datasheet" "~" (id 3) (at 46.99 80.01 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Device:R_Small_US") (at 67.31 67.31 180) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "R5" (id 0) (at 69.85 64.77 0))
    (property "Value" "100K" (id 1) (at 68.58 67.31 0))
    (property "Footprint" "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (id 2) (at 67.31 67.31 0))
    (property "Datasheet" "~" (id 3) (at 67.31 67.31 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "power:GND") (at 297.18 210.82 90) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "#PWR0102" (id 0) (at 303.53 210.82 0))
    (property "Value" "GND" (id 1) (at 300.99 210.82 0))
    (property "Footprint" "" (id 2) (at 297.18 210.82 0))
    (property "Datasheet" "" (id 3) (at 297.18 210.82 0))
    (pin "1")
  )
  (symbol (lib_id "power:GND") (at 151.13 163.83 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "#PWR012" (id 0) (at 151.13 170.18 0))
    (property "Value" "GND" (id 1) (at 151.257 168.2242 0))
    (property "Footprint" "" (id 2) (at 151.13 163.83 0))
    (property "Datasheet" "" (id 3) (at 151.13 163.83 0))
    (pin "1")
  )
  (symbol (lib_id "Device:R_Small_US") (at 143.51 86.36 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "R13" (id 0) (at 146.05 83.82 90))
    (property "Value" "100K" (id 1) (at 140.97 83.82 90))
    (property "Footprint" "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (id 2) (at 143.51 86.36 0))
    (property "Datasheet" "~" (id 3) (at 143.51 86.36 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "power:GND") (at 25.4 180.34 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "#PWR0104" (id 0) (at 25.4 186.69 0))
    (property "Value" "GND" (id 1) (at 24.13 184.15 0))
    (property "Footprint" "" (id 2) (at 25.4 180.34 0))
    (property "Datasheet" "" (id 3) (at 25.4 180.34 0))
    (pin "1")
  )
  (symbol (lib_id "Device:R_Small_US") (at 260.35 64.77 270) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "R14" (id 0) (at 257.81 63.5 90))
    (property "Value" "100K" (id 1) (at 266.7 63.5 90))
    (property "Footprint" "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (id 2) (at 260.35 64.77 0))
    (property "Datasheet" "~" (id 3) (at 260.35 64.77 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Device:C_Small") (at 294.64 191.77 0) (mirror y) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "C11" (id 0) (at 299.72 190.5 0))
    (property "Value" "10uF" (id 1) (at 300.99 194.31 0))
    (property "Footprint" "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder" (id 2) (at 294.64 191.77 0))
    (property "Datasheet" "~" (id 3) (at 294.64 191.77 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "power:GND") (at 81.28 139.7 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "#PWR06" (id 0) (at 81.28 146.05 0))
    (property "Value" "GND" (id 1) (at 78.74 139.7 0))
    (property "Footprint" "" (id 2) (at 81.28 139.7 0))
    (property "Datasheet" "" (id 3) (at 81.28 139.7 0))
    (pin "1")
  )
  (symbol (lib_id "Diode:BAT43W-V") (at 255.27 69.85 270) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "D3" (id 0) (at 257.81 68.2624 90))
    (property "Value" "‎B0240R‎" (id 1) (at 257.81 70.8024 90))
    (property "Footprint" "Diode_SMD:D_0603_1608Metric_Pad1.05x0.95mm_HandSolder" (id 2) (at 250.825 69.85 0))
    (property "Datasheet" "http://www.vishay.com/docs/85660/bat42.pdf" (id 3) (at 255.27 69.85 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "power:GND") (at 243.84 71.12 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "#PWR016" (id 0) (at 243.84 77.47 0))
    (property "Value" "GND" (id 1) (at 243.967 75.5142 0))
    (property "Footprint" "" (id 2) (at 243.84 71.12 0))
    (property "Datasheet" "" (id 3) (at 243.84 71.12 0))
    (pin "1")
  )
  (symbol (lib_id "Device:R_Small_US") (at 83.82 83.82 270) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "R8" (id 0) (at 81.28 82.55 90))
    (property "Value" "10K" (id 1) (at 86.36 81.28 90))
    (property "Footprint" "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (id 2) (at 83.82 83.82 0))
    (property "Datasheet" "~" (id 3) (at 83.82 83.82 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "power:GND") (at 106.68 130.81 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "#PWR07" (id 0) (at 106.68 137.16 0))
    (property "Value" "GND" (id 1) (at 105.41 134.62 0))
    (property "Footprint" "" (id 2) (at 106.68 130.81 0))
    (property "Datasheet" "" (id 3) (at 106.68 130.81 0))
    (pin "1")
  )
  (symbol (lib_id "74xGxx:74LVC2G66") (at 55.88 134.62 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "U1" (id 0) (at 52.07 127 0))
    (property "Value" "NL7WB66USG" (id 1) (at 49.53 129.54 0))
    (property "Footprint" "Package_SO:VSSOP-8_2.3x2mm_P0.5mm" (id 2) (at 55.88 134.62 0))
    (property "Datasheet" "http://www.ti.com/lit/sg/scyt129e/scyt129e.pdf" (id 3) (at 55.88 134.62 0))
    (pin "4")
    (pin "8")
    (pin "1")
    (pin "2")
    (pin "7")
    (pin "3")
    (pin "5")
    (pin "6")
  )
  (symbol (lib_id "Transistor_BJT:BC846BS") (at 121.92 97.79 0) (mirror y) (unit 2)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "Q1" (id 0) (at 116.84 96.5199 0))
    (property "Value" "BC846BS" (id 1) (at 116.84 99.0599 0))
    (property "Footprint" "Package_TO_SOT_SMD:SOT-363_SC-70-6" (id 2) (at 116.84 95.25 0))
    (property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/BC846BS.pdf" (id 3) (at 121.92 97.79 0))
    (pin "1")
    (pin "2")
    (pin "6")
    (pin "3")
    (pin "4")
    (pin "5")
  )
  (symbol (lib_id "ProjectLib:R3117N") (at 44.45 172.72 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "U5" (id 0) (at 44.45 163.83 0))
    (property "Value" "R3117N" (id 1) (at 44.45 166.37 0))
    (property "Footprint" "Package_TO_SOT_SMD:SOT-23-5_HandSoldering" (id 2) (at 44.45 182.88 0))
    (property "Datasheet" "" (id 3) (at 44.45 182.88 0))
    (pin "1")
    (pin "2")
    (pin "3")
    (pin "4")
    (pin "5")
  )
  (symbol (lib_id "power:GND") (at 240.03 217.17 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "#PWR017" (id 0) (at 240.03 223.52 0))
    (property "Value" "GND" (id 1) (at 238.76 220.98 0))
    (property "Footprint" "" (id 2) (at 240.03 217.17 0))
    (property "Datasheet" "" (id 3) (at 240.03 217.17 0))
    (pin "1")
  )
  (sheet_instances
    (path (page "1"))
  )
  (symbol_instances
    (path
      (reference "#PWR01") (unit 1) (value "GND") (footprint "")
    )
    (path
      (reference "#PWR02") (unit 1) (value "GND") (footprint "")
    )
    (path
      (reference "#PWR03") (unit 1) (value "GND") (footprint "")
    )
    (path
      (reference "#PWR04") (unit 1) (value "GND") (footprint "")
    )
    (path
      (reference "#PWR05") (unit 1) (value "GND") (footprint "")
    )
    (path
      (reference "#PWR06") (unit 1) (value "GND") (footprint "")
    )
    (path
      (reference "#PWR07") (unit 1) (value "GND") (footprint "")
    )
    (path
      (reference "#PWR08") (unit 1) (value "GND") (footprint "")
    )
    (path
      (reference "#PWR09") (unit 1) (value "GND") (footprint "")
    )
    (path
      (reference "#PWR010") (unit 1) (value "GND") (footprint "")
    )
    (path
      (reference "#PWR011") (unit 1) (value "GND") (footprint "")
    )
    (path
      (reference "#PWR012") (unit 1) (value "GND") (footprint "")
    )
    (path
      (reference "#PWR013") (unit 1) (value "GND") (footprint "")
    )
    (path
      (reference "#PWR014") (unit 1) (value "GND") (footprint "")
    )
    (path
      (reference "#PWR015") (unit 1) (value "GND") (footprint "")
    )
    (path
      (reference "#PWR016") (unit 1) (value "GND") (footprint "")
    )
    (path
      (reference "#PWR017") (unit 1) (value "GND") (footprint "")
    )
    (path
      (reference "#PWR018") (unit 1) (value "GND") (footprint "")
    )
    (path
      (reference "#PWR019") (unit 1) (value "GND") (footprint "")
    )
    (path
      (reference "#PWR020") (unit 1) (value "GND") (footprint "")
    )
    (path
      (reference "#PWR021") (unit 1) (value "GND") (footprint "")
    )
    (path
      (reference "#PWR022") (unit 1) (value "GND") (footprint "")
    )
    (path
      (reference "#PWR023") (unit 1) (value "GND") (footprint "")
    )
    (path
      (reference "#PWR024") (unit 1) (value "GND") (footprint "")
    )
    (path
      (reference "#PWR025") (unit 1) (value "GND") (footprint "")
    )
    (path
      (reference "#PWR0101") (unit 1) (value "GND") (footprint "")
    )
    (path
      (reference "#PWR0102") (unit 1) (value "GND") (footprint "")
    )
    (path
      (reference "#PWR0103") (unit 1) (value "GND") (footprint "")
    )
    (path
      (reference "#PWR0104") (unit 1) (value "GND") (footprint "")
    )
    (path
      (reference "BT1") (unit 1) (value "ML2020_F1AN") (footprint "ProjectFootprints:ML2020_F1AN")
    )
    (path
      (reference "C1") (unit 1) (value "100nF") (footprint "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder")
    )
    (path
      (reference "C2") (unit 1) (value "100nF") (footprint "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder")
    )
    (path
      (reference "C3") (unit 1) (value "10uF") (footprint "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder")
    )
    (path
      (reference "C4") (unit 1) (value "100nF") (footprint "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder")
    )
    (path
      (reference "C5") (unit 1) (value "100nF") (footprint "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder")
    )
    (path
      (reference "C6") (unit 1) (value "11mF CPH3225A") (footprint "Capacitor_SMD:C_1210_3225Metric_Pad1.33x2.70mm_HandSolder")
    )
    (path
      (reference "C7") (unit 1) (value "10uF 100v") (footprint "Capacitor_SMD:C_1206_3216Metric_Pad1.33x1.80mm_HandSolder")
    )
    (path
      (reference "C8") (unit 1) (value "0.47uF") (footprint "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder")
    )
    (path
      (reference "C9") (unit 1) (value "10uF") (footprint "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder")
    )
    (path
      (reference "C10") (unit 1) (value "10pF") (footprint "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder")
    )
    (path
      (reference "C11") (unit 1) (value "10uF") (footprint "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder")
    )
    (path
      (reference "C12") (unit 1) (value "10uF") (footprint "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder")
    )
    (path
      (reference "C13") (unit 1) (value "10uF") (footprint "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder")
    )
    (path
      (reference "C14") (unit 1) (value "10uF") (footprint "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder")
    )
    (path
      (reference "C15") (unit 1) (value "10uF") (footprint "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder")
    )
    (path
      (reference "C16") (unit 1) (value "0.001 uF") (footprint "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder")
    )
    (path
      (reference "D1") (unit 1) (value "‎B0240R‎") (footprint "Diode_SMD:D_0603_1608Metric_Pad1.05x0.95mm_HandSolder")
    )
    (path
      (reference "D2") (unit 1) (value "B120-E3") (footprint "Diode_SMD:D_SMA")
    )
    (path
      (reference "D3") (unit 1) (value "‎B0240R‎") (footprint "Diode_SMD:D_0603_1608Metric_Pad1.05x0.95mm_HandSolder")
    )
    (path
      (reference "D4") (unit 1) (value "‎B0240R‎") (footprint "Diode_SMD:D_0603_1608Metric_Pad1.05x0.95mm_HandSolder")
    )
    (path
      (reference "D5") (unit 1) (value "GREEN") (footprint "LED_SMD:LED_0603_1608Metric_Pad1.05x0.95mm_HandSolder")
    )
    (path
      (reference "D6") (unit 1) (value "DFLS2100") (footprint "Diode_SMD:D_PowerDI-123")
    )
    (path
      (reference "J1") (unit 1) (value "EVNT") (footprint "Connector_PinSocket_1.27mm:PinSocket_1x01_P1.27mm_Vertical")
    )
    (path
      (reference "J2") (unit 1) (value "CLK") (footprint "Connector_PinSocket_1.27mm:PinSocket_1x01_P1.27mm_Vertical")
    )
    (path
      (reference "J3") (unit 1) (value "~{WAKE}") (footprint "Connector_PinSocket_1.27mm:PinSocket_1x01_P1.27mm_Vertical")
    )
    (path
      (reference "L1") (unit 1) (value "MSS7341-123MLD") (footprint "ProjectFootprints:IND_MSS7341-563MLD")
    )
    (path
      (reference "Q1") (unit 2) (value "BC846BS") (footprint "Package_TO_SOT_SMD:SOT-363_SC-70-6")
    )
    (path
      (reference "Q2") (unit 1) (value "BC856BS") (footprint "Package_TO_SOT_SMD:SOT-363_SC-70-6")
    )
    (path
      (reference "Q3") (unit 1) (value "BC846BS") (footprint "Package_TO_SOT_SMD:SOT-363_SC-70-6")
    )
    (path
      (reference "Q4") (unit 1) (value "BC856BS") (footprint "Package_TO_SOT_SMD:SOT-363_SC-70-6")
    )
    (path
      (reference "Q4") (unit 2) (value "BC856BS") (footprint "Package_TO_SOT_SMD:SOT-363_SC-70-6")
    )
    (path
      (reference "R1") (unit 1) (value "100K") (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder")
    )
    (path
      (reference "R2") (unit 1) (value "1M") (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder")
    )
    (path
      (reference "R3") (unit 1) (value "100K") (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder")
    )
    (path
      (reference "R4") (unit 1) (value "100K") (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder")
    )
    (path
      (reference "R5") (unit 1) (value "100K") (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder")
    )
    (path
      (reference "R6") (unit 1) (value "100K") (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder")
    )
    (path
      (reference "R7") (unit 1) (value "100K NS") (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder")
    )
    (path
      (reference "R8") (unit 1) (value "10K") (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder")
    )
    (path
      (reference "R9") (unit 1) (value "10K") (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder")
    )
    (path
      (reference "R10") (unit 1) (value "100K") (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder")
    )
    (path
      (reference "R11") (unit 1) (value "10K") (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder")
    )
    (path
      (reference "R12") (unit 1) (value "100K") (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder")
    )
    (path
      (reference "R13") (unit 1) (value "100K") (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder")
    )
    (path
      (reference "R14") (unit 1) (value "100K") (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder")
    )
    (path
      (reference "R15") (unit 1) (value "100K") (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder")
    )
    (path
      (reference "R16") (unit 1) (value "100K") (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder")
    )
    (path
      (reference "R17") (unit 1) (value "10K") (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder")
    )
    (path
      (reference "R18") (unit 1) (value "562K") (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder")
    )
    (path
      (reference "R19") (unit 1) (value "118K") (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder")
    )
    (path
      (reference "R20") (unit 1) (value "100K") (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder")
    )
    (path
      (reference "R21") (unit 1) (value "1M") (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder")
    )
    (path
      (reference "R22") (unit 1) (value "10K") (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder")
    )
    (path
      (reference "R23") (unit 1) (value "100K NS") (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder")
    )
    (path
      (reference "R25") (unit 1) (value "1M NS") (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder")
    )
    (path
      (reference "SW1") (unit 1) (value "WAKE") (footprint "Button_Switch_SMD:SW_Push_1P1T_NO_CK_KMR2")
    )
    (path
      (reference "U1") (unit 1) (value "NL7WB66USG") (footprint "Package_SO:VSSOP-8_2.3x2mm_P0.5mm")
    )
    (path
      (reference "U1") (unit 2) (value "NL7WB66USG") (footprint "Package_SO:VSSOP-8_2.3x2mm_P0.5mm")
    )
    (path
      (reference "U2") (unit 1) (value "74AUP1G74") (footprint "Package_SO:VSSOP-8_2.3x2mm_P0.5mm")
    )
    (path
      (reference "U3") (unit 1) (value "RTC-RV-3032") (footprint "ProjectFootprints:RTC_RV-3032-C7")
    )
    (path
      (reference "U4") (unit 1) (value "LT3991EMS-ADJ") (footprint "ProjectFootprints:MSOP-10_MSE")
    )
    (path
      (reference "U5") (unit 1) (value "R3117N") (footprint "Package_TO_SOT_SMD:SOT-23-5_HandSoldering")
    )
    (path
      (reference "W1") (unit 1) (value "Wakestr_Slim_v1") (footprint "ProjectFootprints:wakestr_slim_v1")
    )
  )
)
