Date: 20th November 2023
Participants: Henthorn, McGill, Schnittger, Klimov, Sherman, Micallef
Title: Introductory Geo-Sense Meeting


Items discussed:

1. The preferred material for the housing for batteries and interrogator is titanium.
2. The frame hosting the batteries and interrogator needs to be manufactured.
3. A minimum depth rating for the set up is 500 m.
4. South Bay is a company that can make custom cables for this experiment.
5. The ROV is likely required during both deployment and recovery of the prototype.
6. Consider using DeepSeaConnect (ethernet connection) to check if the prototype is working after deployment.
7. In case of deployment or permitting issues, we can consider deploying the system with the interrogator at the coast.

Action items:

1. Identify day/time for weekly meeting: Sherman
2. Contact Sintela for update on interrogator: Sherman
3. Check about the number of channels available on the interrogator, and re-check termination design: Sherman
4. Get in touch with South Bay and ask for cable specifications/quote: Micallef
5. Look for other small scale interrogators: Micallef
6. Quantify the mechanical specification requirements for the cable based on the current deployment strategy: Schnittger

