CLEMCO BEAD BLASTER	-Jim Scholfield						1/10/17
Manual, a close approx.. of what we have-http://www.clemcoindustries.com/images/pdfs/21803m.pdf
The upper regulator (with gauge)  (Master Pneumatic R55) was replaced late 2016 due to excessive air leaking out from under the cap.  This did not solve the problem.   A fault in the pilot regulator under the cabinet was allowing hi pressure supply air to leak back up to the output (80 psi) of the upper regulator forcing  it to bypass.  I rebuilt the pilot regulator 2x with no success so a new one was ordered.  
Most parts, guns, beads, etc can be had from McMaster-Carr.
Abrasive Blasting Gun-HD- 7/16 Nozzle,  MMC-3444K14
Media-Glass/alum oxide, 80 grit,  MMC-31075K22
[bookmark: _GoBack]
