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British Telecom Analog (BTA) – Right Hand
· Pin 1 = Sensor output (+/-10V)
· Pin 2 = GND
· Pin 3 = Vres (resistance reference)
· Pin 4 = AutoIDENT (not supported on all sensors)
· Pin 5 = Power (+5VDC)
· Pin 6 = Sensor output (0-5V)
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British Telecom Digital (BTD) – Left Hand
	POS.
	DEFAULT
	MOTION DETECTOR
	PHOTOGATE
	RADIATION MONITOR
	ROTARY MOTION

	Pin1
	DIO0
	Echo
	Input
	Countinput
	CCWcount

	Pin2
	DIO1
	Init
	
	
	CWcount

	Pin3
	DIO2
	AutoID
	
	
	

	Pin4
	PWR
(5.3V)
	PWR
(5.3V)
	PWR
(5.3V)
	PWR
(5.3V)
	PWR
(5.3V)

	Pin5
	GND
	GND
	GND
	GND
	GND

	Pin6
	DIO3
	
	
	
	X4res.
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British Telecom Analog Connector (RH)
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