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1.0 PreLoad Software
1.1 Make sure stuff used in tank testing is changed for deployment
1.1.1 Program.cs
1.1.1.1 Set initial state at top of State Machine while loop
1.1.1.2 uBlox.Request fix number of tries and time delay in SurfaceOps
1.1.1.3 Comment out all test compiler directives
1.1.2 configFile.cs
1.1.2.1 Set appropriate preMissionDelayTimeout
1.1.2.2 Set appropriate SurfaceOpsTimeout
1.1.2.3 Uncomment SOSetBellowsPosition to correct value
1.1.2.4 Set descendBellowsLimit to bellowsLowerLimit + 3.0;
1.1.3 Clear all breakpoints
1.1.4 Comment out debug statements
1.2 Mission Config
1.2.1 Make sure last ascend has 0.0 depth
1.2.2 usbCable = false
1.2.3 Set SBE41 pump time
1.2.4 Set SBE41 cpCutoff pressure
1.3 Set SORecoveryMode as appropriate
1.4 AnchorPressureMinimum as appropriate
1.5 Test everything with software on deployment computer
2.0 PreLoad Mechanical
2.1 Balllast so lifting plate is at waterline with bellows at SOSetBellowsPosition
3.0 PreDeployment Mechanical
3.1 Remove eye bolts as necessary
3.2 [bookmark: _GoBack]Remove deploy/debug magnet
3.3 Remove Optode rubber cover
3.4 Remove CTD caps
3.5 Check tension screw cover is tight
3.6 Check Swagelok fitting is tight
3.7 Check tapered ring/bellows cover are screwed together tightly
3.8 Check lifting plate is secured properly
3.9 Position USBL beacon/GPS tracker are opposite dive weights
4.0 Review InitMission data
4.1 Check mission is correct
4.2 Check Optode and CTD settings are correct
