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1.0  Software checks
1.1  Clear all breakpoints
1.2  Comment out all  compiler directives

2.0  Mission configuration
2.1  Bellows lower / upper limit  = 
2.2 Surface ops / Recovery mode  bellows position = 
2.3  Recovery mode true/false
2.4  parkdepth/maxPressure/maxProfiles/maxDays/maxHours
2.5  Pre mission delay timeout
2.6  surfaceOps timeout
2.7  Descend/Park/Anchor/Ascend timeout
2.8  Number of SBD retries
2.9  Homer beacon ID Number = 

3.0  Pre-Deployment Mechanical
3.1  Number of ballast bars = 
3.2  Double check lifting bridle
3.3  Remove Optode  cover
3.4  Remove CTD caps
3.5  Remove FLBB cover
3.6  Remove Telonics magnet/Frequency (160.12210 MHz)
3.7  Connector dummy plugs installed
3.8  Remove GPS tracker off magnet
3.9  Check battery bus voltage
3.10 Check humidity trend
3.11 Check internal pressure trend
 
4.0  Deployment
4.1  Mission start time
4.2 Over the side time
4.3  Deployment latitude
4.4  Deployment longitude 
4.5  AB retract fast start time = 
4.6  Descend time = 
