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1.0  Software checks
1.1  Clear all breakpoints
1.2  Comment out all  compiler directives

2.0  Mission configuration
2.1  Bellows upper limit  = 
2.2  Bellows lower limit = 
2.3  Surface ops bellows position = 
2.4  Recovery mode true/false
2.5  Select correct mission
2.6  Pre mission delay timeout
2.7  Surface ops timeout
2.8  Max depth
2.9  Max number of profiles
2.10 Max mission time
2.11 Homer beacon ID Number = 

3.0  Pre-Deployment Mechanical
3.1  Number of ballast bars = 
3.2  Double check lifting bridle
3.3  Remove Optode  cover
3.4  Remove CTD caps
3.5  Remove FLBB cover
3.6  Connector dummy plugs installed
3.7  Remove GPS tracker off magnet
3.8 Check battery bus voltage
3.9  Check humidity trend
3.10  Check internal pressure trend
 
4.0 [bookmark: _GoBack] Deployment
4.1  Over the side time
4.2  Deployment latitude
4.3  Deployment longitude 
4.4  AB retract fast start time = 
4.5  Descend time = 
