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1.0  Software checks
____Gene/Eric__Clear breakpoints			______Comment out compiler directives

2.0  Mission configuration
_____________Bellows upper/lower limit		______00:01:00___Park hours/minutes  
_____50_____ Surface ops bellows position	           ________________Recovery mode BP
_____120_____parkdepth 				________125_____maxPressure
______3______maxProfiles				________________maxDays/Hours
___10:57AM__ Pre mission delay TO			________________Surface ops TO
_____________Descend TimeOut			________________Park TO
_____________Anchor TO				________________Ascend TO
_____________Number of SBD retries		________________ Homer ID
_____________Sample Period

3.0  Pre-Deployment Mechanical
_____Receive SBD message				_____ Receive  GPS tracker message
_____Double check lifting bridle			__Y__ Remove Optode  cover
__Y___Remove CTD caps					__Y__ Remove FLBB cover
__Y___Connector dummy plugs installed		_____Remove GPS tracker off magnet
___________________Number of ballast bars	_____32.75_____Battery bus voltage
_________22.36 %____Humidity/Temp.		_____1225______Int. pressure/Temp.
_____Remove Telonics magnet/Frequency (160.14000MHz)
__Y__Remove ISUS cover
 
4.0  Deployment
________102.4__________Water Depth m 		______ 10:55______Over the side time
_________10:55______Mission start time ($GO)	_______11:01_______Under Surface time
______36,7329_______Deployment lat. ($GO)		____  121.936_________Deployment long. ($GO)
_________10:58_________AB retract fast start time	____11:02______ Descend time
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