[bookmark: _GoBack]1) Buy DM3CS uSD card connector - Gene
	On order
	Received
2) Change COM to COMM or something on top level drawing – Gene
	Done
3) Check LED reverse voltage with enable jumper removed - Paul
4) Get Paul the details of the mode jumper – Gene
	Mode should be pulled high normally and pulled low with a jumper
5) Check bypass caps on processor schematic - Paul
6) Investigate EMMC memory - Eric
7) Remove PTH from motherboard - Paul
8) Investigate system overcurrent fuse size requirements - Ed
9) Find out max current output from both kinds of batteries – Gene
	a) The Li-ion packs are 32X Panasonic 18650B cells in a 8S4P arrangement.  The protection circuit trips at “40-60 Amps”.  I’m checking with the vendor to get more details.
	b) The primary packs are 2X Electrochem 3B0076 cells in series although we can use one of their other DD cells if we’d like.  We have room for 12X packs and I’ve been thinking we’d arrange them as 4S3P.  Their max continuous current is 3A and they are fused at 4A.  So 12A max.
10) Beef up regen diode - Paul
11) Gene and Ed to talk about regen protection
12) Make sure Jose leaves enough trace to cut/jumper on I2C address lines - Paul
13) Develop an I2C address list for all devices - Gene
14) Look at DC/DC converter input caps - Paul
15) Check stability of input PI filter - Paul
16) Check current limit of DC/DC converters - Paul
17) Add up 5V loads - Gene
18) Look at trip time on Elmo power circuit - Paul
19) Check active state for IRQs (hopefully active low) – Gene
	IRQs can be active either low or high also on a falling, leading or both edge(s)
20) Double check connector pinout on motherboard/daughter card - Ed/Paul
21) Check 1.8V on DC clock and see if we can fallback to 3.3 - Ed
22) Maybe add jumper to level translator force on line - Ed
23) Investigate MAX power down functionality - Gene/Brent
	In progress
24) Change JP1 and JP2 (and other jumpers) on daughter card to 0 ohm resistor - Ed
25) Use discrete resistors for RN1 on daughter card - Ed
26) Ed and Paul decide about split power and signal ground - Ed/Paul
27) Consider using same TVS - Ed/Paul
28) Consider using Ed's switch on MB - Paul
29) Review implications of using ADIN on energy monitor IC for daughter card channel voltage – Gene
	Doesn’t appear to be a problem
30) Send out motherboard layout drawing - Jose
31) Make sure silkscreen has pin numbers on connectors - Jose
32) FLT and IRQ lines are active low - Ed/Paul
	See item 19 above

