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Objective: The six I2C buffers on the original motherboard design were found by Eric Martin to have problems with intermittent latch-up and were replaced by a different IC. Eric also found that the pullup resistors on the daughtercard side needed to be a higher value.

[bookmark: _GoBack]All modifications are based on MB schematic sheet 3 v1.5.0. The schematic with the changes applied is v1.6.0.

1) Remove and replace the six TCA4311ADR buffers, U9 through U14, with PCA9511AD.
2) Remove and replace the twelve 2.2 kΩ pullup resistors, R38 through R49, with 10 kΩ resistors. The resistors are SMD 0603 5%, but 1% can be substituted.
