
CPF Internal Sensors Board Engineering Change Order List



ECO A: PTH Sensor Power Up/Logic Line 
1. Remove Q7
2. Jumper Q7-3 pad tp Q7-6 pad
3. Remove R31, R32, R33


ECO B: Remove bus contention signals
1. Cut the trace coming from J9-A2 [rear side]
2. Cut the trace coming from J9-B2 [rear side]

[bookmark: _GoBack]ECO C: Reroute signals from ECO B
1. Remove U9
2. Attach a wire from U9-2 pad to U4-7
3. Attach a wire from J9-B9 to U5-9






