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Board S/N:	2							
Schematic Release:  	E						
PWB Rev:		A						

Application:		BOG CPF SN2				
Config by:		BDJ						
Date:			11JAN17						

1.8/3.3V Config

Default shown is 1.8V operation.

Section				1.8V			3.3V		

Oscillator 		R2  	0 ohm		R1   	open	
UART A (U2) 		R6  	0 ohm		R5   	open	
UART B (U7) 		R28  	0 ohm		R27   	open	
UART C (U12) 		R50  	0 ohm		R49   	open	




Comm A Config - SBECTD

Component			Native Serial		UART			CTD		
U2 (XR20M1280)		remove		install			remove
U3 (Max3244)			install			install			remove
R7				remove		install			remove
R8				install			remove		remove
R9				install			remove		remove
R10				remove		install			remove
R4 (CTD pullup)		remove		remove		install
R17 (Max3244 manual)	install			install			
R18 (Max3244 Auto)		remove		remove		

Address for UART A:
SB1							open
SB2							open
SB3							open
SB4							open
SB5							open
SB6							open
SB7							open
SB8							open

Pwr A Config 
Voltage Select – Both jumpers MUST match.  Default 12V shown.
				12V			5V	
JP1 (input select)		1-2			3-2
JP2 (output select)		1-2			3-2
R23 (voltage scaling)		453k			165k

Amperage select		1.25A			2.5A
Q1				FD8896		IRF7440
R21				0.04Ω			0.02Ω

Energy Monitor
U6				Remove
Address 0xD4 for Energy Monitor A is shown:
SB9				open
SB10				open
SB11				open
SB12				open

Comm B Config BT

Component			Native Serial		UART		
U7 (XR20M1280)		remove		install		
U8 (Max3226)			install			install		
R29				remove		install		
R30				remove		install	
R31				install			remove	
R32				install			remove		
R33 (Max3244 manual)	install			install			
R35 (Max3244 Auto)		remove		remove		

Address for UART B is shown:
SB13							open
SB14							open
SB15							open
SB16							open
SB17							open
SB18							open
SB19							open
SB20							open

Pwr B Config

Voltage Select – Both jumpers MUST match.  Default 12V shown.
				12V			5V	
JP3 (input select)		1-2			3-2
JP4 (output select)		1-2			3-2
R45 (voltage scaling)		453k			165k

Amperage select		1.25A			2.5A
Q2				FD8896		IRF7440
R43				0.04Ω			0.02Ω

Energy Monitor
U10				Remove
Address Energy Monitor B is shown:
SB21				open
SB22				open
SB23				open
SB24				open

Comm C Config ELMO

Component			Native Serial		UART		
U12 (XR20M1280)		remove		install		
U13 (Max3226)		install			install		
R51				remove		install		
R52				remove		install	
R53				install			remove	
R54				install			remove		
R55 (Max3244 manual)	install			install			
R57 (Max3244 Auto)		remove		remove		

Address for UART C is shown:
SB25							open
SB26							open
SB27							open
SB28							open
SB29							open
SB30							open
SB31							open
SB32							open

Pwr C Config

Voltage Select – Both jumpers MUST match.  Default 12V shown.
				12V			5V	
JP5 (input select)		1-2			3-2
JP6 (output select)		1-2			3-2
R68 (voltage scaling)		453k			165k

Amperage select		1.25A			2.5A
Q3				FD8896		IRF7440
R65				0.04Ω			0.02Ω


Address for Energy Monitor C is shown:
SB33				open
SB34				open
SB35				open
SB36				open

