# Static Call Graph for image .\Objects\embed_oop.axf

#<CALLGRAPH># ARM Linker, 5060750: Last Updated: Mon Apr 27 04:55:56 2020

### Maximum Stack Usage = 232 bytes + Unknown(Functions without stacksize, Cycles, Untraceable Function Pointers)

### Call chain for Maximum Stack Depth:

__rt_entry_main ⇒ main ⇒ PowerLed_ctor ⇒ Led_ctor ⇒ __2printf ⇒ _printf_char_file ⇒ _printf_char_common ⇒ __printf

### Functions with no stack information

- __user_initial_stackheap

### Mutually Recursive functions

- NMI_Handler ⇒ NMI_Handler
- HardFault_Handler ⇒ HardFault_Handler
- MemManage_Handler ⇒ MemManage_Handler
- BusFault_Handler ⇒ BusFault_Handler
- UsageFault_Handler ⇒ UsageFault_Handler
- SVC_Handler ⇒ SVC_Handler
- DebugMon_Handler ⇒ DebugMon_Handler
- PendSV_Handler ⇒ PendSV_Handler
- SysTick_Handler ⇒ SysTick_Handler
- ADC_IRQHandler ⇒ ADC_IRQHandler

  ### Function Pointers

  - ADC_IRQHandler from startup_stm32f411xe.o(.text) referenced from startup_stm32f411xe.o(RESET)
  - BusFault_Handler from startup_stm32f411xe.o(.text) referenced from startup_stm32f411xe.o(RESET)
  - DMA1_Stream0_IRQHandler from startup_stm32f411xe.o(.text) referenced from startup_stm32f411xe.o(RESET)
  - DMA1_Stream1_IRQHandler from startup_stm32f411xe.o(.text) referenced from startup_stm32f411xe.o(RESET)
  - DMA1_Stream2_IRQHandler from startup_stm32f411xe.o(.text) referenced from startup_stm32f411xe.o(RESET)
  - DMA1_Stream3_IRQHandler from startup_stm32f411xe.o(.text) referenced from startup_stm32f411xe.o(RESET)
  - DMA1_Stream4_IRQHandler from startup_stm32f411xe.o(.text) referenced from startup_stm32f411xe.o(RESET)
  - DMA1_Stream5_IRQHandler from startup_stm32f411xe.o(.text) referenced from startup_stm32f411xe.o(RESET)
  - DMA1_Stream6_IRQHandler from startup_stm32f411xe.o(.text) referenced from startup_stm32f411xe.o(RESET)
  - DMA1_Stream7_IRQHandler from startup_stm32f411xe.o(.text) referenced from startup_stm32f411xe.o(RESET)
  - DMA2_Stream0_IRQHandler from startup_stm32f411xe.o(.text) referenced from startup_stm32f411xe.o(RESET)
  - DMA2_Stream1_IRQHandler from startup_stm32f411xe.o(.text) referenced from startup_stm32f411xe.o(RESET)
  - DMA2_Stream2_IRQHandler from startup_stm32f411xe.o(.text) referenced from startup_stm32f411xe.o(RESET)
  - DMA2_Stream3_IRQHandler from startup_stm32f411xe.o(.text) referenced from startup_stm32f411xe.o(RESET)
  - DMA2_Stream4_IRQHandler from startup_stm32f411xe.o(.text) referenced from startup_stm32f411xe.o(RESET)
  - DMA2_Stream5_IRQHandler from startup_stm32f411xe.o(.text) referenced from startup_stm32f411xe.o(RESET)
  - DMA2_Stream6_IRQHandler from startup_stm32f411xe.o(.text) referenced from startup_stm32f411xe.o(RESET)
  - DMA2_Stream7_IRQHandler from startup_stm32f411xe.o(.text) referenced from startup_stm32f411xe.o(RESET)
  - DebugMon_Handler from startup_stm32f411xe.o(.text) referenced from startup_stm32f411xe.o(RESET)
  - EXTI0_IRQHandler from startup_stm32f411xe.o(.text) referenced from startup_stm32f411xe.o(RESET)
  - EXTI15_10_IRQHandler from startup_stm32f411xe.o(.text) referenced from startup_stm32f411xe.o(RESET)
  - EXTI1_IRQHandler from startup_stm32f411xe.o(.text) referenced from startup_stm32f411xe.o(RESET)
  - EXTI2_IRQHandler from startup_stm32f411xe.o(.text) referenced from startup_stm32f411xe.o(RESET)
  - EXTI3_IRQHandler from startup_stm32f411xe.o(.text) referenced from startup_stm32f411xe.o(RESET)
  - EXTI4_IRQHandler from startup_stm32f411xe.o(.text) referenced from startup_stm32f411xe.o(RESET)
  - EXTI9_5_IRQHandler from startup_stm32f411xe.o(.text) referenced from startup_stm32f411xe.o(RESET)
  - FLASH_IRQHandler from startup_stm32f411xe.o(.text) referenced from startup_stm32f411xe.o(RESET)
  - FPU_IRQHandler from startup_stm32f411xe.o(.text) referenced from startup_stm32f411xe.o(RESET)
  - HardFault_Handler from startup_stm32f411xe.o(.text) referenced from startup_stm32f411xe.o(RESET)
  - I2C1_ER_IRQHandler from startup_stm32f411xe.o(.text) referenced from startup_stm32f411xe.o(RESET)
  - I2C1_EV_IRQHandler from startup_stm32f411xe.o(.text) referenced from startup_stm32f411xe.o(RESET)
  - I2C2_ER_IRQHandler from startup_stm32f411xe.o(.text) referenced from startup_stm32f411xe.o(RESET)
  - I2C2_EV_IRQHandler from startup_stm32f411xe.o(.text) referenced from startup_stm32f411xe.o(RESET)
  - I2C3_ER_IRQHandler from startup_stm32f411xe.o(.text) referenced from startup_stm32f411xe.o(RESET)
  - I2C3_EV_IRQHandler from startup_stm32f411xe.o(.text) referenced from startup_stm32f411xe.o(RESET)
  - MedicalLed_computeEfficiency from medicalled.o(i.MedicalLed_computeEfficiency) referenced from medicalled.o(.constdata)
  - MedicalLed_runDiagnostics from medicalled.o(i.MedicalLed_runDiagnostics) referenced from medicalled.o(.constdata)
  - MemManage_Handler from startup_stm32f411xe.o(.text) referenced from startup_stm32f411xe.o(RESET)
  - NMI_Handler from startup_stm32f411xe.o(.text) referenced from startup_stm32f411xe.o(RESET)
  - OTG_FS_IRQHandler from startup_stm32f411xe.o(.text) referenced from startup_stm32f411xe.o(RESET)
  - OTG_FS_WKUP_IRQHandler from startup_stm32f411xe.o(.text) referenced from startup_stm32f411xe.o(RESET)
  - PVD_IRQHandler from startup_stm32f411xe.o(.text) referenced from startup_stm32f411xe.o(RESET)
  - PendSV_Handler from startup_stm32f411xe.o(.text) referenced from startup_stm32f411xe.o(RESET)
  - PowerLed_computeEfficiency from powerled.o(i.PowerLed_computeEfficiency) referenced from powerled.o(.constdata)
  - PowerLed_runDiagnostics from powerled.o(i.PowerLed_runDiagnostics) referenced from powerled.o(.constdata)
  - RCC_IRQHandler from startup_stm32f411xe.o(.text) referenced from startup_stm32f411xe.o(RESET)
  - RTC_Alarm_IRQHandler from startup_stm32f411xe.o(.text) referenced from startup_stm32f411xe.o(RESET)
  - RTC_WKUP_IRQHandler from startup_stm32f411xe.o(.text) referenced from startup_stm32f411xe.o(RESET)
  - Reset_Handler from startup_stm32f411xe.o(.text) referenced from startup_stm32f411xe.o(RESET)
  - SDIO_IRQHandler from startup_stm32f411xe.o(.text) referenced from startup_stm32f411xe.o(RESET)
  - SPI1_IRQHandler from startup_stm32f411xe.o(.text) referenced from startup_stm32f411xe.o(RESET)
  - SPI2_IRQHandler from startup_stm32f411xe.o(.text) referenced from startup_stm32f411xe.o(RESET)
  - SPI3_IRQHandler from startup_stm32f411xe.o(.text) referenced from startup_stm32f411xe.o(RESET)
  - SPI4_IRQHandler from startup_stm32f411xe.o(.text) referenced from startup_stm32f411xe.o(RESET)
  - SPI5_IRQHandler from startup_stm32f411xe.o(.text) referenced from startup_stm32f411xe.o(RESET)
  - SVC_Handler from startup_stm32f411xe.o(.text) referenced from startup_stm32f411xe.o(RESET)
  - SysTick_Handler from startup_stm32f411xe.o(.text) referenced from startup_stm32f411xe.o(RESET)
  - SystemInit from system_stm32f4xx.o(i.SystemInit) referenced from startup_stm32f411xe.o(.text)
  - TAMP_STAMP_IRQHandler from startup_stm32f411xe.o(.text) referenced from startup_stm32f411xe.o(RESET)
  - TIM1_BRK_TIM9_IRQHandler from startup_stm32f411xe.o(.text) referenced from startup_stm32f411xe.o(RESET)
  - TIM1_CC_IRQHandler from startup_stm32f411xe.o(.text) referenced from startup_stm32f411xe.o(RESET)
  - TIM1_TRG_COM_TIM11_IRQHandler from startup_stm32f411xe.o(.text) referenced from startup_stm32f411xe.o(RESET)
  - TIM1_UP_TIM10_IRQHandler from startup_stm32f411xe.o(.text) referenced from startup_stm32f411xe.o(RESET)
  - TIM2_IRQHandler from startup_stm32f411xe.o(.text) referenced from startup_stm32f411xe.o(RESET)
  - TIM3_IRQHandler from startup_stm32f411xe.o(.text) referenced from startup_stm32f411xe.o(RESET)
  - TIM4_IRQHandler from startup_stm32f411xe.o(.text) referenced from startup_stm32f411xe.o(RESET)
  - TIM5_IRQHandler from startup_stm32f411xe.o(.text) referenced from startup_stm32f411xe.o(RESET)
  - USART1_IRQHandler from startup_stm32f411xe.o(.text) referenced from startup_stm32f411xe.o(RESET)
  - USART2_IRQHandler from startup_stm32f411xe.o(.text) referenced from startup_stm32f411xe.o(RESET)
  - USART6_IRQHandler from startup_stm32f411xe.o(.text) referenced from startup_stm32f411xe.o(RESET)
  - UsageFault_Handler from startup_stm32f411xe.o(.text) referenced from startup_stm32f411xe.o(RESET)
  - WWDG_IRQHandler from startup_stm32f411xe.o(.text) referenced from startup_stm32f411xe.o(RESET)
  - __main from __main.o(!!!main) referenced from startup_stm32f411xe.o(.text)
  - _printf_input_char from _printf_char_common.o(.text) referenced from _printf_char_common.o(.text)
  - compute_efficiency from led.o(i.compute_efficiency) referenced from led.o(.constdata)
  - fputc from uart.o(i.fputc) referenced from _printf_char_file.o(.text)
  - run_diagnostics from led.o(i.run_diagnostics) referenced from led.o(.constdata)

  ### Global Symbols

  __main (Thumb, 8 bytes, Stack size 0 bytes, __main.o(!!!main))
  [Calls]

  - >> __rt_entry
  - >> __scatterload

  __scatterload (Thumb, 0 bytes, Stack size unknown bytes, __scatter.o(!!!scatter))
  [Called By]

  - >> __main

  __scatterload_rt2 (Thumb, 44 bytes, Stack size unknown bytes, __scatter.o(!!!scatter), UNUSED)
  [Calls]

  - >> __rt_entry

  __scatterload_rt2_thumb_only (Thumb, 0 bytes, Stack size unknown bytes, __scatter.o(!!!scatter), UNUSED)

  __scatterload_null (Thumb, 0 bytes, Stack size unknown bytes, __scatter.o(!!!scatter), UNUSED)

  __scatterload_copy (Thumb, 26 bytes, Stack size unknown bytes, __scatter_copy.o(!!handler_copy), UNUSED)
  [Calls]

  - >> __scatterload_copy
  [Called By]
  - >> __scatterload_copy

  __scatterload_zeroinit (Thumb, 28 bytes, Stack size unknown bytes, __scatter_zi.o(!!handler_zi), UNUSED)

  _printf_d (Thumb, 0 bytes, Stack size unknown bytes, _printf_d.o(.ARM.Collect$$_printf_percent$$00000009))
  [Stack]

  - Max Depth = 56 + Unknown Stack Size
  - Call Chain = _printf_d ⇒ _printf_int_dec ⇒ _printf_int_common
  [Calls]
  - >> _printf_int_dec

  _printf_percent (Thumb, 0 bytes, Stack size unknown bytes, _printf_percent.o(.ARM.Collect$$_printf_percent$$00000000))
  [Called By]

  - >> __printf

  _printf_percent_end (Thumb, 0 bytes, Stack size unknown bytes, _printf_percent_end.o(.ARM.Collect$$_printf_percent$$00000017))

  __rt_lib_init (Thumb, 0 bytes, Stack size unknown bytes, libinit.o(.ARM.Collect$$libinit$$00000000))
  [Called By]

  - >> __rt_entry_li

  __rt_lib_init_fp_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000001))
  [Calls]

  - >> _fp_init

  __rt_lib_init_alloca_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$0000002E))

  __rt_lib_init_argv_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$0000002C))

  __rt_lib_init_atexit_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$0000001B))

  __rt_lib_init_clock_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000021))

  __rt_lib_init_cpp_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000032))

  __rt_lib_init_exceptions_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000030))

  __rt_lib_init_fp_trap_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$0000001F))

  __rt_lib_init_getenv_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000023))

  __rt_lib_init_heap_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$0000000A))

  __rt_lib_init_lc_collate_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000011))

  __rt_lib_init_lc_ctype_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000013))

  __rt_lib_init_lc_monetary_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000015))

  __rt_lib_init_lc_numeric_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000017))

  __rt_lib_init_lc_time_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000019))

  __rt_lib_init_preinit_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000004))

  __rt_lib_init_rand_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$0000000E))

  __rt_lib_init_return (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000033))

  __rt_lib_init_signal_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$0000001D))

  __rt_lib_init_stdio_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000025))

  __rt_lib_init_user_alloc_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$0000000C))

  __rt_lib_shutdown (Thumb, 0 bytes, Stack size unknown bytes, libshutdown.o(.ARM.Collect$$libshutdown$$00000000))
  [Called By]

  - >> __rt_exit_ls

  __rt_lib_shutdown_cpp_1 (Thumb, 0 bytes, Stack size unknown bytes, libshutdown2.o(.ARM.Collect$$libshutdown$$00000002))

  __rt_lib_shutdown_fp_trap_1 (Thumb, 0 bytes, Stack size unknown bytes, libshutdown2.o(.ARM.Collect$$libshutdown$$00000007))

  __rt_lib_shutdown_heap_1 (Thumb, 0 bytes, Stack size unknown bytes, libshutdown2.o(.ARM.Collect$$libshutdown$$0000000F))

  __rt_lib_shutdown_return (Thumb, 0 bytes, Stack size unknown bytes, libshutdown2.o(.ARM.Collect$$libshutdown$$00000010))

  __rt_lib_shutdown_signal_1 (Thumb, 0 bytes, Stack size unknown bytes, libshutdown2.o(.ARM.Collect$$libshutdown$$0000000A))

  __rt_lib_shutdown_stdio_1 (Thumb, 0 bytes, Stack size unknown bytes, libshutdown2.o(.ARM.Collect$$libshutdown$$00000004))

  __rt_lib_shutdown_user_alloc_1 (Thumb, 0 bytes, Stack size unknown bytes, libshutdown2.o(.ARM.Collect$$libshutdown$$0000000C))

  __rt_entry (Thumb, 0 bytes, Stack size unknown bytes, __rtentry.o(.ARM.Collect$$rtentry$$00000000))
  [Called By]

  - >> __main
  - >> __scatterload_rt2

  __rt_entry_presh_1 (Thumb, 0 bytes, Stack size unknown bytes, __rtentry2.o(.ARM.Collect$$rtentry$$00000002))

  __rt_entry_sh (Thumb, 0 bytes, Stack size unknown bytes, __rtentry4.o(.ARM.Collect$$rtentry$$00000004))
  [Stack]

  - Max Depth = 8 + Unknown Stack Size
  - Call Chain = __rt_entry_sh ⇒ __user_setup_stackheap
  [Calls]
  - >> __user_setup_stackheap

  __rt_entry_li (Thumb, 0 bytes, Stack size unknown bytes, __rtentry2.o(.ARM.Collect$$rtentry$$0000000A))
  [Calls]

  - >> __rt_lib_init

  __rt_entry_postsh_1 (Thumb, 0 bytes, Stack size unknown bytes, __rtentry2.o(.ARM.Collect$$rtentry$$00000009))

  __rt_entry_main (Thumb, 0 bytes, Stack size unknown bytes, __rtentry2.o(.ARM.Collect$$rtentry$$0000000D))
  [Stack]

  - Max Depth = 232 + Unknown Stack Size
  - Call Chain = __rt_entry_main ⇒ main ⇒ PowerLed_ctor ⇒ Led_ctor ⇒ __2printf ⇒ _printf_char_file ⇒ _printf_char_common ⇒ __printf
  [Calls]
  - >> exit
  - >> main

  __rt_entry_postli_1 (Thumb, 0 bytes, Stack size unknown bytes, __rtentry2.o(.ARM.Collect$$rtentry$$0000000C))

  __rt_exit (Thumb, 0 bytes, Stack size unknown bytes, rtexit.o(.ARM.Collect$$rtexit$$00000000))
  [Called By]

  - >> exit

  __rt_exit_ls (Thumb, 0 bytes, Stack size unknown bytes, rtexit2.o(.ARM.Collect$$rtexit$$00000003))
  [Calls]

  - >> __rt_lib_shutdown

  __rt_exit_prels_1 (Thumb, 0 bytes, Stack size unknown bytes, rtexit2.o(.ARM.Collect$$rtexit$$00000002))

  __rt_exit_exit (Thumb, 0 bytes, Stack size unknown bytes, rtexit2.o(.ARM.Collect$$rtexit$$00000004))
  [Calls]

  - >> _sys_exit

  Reset_Handler (Thumb, 8 bytes, Stack size 0 bytes, startup_stm32f411xe.o(.text))

  NMI_Handler (Thumb, 2 bytes, Stack size 0 bytes, startup_stm32f411xe.o(.text))
  [Calls]

  - >> NMI_Handler
  [Called By]
  - >> NMI_Handler
  [Address Reference Count : 1]
  - startup_stm32f411xe.o(RESET)

  HardFault_Handler (Thumb, 2 bytes, Stack size 0 bytes, startup_stm32f411xe.o(.text))
  [Calls]

  - >> HardFault_Handler
  [Called By]
  - >> HardFault_Handler
  [Address Reference Count : 1]
  - startup_stm32f411xe.o(RESET)

  MemManage_Handler (Thumb, 2 bytes, Stack size 0 bytes, startup_stm32f411xe.o(.text))
  [Calls]

  - >> MemManage_Handler
  [Called By]
  - >> MemManage_Handler
  [Address Reference Count : 1]
  - startup_stm32f411xe.o(RESET)

  BusFault_Handler (Thumb, 2 bytes, Stack size 0 bytes, startup_stm32f411xe.o(.text))
  [Calls]

  - >> BusFault_Handler
  [Called By]
  - >> BusFault_Handler
  [Address Reference Count : 1]
  - startup_stm32f411xe.o(RESET)

  UsageFault_Handler (Thumb, 2 bytes, Stack size 0 bytes, startup_stm32f411xe.o(.text))
  [Calls]

  - >> UsageFault_Handler
  [Called By]
  - >> UsageFault_Handler
  [Address Reference Count : 1]
  - startup_stm32f411xe.o(RESET)

  SVC_Handler (Thumb, 2 bytes, Stack size 0 bytes, startup_stm32f411xe.o(.text))
  [Calls]

  - >> SVC_Handler
  [Called By]
  - >> SVC_Handler
  [Address Reference Count : 1]
  - startup_stm32f411xe.o(RESET)

  DebugMon_Handler (Thumb, 2 bytes, Stack size 0 bytes, startup_stm32f411xe.o(.text))
  [Calls]

  - >> DebugMon_Handler
  [Called By]
  - >> DebugMon_Handler
  [Address Reference Count : 1]
  - startup_stm32f411xe.o(RESET)

  PendSV_Handler (Thumb, 2 bytes, Stack size 0 bytes, startup_stm32f411xe.o(.text))
  [Calls]

  - >> PendSV_Handler
  [Called By]
  - >> PendSV_Handler
  [Address Reference Count : 1]
  - startup_stm32f411xe.o(RESET)

  SysTick_Handler (Thumb, 2 bytes, Stack size 0 bytes, startup_stm32f411xe.o(.text))
  [Calls]

  - >> SysTick_Handler
  [Called By]
  - >> SysTick_Handler
  [Address Reference Count : 1]
  - startup_stm32f411xe.o(RESET)

  ADC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f411xe.o(.text))
  [Calls]

  - >> ADC_IRQHandler
  [Called By]
  - >> ADC_IRQHandler
  [Address Reference Count : 1]
  - startup_stm32f411xe.o(RESET)

  DMA1_Stream0_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f411xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f411xe.o(RESET)

  DMA1_Stream1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f411xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f411xe.o(RESET)

  DMA1_Stream2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f411xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f411xe.o(RESET)

  DMA1_Stream3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f411xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f411xe.o(RESET)

  DMA1_Stream4_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f411xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f411xe.o(RESET)

  DMA1_Stream5_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f411xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f411xe.o(RESET)

  DMA1_Stream6_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f411xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f411xe.o(RESET)

  DMA1_Stream7_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f411xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f411xe.o(RESET)

  DMA2_Stream0_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f411xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f411xe.o(RESET)

  DMA2_Stream1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f411xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f411xe.o(RESET)

  DMA2_Stream2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f411xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f411xe.o(RESET)

  DMA2_Stream3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f411xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f411xe.o(RESET)

  DMA2_Stream4_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f411xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f411xe.o(RESET)

  DMA2_Stream5_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f411xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f411xe.o(RESET)

  DMA2_Stream6_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f411xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f411xe.o(RESET)

  DMA2_Stream7_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f411xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f411xe.o(RESET)

  EXTI0_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f411xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f411xe.o(RESET)

  EXTI15_10_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f411xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f411xe.o(RESET)

  EXTI1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f411xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f411xe.o(RESET)

  EXTI2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f411xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f411xe.o(RESET)

  EXTI3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f411xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f411xe.o(RESET)

  EXTI4_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f411xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f411xe.o(RESET)

  EXTI9_5_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f411xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f411xe.o(RESET)

  FLASH_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f411xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f411xe.o(RESET)

  FPU_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f411xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f411xe.o(RESET)

  I2C1_ER_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f411xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f411xe.o(RESET)

  I2C1_EV_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f411xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f411xe.o(RESET)

  I2C2_ER_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f411xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f411xe.o(RESET)

  I2C2_EV_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f411xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f411xe.o(RESET)

  I2C3_ER_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f411xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f411xe.o(RESET)

  I2C3_EV_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f411xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f411xe.o(RESET)

  OTG_FS_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f411xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f411xe.o(RESET)

  OTG_FS_WKUP_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f411xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f411xe.o(RESET)

  PVD_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f411xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f411xe.o(RESET)

  RCC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f411xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f411xe.o(RESET)

  RTC_Alarm_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f411xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f411xe.o(RESET)

  RTC_WKUP_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f411xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f411xe.o(RESET)

  SDIO_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f411xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f411xe.o(RESET)

  SPI1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f411xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f411xe.o(RESET)

  SPI2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f411xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f411xe.o(RESET)

  SPI3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f411xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f411xe.o(RESET)

  SPI4_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f411xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f411xe.o(RESET)

  SPI5_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f411xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f411xe.o(RESET)

  TAMP_STAMP_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f411xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f411xe.o(RESET)

  TIM1_BRK_TIM9_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f411xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f411xe.o(RESET)

  TIM1_CC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f411xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f411xe.o(RESET)

  TIM1_TRG_COM_TIM11_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f411xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f411xe.o(RESET)

  TIM1_UP_TIM10_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f411xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f411xe.o(RESET)

  TIM2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f411xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f411xe.o(RESET)

  TIM3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f411xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f411xe.o(RESET)

  TIM4_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f411xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f411xe.o(RESET)

  TIM5_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f411xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f411xe.o(RESET)

  USART1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f411xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f411xe.o(RESET)

  USART2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f411xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f411xe.o(RESET)

  USART6_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f411xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f411xe.o(RESET)

  WWDG_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f411xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f411xe.o(RESET)

  __user_initial_stackheap (Thumb, 0 bytes, Stack size unknown bytes, startup_stm32f411xe.o(.text))
  [Called By]

  - >> __user_setup_stackheap

  __2printf (Thumb, 20 bytes, Stack size 24 bytes, noretval__2printf.o(.text))
  [Stack]

  - Max Depth = 128 + Unknown Stack Size
  - Call Chain = __2printf ⇒ _printf_char_file ⇒ _printf_char_common ⇒ __printf
  [Calls]
  - >> _printf_char_file
  [Called By]
  - >> MedicalLed_runDiagnostics
  - >> MedicalLed_computeEfficiency
  - >> PowerLed_runDiagnostics
  - >> PowerLed_computeEfficiency
  - >> Led_ctor

  __printf (Thumb, 104 bytes, Stack size 24 bytes, __printf.o(.text))
  [Stack]

  - Max Depth = 24 + Unknown Stack Size
  - Call Chain = __printf
  [Calls]
  - >> _printf_percent
  [Called By]
  - >> _printf_char_common

  _printf_int_dec (Thumb, 104 bytes, Stack size 24 bytes, _printf_dec.o(.text))
  [Stack]

  - Max Depth = 56
  - Call Chain = _printf_int_dec ⇒ _printf_int_common
  [Calls]
  - >> _printf_int_common
  [Called By]
  - >> _printf_d

  __use_two_region_memory (Thumb, 2 bytes, Stack size 0 bytes, heapauxi.o(.text), UNUSED)

  __rt_heap_escrow$2region (Thumb, 2 bytes, Stack size 0 bytes, heapauxi.o(.text), UNUSED)

  __rt_heap_expand$2region (Thumb, 2 bytes, Stack size 0 bytes, heapauxi.o(.text), UNUSED)

  _printf_int_common (Thumb, 178 bytes, Stack size 32 bytes, _printf_intcommon.o(.text))
  [Stack]

  - Max Depth = 32
  - Call Chain = _printf_int_common
  [Called By]
  - >> _printf_int_dec

  _printf_char_file (Thumb, 32 bytes, Stack size 16 bytes, _printf_char_file.o(.text))
  [Stack]

  - Max Depth = 104 + Unknown Stack Size
  - Call Chain = _printf_char_file ⇒ _printf_char_common ⇒ __printf
  [Calls]
  - >> _printf_char_common
  - >> ferror
  [Called By]
  - >> __2printf

  ferror (Thumb, 8 bytes, Stack size 0 bytes, ferror.o(.text))
  [Called By]

  - >> _printf_char_file

  _printf_char_common (Thumb, 32 bytes, Stack size 64 bytes, _printf_char_common.o(.text))
  [Stack]

  - Max Depth = 88 + Unknown Stack Size
  - Call Chain = _printf_char_common ⇒ __printf
  [Calls]
  - >> __printf
  [Called By]
  - >> _printf_char_file

  __user_setup_stackheap (Thumb, 74 bytes, Stack size 8 bytes, sys_stackheap_outer.o(.text))
  [Stack]

  - Max Depth = 8 + Unknown Stack Size
  - Call Chain = __user_setup_stackheap
  [Calls]
  - >> __user_perproc_libspace
  - >> __user_initial_stackheap
  [Called By]
  - >> __rt_entry_sh

  exit (Thumb, 18 bytes, Stack size 8 bytes, exit.o(.text))
  [Stack]

  - Max Depth = 8 + Unknown Stack Size
  - Call Chain = exit
  [Calls]
  - >> __rt_exit
  [Called By]
  - >> __rt_entry_main

  __user_libspace (Thumb, 8 bytes, Stack size 0 bytes, libspace.o(.text), UNUSED)

  __user_perproc_libspace (Thumb, 0 bytes, Stack size 0 bytes, libspace.o(.text))
  [Called By]

  - >> __user_setup_stackheap

  __user_perthread_libspace (Thumb, 0 bytes, Stack size 0 bytes, libspace.o(.text), UNUSED)

  _sys_exit (Thumb, 8 bytes, Stack size 0 bytes, sys_exit.o(.text))
  [Called By]

  - >> __rt_exit_exit

  __I$use$semihosting (Thumb, 0 bytes, Stack size 0 bytes, use_no_semi.o(.text), UNUSED)

  __use_no_semihosting_swi (Thumb, 2 bytes, Stack size 0 bytes, use_no_semi.o(.text), UNUSED)

  __semihosting_library_function (Thumb, 0 bytes, Stack size unknown bytes, indicate_semi.o(.text), UNUSED)

  Led_ctor (Thumb, 312 bytes, Stack size 16 bytes, led.o(i.Led_ctor))
  [Stack]

  - Max Depth = 144 + Unknown Stack Size
  - Call Chain = Led_ctor ⇒ __2printf ⇒ _printf_char_file ⇒ _printf_char_common ⇒ __printf
  [Calls]
  - >> __2printf
  [Called By]
  - >> PowerLed_ctor
  - >> MedicalLed_ctor
  - >> main

  MedicalLed_computeEfficiency (Thumb, 58 bytes, Stack size 32 bytes, medicalled.o(i.MedicalLed_computeEfficiency))
  [Stack]

  - Max Depth = 160 + Unknown Stack Size
  - Call Chain = MedicalLed_computeEfficiency ⇒ __2printf ⇒ _printf_char_file ⇒ _printf_char_common ⇒ __printf
  [Calls]
  - >> __2printf
  [Address Reference Count : 1]
  - medicalled.o(.constdata)

  MedicalLed_ctor (Thumb, 32 bytes, Stack size 24 bytes, medicalled.o(i.MedicalLed_ctor))
  [Stack]

  - Max Depth = 168 + Unknown Stack Size
  - Call Chain = MedicalLed_ctor ⇒ Led_ctor ⇒ __2printf ⇒ _printf_char_file ⇒ _printf_char_common ⇒ __printf
  [Calls]
  - >> Led_ctor
  [Called By]
  - >> main

  MedicalLed_runDiagnostics (Thumb, 24 bytes, Stack size 16 bytes, medicalled.o(i.MedicalLed_runDiagnostics))
  [Stack]

  - Max Depth = 144 + Unknown Stack Size
  - Call Chain = MedicalLed_runDiagnostics ⇒ __2printf ⇒ _printf_char_file ⇒ _printf_char_common ⇒ __printf
  [Calls]
  - >> __2printf
  [Address Reference Count : 1]
  - medicalled.o(.constdata)

  PowerLed_computeEfficiency (Thumb, 40 bytes, Stack size 24 bytes, powerled.o(i.PowerLed_computeEfficiency))
  [Stack]

  - Max Depth = 152 + Unknown Stack Size
  - Call Chain = PowerLed_computeEfficiency ⇒ __2printf ⇒ _printf_char_file ⇒ _printf_char_common ⇒ __printf
  [Calls]
  - >> __2printf
  [Address Reference Count : 1]
  - powerled.o(.constdata)

  PowerLed_ctor (Thumb, 44 bytes, Stack size 32 bytes, powerled.o(i.PowerLed_ctor))
  [Stack]

  - Max Depth = 176 + Unknown Stack Size
  - Call Chain = PowerLed_ctor ⇒ Led_ctor ⇒ __2printf ⇒ _printf_char_file ⇒ _printf_char_common ⇒ __printf
  [Calls]
  - >> Led_ctor
  [Called By]
  - >> main

  PowerLed_runDiagnostics (Thumb, 26 bytes, Stack size 16 bytes, powerled.o(i.PowerLed_runDiagnostics))
  [Stack]

  - Max Depth = 144 + Unknown Stack Size
  - Call Chain = PowerLed_runDiagnostics ⇒ __2printf ⇒ _printf_char_file ⇒ _printf_char_common ⇒ __printf
  [Calls]
  - >> __2printf
  [Address Reference Count : 1]
  - powerled.o(.constdata)

  SystemInit (Thumb, 82 bytes, Stack size 0 bytes, system_stm32f4xx.o(i.SystemInit))
  [Address Reference Count : 1]

  - startup_stm32f411xe.o(.text)

  USART2_Init (Thumb, 112 bytes, Stack size 0 bytes, uart.o(i.USART2_Init))
  [Called By]

  - >> main

  USART2_write (Thumb, 24 bytes, Stack size 0 bytes, uart.o(i.USART2_write))
  [Called By]

  - >> fputc

  computeLedEffs (Thumb, 32 bytes, Stack size 16 bytes, led.o(i.computeLedEffs))
  [Stack]

  - Max Depth = 16
  - Call Chain = computeLedEffs
  [Called By]
  - >> main

  fputc (Thumb, 14 bytes, Stack size 8 bytes, uart.o(i.fputc))
  [Stack]

  - Max Depth = 8
  - Call Chain = fputc
  [Calls]
  - >> USART2_write
  [Address Reference Count : 1]
  - _printf_char_file.o(.text)

  main (Thumb, 94 bytes, Stack size 56 bytes, main.o(i.main))
  [Stack]

  - Max Depth = 232 + Unknown Stack Size
  - Call Chain = main ⇒ PowerLed_ctor ⇒ Led_ctor ⇒ __2printf ⇒ _printf_char_file ⇒ _printf_char_common ⇒ __printf
  [Calls]
  - >> computeLedEffs
  - >> USART2_Init
  - >> PowerLed_ctor
  - >> MedicalLed_ctor
  - >> Led_ctor
  [Called By]
  - >> __rt_entry_main

  _fp_init (Thumb, 10 bytes, Stack size 0 bytes, fpinit.o(x$fpl$fpinit))
  [Called By]

  - >> __rt_lib_init_fp_1

  __fplib_config_fpu_vfp (Thumb, 0 bytes, Stack size unknown bytes, fpinit.o(x$fpl$fpinit), UNUSED)

  __fplib_config_pureend_doubles (Thumb, 0 bytes, Stack size unknown bytes, fpinit.o(x$fpl$fpinit), UNUSED)

  ### Local Symbols

  compute_efficiency (Thumb, 6 bytes, Stack size 0 bytes, led.o(i.compute_efficiency))
  [Address Reference Count : 1]

  - led.o(.constdata)

  run_diagnostics (Thumb, 2 bytes, Stack size 0 bytes, led.o(i.run_diagnostics))
  [Address Reference Count : 1]

  - led.o(.constdata)

  _printf_input_char (Thumb, 10 bytes, Stack size 0 bytes, _printf_char_common.o(.text))
  [Address Reference Count : 1]

  - _printf_char_common.o(.text)

  ### Undefined Global Symbols