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Model name: FFS PipeSch40x8.0-cpfV2
Current Configuration: Default

	Solid Bodies

	Document Name and Reference
	Treated As
	Volumetric Properties
	Document Path/Date Modified

	Mirror1
[image: ]
	Solid Body
	Mass:8.56675 kg
Volume:0.00317287 m^3
Density:2700 kg/m^3
Weight:83.9541 N

	X:\CPF\Mechanical Engr\Farley\CPF2015Feb03\FFS PipeSch40x8.0-cpfV2.SLDPRT
May 12 13:58:25 2015
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	Study name
	12May2015 7 Ring - 3in - 8-375 Dia Buckling

	Analysis type
	Buckling

	Mesh type
	Solid Mesh

	Number of modes
	1

	Solver type
	Direct sparse solver

	Incompatible bonding options
	Automatic

	Thermal Effect: 
	On

	Thermal option
	Include temperature loads

	Zero strain temperature
	298 Kelvin

	Include fluid pressure effects from SOLIDWORKS Flow Simulation
	Off

	Soft Spring: 
	On

	Result folder
	SOLIDWORKS document (X:\CPF\Mechanical Engr\Farley\CPF2015Feb03)
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	Unit system:
	SI (MKS)

	Length/Displacement
	mm

	Temperature
	Kelvin

	Angular velocity
	Rad/sec

	Pressure/Stress
	N/m^2
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	Model Reference
	Properties
	Components
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		Name:
	6061-T6 (SS)

	Model type:
	Linear Elastic Isotropic

	Default failure criterion:
	Unknown

	Yield strength:
	2.75e+008 N/m^2

	Tensile strength:
	3.1e+008 N/m^2

	Mass density:
	2700 kg/m^3

	Elastic modulus:
	6.9e+010 N/m^2

	Poisson's ratio:
	0.33  

	Thermal expansion coefficient:
	2.4e-005 /Kelvin



	SolidBody 1(Mirror1)(FFS PipeSch40x8.0-cpfV2)

	Curve Data:N/A
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	Fixture name
	Fixture Image
	Fixture Details

	On Cylindrical Faces-1
	[image: ]
		Entities:
	2 face(s)

	Type:
	On Cylindrical Faces

	Translation:
	-0.002, ---, ---

	Units:
	in




	On Flat Faces-1
	[image: ]
		Entities:
	1 face(s)

	Type:
	On Flat Faces

	Translation:
	0, ---, ---

	Units:
	in






	Load name
	Load Image
	Load Details

	Force-1
	[image: ]
		Entities:
	2 face(s)

	Type:
	Apply normal force

	Value:
	23289 lbf




	Force-2
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		Entities:
	2 face(s)

	Type:
	Apply normal force

	Value:
	20531 lbf




	Pressure-1
	[image: ]
		Entities:
	33 face(s)

	Type:
	Normal to selected face

	Value:
	750

	Units:
	psi

	Phase Angle:
	0

	Units:
	deg
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	Mesh type
	Solid Mesh

	Mesher Used: 
	Curvature based mesh

	Jacobian points
	4 Points

	Maximum element size
	0.856957 in

	Minimum element size
	0.171391 in

	Mesh Quality
	High



Mesh information - Details
	Total Nodes
	47408

	Total Elements
	23865

	Maximum Aspect Ratio
	660.87

	% of elements with Aspect Ratio < 3
	26.4

	% of elements with Aspect Ratio > 10
	24.2

	% of distorted elements(Jacobian)
	0

	Time to complete mesh(hh;mm;ss): 
	00:00:07

	Computer name: 
	ENIGMA
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	Name
	Type
	Min
	Max

	Amplitude1
	AMPRES: Resultant Amplitude Plot for Mode Shape: 1(Load Factor = 1.37854)
	5.21647e-008 
Node: 8220
	0.000245765 
Node: 18428
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FFS PipeSch40x8.0-cpfV2-12May2015 7 Ring - 3in - 8-375 Dia Buckling-Amplitude-Amplitude1



Mode List
	Mode Number
	Load Factor

	1
	1.3785
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Model name:FFS PipeSchd0c.0-cpv2
Study name:12May2015 7 Ring - 3n - 8-375 Dia Buckling(-Default)
Mesh type: Solid Mesh
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Model name:FFS PipeSchd0c.0-cpv2
Study name:12May2015 7 Ring - 3in - 8-375 Dia Buckling(-Default)
Plot type: Buckling Amplitudel

Mo Shape : 1 Load Factor

Deformation scale: 50
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