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Model name: FFS topFlange-cpfV2
Current Configuration: Default

	Solid Bodies

	Document Name and Reference
	Treated As
	Volumetric Properties
	Document Path/Date Modified

	Split Line6
[image: ]
	Solid Body
	Mass:3.53825 lb
Volume:36.2735 in^3
Density:0.0975437 lb/in^3
Weight:3.53585 lbf

	X:\CPF\Mechanical Engr\Farley\CPF2015Feb03\FFS topFlange-cpfV2.SLDPRT
Apr 08 16:03:13 2015
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	Study name
	30Mar2015 Top Flange Cap with Holes Static Study 2

	Analysis type
	Static

	Mesh type
	Solid Mesh

	Thermal Effect: 
	On

	Thermal option
	Include temperature loads

	Zero strain temperature
	77 Fahrenheit

	Include fluid pressure effects from SolidWorks Flow Simulation
	Off

	Solver type
	FFEPlus

	Inplane Effect: 
	Off

	Soft Spring: 
	Off

	Inertial Relief: 
	Off

	Incompatible bonding options
	Automatic

	Large displacement
	On

	Compute free body forces
	On

	Friction
	Off

	Use Adaptive Method: 
	Off

	Result folder
	SolidWorks document (X:\CPF\Mechanical Engr\Farley\CPF2015Feb03)
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	Unit system:
	English (IPS)

	Length/Displacement
	in

	Temperature
	Fahrenheit

	Angular velocity
	Hertz

	Pressure/Stress
	psi
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	Model Reference
	Properties
	Components
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		Name:
	6061-T6 (SS)

	Model type:
	Linear Elastic Isotropic

	Default failure criterion:
	Unknown

	Yield strength:
	39885.4 psi

	Tensile strength:
	44961.7 psi

	Elastic modulus:
	1.00076e+007 psi

	Poisson's ratio:
	0.33  

	Mass density:
	0.0975437 lb/in^3

	Shear modulus:
	3.77098e+006 psi

	Thermal expansion coefficient:
	1.33333e-005 /Fahrenheit



	SolidBody 1(9/32 (Split Line6)(FFS topFlange-cpfV2)

	Curve Data:N/A
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	Fixture name
	Fixture Image
	Fixture Details

	Fixed-1
	[image: ]
		Entities:
	5 face(s)

	Type:
	Fixed Geometry




	Resultant Forces
	Components
	X
	Y
	Z
	Resultant

	Reaction force(lbf)
	0.00500826
	35067.5
	-0.00366872
	35067.5

	Reaction Moment(lbf.in)
	0
	0
	0
	0


 



	Load name
	Load Image
	Load Details

	Pressure-1
	[image: ]
		Entities:
	13 face(s)

	Type:
	Normal to selected face

	Value:
	750

	Units:
	psi

	Phase Angle:
	0

	Units:
	deg
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	Mesh type
	Solid Mesh

	Mesher Used: 
	Curvature based mesh

	Jacobian points
	16 Points

	Maximum element size
	0.1 in

	Minimum element size
	0.02 in

	Mesh Quality
	Draft Quality Mesh



Mesh Information - Details
	Total Nodes
	159100

	Total Elements
	778086

	Maximum Aspect Ratio
	213.71

	% of elements with Aspect Ratio < 3
	96

	% of elements with Aspect Ratio > 10
	0.536

	Time to complete mesh(hh;mm;ss): 
	00:01:23

	Computer name: 
	ENIGMA
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Mesh Control Information:
	Mesh Control Name
	Mesh Control Image
	Mesh Control Details

	Control-1
	[image: ]
		Entities:
	11 face(s)

	Units:
	in

	Size:
	0.0827772

	Ratio:
	1.5




	Control-7
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		Entities:
	3 face(s)

	Units:
	in

	Size:
	0.05

	Ratio:
	1.5




	Control-8
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		Entities:
	67 face(s)

	Units:
	in

	Size:
	0.09

	Ratio:
	1.5
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Reaction Forces
	Selection set
	Units
	Sum X
	Sum Y
	Sum Z
	Resultant

	Entire Model
	lbf
	0.00500826
	35067.5
	-0.00366872
	35067.5


Reaction Moments
	Selection set
	Units
	Sum X
	Sum Y
	Sum Z
	Resultant

	Entire Model
	lbf.in
	0
	0
	0
	0
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	Name
	Type
	Min
	Max

	Stress1
	VON: von Mises Stress
	180.392 psi
Node: 35361
	391980 psi
Node: 15736
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FFS topFlange-cpfV2-30Mar2015 Top Flange Cap with Holes Static Study 2-Stress-Stress1



	Name
	Type
	Min
	Max

	Displacement1
	URES: Resultant Displacement
	0 in
Node: 15579
	0.11256 in
Node: 690
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FFS topFlange-cpfV2-30Mar2015 Top Flange Cap with Holes Static Study 2-Displacement-Displacement1



	Name
	Type
	Min
	Max

	Strain1
	ESTRN: Equivalent Strain
	1.18094e-005 
Element: 570480
	0.0413941 
Element: 289127
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FFS topFlange-cpfV2-30Mar2015 Top Flange Cap with Holes Static Study 2-Strain-Strain1



	Name
	Type

	Displacement1{1}
	Deformed Shape
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FFS topFlange-cpfV2-30Mar2015 Top Flange Cap with Holes Static Study 2-Displacement-Displacement1{1}



	Name
	Type
	Min
	Max

	Factor of Safety1
	Automatic
	0.101754 
Node: 15736
	1.25 
Node: 1
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FFS topFlange-cpfV2-30Mar2015 Top Flange Cap with Holes Static Study 2-Factor of Safety-Factor of Safety1
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	Top VIew Stress 1


	Image Comments:

	Orange and Red are High Stress Areas
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	Bottom View Stress 2


	Image Comments:

	Orange and Red are High Stress Areas
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Back View of Top Flange Cap
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