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Model name: housingBase-cpfV2
Current Configuration: withBellows

	Solid Bodies

	Document Name and Reference
	Treated As
	Volumetric Properties
	Document Path/Date Modified

	Boss-Extrude1
[image: ]
	Solid Body
	Mass:1.57435 kg
Volume:0.000583093 m^3
Density:2700 kg/m^3
Weight:15.4286 N

	X:\CPF\Mechanical Engr\Farley\CPF2015Feb03\housingBase-cpfV2.SLDPRT
Jun 11 13:50:30 2015
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	Study name
	11June2015 housingBase-cpfV2 Static 1

	Analysis type
	Static

	Mesh type
	Solid Mesh

	Thermal Effect: 
	On

	Thermal option
	Include temperature loads

	Zero strain temperature
	298 Kelvin

	Include fluid pressure effects from SOLIDWORKS Flow Simulation
	Off

	Solver type
	FFEPlus

	Inplane Effect: 
	Off

	Soft Spring: 
	On

	Inertial Relief: 
	Off

	Incompatible bonding options
	Automatic

	Large displacement
	Off

	Compute free body forces
	On

	Friction
	Off

	Use Adaptive Method: 
	Off

	Result folder
	SOLIDWORKS document (X:\CPF\Mechanical Engr\Farley\CPF2015Feb03)
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	Unit system:
	SI (MKS)

	Length/Displacement
	mm

	Temperature
	Kelvin

	Angular velocity
	Rad/sec

	Pressure/Stress
	N/m^2
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	Model Reference
	Properties
	Components
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		Name:
	6061-T6 (SS)

	Model type:
	Linear Elastic Isotropic

	Default failure criterion:
	Unknown

	Yield strength:
	2.75e+008 N/m^2

	Tensile strength:
	3.1e+008 N/m^2

	Elastic modulus:
	6.9e+010 N/m^2

	Poisson's ratio:
	0.33  

	Mass density:
	2700 kg/m^3

	Shear modulus:
	2.6e+010 N/m^2

	Thermal expansion coefficient:
	2.4e-005 /Kelvin



	SolidBody 1(Boss-Extrude1)(housingBase-cpfV2)

	Curve Data:N/A
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	Fixture name
	Fixture Image
	Fixture Details

	Fixed-1
	[image: ]
		Entities:
	1 edge(s)

	Type:
	Fixed Geometry




	Resultant Forces
	Components
	X
	Y
	Z
	Resultant

	Reaction force(N)
	0.598572
	-152126
	8.61084
	152126

	Reaction Moment(N.m)
	0
	0
	0
	0


 



	Load name
	Load Image
	Load Details

	Pressure-1
	[image: ]
		Entities:
	14 face(s)

	Type:
	Normal to selected face

	Value:
	750

	Units:
	psi

	Phase Angle:
	0

	Units:
	deg
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	Mesh type
	Solid Mesh

	Mesher Used: 
	Standard mesh

	Automatic Transition: 
	Off

	Include Mesh Auto Loops: 
	Off

	Jacobian points
	4 Points

	Element Size
	0.2 in

	Tolerance
	0.01 in

	Mesh Quality
	High



Mesh information - Details
	Total Nodes
	56482

	Total Elements
	36209

	Maximum Aspect Ratio
	13.9

	% of elements with Aspect Ratio < 3
	95.5

	% of elements with Aspect Ratio > 10
	0.102

	% of distorted elements(Jacobian)
	0

	Time to complete mesh(hh;mm;ss): 
	00:00:07

	Computer name: 
	ENIGMA
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Reaction forces
	Selection set
	Units
	Sum X
	Sum Y
	Sum Z
	Resultant

	Entire Model
	N
	0.598572
	-152126
	8.61084
	152126


Reaction Moments
	Selection set
	Units
	Sum X
	Sum Y
	Sum Z
	Resultant

	Entire Model
	N.m
	0
	0
	0
	0
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	Name
	Type
	Min
	Max

	Stress1
	VON: von Mises Stress
	59.4122 psi
Node: 39423
	44530.4 psi
Node: 7

	[image: ]
housingBase-cpfV2-11June2015 housingBase-cpfV2 Static 1-Stress-Stress1



	Name
	Type
	Min
	Max

	Displacement1
	URES:   Resultant Displacement
	0 mm
Node: 253
	0.632832 mm
Node: 26587
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housingBase-cpfV2-11June2015 housingBase-cpfV2 Static 1-Displacement-Displacement1



	Name
	Type
	Min
	Max

	Strain1
	ESTRN: Equivalent Strain
	1.56989e-005 
Element: 13655
	0.00335553 
Element: 8597
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housingBase-cpfV2-11June2015 housingBase-cpfV2 Static 1-Strain-Strain1



	Name
	Type
	Min
	Max

	Factor of Safety1
	Automatic
	0.895688 
Node: 7
	5 
Node: 23
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housingBase-cpfV2-11June2015 housingBase-cpfV2 Static 1-Factor of Safety-Factor of Safety1
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