# gsw_cp_ice

    isobaric heat capacity of ice

## Contents

- USAGE:
- DESCRIPTION:
- INPUT:
- OUTPUT:
- EXAMPLE:
- AUTHOR:
- VERSION NUMBER:
- REFERENCES:

## USAGE:

    cp_ice = gsw_cp_ice(t,p)

## DESCRIPTION:

    Calculates the isobaric heat capacity of ice.

## INPUT:

    t    =   in-situ temperature (ITS-90)                          [ deg C ]
    p    =   sea pressure                                           [ dbar ]
            ( ie. absolute pressure - 10.1325 dbar )

    p may have dimensions 1x1 or Mx1 or 1xN or MxN, where t is MxN.

## OUTPUT:

    cp_ice   =   heat capacity of ice                           [ J/(kg*K) ]

## EXAMPLE:

    t = [-10.7856; -13.4329; -12.8103; -12.2600;  -10.8863;  -8.4036;]
    p = [      10;       50;      125;      250;       600;     1000;]

    cp_ice = gsw_cp_ice(t,p)

    cp_ice =

      1.0e+003 *

       2.017314262094657
       1.997830122682709
       2.002281331375396
       2.006127319545421
       2.015676303959609
       2.033308170371559

## AUTHOR:

    Trevor McDougall and Paul Barker        [ help@teos-10.org ]

## VERSION NUMBER:

    3.05 (16th February, 2015)

## REFERENCES:

    IOC, SCOR and IAPSO, 2010: The international thermodynamic equation of
     seawater - 2010: Calculation and use of thermodynamic properties.
     Intergovernmental Oceanographic Commission, Manuals and Guides No. 56,
     UNESCO (English), 196 pp.  Available from the TEOS-10 web site.

    The software is available from http://www.TEOS-10.org