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1.0 Software
1.1 Make sure stuff used in tank testing is changed for deployment
1.1.1 Program.cs
1.1.1.1 Set initial state at top of State Machine while loop
1.1.1.2 uBlox.Request fix number of tries and time delay in SurfaceOps
1.1.2 configFile.cs
1.1.2.1 Set appropriate preMissionDelayTimeout
1.1.2.2 Set appropriate SurfaceOpsTimeout
1.1.2.3 Uncomment SOSetBellowsPosition to correct value
1.1.3 Clear all breakpoints
1.1.4 Comment out debug statements
1.2 Mission Config
1.2.1 Make sure last ascend has 0.0 depth
1.2.2 usbCable = false
1.2.3 Set SBE41 pump time
1.2.4 Set SBE41 cpCutoff pressure
1.3 Set SORecoveryMode as appropriate
2.0 Balllast so mark on antenna stem is at waterline with bellows at SOSetBellowsPosition
3.0 Remove eye bolts as necessary
4.0 Remove Optode rubber cover
5.0 Remove CTD caps
6.0 Check tension screw cover is tight
7.0 Check Swagelok fitting is tight
8.0 Check tapered ring/bellows cover are screwed together tightly
9.0 Check lifting plate is secured properly
10.0 [bookmark: _GoBack]Check Optode and CTD settings are correct
