[bookmark: _GoBack]Here we present the initial work that has been done to develop a biogeochemical profiling float optimized to operate over on the continental shelf and upper slope.  The continental shelves and slopes comprise only 5 to 10 % of the ocean, but they contribute half of the global new primary production (Benway et al., 2015).  Variability in this new primary production can be a major control on air-sea CO2 flux (Evans et al., 2015).  The disproportionately high new primary production in coastal systems supports the vast majority of global fish production (Ryther, 1969), which may be significantly impacted by future climate change (Brander, 2007). As a result, one of the key recommendations in the Coastal Carbon Synthesis Science Plan For Carbon Cycle Research In North American Coastal Waters (Benway et al., 2016) is “Further development of event-scale observing capacity (e.g., novel autonomous platforms) in all continental margin systems to better quantify impacts of episodic events on coastal carbon budgets”.  The Coastal Profiling Float (CPF) targets this recommendation with the specific goal of supporting coastal zone ecosystem observing missions using a large array of CPFs over spatial scales from 10s to 1000s of kilometers and time scales on the order of years at an economically sustainable cost.  Results from pilot science missions will be presented in this talk. The CPF carries a suite of biogeochemical instruments (CTD, Oxygen, pH, Nitrate, Optical Radiometer, Fluorometer and Backscatter) and can follow a user specified depth and sampling profile from 500 meters deep to the surface including the capability to park on the seabed or at a user specified depth.  The results of each CPF profile are transmitted back to shore in near real time using the Iridium satellite network.  New missions can also be downloaded to the CPF from shore.  Working in the coastal zone presents a variety of challenges that drove the need for significantly better buoyancy control in the CPF.  The CPF buoyancy engine can change its displacement by 3.5 liters allowing it to anchor (and more importantly de-anchor) on the seabed and profile through pycnoclines from almost any ocean density through freshwater.  The large volume control allows for profiling velocities in excess of 50 cm/sec and minimizes the need for precise ballasting. In addition, the CPF supports user defined profile trajectories requiring precise depth and velocity control with minimal depth overshoot enabling missions in a few 10s of meters of water depth.  The current CPF design is relatively configurable and we have run missions with a variety of other instruments including a large sediment trap. We have also run science missions in non-coastal waters where the CPF performs as a Lagrangian drifter at depths up to 500 meters. In addition, the CPF has the potential to operate in Arctic waters where large density gradients require the large volume change capability of the CPF buoyancy engine. 

