CPF Production Checkout Form
Revision 2.0

[bookmark: CPFSN]Unit SN: 

2019 MBARI CPF Project 901206


Installation
LHE (SN:      )
[bookmark: Check1]|_|  6 Batteries Installed
|_|  SB1-10 unconnected
|_|  JP1 removed for Sleep enabled
|_|  JP2-3 2-2 for logic control
|_|  Fuses installed (3 places)

Motherboard (SN:      )
|_|  SD Card Inserted (Size:      )
|_|  JP1, JP2 Removed (LED Disable)
|_|  JP3 MODE wired for USB MODE
|_|  USB client harness installed
	
Daughtercards
|_|  SN2 in SLOT-1 (SN:      )
|_|  SN1 in SLOT-2 (SN:      )
|_|  SN3 in SLOT-3 (SN:      )
|_|  BTB on mount: Configured for RS232, LED resistors removed, 
(SN:      )
|_|  ISB in SLOT-6 (SN:      )

Upper Assembly Hardware
[bookmark: Text3]|_|  MSC/ISUS/DuraFet (SN’s:      )
|_|  SBE Board (SN:      )
|_|  GPS (SN:      )
|_|  Iridium Modem
	(SN:      )
	(IMEI:      )
	(SIM:      )
|_|  GPS/Iridium subsystem deck test

Lower Assembly Hardware
|_|  String pot & ADC (SN:      )
|_|  ELMO & Motor (SN:      )
|_|  Motorized Valve
	Arrow pointing toward pump
|_|  Bellows Plumbed

Wire Harness Check
[bookmark: _GoBack]|_|  WH-Battery Charger
|_|  WH-BT Console
|_|  WH-CTD Pwr/Comms
|_|  WH-FLBB
|_|  WH-GPS
|_|  WH-Iridium Comms
|_|  WH-LHE to MoBo Pwer/ISB
|_|  WH-Mot Valve
|_|  WH-MSC
|_|  WH-other msc 
|_|  WH-OCR504
|_|  WH-On/Off Switches
|_|  WH-Optode
|_|  WH-Pos Xducer
|_|  WH-PTH
|_|  WH-Pump Motor
|_|  WH-ucComms

Pre-oil Fill
|_|  Motherboard SW Checkout
|_|  Energy Monitor BATT
|_|  12V Control
|_|  5V Control

Sensor Functionality
|_|  SLOT1-J5 to SLOT5 BT Console PWR/TELEM
|_|  SLOT1-J2 CTD PWR/TELEM
|_|  SLOT1-J4 Pump PWR/TELEM
|_|  SLOT2-J2-J3 Iridium PWR/TELEM
|_|  SLOT2-J4 MSC PWR/TELEM
|_|  SLOT2-J5 Optode PWR/TELEM (SN:      )
|_|  SLOT3-J4 OCR PWR/TELEM (SN:      )
|_|  SLOT3-J5 FLBB PWR/TELEM (SN:      )
|_|  SLOT6-J1 GPS PWR/TELEM (SN:      )
|_|  SLOT6-J2 Bellows Position PWR/TELEM
|_|  SLOT3-J6 Mot Valve PWR/DIO (SN:      )
|_|  SLOT6-J8 Attached

LHE
|_|  LHE Battery Polling
|_|  LHE Sleep Test
|_|  LHE Pump PWR/TELEM
|_|  LHE Pump Energy Monitor
|_|  Charging Cycle through Endcap

Calibrations
|_|  String Pot Calibration:
[bookmark: Text1][bookmark: Text2]	SLOPE:<slope> INTERCEPT:<intercept>
|_|  MSC Calibrations
|_|  Environmental Sensors on ISB

Closed Unit Deck Test
|_|  Iridium Deck Test
|_|  GPS Deck Test
|_|  Bluetooth Deck Test

Oil Filled
Benchtop
|_|  Fill Oil
|_|  Pump/Motor Calibration
|_|  Pump Bellows Cycling (10x)
|_|  Install desiccant packs
|_|  Close Unit
Tank Tests
Surface Operations
|_|  Bluetooth
|_|  Temperature & Humidity Good (<25%RH)
|_|  GPS [ATTEMPT]
|_|  IRIDIUM SBD [ATTEMPT]
|_|  IRIDIUM SBD [ATTEMPT]
Buoyancy Operations
|_|  Ballast Tests
|_|  SurfaceOps Bellows Position
|_|  Descent/Ascent
|_|  Velocity Control
|_|  Depth Holding
|_|  Profile Control
|_|  Sampling Profile

Configuration File Options
TBD


